type rlsservice, domain;
type rlsservice_exec, exec_type, vendor_file_type, file_type;

init_daemon_domain(rlsservice)
vndbinder_use(rlsservice)
add_service(rlsservice, rls_service)


# access rainbow sensor calibration files
allow rlsservice persist_file:dir search;
allow rlsservice persist_camera_file:dir search;
allow rlsservice persist_camera_file:file r_file_perms;
allow rlsservice mnt_vendor_file:dir search;

# access device files
allow rlsservice rls_device:chr_file rw_file_perms;

binder_call(rlsservice, hal_camera_default)
binder_call(rlsservice, servicemanager)


# Allow access to display backlight information
allow rlsservice sysfs_leds:dir search;
allow rlsservice sysfs_leds:file r_file_perms;

# Allow access to always-on compute device node
allow rlsservice device:dir r_file_perms;
allow rlsservice aoc_device:chr_file rw_file_perms;

# For observing apex file changes
allow rlsservice apex_info_file:file r_file_perms;

# Allow read camera property
get_prop(rlsservice, vendor_camera_prop);

# Allow rlsservice bugreport generation
allow rlsservice dumpstate:fd use;
allow rlsservice dumpstate:fifo_file write;