&soc {
	tlmm: pinctrl@3100000 {
		compatible = "qcom,sm8150-pinctrl";
		reg = <0x03100000 0x300000>,
		      <0x03500000 0x300000>,
		      <0x03900000 0x300000>,
		      <0x03D00000 0x300000>;
		reg-names = "west", "east", "north", "south";
		interrupts = <GIC_SPI 208 IRQ_TYPE_LEVEL_HIGH>;
		gpio-ranges = <&tlmm 0 0 176>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
		wakeup-parent = <&pdc>;

		ufs_dev_reset_assert: ufs_dev_reset_assert {
			config {
				pins = "ufs_reset";
				bias-pull-down;		/* default: pull down */
				/*
				 * UFS_RESET driver strengths are having
				 * different values/steps compared to typical
				 * GPIO drive strengths.
				 *
				 * Following table clarifies:
				 *
				 * HDRV value | UFS_RESET | Typical GPIO
				 *   (dec)    |   (mA)    |    (mA)
				 *     0      |   0.8     |    2
				 *     1      |   1.55    |    4
				 *     2      |   2.35    |    6
				 *     3      |   3.1     |    8
				 *     4      |   3.9     |    10
				 *     5      |   4.65    |    12
				 *     6      |   5.4     |    14
				 *     7      |   6.15    |    16
				 *
				 * POR value for UFS_RESET HDRV is 3 which means
				 * 3.1mA and we want to use that. Hence just
				 * specify 8mA to "drive-strength" binding and
				 * that should result into writing 3 to HDRV
				 * field.
				 */
				drive-strength = <8>;	/* default: 3.1 mA */
				output-low; /* active low reset */
			};
		};

		ufs_dev_reset_deassert: ufs_dev_reset_deassert {
			config {
				pins = "ufs_reset";
				bias-pull-down;		/* default: pull down */
				/*
				 * default: 3.1 mA
				 * check comments under ufs_dev_reset_assert
				 */
				drive-strength = <8>;
				output-high; /* active low reset */
			};
		};

		sdc2_on: sdc2_on {
			clk {
				pins = "sdc2_clk";
				bias-disable;		/* NO pull */
				drive-strength = <16>;	/* 16 MA */
			};

			cmd {
				pins = "sdc2_cmd";
				bias-pull-up;		/* pull up */
				drive-strength = <16>;	/* 16 MA */
			};

			data {
				pins = "sdc2_data";
				bias-pull-up;		/* pull up */
				drive-strength = <16>;	/* 16 MA */
			};

			sd-cd {
				pins = "gpio96";
				bias-pull-up;           /* pull up */
				drive-strength = <2>;   /* 2 MA */
			};
		};

		sdc2_off: sdc2_off {
			clk {
				pins = "sdc2_clk";
				bias-disable;		/* NO pull */
				drive-strength = <2>;	/* 2 MA */
			};

			cmd {
				pins = "sdc2_cmd";
				bias-pull-up;		/* pull up */
				drive-strength = <2>;	/* 2 MA */
			};

			data {
				pins = "sdc2_data";
				bias-pull-up;		/* pull up */
				drive-strength = <2>;	/* 2 MA */
			};

			sd-cd {
				pins = "gpio96";
				bias-pull-up;           /* pull up */
				drive-strength = <2>;   /* 2 MA */
			};
		};

		pmx_ts_active {
			ts_active: ts_active {
					mux {
						pins = "gpio122", "gpio54";
						function = "gpio";
					};

					config {
						pins = "gpio122", "gpio54";
						drive-strength = <8>;
						bias-pull-up;
					};
			};
		};

		pmx_ts_int_suspend {
			ts_int_suspend: ts_int_suspend {
				mux {
					pins = "gpio122";
					function = "gpio";
				};

				config {
					pins = "gpio122";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		pmx_ts_reset_suspend {
			ts_reset_suspend: ts_reset_suspend {
				mux {
					pins = "gpio54";
					function = "gpio";
				};

				config {
					pins = "gpio54";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		pcie0 {
			pcie0_clkreq_default: pcie0_clkreq_default {
				mux {
					pins = "gpio36";
					function = "pci_e0";
				};

				config {
					pins = "gpio36";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			pcie0_clkreq_sleep: pcie0_clkreq_sleep {
				mux {
					pins = "gpio36";
					function = "gpio";
				};

				config {
					pins = "gpio36";
					drive-strength = <2>;
					bias-pull-up;
					input-enable;
				};
			};

			pcie0_perst_default: pcie0_perst_default {
				mux {
					pins = "gpio35";
					function = "gpio";
				};

				config {
					pins = "gpio35";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			pcie0_wake_default: pcie0_wake_default {
				mux {
					pins = "gpio37";
					function = "gpio";
				};

				config {
					pins = "gpio37";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		pcie1 {
			pcie1_clkreq_default: pcie1_clkreq_default {
				mux {
					pins = "gpio103";
					function = "pci_e1";
				};

				config {
					pins = "gpio103";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			pcie1_perst_default: pcie1_perst_default {
				mux {
					pins = "gpio102";
					function = "gpio";
				};

				config {
					pins = "gpio102";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			pcie1_wake_default: pcie1_wake_default {
				mux {
					pins = "gpio104";
					function = "gpio";
				};

				config {
					pins = "gpio104";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		cnss_pins {
			cnss_wlan_en_active: cnss_wlan_en_active {
				mux {
					pins = "gpio169";
					function = "gpio";
				};

				config {
					pins = "gpio169";
					drive-strength = <16>;
					output-high;
					bias-pull-up;
				};
			};

			cnss_wlan_en_sleep: cnss_wlan_en_sleep {
				mux {
					pins = "gpio169";
					function = "gpio";
				};

				config {
					pins = "gpio169";
					drive-strength = <2>;
					output-low;
					bias-pull-down;
				};
			};
		};

		pcie_ep {
			pcie_ep_clkreq_default: pcie_ep_clkreq_default {
				mux {
					pins = "gpio103";
					function = "pci_e1";
				};

				config {
					pins = "gpio103";
					drive-strength = <2>;
					bias-disable;
				};
			};

			pcie_ep_perst_default: pcie_ep_perst_default {
				mux {
					pins = "gpio102";
					function = "gpio";
				};

				config {
					pins = "gpio102";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			pcie_ep_wake_default: pcie_ep_wake_default {
				mux {
					pins = "gpio104";
					function = "gpio";
				};

				config {
					pins = "gpio104";
					drive-strength = <2>;
					bias-disable;
				};
			};
		};

		wil6210_refclk3_en_pin: wil6210_refclk3_en_pin {
			mux {
				pins = "gpio87";
				function = "gpio";
			};

			config {
				pins = "gpio87";
				bias-pull-down;		/* PULL DOWN */
				drive-strength = <2>;	/* 2 MA */
			};
		};

		/* SE0 pin mappings */
		qupv3_se0_i2c_pins: qupv3_se0_i2c_pins {
			qupv3_se0_i2c_active: qupv3_se0_i2c_active {
				mux {
					pins = "gpio0", "gpio1";
					function = "qup0";
				};

				config {
					pins = "gpio0", "gpio1";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se0_i2c_sleep: qupv3_se0_i2c_sleep {
				mux {
					pins = "gpio0", "gpio1";
					function = "gpio";
				};

				config {
					pins = "gpio0", "gpio1";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se0_spi_pins: qupv3_se0_spi_pins {
			qupv3_se0_spi_active: qupv3_se0_spi_active {
				mux {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					function = "qup0";
				};

				config {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se0_spi_sleep: qupv3_se0_spi_sleep {
				mux {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					function = "gpio";
				};

				config {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 1 pin mappings */
		qupv3_se1_i2c_pins: qupv3_se1_i2c_pins {
			qupv3_se1_i2c_active: qupv3_se1_i2c_active {
				mux {
					pins = "gpio114", "gpio115";
					function = "qup1";
				};

				config {
					pins = "gpio114", "gpio115";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se1_i2c_sleep: qupv3_se1_i2c_sleep {
				mux {
					pins = "gpio114", "gpio115";
					function = "gpio";
				};

				config {
					pins = "gpio114", "gpio115";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se1_spi_pins: qupv3_se1_spi_pins {
			qupv3_se1_spi_active: qupv3_se1_spi_active {
				mux {
					pins = "gpio114", "gpio115", "gpio116",
								"gpio117";
					function = "qup1";
				};

				config {
					pins = "gpio114", "gpio115", "gpio116",
								"gpio117";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se1_spi_sleep: qupv3_se1_spi_sleep {
				mux {
					pins = "gpio114", "gpio115", "gpio116",
								"gpio117";
					function = "gpio";
				};

				config {
					pins = "gpio114", "gpio115", "gpio116",
								"gpio117";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 2 pin mappings */
		qupv3_se2_i2c_pins: qupv3_se2_i2c_pins {
			qupv3_se2_i2c_active: qupv3_se2_i2c_active {
				mux {
					pins = "gpio126", "gpio127";
					function = "qup2";
				};

				config {
					pins = "gpio126", "gpio127";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se2_i2c_sleep: qupv3_se2_i2c_sleep {
				mux {
					pins = "gpio126", "gpio127";
					function = "gpio";
				};

				config {
					pins = "gpio126", "gpio127";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se2_spi_pins: qupv3_se2_spi_pins {
			qupv3_se2_spi_active: qupv3_se2_spi_active {
				mux {
					pins = "gpio126", "gpio127", "gpio128",
								"gpio129";
					function = "qup2";
				};

				config {
					pins = "gpio126", "gpio127", "gpio128",
								"gpio129";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se2_spi_sleep: qupv3_se2_spi_sleep {
				mux {
					pins = "gpio126", "gpio127", "gpio128",
								"gpio129";
					function = "gpio";
				};

				config {
					pins = "gpio126", "gpio127", "gpio128",
								"gpio129";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 3 pin mappings */
		qupv3_se3_i2c_pins: qupv3_se3_i2c_pins {
			qupv3_se3_i2c_active: qupv3_se3_i2c_active {
				mux {
					pins = "gpio144", "gpio145";
					function = "qup3";
				};

				config {
					pins = "gpio144", "gpio145";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se3_i2c_sleep: qupv3_se3_i2c_sleep {
				mux {
					pins = "gpio144", "gpio145";
					function = "gpio";
				};

				config {
					pins = "gpio144", "gpio145";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se3_spi_pins: qupv3_se3_spi_pins {
			qupv3_se3_spi_active: qupv3_se3_spi_active {
				mux {
					pins = "gpio144", "gpio145", "gpio146",
								"gpio147";
					function = "qup3";
				};

				config {
					pins = "gpio144", "gpio145", "gpio146",
								"gpio147";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se3_spi_sleep: qupv3_se3_spi_sleep {
				mux {
					pins = "gpio145", "gpio146", "gpio147";
					function = "qup3";
				};

				config {
					pins = "gpio145", "gpio146", "gpio147";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se3_spi_miso_sleep: qupv3_se3_spi_miso_sleep {
				mux {
					pins = "gpio144";
					function = "qup3";
				};

				config {
					pins = "gpio144";
					drive-strength = <6>;
					bias-pull-down; /* pull down */
				};
			};
		};

		ss5_pwr_ctrl_pins: ss5_pwr_ctrl_pins {
			ss5_pwr_ctrl_rst_on: ss5_pwr_ctrl_rst_on {
				mux {
					pins = "gpio11", "gpio39", "gpio40";
					function = "gpio";
				};

				config {
					pins = "gpio11", "gpio39", "gpio40";
					drive-strength = <2>; /* 2 mA */
					bias-pull-up;
					output-high;
				};
			};

			ss5_pwr_ctrl_rst_off: ss5_pwr_ctrl_off {
				mux {
					pins = "gpio11", "gpio39", "gpio40";
					function = "gpio";
				};

				config {
					pins = "gpio11", "gpio39", "gpio40";
					drive-strength = <2>; /* 2 mA */
					bias-pull-down;
					output-low;
				};
			};
		};

		/* SE 4 pin mappings */
		qupv3_se4_i2c_pins: qupv3_se4_i2c_pins {
			qupv3_se4_i2c_active: qupv3_se4_i2c_active {
				mux {
					pins = "gpio51", "gpio52";
					function = "qup4";
				};

				config {
					pins = "gpio51", "gpio52";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se4_i2c_sleep: qupv3_se4_i2c_sleep {
				mux {
					pins = "gpio51", "gpio52";
					function = "gpio";
				};

				config {
					pins = "gpio51", "gpio52";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se4_spi_pins: qupv3_se4_spi_pins {
			qupv3_se4_spi_active: qupv3_se4_spi_active {
				mux {
					pins = "gpio51", "gpio52", "gpio53",
								"gpio54";
					function = "qup4";
				};

				config {
					pins = "gpio51", "gpio52", "gpio53",
								"gpio54";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se4_spi_sleep: qupv3_se4_spi_sleep {
				mux {
					pins = "gpio51", "gpio52", "gpio53",
								"gpio54";
					function = "gpio";
				};

				config {
					pins = "gpio51", "gpio52", "gpio53",
								"gpio54";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 5 pin mappings */
		qupv3_se5_i2c_pins: qupv3_se5_i2c_pins {
			qupv3_se5_i2c_active: qupv3_se5_i2c_active {
				mux {
					pins = "gpio121", "gpio122";
					function = "qup5";
				};

				config {
					pins = "gpio121", "gpio122";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se5_i2c_sleep: qupv3_se5_i2c_sleep {
				mux {
					pins = "gpio121", "gpio122";
					function = "gpio";
				};

				config {
					pins = "gpio121", "gpio122";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se5_spi_pins: qupv3_se5_spi_pins {
			qupv3_se5_spi_active: qupv3_se5_spi_active {
				mux {
					pins = "gpio119", "gpio120", "gpio121",
								"gpio122";
					function = "qup5";
				};

				config {
					pins = "gpio119", "gpio120", "gpio121",
								"gpio122";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se5_spi_sleep: qupv3_se5_spi_sleep {
				mux {
					pins = "gpio119", "gpio120", "gpio121",
								"gpio122";
					function = "gpio";
				};

				config {
					pins = "gpio119", "gpio120", "gpio121",
								"gpio122";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 6 pin mappings */
		qupv3_se6_i2c_pins: qupv3_se6_i2c_pins {
			qupv3_se6_i2c_active: qupv3_se6_i2c_active {
				mux {
					pins = "gpio6", "gpio7";
					function = "qup6";
				};

				config {
					pins = "gpio6", "gpio7";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se6_i2c_sleep: qupv3_se6_i2c_sleep {
				mux {
					pins = "gpio6", "gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio7";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se6_spi_pins: qupv3_se6_spi_pins {
			qupv3_se6_spi_active: qupv3_se6_spi_active {
				mux {
					pins = "gpio4", "gpio5", "gpio6",
								"gpio7";
					function = "qup6";
				};

				config {
					pins = "gpio4", "gpio5", "gpio6",
								"gpio7";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se6_spi_sleep: qupv3_se6_spi_sleep {
				mux {
					pins = "gpio4", "gpio5", "gpio6",
								"gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio4", "gpio5", "gpio6",
								"gpio7";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 7 pin mappings */
		qupv3_se7_i2c_pins: qupv3_se7_i2c_pins {
			qupv3_se7_i2c_active: qupv3_se7_i2c_active {
				mux {
					pins = "gpio98", "gpio99";
					function = "qup7";
				};

				config {
					pins = "gpio98", "gpio99";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se7_i2c_sleep: qupv3_se7_i2c_sleep {
				mux {
					pins = "gpio98", "gpio99";
					function = "gpio";
				};

				config {
					pins = "gpio98", "gpio99";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se7_spi_pins: qupv3_se7_spi_pins {
			qupv3_se7_spi_active: qupv3_se7_spi_active {
				mux {
					pins = "gpio98", "gpio99", "gpio100",
								"gpio101";
					function = "qup7";
				};

				config {
					pins = "gpio98", "gpio99", "gpio100",
								"gpio101";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se7_spi_sleep: qupv3_se7_spi_sleep {
				mux {
					pins = "gpio98", "gpio99", "gpio100",
								"gpio101";
					function = "gpio";
				};

				config {
					pins = "gpio98", "gpio99", "gpio100",
								"gpio101";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* QUPv3 North instances */
		/* SE 8 pin mappings */
		qupv3_se8_i2c_pins: qupv3_se8_i2c_pins {
			qupv3_se8_i2c_active: qupv3_se8_i2c_active {
				mux {
					pins = "gpio88", "gpio89";
					function = "qup8";
				};

				config {
					pins = "gpio88", "gpio89";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se8_i2c_sleep: qupv3_se8_i2c_sleep {
				mux {
					pins = "gpio88", "gpio89";
					function = "gpio";
				};

				config {
					pins = "gpio88", "gpio89";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se8_spi_pins: qupv3_se8_spi_pins {
			qupv3_se8_spi_active: qupv3_se8_spi_active {
				mux {
					pins = "gpio88", "gpio89", "gpio90",
								"gpio91";
					function = "qup8";
				};

				config {
					pins = "gpio88", "gpio89", "gpio90",
								"gpio91";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se8_spi_sleep: qupv3_se8_spi_sleep {
				mux {
					pins = "gpio88", "gpio89", "gpio90",
								"gpio91";
					function = "gpio";
				};

				config {
					pins = "gpio88", "gpio89", "gpio90",
								"gpio91";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 9 pin mappings */
		qupv3_se9_i2c_pins: qupv3_se9_i2c_pins {
			qupv3_se9_i2c_active: qupv3_se9_i2c_active {
				mux {
					pins = "gpio39", "gpio40";
					function = "qup9";
				};

				config {
					pins = "gpio39", "gpio40";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se9_i2c_sleep: qupv3_se9_i2c_sleep {
				mux {
					pins = "gpio39", "gpio40";
					function = "gpio";
				};

				config {
					pins = "gpio39", "gpio40";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se9_spi_pins: qupv3_se9_spi_pins {
			qupv3_se9_spi_active: qupv3_se9_spi_active {
				mux {
					pins = "gpio39", "gpio40", "gpio41",
								"gpio42";
					function = "qup9";
				};

				config {
					pins = "gpio39", "gpio40", "gpio41",
								"gpio42";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se9_spi_sleep: qupv3_se9_spi_sleep {
				mux {
					pins = "gpio39", "gpio40", "gpio41",
								"gpio42";
					function = "gpio";
				};

				config {
					pins = "gpio39", "gpio40", "gpio41",
								"gpio42";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se9_2uart_pins: qupv3_se9_2uart_pins {
			qupv3_se9_2uart_default: qupv3_se9_2uart_default {
				mux {
					pins = "gpio41", "gpio42";
					function = "gpio";
				};

				config {
					pins = "gpio41", "gpio42";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se9_2uart_active: qupv3_se9_2uart_active {
				mux {
					pins = "gpio41", "gpio42";
					function = "qup9";
				};

				config {
					pins = "gpio41", "gpio42";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se9_2uart_sleep: qupv3_se9_2uart_sleep {
				mux {
					pins = "gpio41", "gpio42";
					function = "gpio";
				};

				config {
					pins = "gpio41", "gpio42";
					drive-strength = <2>;
					bias-disable;
				};
			};
		};

		nfc {
			nfc_int_active: nfc_int_active {
				/* active state */
				mux {
					/* GPIO 47 NFC Read Interrupt */
					pins = "gpio47";
					function = "gpio";
				};

				config {
					pins = "gpio47";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_int_suspend: nfc_int_suspend {
				/* sleep state */
				mux {
					/* GPIO 47 NFC Read Interrupt */
					pins = "gpio47";
					function = "gpio";
				};

				config {
					pins = "gpio47";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_enable_active: nfc_enable_active {
				/* active state */
				mux {
					/* 41: NFC ENABLE 42:ESE Enable */
					pins = "gpio41", "gpio42", "gpio48";
					function = "gpio";
				};

				config {
					pins = "gpio41", "gpio42", "gpio48";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_enable_suspend: nfc_enable_suspend {
				/* sleep state */
				mux {
					/* 41: NFC ENABLE 42:ESE Enable */
					pins = "gpio41", "gpio42", "gpio48";
					function = "gpio";
				};

				config {
					pins = "gpio41", "gpio42", "gpio48";
					drive-strength = <2>; /* 2 MA */
					bias-disable;
				};
			};

			nfc_clk_req_active: nfc_clk_req_active {
				/* active state */
				mux {
					/* 113: NFC CLOCK REQUEST */
					pins = "gpio113";
					function = "gpio";
				};

				config {
					pins = "gpio113";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_clk_req_suspend: nfc_clk_req_suspend {
				/* sleep state */
				mux {
					/* 113: NFC CLOCK REQUEST */
					pins = "gpio113";
					function = "gpio";
				};

				config {
					pins = "gpio113";
					drive-strength = <2>; /* 2 MA */
					bias-disable;
				};
			};
		};

		/* SE 10 pin mappings */
		qupv3_se10_i2c_pins: qupv3_se10_i2c_pins {
			qupv3_se10_i2c_active: qupv3_se10_i2c_active {
				mux {
					pins = "gpio9", "gpio10";
					function = "qup10";
				};

				config {
					pins = "gpio9", "gpio10";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se10_i2c_sleep: qupv3_se10_i2c_sleep {
				mux {
					pins = "gpio9", "gpio10";
					function = "gpio";
				};

				config {
					pins = "gpio9", "gpio10";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se10_spi_pins: qupv3_se10_spi_pins {
			qupv3_se10_spi_active: qupv3_se10_spi_active {
				mux {
					pins = "gpio9", "gpio10", "gpio11",
								"gpio12";
					function = "qup10";
				};

				config {
					pins = "gpio9", "gpio10", "gpio11",
								"gpio12";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se10_spi_sleep: qupv3_se10_spi_sleep {
				mux {
					pins = "gpio9", "gpio10", "gpio11",
								"gpio12";
					function = "gpio";
				};

				config {
					pins = "gpio9", "gpio10", "gpio11",
								"gpio12";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 11 pin mappings */
		qupv3_se11_i2c_pins: qupv3_se11_i2c_pins {
			qupv3_se11_i2c_active: qupv3_se11_i2c_active {
				mux {
					pins = "gpio94", "gpio95";
					function = "qup11";
				};

				config {
					pins = "gpio94", "gpio95";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se11_i2c_sleep: qupv3_se11_i2c_sleep {
				mux {
					pins = "gpio94", "gpio95";
					function = "gpio";
				};

				config {
					pins = "gpio94", "gpio95";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se11_spi_pins: qupv3_se11_spi_pins {
			qupv3_se11_spi_active: qupv3_se11_spi_active {
				mux {
					pins = "gpio92", "gpio93", "gpio94",
								"gpio95";
					function = "qup11";
				};

				config {
					pins = "gpio92", "gpio93", "gpio94",
								"gpio95";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se11_spi_sleep: qupv3_se11_spi_sleep {
				mux {
					pins = "gpio92", "gpio93", "gpio94",
								"gpio95";
					function = "gpio";
				};

				config {
					pins = "gpio92", "gpio93", "gpio94",
								"gpio95";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 12 pin mappings */
		qupv3_se12_i2c_pins: qupv3_se12_i2c_pins {
			qupv3_se12_i2c_active: qupv3_se12_i2c_active {
				mux {
					pins = "gpio83", "gpio84";
					function = "qup12";
				};

				config {
					pins = "gpio83", "gpio84";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se12_i2c_sleep: qupv3_se12_i2c_sleep {
				mux {
					pins = "gpio83", "gpio84";
					function = "gpio";
				};

				config {
					pins = "gpio83", "gpio84";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se12_spi_pins: qupv3_se12_spi_pins {
			qupv3_se12_spi_active: qupv3_se12_spi_active {
				mux {
					pins = "gpio83", "gpio84", "gpio85",
								"gpio86";
					function = "qup12";
				};

				config {
					pins = "gpio83", "gpio84", "gpio85",
								"gpio86";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se12_spi_sleep: qupv3_se12_spi_sleep {
				mux {
					pins = "gpio83", "gpio84", "gpio85",
								"gpio86";
					function = "gpio";
				};

				config {
					pins = "gpio83", "gpio84", "gpio85",
								"gpio86";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se12_2uart_pins: qupv3_se12_2uart_pins {
			qupv3_se12_2uart_active: qupv3_se12_2uart_active {
				mux {
					pins = "gpio85", "gpio86";
					function = "qup12";
				};

				config {
					pins = "gpio85", "gpio86";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se12_2uart_sleep: qupv3_se12_2uart_sleep {
				mux {
					pins = "gpio85", "gpio86";
					function = "gpio";
				};

				config {
					pins = "gpio85", "gpio86";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		/* SE 13 pin mappings */
		qupv3_se13_i2c_pins: qupv3_se13_i2c_pins {
			qupv3_se13_i2c_active: qupv3_se13_i2c_active {
				mux {
					pins = "gpio86", "gpio85";
					function = "qup16";
				};

				config {
					pins = "gpio86", "gpio85";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se13_i2c_sleep: qupv3_se13_i2c_sleep {
				mux {
					pins = "gpio86", "gpio85";
					function = "gpio";
				};

				config {
					pins = "gpio86", "gpio85";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se13_spi_pins: qupv3_se13_spi_pins {
			qupv3_se13_spi_active: qupv3_se13_spi_active {
				mux {
					pins = "gpio83", "gpio84", "gpio85",
								"gpio86";
					function = "qup16";
				};

				config {
					pins = "gpio83", "gpio84", "gpio85",
								"gpio86";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se13_spi_sleep: qupv3_se13_spi_sleep {
				mux {
					pins = "gpio83", "gpio84", "gpio85",
								"gpio86";
					function = "gpio";
				};

				config {
					pins = "gpio83", "gpio84", "gpio85",
								"gpio86";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 14 pin mappings */
		qupv3_se14_i2c_pins: qupv3_se14_i2c_pins {
			qupv3_se14_i2c_active: qupv3_se14_i2c_active {
				mux {
					pins = "gpio55", "gpio56";
					function = "qup17";
				};

				config {
					pins = "gpio55", "gpio56";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se14_i2c_sleep: qupv3_se14_i2c_sleep {
				mux {
					pins = "gpio55", "gpio56";
					function = "gpio";
				};

				config {
					pins = "gpio55", "gpio56";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se14_spi_pins: qupv3_se14_spi_pins {
			qupv3_se14_spi_active: qupv3_se14_spi_active {
				mux {
					pins = "gpio55", "gpio56", "gpio57",
								"gpio58";
					function = "qup17";
				};

				config {
					pins = "gpio55", "gpio56", "gpio57",
								"gpio58";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se14_spi_sleep: qupv3_se14_spi_sleep {
				mux {
					pins = "gpio55", "gpio56", "gpio57",
								"gpio58";
					function = "gpio";
				};

				config {
					pins = "gpio55", "gpio56", "gpio57",
								"gpio58";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 15 pin mappings */
		qupv3_se15_i2c_pins: qupv3_se15_i2c_pins {
			qupv3_se15_i2c_active: qupv3_se15_i2c_active {
				mux {
					pins = "gpio23", "gpio24";
					function = "qup18";
				};

				config {
					pins = "gpio23", "gpio24";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se15_i2c_sleep: qupv3_se15_i2c_sleep {
				mux {
					pins = "gpio23", "gpio24";
					function = "gpio";
				};

				config {
					pins = "gpio23", "gpio24";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se15_spi_pins: qupv3_se15_spi_pins {
			qupv3_se15_spi_active: qupv3_se15_spi_active {
				mux {
					pins = "gpio23", "gpio24", "gpio25",
								"gpio26";
					function = "qup18";
				};

				config {
					pins = "gpio23", "gpio24", "gpio25",
								"gpio26";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se15_spi_sleep: qupv3_se15_spi_sleep {
				mux {
					pins = "gpio23", "gpio24", "gpio25",
								"gpio26";
					function = "gpio";
				};

				config {
					pins = "gpio23", "gpio24", "gpio25",
								"gpio26";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 16 pin mappings */
		qupv3_se16_i2c_pins: qupv3_se16_i2c_pins {
			qupv3_se16_i2c_active: qupv3_se16_i2c_active {
				mux {
					pins = "gpio57", "gpio58";
					function = "qup19";
				};

				config {
					pins = "gpio57", "gpio58";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se16_i2c_sleep: qupv3_se16_i2c_sleep {
				mux {
					pins = "gpio57", "gpio58";
					function = "gpio";
				};

				config {
					pins = "gpio57", "gpio58";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se16_spi_pins: qupv3_se16_spi_pins {
			qupv3_se16_spi_active: qupv3_se16_spi_active {
				mux {
					pins = "gpio55", "gpio56", "gpio57",
								"gpio58";
					function = "qup19";
				};

				config {
					pins = "gpio55", "gpio56", "gpio57",
								"gpio58";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se16_spi_sleep: qupv3_se16_spi_sleep {
				mux {
					pins = "gpio55", "gpio56", "gpio57",
								"gpio58";
					function = "gpio";
				};

				config {
					pins = "gpio55", "gpio56", "gpio57",
								"gpio58";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 17 pin mappings */
		qupv3_se17_i2c_pins: qupv3_se17_i2c_pins {
			qupv3_se17_i2c_active: qupv3_se17_i2c_active {
				mux {
					pins = "gpio43", "gpio44";
					function = "qup13";
				};

				config {
					pins = "gpio43", "gpio44";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se17_i2c_sleep: qupv3_se17_i2c_sleep {
				mux {
					pins = "gpio43", "gpio44";
					function = "gpio";
				};

				config {
					pins = "gpio43", "gpio44";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se17_spi_pins: qupv3_se17_spi_pins {
			qupv3_se17_spi_active: qupv3_se17_spi_active {
				mux {
					pins = "gpio43", "gpio44", "gpio45",
								"gpio46";
					function = "qup13";
				};

				config {
					pins = "gpio43", "gpio44", "gpio45",
								"gpio46";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se17_spi_sleep: qupv3_se17_spi_sleep {
				mux {
					pins = "gpio43", "gpio44", "gpio45",
								"gpio46";
					function = "gpio";
				};

				config {
					pins = "gpio43", "gpio44", "gpio45",
								"gpio46";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se17_4uart_pins: qupv3_se17_4uart_pins {
			qupv3_se17_default_tx: qupv3_se17_default_tx {
				mux {
					pins = "gpio45";
					function = "gpio";
				};

				config {
					pins = "gpio45";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			qupv3_se17_default_ctsrtsrx:
				qupv3_se17_default_ctsrtsrx {
				mux {
					pins = "gpio43", "gpio44", "gpio46";
					function = "gpio";
				};

				config {
					pins = "gpio43", "gpio44", "gpio46";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			qupv3_se17_ctsrx: qupv3_se17_ctsrx {
				mux {
					pins = "gpio43", "gpio46";
					function = "qup13";
				};

				config {
					pins = "gpio43", "gpio46";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se17_rts: qupv3_se17_rts {
				mux {
					pins = "gpio44";
					function = "qup13";
				};

				config {
					pins = "gpio44";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			qupv3_se17_tx: qupv3_se17_tx {
				mux {
					pins = "gpio45";
					function = "qup13";
				};

				config {
					pins = "gpio45";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		/* SE 18 pin mappings */
		qupv3_se18_i2c_pins: qupv3_se18_i2c_pins {
			qupv3_se18_i2c_active: qupv3_se18_i2c_active {
				mux {
					pins = "gpio47", "gpio48";
					function = "qup14";
				};

				config {
					pins = "gpio47", "gpio48";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se18_i2c_sleep: qupv3_se18_i2c_sleep {
				mux {
					pins = "gpio47", "gpio48";
					function = "gpio";
				};

				config {
					pins = "gpio47", "gpio48";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se18_spi_pins: qupv3_se18_spi_pins {
			qupv3_se18_spi_active: qupv3_se18_spi_active {
				mux {
					pins = "gpio47", "gpio48", "gpio49",
								"gpio50";
					function = "qup14";
				};

				config {
					pins = "gpio47", "gpio48", "gpio49",
								"gpio50";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se18_spi_sleep: qupv3_se18_spi_sleep {
				mux {
					pins = "gpio47", "gpio48", "gpio49",
								"gpio50";
					function = "gpio";
				};

				config {
					pins = "gpio47", "gpio48", "gpio49",
								"gpio50";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* SE 19 pin mappings */
		qupv3_se19_i2c_pins: qupv3_se19_i2c_pins {
			qupv3_se19_i2c_active: qupv3_se19_i2c_active {
				mux {
					pins = "gpio27", "gpio28";
					function = "qup15";
				};

				config {
					pins = "gpio27", "gpio28";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se19_i2c_sleep: qupv3_se19_i2c_sleep {
				mux {
					pins = "gpio27", "gpio28";
					function = "gpio";
				};

				config {
					pins = "gpio27", "gpio28";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se19_spi_pins: qupv3_se19_spi_pins {
			qupv3_se19_spi_active: qupv3_se19_spi_active {
				mux {
					pins = "gpio27", "gpio28", "gpio29",
								"gpio30";
					function = "qup15";
				};

				config {
					pins = "gpio27", "gpio28", "gpio29",
								"gpio30";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se19_spi_sleep: qupv3_se19_spi_sleep {
				mux {
					pins = "gpio27", "gpio28", "gpio29",
								"gpio30";
					function = "gpio";
				};

				config {
					pins = "gpio27", "gpio28", "gpio29",
								"gpio30";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		aqt_intr {
			aqt_intr_default: aqt_intr_default {
				mux {
					pins = "gpio125";
					function = "gpio";
				};

				config {
					pins = "gpio125";
					drive-strength = <2>; /* 2 mA */
					bias-pull-down; /* pull down */
					input-enable;
				};
			};
		};

		wcd9xxx_intr {
			wcd_intr_default: wcd_intr_default {
				 mux {
					pins = "gpio123";
					function = "gpio";
				};

				config {
					pins = "gpio123";
					drive-strength = <2>; /* 2 mA */
					bias-pull-down; /* pull down */
					input-enable;
				};
			};
		};

		cdc_reset_ctrl {
			cdc_reset_sleep: cdc_reset_sleep {
				mux {
					pins = "gpio143";
					function = "gpio";
				};

				config {
					pins = "gpio143";
					drive-strength = <2>;
					bias-disable;
					output-low;
				};
			};

			cdc_reset_active:cdc_reset_active {
				mux {
					pins = "gpio143";
					function = "gpio";
				};

				config {
					pins = "gpio143";
					drive-strength = <8>;
					bias-pull-down;
					output-high;
				};
			};
		};

		sec_aux_pcm {
			sec_aux_pcm_sleep: sec_aux_pcm_sleep {
				mux {
					pins = "gpio126", "gpio127";
					function = "gpio";
				};

				config {
					pins = "gpio126", "gpio127";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_aux_pcm_active: sec_aux_pcm_active {
				mux {
					pins = "gpio126", "gpio127";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio126", "gpio127";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_aux_pcm_din {
			sec_aux_pcm_din_sleep: sec_aux_pcm_din_sleep {
				mux {
					pins = "gpio128";
					function = "gpio";
				};

				config {
					pins = "gpio128";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_aux_pcm_din_active: sec_aux_pcm_din_active {
				mux {
					pins = "gpio128";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio128";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_aux_pcm_dout {
			sec_aux_pcm_dout_sleep: sec_aux_pcm_dout_sleep {
				mux {
					pins = "gpio129";
					function = "gpio";
				};

				config {
					pins = "gpio129";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_aux_pcm_dout_active: sec_aux_pcm_dout_active {
				mux {
					pins = "gpio129";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio129";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_aux_pcm {
			tert_aux_pcm_sleep: tert_aux_pcm_sleep {
				mux {
					pins = "gpio133", "gpio134";
					function = "gpio";
				};

				config {
					pins = "gpio133", "gpio134";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_aux_pcm_active: tert_aux_pcm_active {
				mux {
					pins = "gpio133", "gpio134";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio133", "gpio134";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		tert_aux_pcm_din {
			tert_aux_pcm_din_sleep: tert_aux_pcm_din_sleep {
				mux {
					pins = "gpio135";
					function = "gpio";
				};

				config {
					pins = "gpio135";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_aux_pcm_din_active: tert_aux_pcm_din_active {
				mux {
					pins = "gpio135";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio135";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_aux_pcm_dout {
			tert_aux_pcm_dout_sleep: tert_aux_pcm_dout_sleep {
				mux {
					pins = "gpio131";
					function = "gpio";
				};

				config {
					pins = "gpio131";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_aux_pcm_dout_active: tert_aux_pcm_dout_active {
				mux {
					pins = "gpio131";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio131";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quat_aux_pcm {
			quat_aux_pcm_sleep: quat_aux_pcm_sleep {
				mux {
					pins = "gpio137", "gpio138";
					function = "gpio";
				};

				config {
					pins = "gpio137", "gpio138";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_aux_pcm_active: quat_aux_pcm_active {
				mux {
					pins = "gpio137", "gpio138";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio137", "gpio138";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		quat_aux_pcm_din {
			quat_aux_pcm_din_sleep: quat_aux_pcm_din_sleep {
				mux {
					pins = "gpio139";
					function = "gpio";
				};

				config {
					pins = "gpio139";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_aux_pcm_din_active: quat_aux_pcm_din_active {
				mux {
					pins = "gpio139";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio139";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quat_aux_pcm_dout {
			quat_aux_pcm_dout_sleep: quat_aux_pcm_dout_sleep {
				mux {
					pins = "gpio140";
					function = "gpio";
				};

				config {
					pins = "gpio140";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_aux_pcm_dout_active: quat_aux_pcm_dout_active {
				mux {
					pins = "gpio140";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio140";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_aux_pcm_clk {
			pri_aux_pcm_clk_sleep: pri_aux_pcm_clk_sleep {
				mux {
					pins = "gpio144";
					function = "gpio";
				};

				config {
					pins = "gpio144";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_aux_pcm_clk_active: pri_aux_pcm_clk_active {
				mux {
					pins = "gpio144";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio144";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_aux_pcm_sync {
			pri_aux_pcm_sync_sleep: pri_aux_pcm_sync_sleep {
				mux {
					pins = "gpio145";
					function = "gpio";
				};

				config {
					pins = "gpio145";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_aux_pcm_sync_active: pri_aux_pcm_sync_active {
				mux {
					pins = "gpio145";
					function = "pri_mi2s_ws";
				};

				config {
					pins = "gpio145";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_aux_pcm_din {
			pri_aux_pcm_din_sleep: pri_aux_pcm_din_sleep {
				mux {
					pins = "gpio146";
					function = "gpio";
				};

				config {
					pins = "gpio146";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_aux_pcm_din_active: pri_aux_pcm_din_active {
				mux {
					pins = "gpio146";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio146";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_aux_pcm_dout {
			pri_aux_pcm_dout_sleep: pri_aux_pcm_dout_sleep {
				mux {
					pins = "gpio147";
					function = "gpio";
				};

				config {
					pins = "gpio147";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_aux_pcm_dout_active: pri_aux_pcm_dout_active {
				mux {
					pins = "gpio147";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio147";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quin_aux_pcm {
			quin_aux_pcm_sleep: quin_aux_pcm_sleep {
				mux {
					pins = "gpio149", "gpio151";
					function = "gpio";
				};

				config {
					pins = "gpio149", "gpio151";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_aux_pcm_active: quin_aux_pcm_active {
				mux {
					pins = "gpio149", "gpio151";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio149", "gpio151";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		quin_aux_pcm_din {
			quin_aux_pcm_din_sleep: quin_aux_pcm_din_sleep {
				mux {
					pins = "gpio150";
					function = "gpio";
				};

				config {
					pins = "gpio150";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_aux_pcm_din_active: quin_aux_pcm_din_active {
				mux {
					pins = "gpio150";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio150";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quin_aux_pcm_dout {
			quin_aux_pcm_dout_sleep: quin_aux_pcm_dout_sleep {
				mux {
					pins = "gpio152";
					function = "gpio";
				};

				config {
					pins = "gpio152";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_aux_pcm_dout_active: quin_aux_pcm_dout_active {
				mux {
					pins = "gpio152";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio152";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_tdm {
			sec_tdm_sleep: sec_tdm_sleep {
				mux {
					pins = "gpio126", "gpio127";
					function = "gpio";
				};

				config {
					pins = "gpio126", "gpio127";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_tdm_active: sec_tdm_active {
				mux {
					pins = "gpio126", "gpio127";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio126", "gpio127";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_tdm_din {
			sec_tdm_din_sleep: sec_tdm_din_sleep {
				mux {
					pins = "gpio128";
					function = "gpio";
				};

				config {
					pins = "gpio128";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_tdm_din_active: sec_tdm_din_active {
				mux {
					pins = "gpio128";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio128";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_tdm_dout {
			sec_tdm_dout_sleep: sec_tdm_dout_sleep {
				mux {
					pins = "gpio129";
					function = "gpio";
				};

				config {
					pins = "gpio129";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_tdm_dout_active: sec_tdm_dout_active {
				mux {
					pins = "gpio129";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio129";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		tert_tdm {
			tert_tdm_sleep: tert_tdm_sleep {
				mux {
					pins = "gpio133", "gpio134";
					function = "gpio";
				};

				config {
					pins = "gpio133", "gpio134";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_tdm_active: tert_tdm_active {
				mux {
					pins = "gpio133", "gpio134";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio133", "gpio134";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		tert_tdm_din {
			tert_tdm_din_sleep: tert_tdm_din_sleep {
				mux {
					pins = "gpio135";
					function = "gpio";
				};

				config {
					pins = "gpio135";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_tdm_din_active: tert_tdm_din_active {
				mux {
					pins = "gpio135";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio135";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_tdm_dout {
			tert_tdm_dout_sleep: tert_tdm_dout_sleep {
				mux {
					pins = "gpio131";
					function = "gpio";
				};

				config {
					pins = "gpio131";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_tdm_dout_active: tert_tdm_dout_active {
				mux {
					pins = "gpio131";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio131";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		quat_tdm {
			quat_tdm_sleep: quat_tdm_sleep {
				mux {
					pins = "gpio137", "gpio138";
					function = "gpio";
				};

				config {
					pins = "gpio137", "gpio138";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_tdm_active: quat_tdm_active {
				mux {
					pins = "gpio137", "gpio138";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio137", "gpio138";
					drive-strength = <6>;   /* 6 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		quat_tdm_din {
			quat_tdm_din_sleep: quat_tdm_din_sleep {
				mux {
					pins = "gpio139", "gpio141";
					function = "gpio";
				};

				config {
					pins = "gpio139", "gpio141";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_tdm_din_active: quat_tdm_din_active {
				mux {
					pins = "gpio139", "gpio141";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio139", "gpio141";
					drive-strength = <4>;   /* 4 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quat_tdm_dout {
			quat_tdm_dout_sleep: quat_tdm_dout_sleep {
				mux {
					pins = "gpio140", "gpio142";
					function = "gpio";
				};

				config {
					pins = "gpio140", "gpio142";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_tdm_dout_active: quat_tdm_dout_active {
				mux {
					pins = "gpio140", "gpio142";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio140", "gpio142";
					drive-strength = <4>;   /* 4 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_tdm_clk {
			pri_tdm_clk_sleep: pri_tdm_clk_sleep {
				mux {
					pins = "gpio144";
					function = "gpio";
				};

				config {
					pins = "gpio144";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_tdm_clk_active: pri_tdm_clk_active {
				mux {
					pins = "gpio144";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio144";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_tdm_sync {
			pri_tdm_sync_sleep: pri_tdm_sync_sleep {
				mux {
					pins = "gpio145";
					function = "gpio";
				};

				config {
					pins = "gpio145";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_tdm_sync_active: pri_tdm_sync_active {
				mux {
					pins = "gpio145";
					function = "pri_mi2s_ws";
				};

				config {
					pins = "gpio145";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_tdm_din {
			pri_tdm_din_sleep: pri_tdm_din_sleep {
				mux {
					pins = "gpio146";
					function = "gpio";
				};

				config {
					pins = "gpio146";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_tdm_din_active: pri_tdm_din_active {
				mux {
					pins = "gpio146";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio146";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_tdm_dout {
			pri_tdm_dout_sleep: pri_tdm_dout_sleep {
				mux {
					pins = "gpio147";
					function = "gpio";
				};

				config {
					pins = "gpio147";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_tdm_dout_active: pri_tdm_dout_active {
				mux {
					pins = "gpio147";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio147";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quin_tdm {
			quin_tdm_sleep: quin_tdm_sleep {
				mux {
					pins = "gpio149", "gpio151";
					function = "gpio";
				};

				config {
					pins = "gpio149", "gpio151";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_tdm_active: quin_tdm_active {
				mux {
					pins = "gpio149", "gpio151";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio149", "gpio151";
					drive-strength = <2>;   /* 2 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		quin_tdm_din {
			quin_tdm_din_sleep: quin_tdm_din_sleep {
				mux {
					pins = "gpio150";
					function = "gpio";
				};

				config {
					pins = "gpio150";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_tdm_din_active: quin_tdm_din_active {
				mux {
					pins = "gpio150";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio150";
					drive-strength = <4>;   /* 4 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quin_tdm_dout {
			quin_tdm_dout_sleep: quin_tdm_dout_sleep {
				mux {
					pins = "gpio152";
					function = "gpio";
				};

				config {
					pins = "gpio152";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_tdm_dout_active: quin_tdm_dout_active {
				mux {
					pins = "gpio152";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio152";
					drive-strength = <4>;   /* 4 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		sec_mi2s_mclk {
			sec_mi2s_mclk_sleep: sec_mi2s_mclk_sleep {
				mux {
					pins = "gpio130";
					function = "gpio";
				};

				config {
					pins = "gpio130";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_mi2s_mclk_active: sec_mi2s_mclk_active {
				mux {
					pins = "gpio130";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio130";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_mi2s {
			sec_mi2s_sleep: sec_mi2s_sleep {
				mux {
					pins = "gpio126", "gpio127";
					function = "gpio";
				};

				config {
					pins = "gpio126", "gpio127";
					drive-strength = <2>;   /* 2 mA */
					bias-disable;         /* NO PULL */
					input-enable;
				};
			};

			sec_mi2s_active: sec_mi2s_active {
				mux {
					pins = "gpio126", "gpio127";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio126", "gpio127";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_mi2s_sd0 {
			sec_mi2s_sd0_sleep: sec_mi2s_sd0_sleep {
				mux {
					pins = "gpio128";
					function = "gpio";
				};

				config {
					pins = "gpio128";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_mi2s_sd0_active: sec_mi2s_sd0_active {
				mux {
					pins = "gpio128";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio128";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_mi2s_sd1 {
			sec_mi2s_sd1_sleep: sec_mi2s_sd1_sleep {
				mux {
					pins = "gpio129";
					function = "gpio";
				};

				config {
					pins = "gpio129";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_mi2s_sd1_active: sec_mi2s_sd1_active {
				mux {
					pins = "gpio129";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio129";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_mi2s_mclk {
			tert_mi2s_mclk_sleep: tert_mi2s_mclk_sleep {
				mux {
					pins = "gpio132";
					function = "gpio";
				};

				config {
					pins = "gpio132";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_mi2s_mclk_active: tert_mi2s_mclk_active {
				mux {
					pins = "gpio132";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio132";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_mi2s {
			tert_mi2s_sleep: tert_mi2s_sleep {
				mux {
					pins = "gpio133", "gpio134";
					function = "gpio";
				};

				config {
					pins = "gpio133", "gpio134";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_mi2s_active: tert_mi2s_active {
				mux {
					pins = "gpio133", "gpio134";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio133", "gpio134";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		tert_mi2s_sd0 {
			tert_mi2s_sd0_sleep: tert_mi2s_sd0_sleep {
				mux {
					pins = "gpio135";
					function = "gpio";
				};

				config {
					pins = "gpio135";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_mi2s_sd0_active: tert_mi2s_sd0_active {
				mux {
					pins = "gpio135";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio135";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_mi2s_sd1 {
			tert_mi2s_sd1_sleep: tert_mi2s_sd1_sleep {
				mux {
					pins = "gpio131";
					function = "gpio";
				};

				config {
					pins = "gpio131";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_mi2s_sd1_active: tert_mi2s_sd1_active {
				mux {
					pins = "gpio131";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio131";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quat_mi2s_mclk {
			quat_mi2s_mclk_sleep: quat_mi2s_mclk_sleep {
				mux {
					pins = "gpio136";
					function = "gpio";
				};

				config {
					pins = "gpio136";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_mi2s_mclk_active: quat_mi2s_mclk_active {
				mux {
					pins = "gpio136";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio136";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quat_mi2s {
			quat_mi2s_sleep: quat_mi2s_sleep {
				mux {
					pins = "gpio137", "gpio138";
					function = "gpio";
				};

				config {
					pins = "gpio137", "gpio138";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_mi2s_active: quat_mi2s_active {
				mux {
					pins = "gpio137", "gpio138";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio137", "gpio138";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		quat_mi2s_sd0 {
			quat_mi2s_sd0_sleep: quat_mi2s_sd0_sleep {
				mux {
					pins = "gpio139";
					function = "gpio";
				};

				config {
					pins = "gpio139";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_mi2s_sd0_active: quat_mi2s_sd0_active {
				mux {
					pins = "gpio139";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio139";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quat_mi2s_sd1 {
			quat_mi2s_sd1_sleep: quat_mi2s_sd1_sleep {
				mux {
					pins = "gpio140";
					function = "gpio";
				};

				config {
					pins = "gpio140";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_mi2s_sd1_active: quat_mi2s_sd1_active {
				mux {
					pins = "gpio140";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio140";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quat_mi2s_sd2 {
			quat_mi2s_sd2_sleep: quat_mi2s_sd2_sleep {
				mux {
					pins = "gpio141";
					function = "gpio";
				};

				config {
					pins = "gpio141";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_mi2s_sd2_active: quat_mi2s_sd2_active {
				mux {
					pins = "gpio141";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio141";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quat_mi2s_sd3 {
			quat_mi2s_sd3_sleep: quat_mi2s_sd3_sleep {
				mux {
					pins = "gpio142";
					function = "gpio";
				};

				config {
					pins = "gpio142";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quat_mi2s_sd3_active: quat_mi2s_sd3_active {
				mux {
					pins = "gpio142";
					function = "qua_mi2s";
				};

				config {
					pins = "gpio142";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_mi2s_mclk {
			pri_mi2s_mclk_sleep: pri_mi2s_mclk_sleep {
				mux {
					pins = "gpio143";
					function = "gpio";
				};

				config {
					pins = "gpio143";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_mclk_active: pri_mi2s_mclk_active {
				mux {
					pins = "gpio143";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio143";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_mi2s_sck {
			pri_mi2s_sck_sleep: pri_mi2s_sck_sleep {
				mux {
					pins = "gpio144";
					function = "gpio";
				};

				config {
					pins = "gpio144";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_sck_active: pri_mi2s_sck_active {
				mux {
					pins = "gpio144";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio144";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_mi2s_ws {
			pri_mi2s_ws_sleep: pri_mi2s_ws_sleep {
				mux {
					pins = "gpio145";
					function = "gpio";
				};

				config {
					pins = "gpio145";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_ws_active: pri_mi2s_ws_active {
				mux {
					pins = "gpio145";
					function = "pri_mi2s_ws";
				};

				config {
					pins = "gpio145";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_mi2s_sd0 {
			pri_mi2s_sd0_sleep: pri_mi2s_sd0_sleep {
				mux {
					pins = "gpio146";
					function = "gpio";
				};

				config {
					pins = "gpio146";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_sd0_active: pri_mi2s_sd0_active {
				mux {
					pins = "gpio146";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio146";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_mi2s_sd1 {
			pri_mi2s_sd1_sleep: pri_mi2s_sd1_sleep {
				mux {
					pins = "gpio147";
					function = "gpio";
				};

				config {
					pins = "gpio147";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_sd1_active: pri_mi2s_sd1_active {
				mux {
					pins = "gpio147";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio147";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quin_mi2s_mclk {
			quin_mi2s_mclk_sleep: quin_mi2s_mclk_sleep {
				mux {
					pins = "gpio148";
					function = "gpio";
				};

				config {
					pins = "gpio148";
					drive-strength = <2>; /* 2 mA */
					bias-pull-down;       /* PULL DOWN */
				};
			};

			quin_mi2s_mclk_active: quin_mi2s_mclk_active {
				mux {
					pins = "gpio148";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio148";
					drive-strength = <8>; /* 8 mA */
					bias-disable;         /* NO PULL */
				};
			};
		};

		quin_mi2s {
			quin_mi2s_sleep: quin_mi2s_sleep {
				mux {
					pins = "gpio149", "gpio151";
					function = "gpio";
				};

				config {
					pins = "gpio149", "gpio151";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_mi2s_active: quin_mi2s_active {
				mux {
					pins = "gpio149", "gpio151";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio149", "gpio151";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		quin_mi2s_sd0 {
			quin_mi2s_sd0_sleep: quin_mi2s_sd0_sleep {
				mux {
					pins = "gpio150";
					function = "gpio";
				};

				config {
					pins = "gpio150";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_mi2s_sd0_active: quin_mi2s_sd0_active {
				mux {
					pins = "gpio150";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio150";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		quin_mi2s_sd1 {
			quin_mi2s_sd1_sleep: quin_mi2s_sd1_sleep {
				mux {
					pins = "gpio152";
					function = "gpio";
				};

				config {
					pins = "gpio152";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			quin_mi2s_sd1_active: quin_mi2s_sd1_active {
				mux {
					pins = "gpio152";
					function = "spkr_i2s";
				};

				config {
					pins = "gpio152";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pmx_sde: pmx_sde {
			sde_dsi_active: sde_dsi_active {
				mux {
					pins = "gpio6", "gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio7";
					drive-strength = <8>;   /* 8 mA */
					bias-disable = <0>;   /* no pull */
				};
			};

			sde_dsi_suspend: sde_dsi_suspend {
				mux {
					pins = "gpio6", "gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio7";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_dsi1_active: sde_dsi1_active {
				mux {
					pins = "gpio130";
					function = "gpio";
				};

				config {
					pins = "gpio130";
					drive-strength = <8>;   /* 8 mA */
					bias-disable = <0>;   /* no pull */
				};
			};

			sde_dsi1_suspend: sde_dsi1_suspend {
				mux {
					pins = "gpio130";
					function = "gpio";
				};

				config {
					pins = "gpio130";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};
		};

		pmx_sde_te {
			sde_te_active: sde_te_active {
				mux {
					pins = "gpio8";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio8";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_te_suspend: sde_te_suspend {
				mux {
					pins = "gpio8";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio8";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_te1_active: sde_te1_active {
				mux {
					pins = "gpio9";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio9";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_te1_suspend: sde_te1_suspend {
				mux {
					pins = "gpio9";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio9";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};
		};

		/* add pins for DisplayPort */
		sde_dp_usbplug_cc_active: sde_dp_usbplug_cc_active {
				mux {
					pins = "gpio38";
					function = "gpio";
				};

				config {
					pins = "gpio38";
					bias-disable;
					drive-strength = <16>;
				};
		};

		sde_dp_usbplug_cc_suspend: sde_dp_usbplug_cc_suspend {
				mux {
					pins = "gpio38";
					function = "gpio";
				};

				config {
					pins = "gpio38";
					bias-pull-down;
					drive-strength = <2>;
				};
		};

		ap2mdm {
			ap2mdm_active: ap2mdm_active {
				mux {
					/* ap2mdm-status
					 * ap2mdm-errfatal
					 * ap2mdm-vddmin
					 */
					pins = "gpio135", "gpio141";
					function = "gpio";
				};

				config {
					pins = "gpio135", "gpio141";
					drive-strength = <16>;
					bias-disable;
				};
			};

			ap2mdm_sleep: ap2mdm_sleep {
				mux {
					/* ap2mdm-status
					 * ap2mdm-errfatal
					 * ap2mdm-vddmin
					 */
					pins = "gpio135", "gpio141";
					function = "gpio";
				};

				config {
					pins = "gpio135", "gpio141";
					drive-strength = <8>;
					bias-disable;
				};

			};
		};

		mdm2ap {
			mdm2ap_active: mdm2ap_active {
				mux {
					/* mdm2ap-status
					 * mdm2ap-errfatal
					 * mdm2ap-vddmin
					 */
					pins = "gpio142", "gpio53";
					function = "gpio";
				};

				config {
					pins = "gpio142", "gpio53";
					drive-strength = <8>;
					bias-disable;
				};
			};

			mdm2ap_sleep: mdm2ap_sleep {
				mux {
					/* mdm2ap-status
					 * mdm2ap-errfatal
					 * mdm2ap-vddmin
					 */
					pins = "gpio142", "gpio53";
					function = "gpio";
				};

				config {
					pins = "gpio142", "gpio53";
					drive-strength = <8>;
					bias-disable;
				};
			};
		};

		fsa_usbc_ana_en_n@100 {
			fsa_usbc_ana_en: fsa_usbc_ana_en {
				mux {
					pins = "gpio100";
					function = "gpio";
				};

				config {
					pins = "gpio100";
					drive-strength = <2>;
					bias-disable;
					output-low;
				};
			};
		};

		cam_sensor_mclk0_active: cam_sensor_mclk0_active {
			/* MCLK0 */
			mux {
				pins = "gpio13";
				function = "cam_mclk";
			};

			config {
				pins = "gpio13";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk0_suspend: cam_sensor_mclk0_suspend {
			/* MCLK0 */
			mux {
				pins = "gpio13";
				function = "cam_mclk";
			};

			config {
				pins = "gpio13";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk1_active: cam_sensor_mclk1_active {
			/* MCLK1 */
			mux {
				pins = "gpio14";
				function = "cam_mclk";
			};

			config {
				pins = "gpio14";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk1_suspend: cam_sensor_mclk1_suspend {
			/* MCLK1 */
			mux {
				pins = "gpio14";
				function = "cam_mclk";
			};

			config {
				pins = "gpio14";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk2_active: cam_sensor_mclk2_active {
			/* MCLK2 */
			mux {
				pins = "gpio15";
				function = "cam_mclk";
			};

			config {
				pins = "gpio15";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk2_suspend: cam_sensor_mclk2_suspend {
			/* MCLK2 */
			mux {
				pins = "gpio15";
				function = "cam_mclk";
			};

			config {
				pins = "gpio15";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk3_active: cam_sensor_mclk3_active {
			/* MCLK3 */
			mux {
				pins = "gpio16";
				function = "cam_mclk";
			};

			config {
				pins = "gpio16";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk3_suspend: cam_sensor_mclk3_suspend {
			/* MCLK3 */
			mux {
				pins = "gpio16";
				function = "cam_mclk";
			};

			config {
				pins = "gpio16";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor0_active: cam_sensor0_active {
			/* intr gpio for bridge chip 0 */
			mux {
				pins = "gpio13";
				function = "gpio";
			};

			config {
				pins = "gpio13";
				bias-pull-up; /* PULL UP */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor0_suspend: cam_sensor0_suspend {
			/* intr gpio for bridge chip 0 */
			mux {
				pins = "gpio13";
				function = "gpio";
			};

			config {
				pins = "gpio13";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor1_active: cam_sensor1_active {
			/* intr gpio for bridge chip 1 */
			mux {
				pins = "gpio14";
				function = "gpio";
			};

			config {
				pins = "gpio14";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor1_suspend: cam_sensor1_suspend {
			/* intr gpio for bridge chip 1 */
			mux {
				pins = "gpio14";
				function = "gpio";
			};

			config {
				pins = "gpio14";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor2_active: cam_sensor2_active {
			/* intr gpio for bridge chip 2 */
			mux {
				pins = "gpio15";
				function = "gpio";
			};

			config {
				pins = "gpio15";
				bias-pull-up; /* PULL UP */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor2_suspend: cam_sensor2_suspend {
			/* intr gpio for bridge chip 2 */
			mux {
				pins = "gpio15";
				function = "gpio";
			};

			config {
				pins = "gpio15";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor3_active: cam_sensor3_active {
			/* intr gpio for bridge chip 3 */
			mux {
				pins = "gpio16";
				function = "gpio";
			};

			config {
				pins = "gpio16";
				bias-pull-up; /* PULL UP */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor3_suspend: cam_sensor3_suspend {
			/* intr gpio for bridge chip 3 */
			mux {
				pins = "gpio16";
				function = "gpio";
			};

			config {
				pins = "gpio16";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_eldo2_default: cam_sensor_eldo2_default {
			/* AVDD ELDO2 */
			mux {
				pins = "gpio11";
				function = "gpio";
			};

			config {
				pins = "gpio11";
				bias-disable; /* NO PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		camera_vaf_en_default: camera_vaf_en_default {
			/*  VAF ELDO1 */
			mux {
				pins = "gpio29";
				function = "gpio";
			};

			config {
				pins = "gpio29";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		camera_vana_en_default: camera_vana_en_default {
			 /*  VANA ELDO2 */
			 mux {
				pins = "gpio11";
				function = "gpio";
			};

			config {
				pins = "gpio11";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_active_rear: cam_sensor_active_rear {
			/* RESET REAR2 */
			mux {
				pins = "gpio28";
				function = "gpio";
			};

			config {
				pins = "gpio28";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rear: cam_sensor_suspend_rear {
			/* RESET REAR2 */
			mux {
				pins = "gpio28";
				function = "gpio";
			};

			config {
				pins = "gpio28";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_rear_aux: cam_sensor_active_rear_aux {
			/* RESET REARAUX */
			mux {
				pins = "gpio30";
				function = "gpio";
			};

			config {
				pins = "gpio30";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rear_aux: cam_sensor_suspend_rear_aux {
			/* RESET REARAUX */
			mux {
				pins = "gpio30";
				function = "gpio";
			};

			config {
				pins = "gpio30";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_front: cam_sensor_active_front {
			/* RESET FRONT */
			mux {
				pins = "gpio12";
				function = "gpio";
			};

			config {
				pins = "gpio12";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_front: cam_sensor_suspend_front {
			/* RESET FRONT */
			mux {
				pins = "gpio12";
				function = "gpio";
			};

			config {
				pins = "gpio12";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_iris: cam_sensor_active_iris {
			/* RESET IRIS */
			mux {
				pins = "gpio23", "gpio26";
				function = "gpio";
			};

			config {
				pins = "gpio23", "gpio26";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_iris: cam_sensor_suspend_iris {
			/* RESET IRIS */
			mux {
				pins = "gpio23", "gpio26";
				function = "gpio";
			};

			config {
				pins = "gpio23", "gpio26";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cci0_active: cci0_active {
			mux {
				/* CLK, DATA */
				pins = "gpio17","gpio18"; // Only 2
				function = "cci_i2c";
			};

			config {
				pins = "gpio17","gpio18";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci0_suspend: cci0_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio17","gpio18";
				function = "cci_i2c";
			};

			config {
				pins = "gpio17","gpio18";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci1_active: cci1_active {
			mux {
				/* CLK, DATA */
				pins = "gpio19","gpio20";
				function = "cci_i2c";
			};

			config {
				pins = "gpio19","gpio20";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci1_suspend: cci1_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio19","gpio20";
				function = "cci_i2c";
			};

			config {
				pins = "gpio19","gpio20";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci2_active: cci2_active {
			mux {
				/* CLK, DATA */
				pins = "gpio31","gpio32";
				function = "cci_i2c";
			};

			config {
				pins = "gpio31","gpio32";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci2_suspend: cci2_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio31","gpio32";
				function = "cci_i2c";
			};

			config {
				pins = "gpio31","gpio32";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci3_active: cci3_active {
			mux {
				/* CLK, DATA */
				pins = "gpio33","gpio34";
				function = "cci_i2c";
			};

			config {
				pins = "gpio33","gpio34";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci3_suspend: cci3_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio33","gpio34";
				function = "cci_i2c";
			};

			config {
				pins = "gpio33","gpio34";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		tsif0_signals_active: tsif0_signals_active {
			tsif1_clk {
				pins = "gpio88"; /* TSIF0 CLK */
				function = "tsif1_clk";
			};

			tsif1_en {
				pins = "gpio89"; /* TSIF0 Enable */
				function = "tsif1_en";
			};

			tsif1_data {
				pins = "gpio90"; /* TSIF0 DATA */
				function = "tsif1_data";
			};

			signals_cfg {
				pins = "gpio88", "gpio89", "gpio90";
				drive_strength = <2>;	/* 2 mA */
				bias-pull-down;		/* pull down */
			};
		};

		/* sync signal is only used if configured to mode-2 */
		tsif0_sync_active: tsif0_sync_active {
			tsif1_sync {
				pins = "gpio91";	/* TSIF0 SYNC */
				function = "tsif1_sync";
				drive_strength = <2>;	/* 2 mA */
				bias-pull-down;		/* pull down */
			};
		};

		tsif1_signals_active: tsif1_signals_active {
			tsif2_clk {
				pins = "gpio92"; /* TSIF1 CLK */
				function = "tsif2_clk";
			};

			tsif2_en {
				pins = "gpio93"; /* TSIF1 Enable */
				function = "tsif2_en";
			};

			tsif2_data {
				pins = "gpio94"; /* TSIF1 DATA */
				function = "tsif2_data";
			};

			signals_cfg {
				pins = "gpio92", "gpio93", "gpio94";
				drive_strength = <2>;	/* 2 mA */
				bias-pull-down;		/* pull down */
			};
		};

		/* sync signal is only used if configured to mode-2 */
		tsif1_sync_active: tsif1_sync_active {
			tsif2_sync {
				pins = "gpio95";	/* TSIF1 SYNC */
				function = "tsif2_sync";
				drive_strength = <2>;	/* 2 mA */
				bias-pull-down;		/* pull down */
			};
		};

		trigout_a: trigout_a {
			mux {
				pins = "gpio49";
				function = "qdss_cti";
			};

			config {
				pins = "gpio49";
				drive-strength = <2>;
				bias-disable;
			};
		};

		usb2_id_det_default: usb2_id_det_default {
			config {
				pins = "gpio101";
				function = "gpio";
				input-enable;
				bias-pull-up;
			};
		};

		hs1_i2s_mclk {
			hs1_i2s_mclk_sleep: hs1_i2s_mclk_sleep {
				mux {
					pins = "gpio155";
					function = "gpio";
				};

				config {
					pins = "gpio155";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs1_i2s_mclk_active: hs1_i2s_mclk_active {
				mux {
					pins = "gpio155";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio155";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs1_i2s_sck {
			hs1_i2s_sck_sleep: hs1_i2s_sck_sleep {
				mux {
					pins = "gpio156";
					function = "gpio";
				};

				config {
					pins = "gpio156";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs1_i2s_sck_active: hs1_i2s_sck_active {
				mux {
					pins = "gpio156";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio156";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs1_i2s_ws {
			hs1_i2s_ws_sleep: hs1_i2s_ws_sleep {
				mux {
					pins = "gpio157";
					function = "gpio";
				};

				config {
					pins = "gpio157";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs1_i2s_ws_active: hs1_i2s_ws_active {
				mux {
					pins = "gpio157";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio157";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs1_i2s_data0 {
			hs1_i2s_data0_sleep: hs1_i2s_data0_sleep {
				mux {
					pins = "gpio158";
					function = "gpio";
				};

				config {
					pins = "gpio158";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs1_i2s_data0_active: hs1_i2s_data0_active {
				mux {
					pins = "gpio158";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio158";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs1_i2s_data1 {
			hs1_i2s_data1_sleep: hs1_i2s_data1_sleep {
				mux {
					pins = "gpio159";
					function = "gpio";
				};

				config {
					pins = "gpio159";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs1_i2s_data1_active: hs1_i2s_data1_active {
				mux {
					pins = "gpio159";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio159";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					input-enable;
				};
			};
		};

		hs2_i2s_mclk {
			hs2_i2s_mclk_sleep: hs2_i2s_mclk_sleep {
				mux {
					pins = "gpio160";
					function = "gpio";
				};

				config {
					pins = "gpio160";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs2_i2s_mclk_active: hs2_i2s_mclk_active {
				mux {
					pins = "gpio160";
					function = "hs2_mi2s";
				};

				config {
					pins = "gpio160";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs2_i2s_sck {
			hs2_i2s_sck_sleep: hs2_i2s_sck_sleep {
				mux {
					pins = "gpio161";
					function = "gpio";
				};

				config {
					pins = "gpio161";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs2_i2s_sck_active: hs2_i2s_sck_active {
				mux {
					pins = "gpio161";
					function = "hs2_mi2s";
				};

				config {
					pins = "gpio161";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs2_i2s_ws {
			hs2_i2s_ws_sleep: hs2_i2s_ws_sleep {
				mux {
					pins = "gpio162";
					function = "gpio";
				};

				config {
					pins = "gpio162";
					drive-strength = <2>;   /* 8 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs2_i2s_ws_active: hs2_i2s_ws_active {
				mux {
					pins = "gpio162";
					function = "hs2_mi2s";
				};

				config {
					pins = "gpio162";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs2_i2s_data0 {
			hs2_i2s_data0_sleep: hs2_i2s_data0_sleep {
				mux {
					pins = "gpio163";
					function = "gpio";
				};

				config {
					pins = "gpio163";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs2_i2s_data0_active: hs2_i2s_data0_active {
				mux {
					pins = "gpio163";
					function = "hs2_mi2s";
				};

				config {
					pins = "gpio163";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs2_i2s_data1 {
			hs2_i2s_data1_sleep: hs2_i2s_data1_sleep {
				mux {
					pins = "gpio164";
					function = "gpio";
				};

				config {
					pins = "gpio164";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs2_i2s_data1_active: hs2_i2s_data1_active {
				mux {
					pins = "gpio164";
					function = "hs2_mi2s";
				};

				config {
					pins = "gpio164";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					input-enable;
				};
			};
		};

		hs3_i2s_mclk {
			hs3_i2s_mclk_sleep: hs3_i2s_mclk_sleep {
				mux {
					pins = "gpio125";
					function = "gpio";
				};

				config {
					pins = "gpio125";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs3_i2s_mclk_active: hs3_i2s_mclk_active {
				mux {
					pins = "gpio125";
					function = "hs3_mi2s";
				};

				config {
					pins = "gpio125";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs3_i2s_sck {
			hs3_i2s_sck_sleep: hs3_i2s_sck_sleep {
				mux {
					pins = "gpio165";
					function = "gpio";
				};

				config {
					pins = "gpio165";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs3_i2s_sck_active: hs3_i2s_sck_active {
				mux {
					pins = "gpio165";
					function = "hs3_mi2s";
				};

				config {
					pins = "gpio165";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs3_i2s_ws {
			hs3_i2s_ws_sleep: hs3_i2s_ws_sleep {
				mux {
					pins = "gpio166";
					function = "gpio";
				};

				config {
					pins = "gpio166";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs3_i2s_ws_active: hs3_i2s_ws_active {
				mux {
					pins = "gpio166";
					function = "hs3_mi2s";
				};

				config {
					pins = "gpio166";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs3_i2s_data0 {
			hs3_i2s_data0_sleep: hs3_i2s_data0_sleep {
				mux {
					pins = "gpio167";
					function = "gpio";
				};

				config {
					pins = "gpio167";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs3_i2s_data0_active: hs3_i2s_data0_active {
				mux {
					pins = "gpio167";
					function = "hs3_mi2s";
				};

				config {
					pins = "gpio167";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		hs3_i2s_data1 {
			hs3_i2s_data1_sleep: hs3_i2s_data1_sleep {
				mux {
					pins = "gpio168";
					function = "gpio";
				};

				config {
					pins = "gpio168";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			hs3_i2s_data1_active: hs3_i2s_data1_active {
				mux {
					pins = "gpio168";
					function = "hs3_mi2s";
				};

				config {
					pins = "gpio168";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					input-enable;
				};
			};
		};

		emac {
			emac_mdc: emac_mdc {
				mux {
					pins = "gpio7";
					function = "rgmii";
				};

				config {
					pins = "gpio7";
					bias-pull-up;
				};
			};

			emac_mdio: emac_mdio {
				mux {
					pins = "gpio59";
					function = "rgmii";
				};

				config {
					pins = "gpio59";
					bias-pull-up;
				};
			};

			emac_rgmii_txd0: emac_rgmii_txd0 {
				mux {
					pins = "gpio122";
					function = "rgmii";
				};

				config {
					pins = "gpio122";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_txd1: emac_rgmii_txd1 {
				mux {
					pins = "gpio4";
					function = "rgmii";
				};

				config {
					pins = "gpio4";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_txd2: emac_rgmii_txd2 {
				mux {
					pins = "gpio5";
					function = "rgmii";
				};

				config {
					pins = "gpio5";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_txd3: emac_rgmii_txd3 {
				mux {
					pins = "gpio6";
					function = "rgmii";
				};

				config {
					pins = "gpio6";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_txc: emac_rgmii_txc {
				mux {
					pins = "gpio114";
					function = "rgmii";
				};

				config {
					pins = "gpio114";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_tx_ctl: emac_rgmii_tx_ctl {
				mux {
					pins = "gpio121";
					function = "rgmii";
				};

				config {
					pins = "gpio121";
					bias-pull-up;
					drive-strength = <16>;
				};
			};


			emac_rgmii_rxd0: emac_rgmii_rxd0 {
				mux {
					pins = "gpio117";
					function = "rgmii";
				};

				config {
					pins = "gpio117";
					bias-disable;  /* NO pull */
					drive-strength = <2>;  /* 2MA */
				};
			};

			emac_rgmii_rxd1: emac_rgmii_rxd1 {
				mux {
					pins = "gpio118";
					function = "rgmii";
				};

				config {
					pins = "gpio118";
					bias-disable;  /* NO pull */
					drive-strength = <2>;
				};
			};

			emac_rgmii_rxd2: emac_rgmii_rxd2 {
				mux {
					pins = "gpio119";
					function = "rgmii";
				};

				config {
					pins = "gpio119";
					bias-disable;	/* NO pull */
					drive-strength = <2>;
				};
			};

			emac_rgmii_rxd3: emac_rgmii_rxd3 {
				mux {
					pins = "gpio120";
					function = "rgmii";
				};

				config {
					pins = "gpio120";
					bias-disable;	/* NO pull */
					drive-strength = <2>;
				};
			};

			emac_rgmii_rxc: emac_rgmii_rxc {
				mux {
					pins = "gpio115";
					function = "rgmii";
				};

				config {
					pins = "gpio115";
					bias-disable;	/* NO pull */
					drive-strength = <2>;
				};
			};

			emac_rgmii_rx_ctl: emac_rgmii_rx_ctl {
				mux {
					pins = "gpio116";
					function = "rgmii";
				};

				config {
					pins = "gpio116";
					bias-disable;  /* NO pull */
					drive-strength = <2>;
				};
			};

			emac_phy_intr: emac_phy_intr {
				mux {
					pins = "gpio124";
					function = "emac_phy";
				};

				config {
					pins = "gpio124";
					bias-disable;  /* NO pull */
					drive-strength = <8>;
				};
			};

			emac_phy_reset_state: emac_phy_reset_state {
				mux {
					pins = "gpio79";
					function = "gpio";
				};

				config {
					pins = "gpio79";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_pin_pps_0: emac_pin_pps_0 {
				mux {
					pins = "gpio81";
					function = "emac_pps";
				};

				config {
					pins = "gpio81";
					drive-strength = <8>;  /* 8 mA */
					bias-disable;  /* NO PULL*/
				};
			};
		};

		bt_en_active: bt_en_active {
			mux {
				pins = "gpio172";
				function = "gpio";
			};

			config {
				pins = "gpio172";
				drive-strength = <2>;
				output-low;
				bias-pull-down;
			};
		};

		conn_power_1p8_active: conn_power_1p8_active {
			mux {
				pins = "gpio173";
				function = "gpio";
			};

			config {
				pins = "gpio173";
				drive-strength = <2>;
				bias-pull-up;
			};
		};

		conn_power_pa_active: conn_power_pa_active {
			mux {
				pins = "gpio174";
				function = "gpio";
			};

			config {
				pins = "gpio174";
				drive-strength = <2>;
				bias-pull-up;
			};
		};

		usb2phy_ac_en1_default: usb2phy_ac_en1_default {
			mux {
				pins = "gpio113";
				function = "usb2phy_ac";
			};

			config {
				pins = "gpio113";
				drive-strength = <2>;
				bias-disable;
			};
		};

		usb2phy_ac_en2_default: usb2phy_ac_en2_default {
			mux {
				pins = "gpio123";
				function = "usb2phy_ac";
			};

			config {
				pins = "gpio123";
				drive-strength = <2>;
				bias-disable;
			};
		};

		audio_ioexp_reset_active: audio_ioexp_reset_active {
			mux {
				pins = "gpio166";
				function = "gpio";
			};

			config {
				pins = "gpio166";
				drive-strength = <2>;
				bias-disable;
				output-high;
			};
		};

		qcom_clk_led_gp2_pins: qcom_clk_led_gp2_pins {
			qcom_clk_led_gp2_active: qcom_clk_led_gp2_active {
				mux {
					pins = "gpio21";
					function = "gcc_gp2";
				};

				config {
					pins = "gpio21";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qcom_clk_led_gp2_sleep: qqcom_clk_led_gp2_sleep {
				mux {
					pins = "gpio21";
					function = "gpio";
				};

				config {
					pins = "gpio21";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

			sensor_int1_default: sensor_int1_default {
				mux {
					pins = "gpio12";
					function = "gpio";
				};

				config {
					pins = "gpio12";
					drive-strength = <16>; /* 16 mA */
					bias-pull-down; /* pull down */
				};
			};

			sensor_int2_default: sensor_int2_default {
				mux {
					pins = "gpio40";
					function = "gpio";
				};

				config {
					pins = "gpio40";
					drive-strength = <16>; /* 16 ma */
					bias-pull-down; /* pull down */
				};
			};
	};
};
