&soc {
	/* QUPv3 SE Instances
	 * Qup0 0: SE 0
	 * Qup0 1: SE 1
	 * Qup0 2: SE 2
	 * Qup0 3: SE 3
	 * Qup0 4: SE 4
	 * Qup0 5: SE 5
	 * Qup0 6: SE 6
	 * Qup0 7: SE 7
	 */

	/* GPI Instance */
	gpi_dma0: qcom,gpi-dma@4a00000 {
		compatible = "qcom,gpi-dma";
		#dma-cells = <5>;
		reg = <0x4a00000 0x60000>;
		reg-names = "gpi-top";
		iommus = <&apps_smmu 0xf6 0x0>;
		qcom,max-num-gpii = <12>;
		interrupts = <GIC_SPI 335 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 336 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 337 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 338 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 339 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 340 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 341 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 342 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 343 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 344 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 345 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 346 IRQ_TYPE_LEVEL_HIGH>;
		qcom,gpii-mask = <0xf>;
		qcom,ev-factor = <2>;
		qcom,iommu-dma-addr-pool = <0x100000 0x100000>;
		qcom,gpi-ee-offset = <0x10000>;
		status = "ok";
	};

	/* QUPv3_0  wrapper  instance */
	qupv3_0: qcom,qupv3_0_geni_se@4ac0000 {
		compatible = "qcom,geni-se-qup";
		reg = <0x4ac0000 0x2000>;
		#address-cells = <1>;
		#size-cells = <1>;
		clock-names = "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		iommus = <&apps_smmu 0xe3 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0xc0000000>;
		qcom,iommu-geometry = <0x40000000 0x10000000>;
		qcom,iommu-dma = "fastmap";
		ranges;
		status = "ok";

		/* Debug UART Instance */
		qupv3_se6_2uart: qcom,qup_uart@4a98000 {
			compatible = "qcom,geni-debug-uart";
			reg = <0x4a98000 0x4000>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 333 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se";
			clocks = <&gcc GCC_QUPV3_WRAP0_S6_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se6_2uart_tx_active>, <&qupv3_se6_2uart_rx_active>;
			pinctrl-1 = <&qupv3_se6_2uart_sleep>;
			status = "disabled";
		};

		/* HS UART Instance */
		qupv3_se5_4uart: qcom,qup_uart@4a94000 {
			compatible = "qcom,msm-geni-serial-hs";
			reg = <0x4a94000 0x4000>;
			reg-names = "se_phys";
			interrupts-extended = <&intc GIC_SPI 332 IRQ_TYPE_LEVEL_HIGH>,
					<&tlmm 29 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc SLAVE_EBI_CH0>;
			pinctrl-names = "default", "active", "sleep", "shutdown";
			pinctrl-0 = <&qupv3_se5_default_cts>, <&qupv3_se5_default_rts>,
			<&qupv3_se5_default_tx>, <&qupv3_se5_default_rx>;
			pinctrl-1 = <&qupv3_se5_cts>, <&qupv3_se5_rts>,
			<&qupv3_se5_tx>, <&qupv3_se5_rx>;
			pinctrl-2 = <&qupv3_se5_default_cts>, <&qupv3_se5_default_rts>,
			<&qupv3_se5_default_tx>, <&qupv3_se5_default_rx>;
			pinctrl-3 = <&qupv3_se5_default_cts>, <&qupv3_se5_default_rts>,
			<&qupv3_se5_default_tx>, <&qupv3_se5_default_rx>;
			qcom,wakeup-byte = <0xFD>;
			status = "disabled";
		};

		qupv3_se0_i2c: i2c@4a80000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a80000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 327 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se0_i2c_sda_active>, <&qupv3_se0_i2c_scl_active>;
			pinctrl-1 = <&qupv3_se0_i2c_sleep>;
			dmas = <&gpi_dma0 0 0 3 64 0>,
				<&gpi_dma0 1 0 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		qupv3_se0_spi: spi@4a80000 {
			compatible = "qcom,spi-geni";
			reg = <0x4a80000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 327 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se0_spi_mosi_active>, <&qupv3_se0_spi_miso_active>,
				<&qupv3_se0_spi_clk_active>, <&qupv3_se0_spi_cs_active>;
			pinctrl-1 = <&qupv3_se0_spi_sleep>;
			dmas = <&gpi_dma0 0 0 1 64 0>,
				<&gpi_dma0 1 0 1 64 0>;
			dma-names = "tx", "rx";
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se1_i2c: i2c@4a84000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a84000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 328 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S1_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se1_i2c_sda_active>, <&qupv3_se1_i2c_scl_active>;
			pinctrl-1 = <&qupv3_se1_i2c_sleep>;
			dmas = <&gpi_dma0 1 0 3 64 0>,
				<&gpi_dma0 1 1 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		qupv3_se1_spi: spi@4a84000 {
			compatible = "qcom,spi-geni";
			reg = <0x4a84000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 328 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S1_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se1_spi_mosi_active>, <&qupv3_se1_spi_miso_active>,
				<&qupv3_se1_spi_clk_active>, <&qupv3_se1_spi_cs_active>;
			pinctrl-1 = <&qupv3_se1_spi_sleep>;
			dmas = <&gpi_dma0 0 1 1 64 0>,
				<&gpi_dma0 1 1 1 64 0>;
			dma-names = "tx", "rx";
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se2_i2c: i2c@4a88000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a88000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 329 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se2_i2c_sda_active>, <&qupv3_se2_i2c_scl_active>;
			pinctrl-1 = <&qupv3_se2_i2c_sleep>;
			dmas = <&gpi_dma0 0 2 3 64 0>,
				<&gpi_dma0 1 2 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		qupv3_se2_spi: spi@4a88000 {
			compatible = "qcom,spi-geni";
			reg = <0x4a88000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 329 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se2_spi_mosi_active>, <&qupv3_se2_spi_miso_active>,
				<&qupv3_se2_spi_clk_active>, <&qupv3_se2_spi_cs_active>;
			pinctrl-1 = <&qupv3_se2_spi_sleep>;
			dmas = <&gpi_dma0 0 2 1 64 0>,
				<&gpi_dma0 1 2 1 64 0>;
			dma-names = "tx", "rx";
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se3_i2c: i2c@4a8c000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a8c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 330 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se3_i2c_sda_active>, <&qupv3_se3_i2c_scl_active>;
			pinctrl-1 = <&qupv3_se3_i2c_sleep>;
			dmas = <&gpi_dma0 0 3 3 64 0>,
				<&gpi_dma0 1 3 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		qupv3_se3_spi: spi@4a8c000 {
			compatible = "qcom,spi-geni";
			reg = <0x4a8c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 330 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se3_spi_mosi_active>, <&qupv3_se3_spi_miso_active>,
				<&qupv3_se3_spi_clk_active>, <&qupv3_se3_spi_cs_active>;
			pinctrl-1 = <&qupv3_se3_spi_sleep>;
			dmas = <&gpi_dma0 0 3 1 64 0>,
				<&gpi_dma0 1 3 1 64 0>;
			dma-names = "tx", "rx";
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se4_i2c: i2c@4a90000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a90000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 331 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S4_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se4_i2c_sda_active>, <&qupv3_se4_i2c_scl_active>;
			pinctrl-1 = <&qupv3_se4_i2c_sleep>;
			dmas = <&gpi_dma0 0 4 3 64 0>,
				<&gpi_dma0 1 4 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		qupv3_se4_spi: spi@4a90000 {
			compatible = "qcom,spi-geni";
			reg = <0x4a90000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 331 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S4_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se4_spi_mosi_active>, <&qupv3_se4_spi_miso_active>,
				<&qupv3_se4_spi_clk_active>, <&qupv3_se4_spi_cs_active>;
			pinctrl-1 = <&qupv3_se4_spi_sleep>;
			dmas = <&gpi_dma0 0 4 1 64 0>,
				<&gpi_dma0 1 4 1 64 0>;
			dma-names = "tx", "rx";
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se5_i2c: i2c@4a94000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a94000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 332 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se5_i2c_sda_active>, <&qupv3_se5_i2c_scl_active>;
			pinctrl-1 = <&qupv3_se5_i2c_sleep>;
			dmas = <&gpi_dma0 0 5 3 64 0>,
				<&gpi_dma0 1 5 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		qupv3_se5_spi: spi@4a94000 {
			compatible = "qcom,spi-geni";
			reg = <0x4a94000 0x4000>;
			reg-names = "se_phys";
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 332 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se5_spi_mosi_active>, <&qupv3_se5_spi_miso_active>,
				<&qupv3_se5_spi_clk_active>, <&qupv3_se5_spi_cs_active>;
			pinctrl-1 = <&qupv3_se5_spi_sleep>;
			dmas = <&gpi_dma0 0 5 1 64 0>,
				<&gpi_dma0 1 5 1 64 0>;
			dma-names = "tx", "rx";
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se6_i2c: i2c@4a98000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a98000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 333 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S6_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se6_i2c_sda_active>, <&qupv3_se6_i2c_scl_active>;
			pinctrl-1 = <&qupv3_se6_i2c_sleep>;
			dmas = <&gpi_dma0 0 6 3 64 0>,
				<&gpi_dma0 1 6 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		qupv3_se6_spi: spi@4a98000 {
			compatible = "qcom,spi-geni";
			reg = <0x4a98000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 333 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S6_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se6_spi_mosi_active>, <&qupv3_se6_spi_miso_active>,
				<&qupv3_se6_spi_clk_active>, <&qupv3_se6_spi_cs_active>;
			pinctrl-1 = <&qupv3_se6_spi_sleep>;
			dmas = <&gpi_dma0 0 6 1 64 0>,
				<&gpi_dma0 1 6 1 64 0>;
			dma-names = "tx", "rx";
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se7_i2c_a: i2c_a@4a9c000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a9c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 334 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S7_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc  SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se7_i2c_sda_a>, <&qupv3_se7_i2c_scl_a>;
			pinctrl-1 = <&qupv3_se7_i2c_sleep_a>;
			dmas = <&gpi_dma0 0 7 3 64 0>,
				<&gpi_dma0 1 7 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};

		qupv3_se7_spi_a: spi@4a9c000 {
			compatible = "qcom,spi-geni";
			reg = <0x4a9c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 334 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S7_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se7_spi_mosi_a>, <&qupv3_se7_spi_miso_a>,
				<&qupv3_se7_spi_clk_a>, <&qupv3_se7_spi_cs_a>;
			pinctrl-1 = <&qupv3_se0_spi_sleep>;
			dmas = <&gpi_dma0 0 7 1 64 0>,
				<&gpi_dma0 1 7 1 64 0>;
			dma-names = "tx", "rx";
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se7_i2c_b: i2c_b@4a9c000 {
			compatible = "qcom,i2c-geni";
			reg = <0x4a9c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 334 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S7_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&bimc MASTER_AMPSS_M0 &config_noc SLAVE_QUP_0>,
			<&system_noc MASTER_QUP_0 &bimc SLAVE_EBI_CH0>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se7_i2c_sda_b>, <&qupv3_se7_i2c_scl_b>;
			pinctrl-1 = <&qupv3_se7_i2c_sleep_b>;
			dmas = <&gpi_dma0 0 7 3 64 0>,
				<&gpi_dma0 1 7 3 64 0>;
			dma-names = "tx", "rx";
			status = "disabled";
		};
	};
};
