#include <dt-bindings/regulator/qcom,rpmh-regulator-levels.h>

&apps_rsc_drv2 {
	rpmh-regulator-cxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "cx.lvl";
		proxy-supply = <&VDD_CX_LEVEL>;

		VDD_CX_LEVEL: S1A_LEVEL:
		pm8775_a_s1_level: regulator-pm8775_a-s1-level {
			regulator-name = "pm8775_a_s1_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_CX_LEVEL_AO: S1A_LEVEL_AO:
		pm8775_a_s1_level_ao: regulator-pm8775_a-s1-level-ao {
			regulator-name = "pm8775_a_s1_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-gfxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "gfx.lvl";

		VDD_GFX_LEVEL: S6A_LEVEL:
		pm8775_a_s6_level: regulator-pm8775_a-s6-level {
			regulator-name = "pm8775_a_s6_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-lmxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "lmx.lvl";

		VDD_LPI_MX_LEVEL: L1A_LEVEL:
		pm8775_a_l1_level: regulator-pm8775_a-l1-level {
			regulator-name = "pm8775_a_l1_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-lcxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "lcx.lvl";

		VDD_LPI_CX_LEVEL: L2A_LEVEL:
		pm8775_a_l2_level: regulator-pm8775_a-l2-level {
			regulator-name = "pm8775_a_l2_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-mxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mx.lvl";
		proxy-supply = <&VDD_MXA_LEVEL>;

		VDD_MXA_LEVEL: S1C_LEVEL:
		pm8775_c_s1_level: regulator-pm8775_c-s1-level {
			regulator-name = "pm8775_c_s1_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MXA_LEVEL_AO: S1C_LEVEL_AO:
		pm8775_c_s1_level_ao: regulator-pm8775_c-s1-level-ao {
			regulator-name = "pm8775_c_s1_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-mmcxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mmcx.lvl";
		proxy-supply = <&VDD_MMCX_LEVEL>;

		VDD_MMCX_LEVEL: VDD_MM_LEVEL: S3C_LEVEL:
		pm8775_c_s3_level: regulator-pm8775_c-s3-level {
			regulator-name = "pm8775_c_s3_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MMCX_LEVEL_AO: S3C_LEVEL_AO:
		pm8775_c_s3_level_ao: regulator-pm8775_c-s3-level-ao {
			regulator-name = "pm8775_c_s3_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-nsp0lvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "nsp0.lvl";

		VDD_NSP_0_LEVEL: S6C_LEVEL:
		pm8775_c_s6_level: regulator-pm8775_c-s6-level {
			regulator-name = "pm8775_c_s6_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-mxclvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mxc.lvl";
		proxy-supply = <&VDD_MXC_LEVEL>;

		VDD_MXC_LEVEL: S5E_LEVEL:
		pm8775_e_s5_level: regulator-pm8775_e-s5-level {
			regulator-name = "pm8775_e_s5_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MXC_LEVEL_AO: S5E_LEVEL_AO:
		pm8775_e_s5_level_ao: regulator-pm8775_e-s5-level-ao {
			regulator-name = "pm8775_e_s5_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};

		VDD_MXC_MMCX_VOTER_LEVEL: VDD_MXC_MM_VOTER_LEVEL:
		VDD_MM_MXC_VOTER_LEVEL:
		regulator-pm8775_e-s5-mmcx-voter-level {
			regulator-name = "pm8775_e_s5_mmcx_voter_level";
			vin-supply = <&VDD_MMCX_LEVEL>;
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
		};

		VDD_MXC_GFX_VOTER_LEVEL: VDD_GFX_MXC_VOTER_LEVEL:
		VDD_GX_MXC_VOTER_LEVEL:
		regulator-pm8775_e-s5-gfx-voter-level {
			regulator-name = "pm8775_e_s5_gfx_voter_level";
			pm8775_e_s5_gfx_voter_level-parent-supply =
				<&VDD_GFX_LEVEL>;
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
		};
	};

	rpmh-regulator-ebilvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "ebi.lvl";

		VDD_EBI_LEVEL: S8E_LEVEL:
		pm8775_e_s8_level: regulator-pm8775_e-s8-level {
			regulator-name = "pm8775_e_s8_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-nsp1lvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "nsp1.lvl";

		VDD_NSP_1_LEVEL: S1G_LEVEL:
		pm8775_g_s1_level: regulator-pm8775_g-s1-level {
			regulator-name = "pm8775_g_s1_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-smpa4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpa4";

		S4A:
		pm8775_a_s4: regulator-pm8775_a-s4 {
			regulator-name = "pm8775_a_s4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1620000>;
			regulator-max-microvolt = <2000000>;
			qcom,init-voltage = <1800000>;
		};
	};

	rpmh-regulator-smpa5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpa5";

		S5A:
		pm8775_a_s5: regulator-pm8775_a-s5 {
			regulator-name = "pm8775_a_s5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1850000>;
			regulator-max-microvolt = <2100000>;
			qcom,init-voltage = <1850000>;
		};
	};

	rpmh-regulator-smpa9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpa9";

		S9A:
		pm8775_a_s9: regulator-pm8775_a-s9 {
			regulator-name = "pm8775_a_s9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <535000>;
			regulator-max-microvolt = <1120000>;
			qcom,init-voltage = <1000000>;
		};
	};

	rpmh-regulator-ldoa4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoa4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L4A:
		pm8775_a_l4: regulator-pm8775_a-l4 {
			regulator-name = "pm8775_a_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <788000>;
			regulator-max-microvolt = <1050000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoa5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoa5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L5A:
		pm8775_a_l5: regulator-pm8775_a-l5 {
			regulator-name = "pm8775_a_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <870000>;
			regulator-max-microvolt = <950000>;
			qcom,init-voltage = <870000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoa6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoa6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L6A:
		pm8775_a_l6: regulator-pm8775_a-l6 {
			regulator-name = "pm8775_a_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <870000>;
			regulator-max-microvolt = <970000>;
			qcom,init-voltage = <900000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoa7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoa7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L7A:
		pm8775_a_l7: regulator-pm8775_a-l7 {
			regulator-name = "pm8775_a_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <830000>;
			regulator-max-microvolt = <920000>;
			regulator-always-on;
			qcom,init-voltage = <880000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoa8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoa8";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;

		L8A:
		pm8775_a_l8: regulator-pm8775_a-l8 {
			regulator-name = "pm8775_a_l8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2400000>;
			regulator-max-microvolt = <3300000>;
			qcom,init-voltage = <2960000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoa9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoa9";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L9A:
		pm8775_a_l9: regulator-pm8775_a-l9 {
			regulator-name = "pm8775_a_l9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2970000>;
			regulator-max-microvolt = <3544000>;
			qcom,init-voltage = <3072000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L1C:
		pm8775_c_l1: regulator-pm8775_c-l1 {
			regulator-name = "pm8775_c_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1140000>;
			regulator-max-microvolt = <1260000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L2C:
		pm8775_c_l2: regulator-pm8775_c-l2 {
			regulator-name = "pm8775_c_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <900000>;
			regulator-max-microvolt = <1100000>;
			qcom,init-voltage = <900000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L3C:
		pm8775_c_l3: regulator-pm8775_c-l3 {
			regulator-name = "pm8775_c_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1100000>;
			regulator-max-microvolt = <1300000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L4C:
		pm8775_c_l4: regulator-pm8775_c-l4 {
			regulator-name = "pm8775_c_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1100000>;
			regulator-max-microvolt = <1300000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L5C:
		pm8775_c_l5: regulator-pm8775_c-l5 {
			regulator-name = "pm8775_c_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1100000>;
			regulator-max-microvolt = <1300000>;
			qcom,init-voltage = <1100000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L6C:
		pm8775_c_l6: regulator-pm8775_c-l6 {
			regulator-name = "pm8775_c_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1620000>;
			regulator-max-microvolt = <1980000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L7C:
		pm8775_c_l7: regulator-pm8775_c-l7 {
			regulator-name = "pm8775_c_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1620000>;
			regulator-max-microvolt = <2000000>;
			qcom,init-voltage = <1620000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc8";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;

		L8C:
		pm8775_c_l8: regulator-pm8775_c-l8 {
			regulator-name = "pm8775_c_l8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2400000>;
			regulator-max-microvolt = <3300000>;
			qcom,init-voltage = <2400000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoc9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc9";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L9C:
		pm8775_c_l9: regulator-pm8775_c-l9 {
			regulator-name = "pm8775_c_l9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1650000>;
			regulator-max-microvolt = <2700000>;
			qcom,init-voltage = <1650000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-smpe4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe4";

		S4E:
		pm8775_e_s4: regulator-pm8775_e-s4 {
			regulator-name = "pm8775_e_s4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <970000>;
			regulator-max-microvolt = <1520000>;
			qcom,init-voltage = <1352000>;
		};
	};

	rpmh-regulator-smpe7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe7";

		S7E:
		pm8775_e_s7: regulator-pm8775_e-s7 {
			regulator-name = "pm8775_e_s7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1010000>;
			regulator-max-microvolt = <1170000>;
			qcom,init-voltage = <1100000>;
		};
	};

	rpmh-regulator-smpe9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe9";

		S9E:
		pm8775_e_s9: regulator-pm8775_e-s9 {
			regulator-name = "pm8775_e_s9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <300000>;
			regulator-max-microvolt = <570000>;
			qcom,init-voltage = <500000>;
		};
	};

	rpmh-regulator-ldoe6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;

		L6E:
		pm8775_e_l6: regulator-pm8775_e-l6 {
			regulator-name = "pm8775_e_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1280000>;
			regulator-max-microvolt = <1450000>;
			qcom,init-voltage = <1280000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};

	rpmh-regulator-ldoe8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe8";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;

		L8E:
		pm8775_e_l8: regulator-pm8775_e-l8 {
			regulator-name = "pm8775_e_l8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1950000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode =
				<RPMH_REGULATOR_MODE_LPM>;
		};
	};
};
