#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/soc/qcom,rpmh-rsc.h>
#include <dt-bindings/clock/qcom,rpmh.h>
#include <dt-bindings/clock/qcom,gcc-sm8150.h>
#include <dt-bindings/clock/qcom,aop-qmp.h>
#include <dt-bindings/clock/qcom,camcc-sm8150.h>
#include <dt-bindings/clock/qcom,dispcc-sm8150.h>
#include <dt-bindings/clock/qcom,gpucc-sm8150.h>
#include <dt-bindings/clock/qcom,npucc-sm8150.h>
#include <dt-bindings/clock/qcom,scc-sm8150.h>
#include <dt-bindings/clock/qcom,videocc-sm8150.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interconnect/qcom,icc.h>
#include <dt-bindings/interconnect/qcom,sm8150.h>
#include <dt-bindings/regulator/qcom,rpmh-regulator-levels.h>
#include <dt-bindings/spmi/spmi.h>

/ {
	model = "Qualcomm Technologies, Inc. SM8150";
	compatible = "qcom,sm8150";
	qcom,msm-name = "SM8150 V1";
	qcom,msm-id = <339 0x10000>;
	interrupt-parent = <&intc>;

	#address-cells = <2>;
	#size-cells = <2>;
	memory { device_type = "memory"; reg = <0 0 0 0>; };
	ddr-regions { };

	aliases {
		mmc1 = &sdhc_2; /* SDC2 SD card slot */
		pci-domain0 = &pcie0; /* PCIe0 domain */
		pci-domain1 = &pcie1; /* PCIe1 domain */
		serial0 = &qupv3_se12_2uart;
		hsuart0 = &qupv3_se17_4uart;
		hsuart1 = &qupv3_se9_2uart;
		ufshc1 = &ufshc_mem; /* Embedded UFS slot */
		spi22 = &qupv3_se22_spi;
		i2c7 = &qupv3_se20_i2c;
	};

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		CPU0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0 0x0>;
			enable-method = "psci";
			cpu-idle-states = <&SILVER_OFF>;
			power-domains = <&CPU_PD0>;
			power-domain-names = "psci";
			capacity-dmips-mhz = <1024>;
			i-cache-size = <0x8000>;
			d-cache-size = <0x8000>;
			next-level-cache = <&L2_0>;
			qcom,freq-domain = <&cpufreq_hw 0 4>;
			dynamic-power-coefficient = <100>;
			#cooling-cells = <2>;
			L2_0: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-size = <0x20000>;
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;

				L3_0: l3-cache {
				      compatible = "arm,arch-cache";
				      cache-size = <0x200000>;
				      cache-level = <3>;
				};
			};
		};

		CPU1: cpu@100 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0 0x100>;
			enable-method = "psci";
			cpu-idle-states = <&SILVER_OFF>;
			power-domains = <&CPU_PD1>;
			power-domain-names = "psci";
			capacity-dmips-mhz = <1024>;
			i-cache-size = <0x8000>;
			d-cache-size = <0x8000>;
			next-level-cache = <&L2_1>;
			qcom,freq-domain = <&cpufreq_hw 0 4>;
			dynamic-power-coefficient = <100>;
			L2_1: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-size = <0x20000>;
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU2: cpu@200 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0 0x200>;
			enable-method = "psci";
			cpu-idle-states = <&SILVER_OFF>;
			power-domains = <&CPU_PD2>;
			power-domain-names = "psci";
			capacity-dmips-mhz = <1024>;
			i-cache-size = <0x8000>;
			d-cache-size = <0x8000>;
			next-level-cache = <&L2_2>;
			qcom,freq-domain = <&cpufreq_hw 0 4>;
			dynamic-power-coefficient = <100>;
			L2_2: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-size = <0x20000>;
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU3: cpu@300 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0 0x300>;
			enable-method = "psci";
			cpu-idle-states = <&SILVER_OFF>;
			power-domains = <&CPU_PD3>;
			power-domain-names = "psci";
			capacity-dmips-mhz = <1024>;
			i-cache-size = <0x8000>;
			d-cache-size = <0x8000>;
			next-level-cache = <&L2_3>;
			qcom,freq-domain = <&cpufreq_hw 0 4>;
			dynamic-power-coefficient = <100>;
			L2_3: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-size = <0x20000>;
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU4: cpu@400 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0 0x400>;
			enable-method = "psci";
			cpu-idle-states = <&GOLD_OFF>;
			power-domains = <&CPU_PD4>;
			power-domain-names = "psci";
			capacity-dmips-mhz = <1740>;
			i-cache-size = <0x10000>;
			d-cache-size = <0x10000>;
			next-level-cache = <&L2_4>;
			qcom,freq-domain = <&cpufreq_hw 1 4>;
			dynamic-power-coefficient = <374>;
			#cooling-cells = <2>;
			L2_4: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-size = <0x40000>;
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU5: cpu@500 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0 0x500>;
			enable-method = "psci";
			cpu-idle-states = <&GOLD_OFF>;
			power-domains = <&CPU_PD5>;
			power-domain-names = "psci";
			capacity-dmips-mhz = <1740>;
			i-cache-size = <0x10000>;
			d-cache-size = <0x10000>;
			next-level-cache = <&L2_5>;
			qcom,freq-domain = <&cpufreq_hw 1 4>;
			dynamic-power-coefficient = <374>;
			L2_5: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-size = <0x40000>;
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU6: cpu@600 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0 0x600>;
			enable-method = "psci";
			cpu-idle-states = <&GOLD_OFF>;
			power-domains = <&CPU_PD6>;
			power-domain-names = "psci";
			capacity-dmips-mhz = <1740>;
			i-cache-size = <0x10000>;
			d-cache-size = <0x10000>;
			next-level-cache = <&L2_6>;
			qcom,freq-domain = <&cpufreq_hw 1 4>;
			dynamic-power-coefficient = <374>;
			L2_6: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-size = <0x40000>;
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU7: cpu@700 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0 0x700>;
			enable-method = "psci";
			cpu-idle-states = <&GOLD_OFF>;
			power-domains = <&CPU_PD7>;
			power-domain-names = "psci";
			capacity-dmips-mhz = <1740>;
			i-cache-size = <0x10000>;
			d-cache-size = <0x10000>;
			next-level-cache = <&L2_7>;
			qcom,freq-domain = <&cpufreq_hw 2 4>;
			dynamic-power-coefficient = <431>;
			#cooling-cells = <2>;
			L2_7: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-size = <0x80000>;
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		cpu-map {
			cluster0 {
				core0 {
					cpu = <&CPU0>;
				};

				core1 {
					cpu = <&CPU1>;
				};

				core2 {
					cpu = <&CPU2>;
				};

				core3 {
					cpu = <&CPU3>;
				};
			};

			cluster1 {
				core0 {
					cpu = <&CPU4>;
				};

				core1 {
					cpu = <&CPU5>;
				};

				core2 {
					cpu = <&CPU6>;
				};
			};

			cluster2 {
				core0 {
					cpu = <&CPU7>;
				};
			};
		};
	};

	idle-states {
		SILVER_OFF: silver-c4 {  /* C4 */
			compatible = "arm,idle-state";
			idle-state-name = "rail-pc";
			entry-latency-us = <355>;
			exit-latency-us = <909>;
			min-residency-us = <3934>;
			arm,psci-suspend-param = <0x40000004>;
			local-timer-stop;
		};

		GOLD_OFF: gold-c4 {  /* C4 */
			compatible = "arm,idle-state";
			idle-state-name = "rail-pc";
			entry-latency-us = <2411>;
			exit-latency-us = <1461>;
			min-residency-us = <4488>;
			arm,psci-suspend-param = <0x40000004>;
			local-timer-stop;
		};

		APSS_OFF: cluster-e3 { /* E3 */
			compatible = "domain-idle-state";
			idle-state-name = "llcc-off";
			entry-latency-us = <3263>;
			exit-latency-us = <6562>;
			min-residency-us = <9987>;
			arm,psci-suspend-param = <0x4100c344>;
		};
	};

	psci {
		compatible = "arm,psci-1.0";
		method = "smc";

		CPU_PD0: cpu-pd0 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD1: cpu-pd1 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD2: cpu-pd2 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD3: cpu-pd3 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD4: cpu-pd4 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD5: cpu-pd5 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD6: cpu-pd6 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD7: cpu-pd7 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CLUSTER_PD: cluster-pd {
			#power-domain-cells = <0>;
			domain-idle-states = <&APSS_OFF>;
		};
	};

	chosen: chosen {
		bootargs = "qcom_dma_heaps.enable_bitstream_contig_heap=y kpti=0 ssbd=force-off";
	};

	soc: soc { };

	firmware: firmware { };

	reserved_memory: reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		hyp_mem: hyp_mem {
			no-map;
			reg = <0x0 0x85700000 0x0 0x600000>;
		};

		xbl_mem: xbl_mem {
			no-map;
			reg = <0x0 0x85e00000 0x0 0x100000>;
		};

		aop_mem: memory@85f00000 {
			reg = <0x0 0x85f00000 0x0 0x20000>;
			no-map;
		};

		aop_cmd_db: memory@85f20000 {
			compatible = "qcom,cmd-db";
			reg = <0x0 0x85f20000 0x0 0x20000>;
			no-map;
		};

		smem_region: smem {
			no-map;
			reg = <0x0 0x86000000 0x0 0x200000>;
		};

		removed_regions: removed_regions {
			no-map;
			reg = <0x0 0x86200000 0x0 0x5500000>;
		};

		pil_camera_mem: camera_region {
			no-map;
			reg = <0x0 0x8b700000 0x0 0x500000>;
		};

		pil_wlan_fw_mem: pil_wlan_fw_region {
			no-map;
			reg = <0x0 0x8bc00000 0x0 0x180000>;
		};

		pil_npu_mem: pil_npu_region {
			no-map;
			reg = <0x0 0x8bd80000 0x0 0x80000>;
		};

		rproc_adsp_mem: rproc_adsp_region {
			no-map;
			reg = <0x0 0x8be00000 0x0 0x1a00000>;
		};

		pil_modem_mem: modem_region {
			no-map;
			reg = <0x0 0x8d800000 0x0 0x4c1c000>;
		};

		pil_video_mem: pil_video_region {
			no-map;
			reg = <0x0 0x96e00000 0x0 0x500000>;
		};

		pil_slpi_mem: pil_slpi_region {
			no-map;
			reg = <0x0 0x97300000 0x0 0x1400000>;
		};

		pil_ipa_fw_mem: pil_ipa_fw_region {
			no-map;
			reg = <0x0 0x98700000 0x0 0x10000>;
		};

		pil_ipa_gsi_mem: pil_ipa_gsi_region {
			no-map;
			reg = <0x0 0x98710000 0x0 0x5000>;
		};

		gpu_micro_code_mem: gpu_micro_code_region {
			no-map;
			reg = <0x0 0x98715000 0x0 0x2000>;
		};

		pil_spss_mem: pil_spss_region {
			no-map;
			reg = <0x0 0x98800000 0x0 0x100000>;
		};

		rproc_cdsp_mem: rproc_cdsp_region {
			no-map;
			reg = <0x0 0x98900000 0x0 0x1400000>;
		};

		qseecom_mem: qseecom_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1400000>;
		};

		cdsp_sec_mem: cdsp_sec_regions {
			no-map;
			reg = <0x0 0xa4c00000 0x0 0x3c00000>;
		};

		cont_splash_memory: cont_splash_region {
			reg = <0x0 0x9c000000 0x0 0x2400000>;
			label = "cont_splash_region";
		};

		disp_rdump_memory: disp_rdump_region {
			reg = <0x0 0x9c000000 0x0 0x02400000>;
			label = "disp_rdump_region";
		};

		adsp_mem: adsp_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1000000>;
		};

		cdsp_mem: cdsp_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x400000>;
		};

		user_contig_mem: user_contig_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1000000>;
		};

		qseecom_ta_mem: qseecom_ta_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1000000>;
		};

		sp_mem: sp_region {  /* SPSS-HLOS ION shared mem */
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x800000>;
		};

		secure_display_memory: secure_display_region { /* Secure UI */
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0xA000000>;
		};

		dump_mem: mem_dump_region {
			compatible = "shared-dma-pool";
			reusable;
			size = <0 0x2400000>;
		};

		/* global autoconfigured region for contiguous allocations */
		system_cma: linux,cma {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x2800000>;
			linux,cma-default;
		};
	};

	clocks {
		xo_board: xo-board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <38400000>;
			clock-output-names = "xo_board";
		};

		sleep_clk: sleep-clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32764>;
			clock-output-names = "sleep_clk";
		};
	};
};

&soc {
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0 0 0 0xffffffff>;
	compatible = "simple-bus";

	intc: interrupt-controller@17a00000 {
		compatible = "arm,gic-v3";
		#interrupt-cells = <3>;
		interrupt-controller;
		#redistributor-regions = <1>;
		redistributor-stride = <0x0 0x20000>;
		reg = <0x17a00000 0x10000>,     /* GICD */
		      <0x17a60000 0x100000>;    /* GICR * 8 */
		interrupts = <GIC_PPI 9 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-parent = <&intc>;
	};

	pdc: interrupt-controller@b220000 {
		compatible = "qcom,sm8150-pdc", "qcom,pdc";
		reg = <0xb220000 0x30000>, <0x17c000f0 0x64>;
		qcom,pdc-ranges = <0 480 94>, <94 609 31>, <125 63 1>;
		#interrupt-cells = <2>;
		interrupt-parent = <&intc>;
		interrupt-controller;
	};

	arch_timer: timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 1 (GIC_CPU_MASK_SIMPLE(8) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 2 (GIC_CPU_MASK_SIMPLE(8) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 3 (GIC_CPU_MASK_SIMPLE(8) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 0 (GIC_CPU_MASK_SIMPLE(8) | IRQ_TYPE_LEVEL_LOW)>;
		clock-frequency = <19200000>;
	};

	timer@17c20000 {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "arm,armv7-timer-mem";
		reg = <0x17c20000 0x1000>;
		clock-frequency = <19200000>;

		frame@17c21000 {
			frame-number = <0>;
			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c21000 0x1000>,
			      <0x17c22000 0x1000>;
		};

		frame@17c23000 {
			frame-number = <1>;
			interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c23000 0x1000>;
			status = "disabled";
		};

		frame@17c25000 {
			frame-number = <2>;
			interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c25000 0x1000>;
			status = "disabled";
		};

		frame@17c27000 {
			frame-number = <3>;
			interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c26000 0x1000>;
			status = "disabled";
		};

		frame@17c29000 {
			frame-number = <4>;
			interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c29000 0x1000>;
			status = "disabled";
		};

		frame@17c2b000 {
			frame-number = <5>;
			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c2b000 0x1000>;
			status = "disabled";
		};

		frame@17c2d000 {
			frame-number = <6>;
			interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c2d000 0x1000>;
			status = "disabled";
		};
	};

	qcom,mpm2-sleep-counter@c221000 {
		compatible = "qcom,mpm2-sleep-counter";
		reg = <0xc221000 0x1000>;
		clock-frequency = <32768>;
	};

	qcom,msm-imem@146bf000 {
		compatible = "qcom,msm-imem";
		reg = <0x146bf000 0x1000>;
		ranges = <0x0 0x146bf000 0x1000>;
		#address-cells = <1>;
		#size-cells = <1>;

		mem_dump_table@10 {
			compatible = "qcom,msm-imem-mem_dump_table";
			reg = <0x10 0x8>;
		};

		dload_type@1c {
			compatible = "qcom,msm-imem-dload-type";
			reg = <0x1c 0x4>;
		};

		kaslr_offset@6d0 {
			compatible = "qcom,msm-imem-kaslr_offset";
			reg = <0x6d0 0xc>;
		};

		boot_stats@6b0 {
			compatible = "qcom,msm-imem-boot_stats";
			reg = <0x6b0 0x20>;
		};

		diag_dload@c8 {
			compatible = "qcom,msm-imem-diag-dload";
			reg = <0xc8 0xc8>;
		};
	};

	cpu_pmu: cpu-pmu {
		compatible = "arm,armv8-pmuv3";
		interrupts = <GIC_PPI 5 IRQ_TYPE_LEVEL_HIGH>;
	};

	qcom,msm-rtb {
		compatible = "qcom,msm-rtb";
		qcom,rtb-size = <0x100000>;
	};

	dload_mode {
		compatible = "qcom,dload-mode";
	};

	mini_dump_mode {
		compatible = "qcom,minidump";
		status = "ok";
	};

	vendor_hooks: qcom,cpu-vendor-hooks {
		compatible = "qcom,cpu-vendor-hooks";
	};

	logbuf: qcom,logbuf-vendor-hooks {
		compatible = "qcom,logbuf-vendor-hooks";
	};

	tcsr: syscon@1fc0000 {
		compatible = "syscon";
		reg = <0x1fc0000 0x30000>;
	};

	apps_rsc: rsc@18200000 {
		label = "apps_rsc";
		compatible = "qcom,rpmh-rsc";
		reg = <0x18200000 0x10000>,
		      <0x18210000 0x10000>,
		      <0x18220000 0x10000>;
		reg-names = "drv-0", "drv-1", "drv-2";
		qcom,drv-count = <3>;
		interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
		power-domains = <&CLUSTER_PD>;

		apps_rsc_drv2: drv@2 {
			qcom,drv-id = <2>;
			qcom,tcs-offset = <0xd00>;
			channel@0 {
				qcom,tcs-config = <ACTIVE_TCS    2>,
						  <SLEEP_TCS     3>,
						  <WAKE_TCS      3>,
						  <CONTROL_TCS   1>,
						  <FAST_PATH_TCS 0>;
			};

			rpmhcc: clock-controller {
				compatible = "qcom,sm8150-rpmh-clk";
				#clock-cells = <1>;
				clock-names = "xo";
				clocks = <&xo_board>;
				status = "okay";
			};

			apps_bcm_voter: bcm_voter {
				compatible = "qcom,bcm-voter";
			};
		};
	};

	cluster-device {
		compatible = "qcom,lpm-cluster-dev";
		power-domains = <&CLUSTER_PD>;
	};

	disp_rsc: rsc@af20000 {
		label = "disp_rsc";
		compatible = "qcom,rpmh-rsc";
		reg = <0xaf20000 0x10000>;
		reg-names = "drv-0";
		qcom,drv-count = <1>;
		interrupts = <GIC_SPI 129 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&dispcc DISP_CC_MDSS_RSCC_AHB_CLK>;

		disp_rsc_drv0: drv@0 {
			qcom,drv-id = <0>;
			qcom,tcs-offset = <0x1c00>;
			channel@0 {
				qcom,tcs-config = <SLEEP_TCS     1>,
						  <WAKE_TCS      1>,
						  <ACTIVE_TCS    2>,
						  <CONTROL_TCS   0>,
						  <FAST_PATH_TCS 0>;
			};

			disp_bcm_voter: bcm_voter {
				compatible = "qcom,bcm-voter";
				qcom,tcs-wait = <QCOM_ICC_TAG_AMC>;
			};
		};
	};

	gcc: clock-controller@100000 {
		compatible = "qcom,sm8150-gcc", "syscon";
		reg = <0x100000 0x1f0000>;
		reg-names = "cc_base";
		vdd_cx-supply = <&VDD_CX_LEVEL>;
		vdd_cx_ao-supply = <&VDD_CX_LEVEL_AO>;
		vdd_mm-supply = <&VDD_MMCX_LEVEL>;
		clocks = <&rpmhcc RPMH_CXO_CLK>, <&rpmhcc RPMH_CXO_CLK_A>,
			 <&sleep_clk>;
		clock-names = "bi_tcxo", "bi_tcxo_ao", "sleep_clk";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	videocc: clock-controller@ab00000 {
		compatible = "qcom,sm8150-videocc", "syscon";
		reg = <0xab00000 0x10000>;
		reg-names = "cc_base";
		vdd_mm-supply = <&VDD_MMCX_LEVEL>;
		clocks = <&gcc GCC_VIDEO_AHB_CLK>, <&rpmhcc RPMH_CXO_CLK>;
		clock-names = "iface", "bi_tcxo";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	camcc: clock-controller@ad00000 {
		compatible = "qcom,sm8150-camcc", "syscon";
		reg = <0xad00000 0x10000>;
		reg-names = "cc_base";
		vdd_mx-supply = <&VDD_MX_LEVEL>;
		vdd_mm-supply = <&VDD_MMCX_LEVEL>;
		clocks = <&gcc GCC_CAMERA_AHB_CLK>, <&rpmhcc RPMH_CXO_CLK>;
		clock-names = "iface", "bi_tcxo";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	dispcc: clock-controller@af00000 {
		compatible = "qcom,sm8150-dispcc", "syscon";
		reg = <0xaf00000 0x20000>;
		reg-names = "cc_base";
		vdd_mm-supply = <&VDD_MMCX_LEVEL>;
		clocks = <&gcc GCC_DISP_AHB_CLK>, <&rpmhcc RPMH_CXO_CLK>;
		clock-names = "iface", "bi_tcxo";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	npucc: clock-controller@9910000 {
		compatible = "qcom,sm8150-npucc", "syscon";
		reg = <0x9910000 0x10000>;
		reg-names = "cc_base";
		vdd_cx-supply = <&VDD_CX_LEVEL>;
		vdd_gdsc-supply = <&npu_core_gdsc>;
		clocks =
			<&rpmhcc RPMH_CXO_CLK>,
			<&gcc GCC_NPU_GPLL0_DIV_CLK_SRC>,
			<&gcc GCC_NPU_GPLL0_CLK_SRC>,
			<&gcc GCC_NPU_AXI_CLK>;
		clock-names =
			"bi_tcxo",
			"gcc_npu_gpll0_div_clk_src",
			"gcc_npu_gpll0_clk_src",
			"gcc_npu_axi_clk";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	gpucc: clock-controller@2c90000 {
		compatible = "qcom,sm8150-gpucc", "syscon";
		reg = <0x2c90000 0x9000>;
		reg-names = "cc_base";
		vdd_cx-supply = <&VDD_CX_LEVEL>;
		vdd_mx-supply = <&VDD_MX_LEVEL>;
		clocks =
			<&rpmhcc RPMH_CXO_CLK>,
			<&gcc GCC_GPU_GPLL0_CLK_SRC>,
			<&gcc GCC_GPU_GPLL0_DIV_CLK_SRC>,
			<&gcc GCC_GPU_CFG_AHB_CLK>;
		clock-names = "bi_tcxo",
			"gcc_gpu_gpll0_clk_src",
			"gcc_gpu_gpll0_div_clk_src",
			"iface";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	scc: clock-controller@2b10000 {
		compatible = "qcom,sm8150-scc", "syscon";
		reg = <0x2b10000 0x30000>;
		vdd_scc_cx-supply = <&pm8150_l8_level>;
		clocks = <&rpmhcc RPMH_CXO_CLK>;
		clock-names = "bi_tcxo";
		#clock-cells = <1>;
		status = "disabled";
	};

	cpucc: syscon@182a0000 {
		compatible = "syscon";
		reg = <0x182a0000 0x4>;
	};

	mccc: syscon@90b0000 {
		compatible = "syscon";
		reg = <0x90b0000 0x1000>;
	};

	debugcc: debug-clock-controller@0 {
		compatible = "qcom,sm8150-debugcc";
		qcom,gcc = <&gcc>;
		qcom,videocc = <&videocc>;
		qcom,camcc = <&camcc>;
		qcom,dispcc = <&dispcc>;
		qcom,npucc = <&npucc>;
		qcom,gpucc = <&gpucc>;
		qcom,cpucc = <&cpucc>;
		qcom,mccc = <&mccc>;
		clock-names = "xo_clk_src";
		clocks = <&rpmhcc RPMH_CXO_CLK>;
		#clock-cells = <1>;
	};

	cpufreq_hw: cpufreq@18323000 {
		compatible = "qcom,cpufreq-hw";
		reg = <0x18323000 0x1400>, <0x18325800 0x1400>,
		      <0x18327800 0x1400>;
		reg-names = "freq-domain0", "freq-domain1",
			    "freq-domain2";

		clocks = <&rpmhcc RPMH_CXO_CLK>, <&gcc GPLL0>;
		clock-names = "xo", "alternate";
		qcom,no-accumulative-counter;

		#freq-domain-cells = <2>;
	};

	spmi_bus: qcom,spmi@c440000 {
		compatible = "qcom,spmi-pmic-arb";
		reg = <0xc440000 0x1100>,
		      <0xc600000 0x2000000>,
		      <0xe600000 0x100000>,
		      <0xe700000 0xa0000>,
		      <0xc40a000 0x26000>;
		reg-names = "core", "chnls", "obsrvr", "intr", "cnfg";
		interrupts-extended = <&pdc 1 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "periph_irq";
		interrupt-controller;
		#interrupt-cells = <4>;
		#address-cells = <2>;
		#size-cells = <0>;
		cell-index = <0>;
		qcom,channel = <0>;
		qcom,ee = <0>;
	};

	config_noc: interconnect@1500000 {
		reg = <0x1500000 0x7400>;
		compatible = "qcom,sm8150-config_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	system_noc: interconnect@1620000 {
		reg = <0x1620000 0x19400>;
		compatible = "qcom,sm8150-system_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	camnoc_virt: interconnect@1630000 {
		compatible = "qcom,sm8150-camnoc_virt";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	ipa_virt: interconnect@1640000 {
		compatible = "qcom,sm8150-ipa_virt";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	aggre1_noc: interconnect@16e0000 {
		reg = <0x16E0000 0xD080>;
		compatible = "qcom,sm8150-aggre1_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
		clocks = <&gcc GCC_AGGRE_UFS_PHY_AXI_CLK>,
			<&gcc GCC_AGGRE_USB3_PRIM_AXI_CLK>,
			<&gcc GCC_AGGRE_USB3_SEC_AXI_CLK>;
	};

	aggre2_noc: interconnect@1700000 {
		reg = <0x1700000 0x3B100>;
		compatible = "qcom,sm8150-aggre2_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	compute_noc: interconnect@1724000 {
		reg = <0x1724000 0x10>;
		compatible = "qcom,sm8150-compute_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	mmss_noc: interconnect@1740000 {
		reg = <0x1740000 0x1C100>;
		compatible = "qcom,sm8150-mmss_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos", "disp";
		qcom,bcm-voters = <&apps_bcm_voter>, <&disp_bcm_voter>;
	};

	dc_noc: interconnect@9160000 {
		reg = <0x9160000 0x3200>;
		compatible = "qcom,sm8150-dc_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	gem_noc: interconnect@9680000 {
		reg = <0x9680000 0x3E200>;
		compatible = "qcom,sm8150-gem_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos", "disp";
		qcom,bcm-voters = <&apps_bcm_voter>, <&disp_bcm_voter>;
	};

	mc_virt: interconnect@9690000 {
		compatible = "qcom,sm8150-mc_virt";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos", "disp";
		qcom,bcm-voters = <&apps_bcm_voter>, <&disp_bcm_voter>;
	};

	spmi_debug_bus: qcom,spmi-debug@6b22000 {
		compatible = "qcom,spmi-pmic-arb-debug";
		reg = <0x6b22000 0x60>, <0x7820a8 0x4>;
		reg-names = "core", "fuse";
		clocks = <&aoss_qmp>;
		clock-names = "core_clk";
		qcom,fuse-disable-bit = <24>;
		#address-cells = <2>;
		#size-cells = <0>;
		status = "disabled";

		qcom,pm8150-debug@0 {
			compatible = "qcom,spmi-pmic";
			reg = <0 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pm8150-debug@1 {
			compatible = "qcom,spmi-pmic";
			reg = <1 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pm8150b-debug@2 {
			compatible = "qcom,spmi-pmic";
			reg = <2 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pm8150b-debug@3 {
			compatible = "qcom,spmi-pmic";
			reg = <3 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pm8150l-debug@4 {
			compatible = "qcom,spmi-pmic";
			reg = <4 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pm8150l-debug@5 {
			compatible = "qcom,spmi-pmic";
			reg = <5 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};
	};

	ufsphy_mem: ufsphy_mem@1d87000 {
		reg = <0x1d87000 0xda8>; /* PHY regs */
		reg-names = "phy_mem";
		#phy-cells = <0>;

		lanes-per-direction = <2>;

		clock-names = "ref_clk_src",
			"ref_clk",
			"ref_aux_clk";
		clocks = <&rpmhcc RPMH_CXO_CLK>,
			<&gcc GCC_UFS_MEM_CLKREF_CLK>,
			<&gcc GCC_UFS_PHY_PHY_AUX_CLK>;

		resets = <&ufshc_mem 0>;
		status = "disabled";
	};

	ufshc_mem: ufshc@1d84000 {
		compatible = "qcom,ufshc";
		reg = <0x1d84000 0x2500>,
			  <0x1d90000 0x8000>;
		reg-names = "ufs_mem", "ufs_ice";
		interrupts = <GIC_SPI 265 IRQ_TYPE_LEVEL_HIGH>;
		phys = <&ufsphy_mem>;
		phy-names = "ufsphy";
		#reset-cells = <1>;

		lanes-per-direction = <2>;
		dev-ref-clk-freq = <0>; /* 19.2 MHz */

		clock-names =
			"core_clk",
			"bus_aggr_clk",
			"iface_clk",
			"core_clk_unipro",
			"core_clk_ice",
			"ref_clk",
			"tx_lane0_sync_clk",
			"rx_lane0_sync_clk",
			"rx_lane1_sync_clk";
		clocks =
			<&gcc GCC_UFS_PHY_AXI_CLK>,
			<&gcc GCC_AGGRE_UFS_PHY_AXI_CLK>,
			<&gcc GCC_UFS_PHY_AHB_CLK>,
			<&gcc GCC_UFS_PHY_UNIPRO_CORE_CLK>,
			<&gcc GCC_UFS_PHY_ICE_CORE_CLK>,
			<&rpmhcc RPMH_CXO_CLK>,
			<&gcc GCC_UFS_PHY_TX_SYMBOL_0_CLK>,
			<&gcc GCC_UFS_PHY_RX_SYMBOL_0_CLK>,
			<&gcc GCC_UFS_PHY_RX_SYMBOL_1_CLK>;
		freq-table-hz =
			<37500000 300000000>,
			<0 0>,
			<0 0>,
			<37500000 300000000>,
			<37500000 300000000>,
			<0 0>,
			<0 0>,
			<0 0>,
			<0 0>;
		interconnects = <&aggre1_noc MASTER_UFS_MEM &mc_virt SLAVE_EBI1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_UFS_MEM_CFG>;
		interconnect-names = "ufs-ddr", "cpu-ufs";

		qcom,ufs-bus-bw,name = "ufshc_mem";
		qcom,ufs-bus-bw,num-cases = <26>;
		qcom,ufs-bus-bw,num-paths = <2>;
		qcom,ufs-bus-bw,vectors-KBps =
		/*
		 * During HS G3 UFS runs at nominal voltage corner, vote
		 * higher bandwidth to push other buses in the data path
		 * to run at nominal to achieve max throughput.
		 * 4GBps pushes BIMC to run at nominal.
		 * 200MBps pushes CNOC to run at nominal.
		 * Vote for half of this bandwidth for HS G3 1-lane.
		 * For max bandwidth, vote high enough to push the buses
		 * to run in turbo voltage corner.
		 */
		<0 0>, <0 0>,          /* No vote */
		<922 0>, <1000 0>,     /* PWM G1 */
		<1844 0>, <1000 0>,    /* PWM G2 */
		<3688 0>, <1000 0>,    /* PWM G3 */
		<7376 0>, <1000 0>,    /* PWM G4 */
		<1844 0>, <1000 0>,    /* PWM G1 L2 */
		<3688 0>, <1000 0>,    /* PWM G2 L2 */
		<7376 0>, <1000 0>,    /* PWM G3 L2 */
		<14752 0>, <1000 0>,   /* PWM G4 L2 */
		<127796 0>, <1000 0>,  /* HS G1 RA */
		<255591 0>, <1000 0>,  /* HS G2 RA */
		<2097152 0>, <102400 0>,  /* HS G3 RA */
		<4194304 0>, <204800 0>,  /* HS G4 RA */
		<255591 0>, <1000 0>,  /* HS G1 RA L2 */
		<511181 0>, <1000 0>,  /* HS G2 RA L2 */
		<4194304 0>, <204800 0>, /* HS G3 RA L2 */
		<8388608 0>, <409600 0>, /* HS G4 RA L2 */
		<149422 0>, <1000 0>,  /* HS G1 RB */
		<298189 0>, <1000 0>,  /* HS G2 RB */
		<2097152 0>, <102400 0>,  /* HS G3 RB */
		<4194304 0>, <204800 0>,  /* HS G4 RB */
		<298189 0>, <1000 0>,  /* HS G1 RB L2 */
		<596378 0>, <1000 0>,  /* HS G2 RB L2 */
		/* As UFS working in HS G3 RB L2 mode, aggregated
		 * bandwidth (AB) should take care of providing
		 * optimum throughput requested. However, as tested,
		 * in order to scale up CNOC clock, instantaneous
		 * bindwidth (IB) needs to be given a proper value too.
		 */
		<4194304 0>, <204800 409600>, /* HS G3 RB L2 */
		<8388608 0>, <409600 409600>, /* HS G4 RB L2 */
		<7643136 0>, <307200 0>; /* Max. bandwidth */

		qcom,bus-vector-names = "MIN",
		"PWM_G1_L1", "PWM_G2_L1", "PWM_G3_L1", "PWM_G4_L1",
		"PWM_G1_L2", "PWM_G2_L2", "PWM_G3_L2", "PWM_G4_L2",
		"HS_RA_G1_L1", "HS_RA_G2_L1", "HS_RA_G3_L1", "HS_RA_G4_L1",
		"HS_RA_G1_L2", "HS_RA_G2_L2", "HS_RA_G3_L2", "HS_RA_G4_L2",
		"HS_RB_G1_L1", "HS_RB_G2_L1", "HS_RB_G3_L1", "HS_RB_G4_L1",
		"HS_RB_G1_L2", "HS_RB_G2_L2", "HS_RB_G3_L2", "HS_RB_G4_L2",
		"MAX";

		reset-gpios = <&tlmm 175 GPIO_ACTIVE_LOW>;

		resets = <&gcc GCC_UFS_PHY_BCR>;
		reset-names = "rst";

		iommus = <&apps_smmu 0x300 0x0>;
		qcom,iommu-dma = "bypass";
		dma-coherent;
		qcom,disable-lpm;

		status = "disabled";
		qos0 {
			mask = <0xf0>;
			vote = <44>;
		};

		qos1 {
			mask = <0x0f>;
			vote = <44>;
		};
	};

	sdhc2_opp_table: sdhc2-opp-table {
		compatible = "operating-points-v2";

		opp-100000000 {
			opp-hz = /bits/ 64 <100000000>;
			opp-peak-kBps = <1600000 280000>;
			opp-avg-kBps = <50000 0>;
		};

		opp-202000000 {
			opp-hz = /bits/ 64 <202000000>;
			opp-peak-kBps = <5600000 1500000>;
			opp-avg-kBps = <104000 0>;
		};
	};

	sdhc_2: sdhci@8804000 {
		compatible = "qcom,sdhci-msm-v5";
		reg = <0x8804000 0x1000>;
		reg-names = "hc";

		interrupts = <GIC_SPI 204 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 222 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "hc_irq", "pwr_irq";

		clocks = <&gcc GCC_SDCC2_AHB_CLK>,
			<&gcc GCC_SDCC2_APPS_CLK>;
		clock-names = "iface", "core";

		bus-width = <4>;
		no-sdio;
		no-mmc;
		qcom,restore-after-cx-collapse;

		iommus = <&apps_smmu 0x06A0 0x0>;
		qcom,iommu-dma = "fastmap";
		dma-coherent;

		interconnects = <&aggre2_noc MASTER_SDCC_2 &mc_virt SLAVE_EBI1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_SDCC_2>;
		interconnect-names = "sdhc-ddr","cpu-sdhc";
		operating-points-v2 = <&sdhc2_opp_table>;

		/* DLL HSR settings. Refer go/hsr - <Target> DLL settings */
		qcom,dll-hsr-list = <0x0007642c 0x0 0x10 0x2C010800 0x80040868>;


		status = "disabled";

		qos0 {
			mask = <0x3f>;
			vote = <44>;
		};

		qos1 {
			mask = <0xc0>;
			vote = <44>;
		};
	};

	qcom,rmtfs_sharedmem@0 {
		compatible = "qcom,sharedmem-uio";
		reg = <0x0 0x200000>;
		reg-names = "rmtfs";
		qcom,client-id = <0x00000001>;
		qcom,guard-memory;
	};

	thermal_zones: thermal-zones {
	};

	apcs: syscon@17c0000c {
		compatible = "syscon";
		reg = <0x17c0000c 0x4>;
	};

	apss_shared: mailbox@17c00000 {
		compatible = "qcom,sm8150-apss-shared";
		reg = <0x17c00000 0x1000>;
		#mbox-cells = <1>;
	};

	aoss_qmp: power-controller@c300000 {
		compatible = "qcom,sm8150-aoss-qmp";
		reg = <0x0c300000 0x100000>;
		interrupts = <GIC_SPI 389 IRQ_TYPE_EDGE_RISING>;
		mboxes = <&apss_shared 0>;

		#clock-cells = <0>;
		#power-domain-cells = <1>;
	};

	qmp_aop: qcom,qmp-aop@c300000 {
		compatible = "qcom,qmp-mbox";
		qcom,qmp = <&aoss_qmp>;
		label = "aop";
		#mbox-cells = <1>;
	};

	tcsr_mutex_block: syscon@1f40000 {
		compatible = "syscon";
		reg = <0x1f40000 0x20000>;
	};

	tcsr_mutex: hwlock@1f40000 {
		compatible = "qcom,tcsr-mutex";
		syscon = <&tcsr_mutex_block 0 0x1000>;
		#hwlock-cells = <1>;
	};

	smem: qcom,smem@8600000 {
		compatible = "qcom,smem";
		memory-region = <&smem_region>;
		hwlocks = <&tcsr_mutex 3>;
	};

	sp_scsr: mailbox@188501c {
		compatible = "qcom,sm8150-spcs-global";
		reg = <0x188501c 0x4>;

		#mbox-cells = <1>;
	};

	sp_scsr_block: syscon@1880000 {
		compatible = "syscon";
		reg = <0x1880000 0x10000>;
	};

	intsp: qcom,qsee_irq {
		compatible = "qcom,sm8150-qsee-irq";

		syscon = <&sp_scsr_block>;
		interrupts = <0 348 IRQ_TYPE_LEVEL_HIGH>,
			     <0 349 IRQ_TYPE_LEVEL_HIGH>;

		interrupt-names = "sp_ipc0",
				  "sp_ipc1";

		interrupt-controller;
		#interrupt-cells = <3>;
	};

	qcom,qsee_irq_bridge {
		compatible = "qcom,qsee-ipc-irq-bridge";

		qcom,qsee-ipc-irq-spss {
			qcom,dev-name = "qsee_ipc_irq_spss";
			label = "spss";
			interrupt-parent = <&intsp>;
			interrupts = <1 0 IRQ_TYPE_LEVEL_HIGH>;
		};
	};

	qcom,glinkpkt {
		compatible = "qcom,glinkpkt";

		qcom,glinkpkt-apr-apps2 {
			qcom,glinkpkt-edge = "adsp";
			qcom,glinkpkt-ch-name = "apr_apps2";
			qcom,glinkpkt-dev-name = "apr_apps2";
		};
	};

	qcom,smp2p_sleepstate {
		compatible = "qcom,smp2p-sleepstate";
		qcom,smem-states = <&sleepstate_smp2p_out 0>;
		interrupt-parent = <&sleepstate_smp2p_in>;
		interrupts = <0 0>;
		interrupt-names = "smp2p-sleepstate-in";
	};

	qcom,secure-buffer {
		compatible = "qcom,secure-buffer";
		qcom,vmid-cp-camera-preview-ro;
	};

	cache-controller@9200000 {
		compatible = "qcom,sm8150-llcc";
		reg = <0x9200000 0x1d0000> , <0x9600000 0x50000>;
		reg-names = "llcc_base", "llcc_broadcast_base";
		cap-based-alloc-and-pwr-collapse;
	};

	wdog: qcom,wdt@17c10000 {
		compatible = "qcom,msm-watchdog";
		reg = <0x17c10000 0x1000>;
		reg-names = "wdt-base";
		interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
	};

	qcom,sps {
		compatible = "qcom,msm-sps-4k";
		qcom,pipe-attr-ee;
	};

	qcom,mem-buf {
		compatible = "qcom,mem-buf";
		qcom,mem-buf-capabilities = "supplier";
		qcom,vmid = <3>;
	};

	qcom,mem-buf-msgq {
		compatible = "qcom,mem-buf-msgq";
	};

	soc-sleep-stats@c3f0000 {
		compatible = "qcom,rpmh-sleep-stats-legacy";
		reg = <0xc3f0000 0x400>;
		ss-name = "modem", "adsp", "adsp_island",
			  "cdsp", "slpi", "slpi_island",
			  "apss";
	};

	llcc_pmu: llcc-pmu@90cc000 {
		compatible = "qcom,llcc-pmu-ver2";
		reg = <0x090cc000 0x300>;
		reg-names = "lagg-base";
	};

	adsp_pas: remoteproc-adsp@17300000 {
		compatible = "qcom,sm8150-adsp-pas";
		reg = <0x17300000 0x00100>;
		status = "ok";

		cx-supply = <&VDD_CX_LEVEL>;
		cx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 0>;
		mx-supply = <&VDD_MX_LEVEL>;
		mx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 0>;
		reg-names = "cx", "mx";

		clocks = <&rpmhcc RPMH_CXO_CLK>;
		clock-names = "xo";

		qcom,qmp = <&aoss_qmp>;

		interconnects = <&aggre2_noc MASTER_CRYPTO &mc_virt SLAVE_EBI1>;
		interconnect-names = "crypto_ddr";

		memory-region = <&rproc_adsp_mem>;

		/* Inputs from ssc */
		interrupts-extended = <&intc GIC_SPI 162 IRQ_TYPE_LEVEL_HIGH>,
					<&adsp_smp2p_in 0 0>,
					<&adsp_smp2p_in 2 0>,
					<&adsp_smp2p_in 1 0>,
					<&adsp_smp2p_in 3 0>,
					<&adsp_smp2p_in 7 0>;

		interrupt-names = "wdog",
				"fatal",
				"handover",
				"ready",
				"stop-ack",
				"shutdown-ack";

		/* Outputs to turing */
		qcom,smem-states = <&adsp_smp2p_out 0>;
		qcom,smem-state-names = "stop";

		glink_edge: glink-edge {
			qcom,remote-pid = <2>;
			transport = "smem";
			mboxes = <&apss_shared 8>;
			mbox-names = "adsp_smem";
			interrupts = <GIC_SPI 156 IRQ_TYPE_EDGE_RISING>;

			label = "adsp";
			qcom,glink-label = "lpass";
			cpu-affinity = <1 2>;

			qcom,adsp_qrtr {
				qcom,glink-channels = "IPCRTR";
				qcom,intents = <0x800  5
						0x2000 3
						0x4400 2>;
			};

			qcom,apr_tal_rpmsg {
				qcom,glink-channels = "apr_audio_svc";
				qcom,intents = <0x200 20>;
			};

			qcom,msm_fastrpc_rpmsg {
				compatible = "qcom,msm-fastrpc-rpmsg";
				qcom,glink-channels = "fastrpcglink-apps-dsp";
				qcom,intents = <0x64 64>;
			};

			qcom,adsp_glink_ssr {
				qcom,glink-channels = "glink_ssr";
			};
		};
	};

	cdsp_pas: remoteproc-cdsp@0x8300000 {
		compatible = "qcom,sm8150-cdsp-pas";
		reg = <0x8300000 0x100000>;
		status = "ok";

		cx-supply = <&VDD_CX_LEVEL>;
		cx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 100000>;
		reg-names = "cx";

		clocks = <&rpmhcc RPMH_CXO_CLK>;
		clock-names = "xo";

		qcom,qmp = <&aoss_qmp>;

		interconnects = <&aggre2_noc MASTER_CRYPTO &mc_virt SLAVE_EBI1>;
		interconnect-names = "crypto_ddr";

		memory-region = <&rproc_cdsp_mem>;

		/* Inputs from ssc */
		interrupts-extended = <&intc GIC_SPI 578 IRQ_TYPE_EDGE_RISING>,
					<&cdsp_smp2p_in 0 0>,
					<&cdsp_smp2p_in 2 0>,
					<&cdsp_smp2p_in 1 0>,
					<&cdsp_smp2p_in 3 0>,
					<&cdsp_smp2p_in 7 0>;

		interrupt-names = "wdog",
				"fatal",
				"handover",
				"ready",
				"stop-ack",
				"shutdown-ack";

		/* Outputs to turing */
		qcom,smem-states = <&cdsp_smp2p_out 0>;
		qcom,smem-state-names = "stop";

		glink-edge {
			qcom,remote-pid = <5>;
			transport = "smem";
			mboxes = <&apss_shared 4>;
			mbox-names = "cdsp_smem";
			interrupts = <GIC_SPI 574 IRQ_TYPE_EDGE_RISING>;

			label = "cdsp";
			qcom,glink-label = "cdsp";

			qcom,cdsp_qrtr {
				qcom,glink-channels = "IPCRTR";
				qcom,intents = <0x800  5
						0x2000 3
						0x4400 2>;
			};

			qcom,msm_fastrpc_rpmsg {
				compatible = "qcom,msm-fastrpc-rpmsg";
				qcom,glink-channels = "fastrpcglink-apps-dsp";
				qcom,intents = <0x64 64>;
			};

			qcom,msm_cdsprm_rpmsg {
				compatible = "qcom,msm-cdsprm-rpmsg";
				qcom,glink-channels = "cdsprmglink-apps-dsp";
				qcom,intents = <0x20 12>;
				msm_cdsp_rm: qcom,msm_cdsp_rm {
					compatible = "qcom,msm-cdsp-rm";
					qcom,qos-latency-us = <44>;
					qcom,qos-maxhold-ms = <20>;
					qcom,compute-cx-limit-en;
					qcom,compute-priority-mode = <2>;
					#cooling-cells = <2>;
				};
			};

			qcom,cdsp_glink_ssr {
				qcom,glink-channels = "glink_ssr";
			};
		};
	};

	qcom,pmu {
		compatible = "qcom,pmu";
		qcom,long-counter;
		qcom,pmu-events-tbl =
			< 0x0008 0xFF 0xFF 0xFF >,
			< 0x0011 0xFF 0xFF 0xFF >,
			< 0x0017 0xFF 0xFF 0xFF >,
			< 0x002A 0xFF 0xFF 0xFF >,
			< 0x1000 0xFF 0xFF 0xFF >;
	};

	ddr_freq_table: ddr-freq-table {
		qcom,freq-tbl =
			<  200000 >,
			<  300000 >,
			<  451000 >,
			<  547000 >,
			<  681000 >,
			<  768000 >,
			< 1017000 >,
			< 1296000 >,
			< 1555000 >,
			< 1804000 >,
			< 2092000 >;
	};

	llcc_freq_table: llcc-freq-table {
		qcom,freq-tbl =
			< 150000 >,
			< 200000 >,
			< 403000 >,
			< 533000 >,
			< 666000 >,
			< 777000 >;
	};

	qcom_dcvs: qcom,dcvs {
		compatible = "qcom,dcvs";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		qcom_ddr_dcvs_hw: ddr {
			compatible = "qcom,dcvs-hw";
			qcom,dcvs-hw-type = <0>;
			qcom,bus-width = <4>;
			qcom,freq-tbl = <&ddr_freq_table>;

			ddr_dcvs_sp: sp {
				compatible = "qcom,dcvs-path";
				qcom,dcvs-path-type = <0>;
				interconnects = <&mc_virt MASTER_LLCC
						 &mc_virt SLAVE_EBI1>;
			};
		};

		qcom_llcc_dcvs_hw: llcc {
			compatible = "qcom,dcvs-hw";
			qcom,dcvs-hw-type = <1>;
			qcom,bus-width = <16>;
			qcom,freq-tbl = <&llcc_freq_table>;

			llcc_dcvs_sp: sp {
				compatible = "qcom,dcvs-path";
				qcom,dcvs-path-type = <0>;
				interconnects = <&gem_noc MASTER_APPSS_PROC
						 &gem_noc SLAVE_LLCC>;
			};
		};

		qcom_l3_dcvs_hw: l3 {
			compatible = "qcom,dcvs-hw";
			qcom,dcvs-hw-type = <2>;
			qcom,bus-width = <32>;
			qcom,ftbl-row-size = <0x20>;
			reg = <0x18321000 0x4000>, <0x18321110 0x500>;
			reg-names = "l3-base", "l3tbl-base";

			l3_dcvs_sp: sp {
				compatible = "qcom,dcvs-path";
				qcom,dcvs-path-type = <0>;
				qcom,shared-offset = <0x0920>;
			};
		};
	};

	qcom_memlat: qcom,memlat {
		compatible = "qcom,memlat";

		ddr {
			compatible = "qcom,memlat-grp";
			qcom,target-dev = <&qcom_ddr_dcvs_hw>;
			qcom,sampling-path = <&ddr_dcvs_sp>;
			qcom,miss-ev = <0x1000>;

			silver {
				compatible = "qcom,memlat-mon";
				qcom,cpulist = <&CPU0 &CPU1 &CPU2 &CPU3>;
				qcom,cpufreq-memfreq-tbl =
						<  300000 200000 >,
						<  768000 451000 >,
						< 1075200 547000 >,
						< 1267200 768000 >;
				qcom,sampling-enabled;
			};

			gold {
				compatible = "qcom,memlat-mon";
				qcom,cpulist = <&CPU4 &CPU5 &CPU6 &CPU7>;
				qcom,cpufreq-memfreq-tbl =
						<  300000  200000 >,
						<  576000  451000 >,
						<  768000  547000 >,
						<  960000  768000 >,
						< 1248000 1017000 >,
						< 1728000 1555000 >,
						< 2016000 1804000 >,
						< 2054400 2092000 >;
				qcom,sampling-enabled;
			};

			gold-compute {
				compatible = "qcom,memlat-mon";
				qcom,cpulist = <&CPU4 &CPU5 &CPU6 &CPU7>;
				qcom,cpufreq-memfreq-tbl =
						< 1593600  200000 >,
						< 2016000 1017000 >,
						< 2054400 2092000 >;
				qcom,sampling-enabled;
				qcom,compute-mon;
			};
		};

		llcc {
			compatible = "qcom,memlat-grp";
			qcom,target-dev = <&qcom_llcc_dcvs_hw>;
			qcom,sampling-path = <&llcc_dcvs_sp>;
			qcom,miss-ev = <0x2A>;

			silver {
				compatible = "qcom,memlat-mon";
				qcom,cpulist = <&CPU0 &CPU1 &CPU2 &CPU3>;
				qcom,cpufreq-memfreq-tbl =
						<  300000 150000 >,
						<  768000 200000 >,
						< 1075200 403000 >,
						< 1267200 403000 >;
				qcom,sampling-enabled;
			};

			gold {
				compatible = "qcom,memlat-mon";
				qcom,cpulist = <&CPU4 &CPU5 &CPU6 &CPU7>;
				qcom,cpufreq-memfreq-tbl =
						<  300000 150000 >,
						<  576000 200000 >,
						<  768000 403000 >,
						<  960000 403000 >,
						< 1248000 533000 >,
						< 1728000 666000 >,
						< 2016000 777000 >;
				qcom,sampling-enabled;
			};
		};

		l3 {
			compatible = "qcom,memlat-grp";
			qcom,target-dev = <&qcom_l3_dcvs_hw>;
			qcom,sampling-path = <&l3_dcvs_sp>;
			qcom,miss-ev = <0x17>;

			silver {
				compatible = "qcom,memlat-mon";
				qcom,cpulist = <&CPU0 &CPU1 &CPU2 &CPU3>;
				qcom,cpufreq-memfreq-tbl =
						<  300000 300000 >,
						<  480000 403200 >,
						<  672000 480000 >,
						<  768000 576000 >,
						<  864000 672000 >,
						<  979200 768000 >,
						< 1075200 864000 >,
						< 1267200 960000 >;
				qcom,sampling-enabled;
			};

			gold {
				compatible = "qcom,memlat-mon";
				qcom,cpulist = <&CPU4 &CPU5 &CPU6>;
				qcom,cpufreq-memfreq-tbl =
						<  300000  300000 >,
						<  768000  576000 >,
						< 1152000  768000 >,
						< 1344000  960000 >,
						< 1689600 1228800 >,
						< 2016000 1344000 >;
				qcom,sampling-enabled;
			};

			prime {
				compatible = "qcom,memlat-mon";
				qcom,cpulist = <&CPU7>;
				qcom,cpufreq-memfreq-tbl =
						<  300000  300000 >,
						<  768000  576000 >,
						< 1152000  768000 >,
						< 1344000  960000 >,
						< 1689600 1228800 >,
						< 2016000 1344000 >;
				qcom,sampling-enabled;
			};
		};
	};

	bwmon_llcc: qcom,bwmon-llcc@90b6400 {
		compatible = "qcom,bwmon4";
		reg = <0x90b6400 0x300>, <0x90b6300 0x200>;
		reg-names = "base", "global_base";
		interrupts = <GIC_SPI 581 IRQ_TYPE_LEVEL_HIGH>;
		qcom,mport = <0>;
		qcom,hw-timer-hz = <19200000>;
		qcom,count-unit = <0x10000>;
		qcom,target-dev = <&qcom_llcc_dcvs_hw>;
	};

	bwmon_ddr: qcom,bwmon-ddr@90cd000 {
		compatible = "qcom,bwmon5";
		reg = <0x90cd000 0x1000>;
		reg-names = "base";
		interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
		qcom,hw-timer-hz = <19200000>;
		qcom,count-unit = <0x10000>;
		qcom,target-dev = <&qcom_ddr_dcvs_hw>;
	};

	qcom,chd {
		compatible = "qcom,core-hang-detect";
		label = "core";
		qcom,threshold-arr = <0x18000058 0x18010058 0x18020058 0x18030058
				0x18040058 0x18050058 0x18060058 0x18070058>;
		qcom,config-arr = <0x18000060 0x18010060 0x18020060 0x18030060
				0x18040060 0x18050060 0x18060060 0x18070060>;
	};

	qtee_shmbridge {
		compatible = "qcom,tee-shared-memory-bridge";
		qcom,disable-shmbridge-support;
	};

	qcom_qseecom: qseecom@87900000 {
		compatible = "qcom,qseecom";
		reg = <0x87900000 0x2200000>;
		reg-names = "secapp-region";
		memory-region = <&qseecom_mem>;
		qcom,hlos-num-ce-hw-instances = <1>;
		qcom,hlos-ce-hw-instance = <0>;
		qcom,qsee-ce-hw-instance = <0>;
		qcom,disk-encrypt-pipe-pair = <2>;
		qcom,support-fde;
		qcom,no-clock-support;
		qcom,fde-key-size;
		qcom,appsbl-qseecom-support;
		qcom,commonlib64-loaded-by-uefi;
		qcom,qsee-reentrancy-support = <2>;
	};

	qcom_tzlog: tz-log@146bf720 {
		compatible = "qcom,tz-log";
		reg = <0x146bf720 0x3000>;
		qcom,hyplog-enabled;
		hyplog-address-offset = <0x410>;
		hyplog-size-offset = <0x414>;
	};

	qcom_cedev: qcedev@1de0000 {
		compatible = "qcom,qcedev";
		reg = <0x1de0000 0x20000>,
			<0x1dc4000 0x28000>;
		reg-names = "crypto-base","crypto-bam-base";
		interrupts = <GIC_SPI 272 IRQ_TYPE_LEVEL_HIGH>;
		qcom,bam-pipe-pair = <2>;
		qcom,offload-ops-support;
		qcom,bam-pipe-offload-cpb-hlos = <1>;
		qcom,bam-pipe-offload-hlos-cpb = <3>;
		qcom,bam-pipe-offload-hlos-hlos = <4>;
		qcom,ce-hw-instance = <0>;
		qcom,ce-device = <0>;
		qcom,ce-hw-shared;
		qcom,bam-ee = <0>;
		qcom,smmu-s1-enable;
		qcom,no-clock-support;
		interconnect-names = "data_path";
		interconnects = <&aggre2_noc MASTER_CRYPTO &mc_virt SLAVE_EBI1>;
		iommus = <&apps_smmu 0x0504 0x0011>,
			<&apps_smmu 0x0502 0x0641>,
			<&apps_smmu 0x0514 0x0011>;
		 qcom,iommu-dma = "atomic";
		dma-coherent;

		qcom_cedev_ns_cb {
			compatible = "qcom,qcedev,context-bank";
			label = "ns_context";
			iommus = <&apps_smmu 0x0506 0x0011>,
				<&apps_smmu 0x0508 0x0011>,
				<&apps_smmu 0x0512 0x0000>,
				<&apps_smmu 0x0516 0x0011>,
				<&apps_smmu 0x0518 0x0011>;
			dma-coherent;
		};

		qcom_cedev_s_cb {
			compatible = "qcom,qcedev,context-bank";
			label = "secure_context";
			iommus = <&apps_smmu 0x0513 0x0000>;
			qcom,iommu-vmid = <0x9>;
			qcom,secure-context-bank;
			dma-coherent;
		};
	};

	qcom_rng: qrng@793000 {
		compatible = "qcom,msm-rng";
		reg = <0x793000 0x1000>;
		qcom,no-qrng-config;
		interconnect-names = "data_path";
		interconnects = <&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_PRNG>;
		clock-names = "km_clk_src";
		clocks = <&gcc GCC_PRNG_AHB_CLK>;
	};

	qcom,msm-cdsp-loader {
		compatible = "qcom,cdsp-loader";
		qcom,proc-img-to-load = "cdsp";
		qcom,rproc-handle = <&cdsp_pas>;
	};

	qcom,msm-adsprpc-mem {
		compatible = "qcom,msm-adsprpc-mem-region";
		memory-region = <&adsp_mem>;
	};

	msm_fastrpc: qcom,msm_fastrpc {
		compatible = "qcom,msm-fastrpc-compute";
		qcom,fastrpc-adsp-audio-pdr;
		qcom,rpc-latency-us = <235>;

		qcom,msm_fastrpc_compute_cb1 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x1001 0x0460>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb4 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x1004 0x0460>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb5 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x1005 0x0460>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb6 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x1006 0x0460>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb7 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x1007 0x0460>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb8 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x1008 0x0460>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb2 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x1002 0x0460>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb3 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x1003 0x0460>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb9 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			qcom,secure-context-bank;
			iommus = <&apps_smmu 0x1009 0x0460>;
			qcom,iommu-dma-addr-pool = <0x60000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb10 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "adsprpc-smd";
			iommus = <&apps_smmu 0x1b23 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb11 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "adsprpc-smd";
			iommus = <&apps_smmu 0x1b24 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};

		qcom,msm_fastrpc_compute_cb12 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "adsprpc-smd";
			iommus = <&apps_smmu 0x1b25 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable";
			dma-coherent;
		};
	};

	kryo-erp {
		compatible = "arm,arm64-kryo-cpu-erp";
		interrupts = <GIC_PPI 6 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_PPI 7 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;

		interrupt-names = "l1-l2-faultirq",
				"l1-l2-errirq",
				"l3-scu-errirq",
				"l3-scu-faultirq";
	};
};

&firmware {
	qcom_scm {
		compatible = "qcom,scm";
		qcom,dload-mode = <&tcsr 0x13000>;
	};

	qcom_smcinvoke {
		compatible = "qcom,smcinvoke";
	};

	android {
		compatible = "android,firmware";
		vbmeta {
			compatible = "android,vbmeta";
			parts = "vbmeta,boot,system,vendor,dtbo";
		};

		fstab {
			compatible = "android,fstab";
			vendor {
				compatible = "android,vendor";
				dev = "/dev/block/platform/soc/1d84000.ufshc/by-name/vendor";
				type = "ext4";
				mnt_flags = "ro,barrier=1,discard";
				fsmgr_flags = "wait,slotselect,avb";
				status = "ok";
			};
		};
	};
};

#include "sm8150-regulator.dtsi"
#include "sm8150-pinctrl.dtsi"
#include "sm8150-dma-heaps.dtsi"
#include "sm8150-slpi-pinctrl.dtsi"
#include "sm8150-gdsc.dtsi"
#include "msm-arm-smmu-sm8150.dtsi"
#include "sm8150-smp2p.dtsi"
#include "sm8150-usb.dtsi"
#include "sm8150-debug.dtsi"

&emac_gdsc {
	status = "ok";
};

&pcie_0_gdsc {
	status = "ok";
};

&pcie_1_gdsc {
	status = "ok";
};

&ufs_phy_gdsc {
	status = "ok";
};

&ufs_card_gdsc {
	status = "ok";
};

&usb30_prim_gdsc {
	status = "ok";
};

&usb30_sec_gdsc {
	status = "ok";
};

&hlos1_vote_aggre_noc_mmu_audio_tbu_gdsc {
	status = "ok";
};

&hlos1_vote_aggre_noc_mmu_tbu1_gdsc {
	status = "ok";
};

&hlos1_vote_aggre_noc_mmu_tbu2_gdsc {
	status = "ok";
};

&hlos1_vote_aggre_noc_mmu_pcie_tbu_gdsc {
	status = "ok";
};

&hlos1_vote_mmnoc_mmu_tbu_hf0_gdsc {
	status = "ok";
};

&hlos1_vote_mmnoc_mmu_tbu_sf_gdsc {
	status = "ok";
};

&hlos1_vote_mmnoc_mmu_tbu_hf1_gdsc {
	status = "ok";
};

&hlos1_vote_turing_mmu_tbu0_gdsc {
	status = "ok";
};

&hlos1_vote_turing_mmu_tbu1_gdsc {
	status = "ok";
};

&bps_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_CAMERA_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	qcom,support-hw-trigger;
	status = "ok";
};

&ipe_0_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_CAMERA_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	qcom,support-hw-trigger;
	status = "ok";
};

&ipe_1_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_CAMERA_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	qcom,support-hw-trigger;
	status = "ok";
};

&ife_0_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_CAMERA_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	status = "ok";
};

&ife_1_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_CAMERA_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	status = "ok";
};

&titan_top_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_CAMERA_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	status = "ok";
};

&mdss_core_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_DISP_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	status = "ok";
};

&gpu_cx_gdsc {
	parent-supply = <&VDD_CX_LEVEL>;
	status = "ok";
};

&gpu_gx_gdsc {
	parent-supply = <&VDD_GFX_LEVEL>;
	status = "ok";
};

&mvsc_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_VIDEO_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	status = "ok";
};

&mvs0_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_VIDEO_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	qcom,support-hw-trigger;
	status = "ok";
};

&mvs1_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_VIDEO_AHB_CLK>;
	parent-supply = <&VDD_MMCX_LEVEL>;
	qcom,support-hw-trigger;
	status = "ok";
};

&npu_core_gdsc {
	clock-names = "ahb_clk";
	clocks = <&gcc GCC_NPU_CFG_AHB_CLK>;
	status = "ok";
};

#include "sm8150-pcie.dtsi"
#include "sm8150-qupv3.dtsi"
#include "sm8150-ssc-qupv3.dtsi"

&qupv3_se12_2uart {
	status = "ok";
};

&qupv3_se9_2uart {
	qcom,auto-suspend-disable;
	status = "ok";
};

#include "sm8150-thermal.dtsi"
