&soc {
	slpi_tlmm: slpi_pinctrl@2b40000 {
		compatible = "qcom,slpi-pinctrl";
		reg = <0x2b40000 0x20000>;
		clock-names = "ssc-clk";
		clocks =  <&scc SCC_QUPV3_S_HCLK_CLK>;
		qcom,num-pins = <14>;
		status = "disabled";

		qupv3_se20_i2c_pins: qupv3_se20_i2c_pins {
			qupv3_se20_i2c_active: qupv3_se20_i2c_active {
				mux {
					pins = "gpio0", "gpio1";
					function = "func1";
				};

				config {
					pins = "gpio0", "gpio1";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se20_i2c_sleep: qupv3_se20_i2c_sleep {
				mux {
					pins = "gpio0", "gpio1";
					function = "gpio";
				};

				config {
					pins = "gpio0", "gpio1";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		qupv3_se21_i2c_pins: qupv3_se21_i2c_pins {
			qupv3_se21_i2c_active: qupv3_se21_i2c_active {
				mux {
					pins = "gpio2", "gpio3";
					function = "func1";
				};

				config {
					pins = "gpio2", "gpio3";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se21_i2c_sleep: qupv3_se21_i2c_sleep {
				mux {
					pins = "gpio2", "gpio3";
					function = "gpio";
				};

				config {
					pins = "gpio2", "gpio3";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		qupv3_se22_i2c_pins: qupv3_se22_i2c_pins {
			qupv3_se22_i2c_active: qupv3_se22_i2c_active {
				mux {
					pins = "gpio6", "gpio7";
					function = "func1";
				};

				config {
					pins = "gpio6", "gpio7";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se22_i2c_sleep: qupv3_se22_i2c_sleep {
				mux {
					pins = "gpio6", "gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio7";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		qupv3_se23_i2c_pins: qupv3_se23_i2c_pins {
			qupv3_se23_i2c_active: qupv3_se23_i2c_active {
				mux {
					pins = "gpio8", "gpio9";
					function = "func3";
				};

				config {
					pins = "gpio8", "gpio9";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se23_i2c_sleep: qupv3_se23_i2c_sleep {
				mux {
					pins = "gpio8", "gpio9";
					function = "gpio";
				};

				config {
					pins = "gpio8", "gpio9";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		/* SE21 pin mappings */
		qupv3_se21_spi_pins: qupv3_se21_spi_pins {
			qupv3_se21_spi_active: qupv3_se21_spi_active {
				mux {
					pins = "gpio2", "gpio3", "gpio4",
								"gpio5";
					function = "func1";
				};

				config {
					pins = "gpio2", "gpio3", "gpio4",
								"gpio5";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se21_spi_sleep: qupv3_se21_spi_sleep {
				mux {
					pins = "gpio2", "gpio3", "gpio4",
								"gpio5";
					function = "gpio";
				};

				config {
					pins = "gpio2", "gpio3", "gpio4",
								"gpio5";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		/*SE22 pin mappings*/
		qupv3_se22_spi_pins: qupv3_se22_spi_pins {
			qupv3_se22_spi_active: qupv3_se22_spi_active {
				mux {
					pins = "gpio6", "gpio7", "gpio8",
								"gpio9";
					function = "func1";
				};

				config {
					pins = "gpio6", "gpio7", "gpio8",
								"gpio9";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se22_spi_sleep: qupv3_se22_spi_sleep {
				mux {
					pins = "gpio6", "gpio7", "gpio8",
								"gpio9";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio7", "gpio8",
								"gpio9";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};
	};
};
