#include "kalama-qrd.dtsi"

&sdhc_2 {
	cd-gpios = <&pm8550_gpios 12 GPIO_ACTIVE_HIGH>;
};

&usb_qmp_dp_phy {
	pinctrl-names = "default";
};

&redriver {
	status = "disabled";
};

&regulator_ocp_notifier {
	/delete-property/ periph-bc3-supply;
	/delete-property/ periph-bc4-supply;
	/delete-property/ periph-bc5-supply;
	/delete-property/ periph-bc6-supply;
	/delete-property/ periph-bc7-supply;
};

&pm8550b_eusb2_repeater {
	qcom,param-override-seq =
		/* <value reg_offset> */
		/* Adjust HS trasmit amplitude */
		<0xb 0x51
		/* Squelch detection threshold */
		 0x3 0x54
		/* Tx pre-emphasis tuning */
		 0x3 0x57
		/* HS disconnect threshold */
		 0x6 0x53>;
};

&pcie1 {
	qcom,boot-option = <0x2>;
	qcom,apss-based-l1ss-sleep;
};
