
&qupv3_se0_i2c {
	status = "ok";
	qcom,clk-freq-out = <1000000>;
	#address-cells = <1>;
	#size-cells = <0>;
	nq@28 {
		compatible = "qcom,sn-nci";
		reg = <0x29>;
		qcom,sn-irq = <&tlmm 55 0x00>;
		qcom,sn-ven = <&tlmm 161 0x00>;
		qcom,sn-firm = <&tlmm 159 0x00>;
		qcom,sn-clkreq = <&tlmm 31 0x00>;
		qcom,sn-szone = "enable";
		qcom,sn-vdd-1p8-supply = <&L15B>;
		qcom,sn-vdd-1p8-voltage = <1760000 1800000>;
		qcom,sn-vdd-1p8-current = <157000>;
		interrupt-parent = <&tlmm>;
		interrupts = <55 0>;
		interrupt-names = "nfc_irq";
		pinctrl-names = "nfc_active", "nfc_suspend";
		pinctrl-0 = <&nfc_int_active &nfc_enable_active>;
		pinctrl-1 = <&nfc_int_suspend &nfc_enable_suspend>;
	};
};

&qupv3_se1_spi {
	status = "ok";
	p61@0 {
		compatible = "nxp,p61";
		reg = <0x0>;
		spi-max-frequency = <20000000>;
		nxp,nfcc = "1-0029";
	};
};
