#include <dt-bindings/msm-camera.h>

&tlmm {
	cci0_active: cci0_active {
		mux {
			/* DATA, CLK */
			pins = "gpio70","gpio71"; // Only 2
			function = "cci_i2c";
		};

		config {
			pins = "gpio70","gpio71";
			bias-pull-up; /* PULL UP*/
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci0_suspend: cci0_suspend {
		mux {
			/* DATA, CLK */
			pins = "gpio70","gpio71";
			function = "cci_i2c";
		};

		config {
			pins = "gpio70","gpio71";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci1_active: cci1_active {
		mux {
			/* DATA, CLK */
			pins = "gpio72","gpio73";
			function = "cci_i2c";
		};

		config {
			pins = "gpio72","gpio73";
			bias-pull-up; /* PULL UP*/
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci1_suspend: cci1_suspend {
		mux {
			/* DATA, CLK */
			pins = "gpio72","gpio73";
			function = "cci_i2c";
		};

		config {
			pins = "gpio72","gpio73";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci2_active: cci2_active {
		mux {
			/* DATA, CLK */
			pins = "gpio74","gpio75";
			function = "cci_i2c";
		};

		config {
			pins = "gpio74","gpio75";
			bias-pull-up; /* PULL UP*/
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci2_suspend: cci2_suspend {
		mux {
			/* DATA, CLK */
			pins = "gpio74","gpio75";
			function = "cci_i2c";
		};

		config {
			pins = "gpio74","gpio75";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci3_active: cci3_active {
		mux {
			/* DATA, CLK */
			pins = "gpio76","gpio77";
			function = "cci_i2c";
		};

		config {
			pins = "gpio76","gpio77";
			bias-pull-up; /* PULL UP*/
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci3_suspend: cci3_suspend {
		mux {
			/* DATA, CLK */
			pins = "gpio76","gpio77";
			function = "cci_i2c";
		};

		config {
			pins = "gpio76","gpio77";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
		};

	};

	cam_sensor_mclk0_active: cam_sensor_mclk0_active {
		/* MCLK0 */
		mux {
			pins = "gpio64";
			function = "cam_mclk";
		};

		config {
			pins = "gpio64";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk0_suspend: cam_sensor_mclk0_suspend {
		/* MCLK0 */
		mux {
			pins = "gpio64";
			function = "cam_mclk";
		};

		config {
			pins = "gpio64";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk1_active: cam_sensor_mclk1_active {
		/* MCLK1 */
		mux {
			pins = "gpio65";
			function = "cam_mclk";
		};

		config {
			pins = "gpio65";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk1_suspend: cam_sensor_mclk1_suspend {
		/* MCLK1 */
		mux {
			pins = "gpio65";
			function = "cam_mclk";
		};

		config {
			pins = "gpio65";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk2_active: cam_sensor_mclk2_active {
		/* MCLK2 */
		mux {
			pins = "gpio66";
			function = "cam_mclk";
		};

		config {
			pins = "gpio66";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk2_suspend: cam_sensor_mclk2_suspend {
		/* MCLK2 */
		mux {
			pins = "gpio66";
			function = "cam_mclk";
		};

		config {
			pins = "gpio66";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk3_active: cam_sensor_mclk3_active {
		/* MCLK3 */
		mux {
			pins = "gpio67";
			function = "cam_mclk";
		};

		config {
			pins = "gpio67";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk3_suspend: cam_sensor_mclk3_suspend {
		/* MCLK3 */
		mux {
			pins = "gpio67";
			function = "cam_mclk";
		};

		config {
			pins = "gpio67";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk4_active: cam_sensor_mclk4_active {
		/* MCLK4 */
		mux {
			pins = "gpio68";
			function = "cam_mclk";
		};

		config {
			pins = "gpio68";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk4_suspend: cam_sensor_mclk4_suspend {
		/* MCLK4 */
		mux {
			pins = "gpio68";
			function = "cam_mclk";
		};

		config {
			pins = "gpio68";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk5_active: cam_sensor_mclk5_active {
		/* MCLK5 */
		mux {
			pins = "gpio69";
			function = "cam_mclk";
		};

		config {
			pins = "gpio69";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk5_suspend: cam_sensor_mclk5_suspend {
		/* MCLK5 */
		mux {
			pins = "gpio69";
			function = "cam_mclk";
		};

		config {
			pins = "gpio69";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_active_rst0: cam_sensor_active_rst0 {
		/* RESET REAR */
		mux {
			pins = "gpio20";
			function = "gpio";
		};

		config {
			pins = "gpio20";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst0: cam_sensor_suspend_rst0 {
		/* RESET REAR */
		mux {
			pins = "gpio20";
			function = "gpio";
		};

		config {
			pins = "gpio20";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst1: cam_sensor_active_rst1 {
		/* RESET REARAUX */
		mux {
			pins = "gpio21";
			function = "gpio";
		};

		config {
			pins = "gpio21";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst1: cam_sensor_suspend_rst1 {
		/* RESET REARAUX */
		mux {
			pins = "gpio21";
			function = "gpio";
		};

		config {
			pins = "gpio21";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst2: cam_sensor_active_rst2 {
		/* RESET 2 */
		mux {
			pins = "gpio78";
			function = "gpio";
		};

		config {
			pins = "gpio78";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst2: cam_sensor_suspend_rst2 {
		/* RESET 2 */
		mux {
			pins = "gpio78";
			function = "gpio";
		};

		config {
			pins = "gpio78";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst3: cam_sensor_active_rst3 {
		/* RESET 3 */
		mux {
			pins = "gpio79";
			function = "gpio";
		};

		config {
			pins = "gpio79";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst3: cam_sensor_suspend_rst3 {
		/* RESET 3 */
		mux {
			pins = "gpio79";
			function = "gpio";
		};

		config {
			pins = "gpio79";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst4: cam_sensor_active_rst4 {
		/* RESET 4 */
		mux {
			pins = "gpio80";
			function = "gpio";
		};

		config {
			pins = "gpio80";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst4: cam_sensor_suspend_rst4 {
		/* RESET 4 */
		mux {
			pins = "gpio80";
			function = "gpio";
		};

		config {
			pins = "gpio80";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst5: cam_sensor_active_rst5 {
		/* RESET 5 */
		mux {
			pins = "gpio81";
			function = "gpio";
		};

		config {
			pins = "gpio81";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst5: cam_sensor_suspend_rst5 {
		/* RESET 5 */
		mux {
			pins = "gpio81";
			function = "gpio";
		};

		config {
			pins = "gpio81";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};
};

&soc {
	#address-cells = <1>;
	#size-cells = <1>;
	interrupt-parent = <&intc>;

	qcom,cam-req-mgr {
		compatible = "qcom,cam-req-mgr";
		status = "ok";
	};

	qcom,cam-sync {
		compatible = "qcom,cam-sync";
		status = "ok";
	};

	cam_csiphy0: qcom,csiphy0@ac6a000 {
		cell-index = <0>;
		compatible = "qcom,csiphy-v2.1.1", "qcom,csiphy";
		reg = <0x0ac6a000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0x6a000>;
		interrupt-names = "CSIPHY0";
		interrupts = <GIC_SPI 477 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L10C>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 45100 85200>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy0_clk",
			"csi0phytimer_clk_src",
			"csi0phytimer_clk";
		clocks = <&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_CSIPHY0_CLK>,
			<&camcc CAM_CC_CSI0PHYTIMER_CLK_SRC>,
			<&camcc CAM_CC_CSI0PHYTIMER_CLK>;
		src-clock-name = "csi0phytimer_clk_src";
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		clock-rates =
			<266666667 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>;
		status = "ok";
	};

	cam_csiphy1: qcom,csiphy1@ac6c000 {
		cell-index = <1>;
		compatible = "qcom,csiphy-v2.1.1", "qcom,csiphy";
		reg = <0x0ac6c000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0x6c000>;
		interrupt-names = "CSIPHY1";
		interrupts = <GIC_SPI 478 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L10C>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 45100 85200>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy1_clk",
			"csi1phytimer_clk_src",
			"csi1phytimer_clk";
		clocks = <&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_CSIPHY1_CLK>,
			<&camcc CAM_CC_CSI1PHYTIMER_CLK_SRC>,
			<&camcc CAM_CC_CSI1PHYTIMER_CLK>;
		src-clock-name = "csi1phytimer_clk_src";
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		clock-rates =
			<266666667 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>;
		status = "ok";
	};

	cam_csiphy2: qcom,csiphy2@ac6e000 {
		cell-index = <2>;
		compatible = "qcom,csiphy-v2.1.1", "qcom,csiphy";
		reg = <0x0ac6e000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0x6e000>;
		interrupt-names = "CSIPHY2";
		interrupts = <GIC_SPI 479 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L10C>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 45100 85200>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy2_clk",
			"csi2phytimer_clk_src",
			"csi2phytimer_clk";
		clocks = <&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_CSIPHY2_CLK>,
			<&camcc CAM_CC_CSI2PHYTIMER_CLK_SRC>,
			<&camcc CAM_CC_CSI2PHYTIMER_CLK>;
		src-clock-name = "csi2phytimer_clk_src";
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		clock-rates =
			<266666667 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>;
		status = "ok";
	};

	cam_csiphy3: qcom,csiphy3@ac70000 {
		cell-index = <3>;
		compatible = "qcom,csiphy-v2.1.1", "qcom,csiphy";
		reg = <0x0ac70000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0x70000>;
		interrupt-names = "CSIPHY3";
		interrupts = <GIC_SPI 448 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L10C>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 45100 85200>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy3_clk",
			"csi3phytimer_clk_src",
			"csi3phytimer_clk";
		clocks = <&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_CSIPHY3_CLK>,
			<&camcc CAM_CC_CSI3PHYTIMER_CLK_SRC>,
			<&camcc CAM_CC_CSI3PHYTIMER_CLK>;
		src-clock-name = "csi3phytimer_clk_src";
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		clock-rates =
			<266666667 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>;
		status = "ok";
	};

	cam_csiphy4: qcom,csiphy4@ac72000 {
		cell-index = <4>;
		compatible = "qcom,csiphy-v2.1.1", "qcom,csiphy";
		reg = <0x0ac72000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0x72000>;
		interrupt-names = "CSIPHY4";
		interrupts = <GIC_SPI 122 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L10C>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 45100 85200>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy4_clk",
			"csi4phytimer_clk_src",
			"csi4phytimer_clk";
		clocks = <&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_CSIPHY4_CLK>,
			<&camcc CAM_CC_CSI4PHYTIMER_CLK_SRC>,
			<&camcc CAM_CC_CSI4PHYTIMER_CLK>;
		src-clock-name = "csi4phytimer_clk_src";
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		clock-rates =
			<266666667 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>;
		status = "ok";
	};

	cam_cci0: qcom,cci0@ac4f000 {
		cell-index = <0>;
		compatible = "qcom,cci", "simple-bus";
		reg = <0xac4f000 0x1000>;
		reg-names = "cci";
		reg-cam-base = <0x4f000>;
		interrupt-names = "cci0";
		interrupts = <GIC_SPI 460 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cci_0_clk_src",
			"cci_0_clk";
		clocks = <&camcc CAM_CC_CCI_0_CLK_SRC>,
			<&camcc CAM_CC_CCI_0_CLK>;
		clock-rates = <37500000 0>;
		clock-cntl-level = "lowsvs";
		src-clock-name = "cci_0_clk_src";
		pctrl-idx-mapping = <CCI_MASTER_0 CCI_MASTER_1>;
		pctrl-map-names = "m0", "m1";
		pinctrl-names = "m0_active", "m0_suspend",
			"m1_active", "m1_suspend";
		pinctrl-0 = <&cci0_active>;
		pinctrl-1 = <&cci0_suspend>;
		pinctrl-2 = <&cci1_active>;
		pinctrl-3 = <&cci1_suspend>;
		status = "ok";

		i2c_freq_100Khz_cci0: qcom,i2c_standard_mode {
			hw-thigh = <201>;
			hw-tlow = <174>;
			hw-tsu-sto = <204>;
			hw-tsu-sta = <231>;
			hw-thd-dat = <22>;
			hw-thd-sta = <162>;
			hw-tbuf = <227>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <6>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_400Khz_cci0: qcom,i2c_fast_mode {
			hw-thigh = <38>;
			hw-tlow = <56>;
			hw-tsu-sto = <40>;
			hw-tsu-sta = <40>;
			hw-thd-dat = <22>;
			hw-thd-sta = <35>;
			hw-tbuf = <62>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <6>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_custom_cci0: qcom,i2c_custom_mode {
			hw-thigh = <16>;
			hw-tlow = <22>;
			hw-tsu-sto = <17>;
			hw-tsu-sta = <18>;
			hw-thd-dat = <16>;
			hw-thd-sta = <15>;
			hw-tbuf = <24>;
			hw-scl-stretch-en = <1>;
			hw-trdhld = <3>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_1Mhz_cci0: qcom,i2c_fast_plus_mode {
			hw-thigh = <16>;
			hw-tlow = <22>;
			hw-tsu-sto = <17>;
			hw-tsu-sta = <18>;
			hw-thd-dat = <16>;
			hw-thd-sta = <15>;
			hw-tbuf = <24>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <3>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};
	};

	cam_cci1: qcom,cci1@ac50000 {
		cell-index = <1>;
		compatible = "qcom,cci", "simple-bus";
		reg = <0xac50000 0x1000>;
		reg-names = "cci";
		reg-cam-base = <0x50000>;
		interrupt-names = "cci1";
		interrupts = <GIC_SPI 271 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cci_1_clk_src",
			"cci_1_clk";
		clocks = <&camcc CAM_CC_CCI_1_CLK_SRC>,
			<&camcc CAM_CC_CCI_1_CLK>;
		clock-rates = <37500000 0>;
		clock-cntl-level = "lowsvs";
		src-clock-name = "cci_1_clk_src";
		pctrl-idx-mapping = <CCI_MASTER_0 CCI_MASTER_1>;
		pctrl-map-names = "m0", "m1";
		pinctrl-names = "m0_active", "m0_suspend",
			"m1_active", "m1_suspend";
		pinctrl-0 = <&cci2_active>;
		pinctrl-1 = <&cci2_suspend>;
		pinctrl-2 = <&cci3_active>;
		pinctrl-3 = <&cci3_suspend>;
		status = "ok";

		i2c_freq_100Khz_cci1: qcom,i2c_standard_mode {
			hw-thigh = <201>;
			hw-tlow = <174>;
			hw-tsu-sto = <204>;
			hw-tsu-sta = <231>;
			hw-thd-dat = <22>;
			hw-thd-sta = <162>;
			hw-tbuf = <227>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <6>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_400Khz_cci1: qcom,i2c_fast_mode {
			hw-thigh = <38>;
			hw-tlow = <56>;
			hw-tsu-sto = <40>;
			hw-tsu-sta = <40>;
			hw-thd-dat = <22>;
			hw-thd-sta = <35>;
			hw-tbuf = <62>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <6>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_custom_cci1: qcom,i2c_custom_mode {
			hw-thigh = <16>;
			hw-tlow = <22>;
			hw-tsu-sto = <17>;
			hw-tsu-sta = <18>;
			hw-thd-dat = <16>;
			hw-thd-sta = <15>;
			hw-tbuf = <24>;
			hw-scl-stretch-en = <1>;
			hw-trdhld = <3>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_1Mhz_cci1: qcom,i2c_fast_plus_mode {
			hw-thigh = <16>;
			hw-tlow = <22>;
			hw-tsu-sto = <17>;
			hw-tsu-sta = <18>;
			hw-thd-dat = <16>;
			hw-thd-sta = <15>;
			hw-tbuf = <24>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <3>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};
	};

	cam_csiphy_tpg13: qcom,tpg13@ac97000 {
		cell-index = <13>;
		phy-id     = <0>;
		compatible = "qcom,cam-tpg102";
		reg-names = "tpg0", "cam_cpas_top";
		reg = <0xac97000 0x100>,
			<0xac40000 0x1000>;
		reg-cam-base = <0x97000 0x40000>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy0_clk",
			"csi0phytimer_clk_src",
			"csi0phytimer_clk";
		clocks = <&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_CSIPHY0_CLK>,
			<&camcc CAM_CC_CSI0PHYTIMER_CLK_SRC>,
			<&camcc CAM_CC_CSI0PHYTIMER_CLK>;
		clock-rates =
			<266666667 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "csi0phytimer_clk_src";
		status = "ok";
	};

	cam_csiphy_tpg14: qcom,tpg14@ac98000 {
		cell-index = <14>;
		phy-id     = <1>;
		compatible = "qcom,cam-tpg102";
		reg-names = "tpg1", "cam_cpas_top";
		reg = <0xac98000 0x100>,
			<0xac40000 0x1000>;
		reg-cam-base = <0x98000 0x40000>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy1_clk",
			"csi1phytimer_clk_src",
			"csi1phytimer_clk";
		clocks = <&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_CSIPHY1_CLK>,
			<&camcc CAM_CC_CSI1PHYTIMER_CLK_SRC>,
			<&camcc CAM_CC_CSI1PHYTIMER_CLK>;
		clock-rates =
			<266666667 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>,
			<400000000 0 300000000 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "csi1phytimer_clk_src";
		status = "ok";
	};

	qcom,cam_smmu {
		compatible = "qcom,msm-cam-smmu", "simple-bus";
		status = "ok";
		force_cache_allocs;

		msm_cam_smmu_ife {
			compatible = "qcom,msm-cam-smmu-cb";
			iommus = <&apps_smmu 0x800 0x440>,
				<&apps_smmu 0x840 0x440>,
				<&apps_smmu 0xC00 0x440>,
				<&apps_smmu 0xC40 0x440>;
			qcom,iommu-dma-addr-pool = <0x7400000 0xd8c00000>;
			dma-coherent;
			cam-smmu-label = "ife", "ife-cdm";
			multiple-client-devices;
			ife_iova_mem_map: iova-mem-map {
				/* IO region is approximately 3.4 GB */
				iova-mem-region-io {
					iova-region-name = "io";
					iova-region-start = <0x7400000>;
					iova-region-len = <0xd8c00000>;
					iova-region-id = <0x3>;
					status = "ok";
				};
			};
		};

		msm_cam_smmu_jpeg {
			compatible = "qcom,msm-cam-smmu-cb";
			iommus = <&apps_smmu 0x2040 0x400>,
				<&apps_smmu 0x2440 0x400>;
			cam-smmu-label = "jpeg";
			qcom,iommu-dma-addr-pool = <0x7400000 0xd8c00000>;
			dma-coherent;
			jpeg_iova_mem_map: iova-mem-map {
				/* IO region is approximately 3.4 GB */
				iova-mem-region-io {
					iova-region-name = "io";
					iova-region-start = <0x7400000>;
					iova-region-len = <0xd8c00000>;
					iova-region-id = <0x3>;
					status = "ok";
				};
			};
		};

		msm_cam_icp_fw {
			compatible = "qcom,msm-cam-smmu-fw-dev";
			label="icp";
			memory-region = <&camera_mem>;
		};

		msm_cam_smmu_icp {
			compatible = "qcom,msm-cam-smmu-cb";
			iommus = <&apps_smmu 0x2000 0x400>,
				<&apps_smmu 0x2020 0x400>,
				<&apps_smmu 0x2060 0x400>,
				<&apps_smmu 0x20E2 0x400>,
				<&apps_smmu 0x2400 0x400>,
				<&apps_smmu 0x2420 0x400>,
				<&apps_smmu 0x2460 0x400>,
				<&apps_smmu 0x24E2 0x400>;
			qcom,iommu-dma-addr-pool = <0x10c00000 0xee300000>;
			dma-coherent;
			iova-region-discard = <0xdff00000 0x300000>;
			cam-smmu-label = "icp";
			icp_iova_mem_map: iova-mem-map {
				iova-mem-region-firmware {
					/* Firmware region is 5MB */
					iova-region-name = "firmware";
					iova-region-start = <0x0>;
					iova-region-len = <0x500000>;
					iova-region-id = <0x0>;
					status = "ok";
				};

				iova-mem-region-shared {
					/* Shared region is 150MB long */
					iova-region-name = "shared";
					iova-region-start = <0x7400000>;
					iova-region-len = <0x9600000>;
					iova-region-id = <0x1>;
					status = "ok";
				};

				iova-mem-region-secondary-heap {
					/* Secondary heap region is 1MB long */
					iova-region-name = "secheap";
					iova-region-start = <0x10a00000>;
					iova-region-len = <0x100000>;
					iova-region-id = <0x4>;
					status = "ok";
				};

				iova-mem-region-io {
					/* IO region is approximately 3.7 GB */
					iova-region-name = "io";
					iova-region-start = <0x10c00000>;
					iova-region-len = <0xee300000>;
					iova-region-discard = <0xdff00000 0x300000>;
					iova-region-id = <0x3>;
					status = "ok";
				};

				iova-mem-qdss-region {
					/* QDSS region is appropriate 1MB */
					iova-region-name = "qdss";
					iova-region-start = <0x10b00000>;
					iova-region-len = <0x100000>;
					iova-region-id = <0x5>;
					qdss-phy-addr = <0x16790000>;
					status = "ok";
				};
			};
		};

		msm_cam_smmu_cpas_cdm {
			compatible = "qcom,msm-cam-smmu-cb";
			iommus = <&apps_smmu 0x20C0 0x400>,
				<&apps_smmu 0x24C0 0x400>;
			cam-smmu-label = "cpas-cdm";
			qcom,iommu-dma-addr-pool = <0x7400000 0xd8c00000>;
			dma-coherent;
			cpas_cdm_iova_mem_map: iova-mem-map {
				iova-mem-region-io {
					/* IO region is approximately 3.4 GB */
					iova-region-name = "io";
					iova-region-start = <0x7400000>;
					iova-region-len = <0xd8c00000>;
					iova-region-id = <0x3>;
					status = "ok";
				};
			};
		};

		msm_cam_smmu_secure {
			compatible = "qcom,msm-cam-smmu-cb";
			cam-smmu-label = "cam-secure";
			qcom,secure-cb;
		};
	};

	qcom,cam-cdm-intf {
		compatible = "qcom,cam-cdm-intf";
		cell-index = <0>;
		label = "cam-cdm-intf";
		num-hw-cdm = <1>;
		cdm-client-names = "vfe",
			"jpegdma",
			"jpegenc";
		status = "ok";
	};

	qcom,cpas-cdm0 {
		cell-index = <0>;
		compatible = "qcom,cam-cpas-cdm1_2";
		label = "cpas-cdm";
		reg = <0xac4d000 0x1000>;
		reg-names = "cpas-cdm";
		reg-cam-base = <0x4d000>;
		interrupts = <GIC_SPI 461 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "cpas-cdm";
		regulator-names = "camss";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cam_cc_cpas_slow_ahb_clk",
			"cam_cc_cpas_ahb_clk";
		clocks = <&camcc CAM_CC_SLOW_AHB_CLK_SRC>,
			<&camcc CAM_CC_CPAS_AHB_CLK>;
		clock-rates = <0 0>;
		clock-cntl-level = "svs";
		cdm-client-names = "ife3", "ife4", "dualife";
		status = "ok";
	};

	qcom,ife-cdm0 {
		cell-index = <0>;
		compatible = "qcom,cam-ife-cdm1_2";
		label = "ife-cdm";
		reg = <0xacb4200 0x1000>;
		reg-names = "ife-cdm0";
		reg-cam-base = <0xb4200>;
		interrupts = <GIC_SPI 456 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "ife-cdm0";
		regulator-names = "camss","ife0";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife0-supply = <&cam_cc_ife_0_gdsc>;
		clock-names = "ife_0_ahb",
			"ife_0_areg",
			"ife_clk",
			"ife_axi_clk",
			"cam_cc_cpas_ahb_clk";
		clocks =
			<&camcc CAM_CC_IFE_0_AHB_CLK>,
			<&camcc CAM_CC_IFE_0_AREG_CLK>,
			<&camcc CAM_CC_IFE_0_CLK>,
			<&camcc CAM_CC_IFE_0_AXI_CLK>,
			<&camcc CAM_CC_CPAS_AHB_CLK>;
		clock-rates =
			<0 0 0 0 0>,
			<0 0 0 0 0>,
			<0 0 0 0 0>,
			<0 0 0 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		cdm-client-names = "ife0";
		status = "ok";
	};

	qcom,ife-cdm1 {
		cell-index = <1>;
		compatible = "qcom,cam-ife-cdm1_2";
		label = "ife-cdm";
		reg = <0xacc3200 0x1000>;
		reg-names = "ife-cdm1";
		reg-cam-base = <0xc3200>;
		interrupts = <GIC_SPI 287 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "ife-cdm1";
		regulator-names = "camss","ife1";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife1-supply = <&cam_cc_ife_1_gdsc>;
		clock-names = "ife_1_ahb",
			"ife_1_areg",
			"ife_clk",
			"ife_axi_clk",
			"cam_cc_cpas_ahb_clk";
		clocks =
			<&camcc CAM_CC_IFE_1_AHB_CLK>,
			<&camcc CAM_CC_IFE_1_AREG_CLK>,
			<&camcc CAM_CC_IFE_1_CLK>,
			<&camcc CAM_CC_IFE_1_AXI_CLK>,
			<&camcc CAM_CC_CPAS_AHB_CLK>;
		clock-rates =
			<0 0 0 0 0>,
			<0 0 0 0 0>,
			<0 0 0 0 0>,
			<0 0 0 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		cdm-client-names = "ife1";
		status = "ok";
	};

	qcom,ife-cdm2 {
		cell-index = <2>;
		compatible = "qcom,cam-ife-cdm1_2";
		label = "ife-cdm";
		reg = <0xacef200 0x1000>;
		reg-names = "ife-cdm2";
		reg-cam-base = <0xef200>;
		interrupts = <GIC_SPI 642 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "ife-cdm2";
		regulator-names = "camss","ife2";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife2-supply = <&cam_cc_ife_2_gdsc>;
		clock-names = "ife_2_ahb",
			"ife_2_areg",
			"ife_clk",
			"ife_axi_clk",
			"cam_cc_cpas_ahb_clk";
		clocks =
			<&camcc CAM_CC_IFE_2_AHB_CLK>,
			<&camcc CAM_CC_IFE_2_AREG_CLK>,
			<&camcc CAM_CC_IFE_2_CLK>,
			<&camcc CAM_CC_IFE_2_AXI_CLK>,
			<&camcc CAM_CC_CPAS_AHB_CLK>;
		clock-rates =
			<0 0 0 0 0>,
			<0 0 0 0 0>,
			<0 0 0 0 0>,
			<0 0 0 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		cdm-client-names = "ife2";
		status = "ok";
	};

	qcom,cam-isp {
		compatible = "qcom,cam-isp";
		arch-compat = "ife";
		status = "ok";
	};

	cam_csid0: qcom,csid0 {
		cell-index = <0>;
		compatible = "qcom,csid570";
		reg-names = "csid";
		reg = <0xacb5200 0x1000>;
		reg-cam-base = <0xb5200>;
		interrupt-names = "csid0";
		interrupts = <GIC_SPI 464 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss", "ife0";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife0-supply = <&cam_cc_ife_0_gdsc>;
		clock-names =
			"ife_csid_clk_src",
			"ife_csid_clk",
			"cphy_rx_clk_src",
			"ife_cphy_rx_clk",
			"ife_clk_src",
			"ife_clk",
			"ife_0_areg",
			"ife_0_ahb",
			"ife_axi_clk";
		clocks =
			<&camcc CAM_CC_IFE_0_CSID_CLK_SRC>,
			<&camcc CAM_CC_IFE_0_CSID_CLK>,
			<&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_IFE_0_CPHY_RX_CLK>,
			<&camcc CAM_CC_IFE_0_CLK_SRC>,
			<&camcc CAM_CC_IFE_0_CLK>,
			<&camcc CAM_CC_IFE_0_AREG_CLK>,
			<&camcc CAM_CC_IFE_0_AHB_CLK>,
			<&camcc CAM_CC_IFE_0_AXI_CLK>;
		clock-rates =
			<400000000 0 0 0 338000000 0 100000000 0 0>,
			<400000000 0 0 0 475000000 0 200000000 0 0>,
			<400000000 0 0 0 600000000 0 300000000 0 0>,
			<400000000 0 0 0 720000000 0 400000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe0: qcom,ife0 {
		cell-index = <0>;
		compatible = "qcom,vfe570";
		reg-names = "ife", "cam_camnoc";
		reg = <0xacb4000 0xd000>,
			<0xac42000 0x8000>;
		reg-cam-base = <0xb4000 0x42000>;
		interrupt-names = "ife0";
		interrupts = <GIC_SPI 465 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss", "ife0";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife0-supply = <&cam_cc_ife_0_gdsc>;
		clock-names =
			"ife_0_ahb",
			"ife_0_areg",
			"ife_clk_src",
			"ife_clk",
			"ife_axi_clk";
		clocks =
			<&camcc CAM_CC_IFE_0_AHB_CLK>,
			<&camcc CAM_CC_IFE_0_AREG_CLK>,
			<&camcc CAM_CC_IFE_0_CLK_SRC>,
			<&camcc CAM_CC_IFE_0_CLK>,
			<&camcc CAM_CC_IFE_0_AXI_CLK>;
		clock-rates =
			<0 100000000 338000000 0 0>,
			<0 200000000 475000000 0 0>,
			<0 300000000 600000000 0 0>,
			<0 400000000 720000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_clk_src";
		scl-clk-names = "ife_0_areg";
		clock-control-debugfs = "true";
		clock-names-option =  "ife_dsp_clk";
		clocks-option = <&camcc CAM_CC_IFE_0_DSP_CLK>;
		clock-rates-option = <720000000>;
		ubwc-static-cfg = <0x1016 0x1026>;
		cam_hw_pid = <28 4 16 8>;
		status = "ok";
	};

	cam_csid1: qcom,csid1 {
		cell-index = <1>;
		compatible = "qcom,csid570";
		reg-names = "csid";
		reg = <0xacc4200 0x1000>;
		reg-cam-base = <0xc4200>;
		interrupt-names = "csid1";
		interrupts = <GIC_SPI 466 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss", "ife1";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife1-supply = <&cam_cc_ife_1_gdsc>;
		clock-names =
			"ife_csid_clk_src",
			"ife_csid_clk",
			"cphy_rx_clk_src",
			"ife_cphy_rx_clk",
			"ife_clk_src",
			"ife_clk",
			"ife_1_areg",
			"ife_1_ahb",
			"ife_axi_clk";
		clocks =
			<&camcc CAM_CC_IFE_1_CSID_CLK_SRC>,
			<&camcc CAM_CC_IFE_1_CSID_CLK>,
			<&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_IFE_1_CPHY_RX_CLK>,
			<&camcc CAM_CC_IFE_1_CLK_SRC>,
			<&camcc CAM_CC_IFE_1_CLK>,
			<&camcc CAM_CC_IFE_1_AREG_CLK>,
			<&camcc CAM_CC_IFE_1_AHB_CLK>,
			<&camcc CAM_CC_IFE_1_AXI_CLK>;
		clock-rates =
			<400000000 0 0 0 338000000 0 100000000 0 0>,
			<400000000 0 0 0 475000000 0 200000000 0 0>,
			<400000000 0 0 0 600000000 0 300000000 0 0>,
			<400000000 0 0 0 720000000 0 400000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe1: qcom,ife1 {
		cell-index = <1>;
		compatible = "qcom,vfe570";
		reg-names = "ife", "cam_camnoc";
		reg = <0xacc3000 0xd000>,
			<0xac42000 0x8000>;
		reg-cam-base = <0xc3000 0x42000>;
		interrupt-names = "ife1";
		interrupts = <GIC_SPI 467 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss", "ife1";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife1-supply = <&cam_cc_ife_1_gdsc>;
		clock-names =
			"ife_1_ahb",
			"ife_1_areg",
			"ife_clk_src",
			"ife_clk",
			"ife_axi_clk";
		clocks =
			<&camcc CAM_CC_IFE_1_AHB_CLK>,
			<&camcc CAM_CC_IFE_1_AREG_CLK>,
			<&camcc CAM_CC_IFE_1_CLK_SRC>,
			<&camcc CAM_CC_IFE_1_CLK>,
			<&camcc CAM_CC_IFE_1_AXI_CLK>;
		clock-rates =
			<0 100000000 338000000 0 0>,
			<0 200000000 475000000 0 0>,
			<0 300000000 600000000 0 0>,
			<0 400000000 720000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_clk_src";
		scl-clk-names = "ife_1_areg";
		clock-control-debugfs = "true";
		clock-names-option =  "ife_dsp_clk";
		clocks-option = <&camcc CAM_CC_IFE_1_DSP_CLK>;
		clock-rates-option = <720000000>;
		ubwc-static-cfg = <0x1016 0x1026>;
		cam_hw_pid = <29 5 17 9>;
		status = "ok";
	};

	cam_csid2: qcom,csid2 {
		cell-index = <2>;
		compatible = "qcom,csid570";
		reg-names = "csid";
		reg = <0xacf0200 0x1000>;
		reg-cam-base = <0xf0200>;
		interrupt-names = "csid2";
		interrupts = <GIC_SPI 640 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss", "ife2";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife2-supply = <&cam_cc_ife_2_gdsc>;
		clock-names =
			"ife_csid_clk_src",
			"ife_csid_clk",
			"cphy_rx_clk_src",
			"ife_cphy_rx_clk",
			"ife_clk_src",
			"ife_clk",
			"ife_2_areg",
			"ife_2_ahb",
			"ife_axi_clk";
		clocks =
			<&camcc CAM_CC_IFE_2_CSID_CLK_SRC>,
			<&camcc CAM_CC_IFE_2_CSID_CLK>,
			<&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_IFE_2_CPHY_RX_CLK>,
			<&camcc CAM_CC_IFE_2_CLK_SRC>,
			<&camcc CAM_CC_IFE_2_CLK>,
			<&camcc CAM_CC_IFE_2_AREG_CLK>,
			<&camcc CAM_CC_IFE_2_AHB_CLK>,
			<&camcc CAM_CC_IFE_2_AXI_CLK>;
		clock-rates =
			<400000000 0 0 0 338000000 0 100000000 0 0>,
			<400000000 0 0 0 475000000 0 200000000 0 0>,
			<400000000 0 0 0 600000000 0 300000000 0 0>,
			<400000000 0 0 0 720000000 0 400000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe2: qcom,ife2 {
		cell-index = <2>;
		compatible = "qcom,vfe570";
		reg-names = "ife", "cam_camnoc";
		reg = <0xacef000 0xd000>,
			<0xac42000 0x8000>;
		reg-cam-base = <0xef000 0x42000>;
		interrupt-names = "ife2";
		interrupts = <GIC_SPI 641 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss", "ife2";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		ife2-supply = <&cam_cc_ife_2_gdsc>;
		clock-names =
			"ife_2_ahb",
			"ife_2_areg",
			"ife_clk_src",
			"ife_clk",
			"ife_axi_clk";
		clocks =
			<&camcc CAM_CC_IFE_2_AHB_CLK>,
			<&camcc CAM_CC_IFE_2_AREG_CLK>,
			<&camcc CAM_CC_IFE_2_CLK_SRC>,
			<&camcc CAM_CC_IFE_2_CLK>,
			<&camcc CAM_CC_IFE_2_AXI_CLK>;
		clock-rates =
			<0 100000000 338000000 0 0>,
			<0 200000000 475000000 0 0>,
			<0 300000000 600000000 0 0>,
			<0 400000000 720000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_clk_src";
		scl-clk-names = "ife_2_areg";
		clock-control-debugfs = "true";
		ubwc-static-cfg = <0x1016 0x1026>;
		cam_hw_pid = <30 6 18 10>;
		status = "ok";
	};

	cam_csid_lite0: qcom,csid-lite0 {
		cell-index = <3>;
		compatible = "qcom,csid-lite570";
		reg-names = "csid-lite";
		reg = <0xacd9200 0x1000>;
		reg-cam-base = <0xd9200>;
		interrupt-names = "csid-lite0";
		interrupts = <GIC_SPI 468 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"ife_csid_clk_src",
			"ife_csid_clk",
			"cphy_rx_clk_src",
			"ife_cphy_rx_clk",
			"ife_clk_src",
			"ife_lite_ahb",
			"ife_clk";
		clocks =
			<&camcc CAM_CC_IFE_LITE_CSID_CLK_SRC>,
			<&camcc CAM_CC_IFE_LITE_CSID_CLK>,
			<&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_IFE_LITE_CPHY_RX_CLK>,
			<&camcc CAM_CC_IFE_LITE_CLK_SRC>,
			<&camcc CAM_CC_IFE_LITE_AHB_CLK>,
			<&camcc CAM_CC_IFE_LITE_CLK>;
		clock-rates =
			<400000000 0 0 0 400000000 0 0>,
			<400000000 0 0 0 480000000 0 0>,
			<400000000 0 0 0 480000000 0 0>,
			<400000000 0 0 0 480000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe_lite0: qcom,ife-lite0 {
		cell-index = <3>;
		compatible = "qcom,vfe-lite570";
		reg-names = "ife-lite";
		reg = <0xacd9000 0x2200>;
		reg-cam-base = <0xd9000>;
		interrupt-names = "ife-lite0";
		interrupts = <GIC_SPI 469 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"ife_lite_ahb",
			"ife_lite_axi",
			"ife_clk_src",
			"ife_clk";
		clocks =
			<&camcc CAM_CC_IFE_LITE_AHB_CLK>,
			<&camcc CAM_CC_IFE_LITE_AXI_CLK>,
			<&camcc CAM_CC_IFE_LITE_CLK_SRC>,
			<&camcc CAM_CC_IFE_LITE_CLK>;
		clock-rates =
			<0 0 400000000 0>,
			<0 0 480000000 0>,
			<0 0 480000000 0>,
			<0 0 480000000 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_clk_src";
		clock-control-debugfs = "true";
		cam_hw_pid = <20>;
		status = "ok";
	};

	cam_csid_lite1: qcom,csid-lite1 {
		cell-index = <4>;
		compatible = "qcom,csid-lite570";
		reg-names = "csid-lite";
		reg = <0xacdb400 0x1000>;
		reg-cam-base = <0xdb400>;
		interrupt-names = "csid-lite1";
		interrupts = <GIC_SPI 359 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"ife_csid_clk_src",
			"ife_csid_clk",
			"cphy_rx_clk_src",
			"ife_cphy_rx_clk",
			"ife_clk_src",
			"ife_lite_ahb",
			"ife_clk";
		clocks =
			<&camcc CAM_CC_IFE_LITE_CSID_CLK_SRC>,
			<&camcc CAM_CC_IFE_LITE_CSID_CLK>,
			<&camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&camcc CAM_CC_IFE_LITE_CPHY_RX_CLK>,
			<&camcc CAM_CC_IFE_LITE_CLK_SRC>,
			<&camcc CAM_CC_IFE_LITE_AHB_CLK>,
			<&camcc CAM_CC_IFE_LITE_CLK>;
		clock-rates =
			<400000000 0 0 0 400000000 0 0>,
			<400000000 0 0 0 480000000 0 0>,
			<400000000 0 0 0 480000000 0 0>,
			<400000000 0 0 0 480000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe_lite1: qcom,ife-lite1 {
		cell-index = <4>;
		compatible = "qcom,vfe-lite570";
		reg-names = "ife-lite";
		reg = <0xacdb200 0x2200>;
		reg-cam-base = <0xdb200>;
		interrupt-names = "ife-lite1";
		interrupts = <GIC_SPI 360 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss";
		camss-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"ife_lite_ahb",
			"ife_lite_axi",
			"ife_clk_src",
			"ife_clk";
		clocks =
			<&camcc CAM_CC_IFE_LITE_AHB_CLK>,
			<&camcc CAM_CC_IFE_LITE_AXI_CLK>,
			<&camcc CAM_CC_IFE_LITE_CLK_SRC>,
			<&camcc CAM_CC_IFE_LITE_CLK>;
		clock-rates =
			<0 0 400000000 0>,
			<0 0 480000000 0>,
			<0 0 480000000 0>,
			<0 0 480000000 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		src-clock-name = "ife_clk_src";
		clock-control-debugfs = "true";
		cam_hw_pid = <19>;
		status = "ok";
	};

	qcom,cam-icp {
		compatible = "qcom,cam-icp";
		compat-hw-name = "qcom,icp",
			"qcom,ipe0",
			"qcom,bps";
		num-icp = <1>;
		num-ipe = <1>;
		num-bps = <1>;
		status = "ok";
		icp_pc_en;
		ipe_bps_pc_en;
	};

	cam_icp: qcom,icp {
		cell-index = <0>;
		compatible = "qcom,cam-icp_v1";
		icp-version = <0x0100>;
		reg = <0xac00000 0x6000>,
			<0xac10000 0x8000>,
			<0xac18000 0x3000>;
		reg-names = "icp_qgic", "icp_sierra", "icp_csr";
		reg-cam-base = <0x00000 0x10000 0x18000>;
		interrupts = <GIC_SPI 463 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "icp";
		regulator-names = "camss-vdd";
		camss-vdd-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"soc_fast_ahb",
			"icp_ahb_clk",
			"icp_clk_src",
			"icp_clk";
		src-clock-name = "icp_clk_src";
		clocks =
			<&camcc CAM_CC_FAST_AHB_CLK_SRC>,
			<&camcc CAM_CC_ICP_AHB_CLK>,
			<&camcc CAM_CC_ICP_CLK_SRC>,
			<&camcc CAM_CC_ICP_CLK>;

		clock-rates =
			<100000000 0 400000000 0>,
			<200000000 0 480000000 0>,
			<300000000 0 600000000 0>,
			<400000000 0 600000000 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		fw_name = "CAMERA_ICP_480.elf";
		ubwc-ipe-fetch-cfg = <0x7073 0x707b>;
		ubwc-ipe-write-cfg = <0x161cf 0x161ef>;
		ubwc-bps-fetch-cfg = <0x7073 0x707b>;
		ubwc-bps-write-cfg = <0x161cf 0x161ef>;
		qos-val = <0x00000A0A>;
		status = "ok";
	};

	cam_ipe0: qcom,ipe0 {
		cell-index = <0>;
		compatible = "qcom,cam-ipe";
		reg = <0xac9a000 0x12000>;
		reg-names = "ipe0_top";
		reg-cam-base = <0x9a000>;
		regulator-names = "ipe0-vdd";
		ipe0-vdd-supply = <&cam_cc_ipe_0_gdsc>;
		clock-names =
			"ipe_0_ahb_clk",
			"ipe_0_areg_clk",
			"ipe_0_axi_clk",
			"ipe_0_clk_src",
			"ipe_0_clk";
		src-clock-name = "ipe_0_clk_src";
		clock-control-debugfs = "true";
		clocks =
			<&camcc CAM_CC_IPE_0_AHB_CLK>,
			<&camcc CAM_CC_IPE_0_AREG_CLK>,
			<&camcc CAM_CC_IPE_0_AXI_CLK>,
			<&camcc CAM_CC_IPE_0_CLK_SRC>,
			<&camcc CAM_CC_IPE_0_CLK>;

		clock-rates =
			<0 0 0 300000000 0>,
			<0 0 0 450000000 0>,
			<0 0 0 560000000 0>,
			<0 0 0 700000000 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		status = "ok";
	};

	cam_bps: qcom,bps {
		cell-index = <0>;
		compatible = "qcom,cam-bps";
		reg = <0xac7a000 0x8000>;
		reg-names = "bps_top";
		reg-cam-base = <0x7a000>;
		regulator-names = "bps-vdd";
		bps-vdd-supply = <&cam_cc_bps_gdsc>;
		clock-names =
			"bps_ahb_clk",
			"bps_areg_clk",
			"bps_axi_clk",
			"bps_clk_src",
			"bps_clk";
		src-clock-name = "bps_clk_src";
		clock-control-debugfs = "true";
		clocks =
			<&camcc CAM_CC_BPS_AHB_CLK>,
			<&camcc CAM_CC_BPS_AREG_CLK>,
			<&camcc CAM_CC_BPS_AXI_CLK>,
			<&camcc CAM_CC_BPS_CLK_SRC>,
			<&camcc CAM_CC_BPS_CLK>;

		clock-rates =
			<0 0 0 200000000 0>,
			<0 0 0 400000000 0>,
			<0 0 0 480000000 0>,
			<0 0 0 600000000 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal";
		status = "ok";
	};

	qcom,cam-jpeg {
		compatible = "qcom,cam-jpeg";
		compat-hw-name = "qcom,jpegenc",
			"qcom,jpegdma";
		num-jpeg-enc = <1>;
		num-jpeg-dma = <1>;
		status = "ok";
	};

	cam_jpeg_enc: qcom,jpegenc {
		cell-index = <0>;
		compatible = "qcom,cam_jpeg_enc";
		reg-names = "jpege_hw";
		reg = <0xac53000 0x4000>;
		reg-cam-base = <0x53000>;
		interrupt-names = "jpeg";
		interrupts = <GIC_SPI 474 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss-vdd";
		camss-vdd-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"jpegenc_clk_src",
			"jpegenc_clk";
		clocks =
			<&camcc CAM_CC_JPEG_CLK_SRC>,
			<&camcc CAM_CC_JPEG_CLK>;

		clock-rates = <600000000 0>;
		src-clock-name = "jpegenc_clk_src";
		clock-cntl-level = "nominal";
		cam_hw_pid = <25 26>;
		cam_hw_rd_mid = <0>;
		cam_hw_wr_mid = <1>;
		status = "ok";
	};

	cam_jpeg_dma: qcom,jpegdma {
		cell-index = <0>;
		compatible = "qcom,cam_jpeg_dma";
		reg-names = "jpegdma_hw";
		reg = <0xac57000 0x4000>;
		reg-cam-base = <0x57000>;
		interrupt-names = "jpegdma";
		interrupts = <GIC_SPI 475 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "camss-vdd";
		camss-vdd-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"jpegdma_clk_src",
			"jpegdma_clk";
		clocks =
			<&camcc CAM_CC_JPEG_CLK_SRC>,
			<&camcc CAM_CC_JPEG_CLK>;
		clock-rates = <600000000 0>;
		src-clock-name = "jpegdma_clk_src";
		clock-cntl-level = "nominal";
		cam_hw_pid = <24 27>;
		cam_hw_rd_mid = <0>;
		cam_hw_wr_mid = <1>;
		status = "ok";
	};

	qcom,cam-cpas {
		cell-index = <0>;
		compatible = "qcom,cam-cpas";
		label = "cpas";
		arch-compat = "cpas_top";
		status = "ok";
		reg-names = "cam_cpas_top", "cam_camnoc", "cam_rpmh";
		reg = <0xac40000 0x1000>,
			<0xac42000 0x8000>,
			<0xbbf0000 0x1F00>;
		reg-cam-base = <0x40000 0x42000 0x0BBF0000>;
		cam_hw_fuse = <CAM_CPAS_ISP_FUSE 0x221C8130 0x200000 CAM_CPAS_FEATURE_TYPE_DISABLE 0x4>,
			<CAM_CPAS_ISP_LITE_FUSE 0x221C8130 0x400000 CAM_CPAS_FEATURE_TYPE_DISABLE 0x10>,
			<CAM_CPAS_QCFA_BINNING_ENABLE 0x221C8130 0x1000000 CAM_CPAS_FEATURE_TYPE_DISABLE 0xFF>,
			<CAM_CPAS_MF_HDR_ENABLE 0x221C8130 0x2 CAM_CPAS_FEATURE_TYPE_ENABLE 0xFF>,
			<CAM_CPAS_MP_LIMIT_FUSE 0x221C8130 0x3000 CAM_CPAS_FEATURE_TYPE_VALUE 0xFF>,
			<CAM_CPAS_CSIPHY_FUSE 0x221C8130 0x2000000 CAM_CPAS_FEATURE_TYPE_DISABLE 0x10>;
		interrupt-names = "cpas_camnoc";
		interrupts = <GIC_SPI 459 IRQ_TYPE_EDGE_RISING>;
		camnoc-axi-min-ib-bw = <3000000000>;
		regulator-names = "camss-vdd";
		camss-vdd-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"gcc_axi_hf_clk",
			"gcc_axi_sf_clk",
			"slow_ahb_clk_src",
			"cpas_ahb_clk",
			"cpas_core_ahb_clk",
			"camnoc_axi_clk_src",
			"camnoc_axi_clk";
		clocks =
			<&gcc GCC_CAMERA_HF_AXI_CLK>,
			<&gcc GCC_CAMERA_SF_AXI_CLK>,
			<&camcc CAM_CC_SLOW_AHB_CLK_SRC>,
			<&camcc CAM_CC_CPAS_AHB_CLK>,
			<&camcc CAM_CC_CORE_AHB_CLK>,
			<&camcc CAM_CC_CAMNOC_AXI_CLK_SRC>,
			<&camcc CAM_CC_CAMNOC_AXI_CLK>;
		src-clock-name = "camnoc_axi_clk_src";
		clock-rates =
			<0 0 0 0 0 0 0>,
			<0 0 80000000 0 0 300000000 0>,
			<0 0 80000000 0 0 400000000 0>,
			<0 0 80000000 0 0 400000000 0>,
			<0 0 80000000 0 0 480000000 0>;
		clock-cntl-level = "suspend", "lowsvs", "svs", "svs_l1", "nominal";
		control-camnoc-axi-clk;
		camnoc-bus-width = <32>;
		camnoc-axi-clk-bw-margin-perc = <20>;
		interconnect-names = "cam_ahb";
		interconnects =<&gem_noc MASTER_APPSS_PROC
			&config_noc SLAVE_CAMERA_CFG>;
		rpmh-bcm-info = <12 0x4 0x800 0 4>;
		cam-ahb-num-cases = <8>;
		cam-ahb-bw-KBps =
			<0 0>, <0 76800>, <0 76800>, <0 150000>, <0 150000>,
			<0 300000>, <0 300000>, <0 300000>;
		vdd-corners = <RPMH_REGULATOR_LEVEL_RETENTION
			RPMH_REGULATOR_LEVEL_MIN_SVS
			RPMH_REGULATOR_LEVEL_LOW_SVS
			RPMH_REGULATOR_LEVEL_SVS
			RPMH_REGULATOR_LEVEL_SVS_L1
			RPMH_REGULATOR_LEVEL_NOM
			RPMH_REGULATOR_LEVEL_NOM_L1
			RPMH_REGULATOR_LEVEL_NOM_L2
			RPMH_REGULATOR_LEVEL_TURBO
			RPMH_REGULATOR_LEVEL_TURBO_L1>;
		vdd-corner-ahb-mapping = "suspend", "lowsvs",
			"lowsvs", "svs", "svs_l1",
			"nominal", "nominal", "nominal",
			"turbo", "turbo";
		client-id-based;
		client-names =
			"csiphy0", "csiphy1", "csiphy2", "csiphy3",
			"csiphy4", "cci0", "cci1",
			"csid0", "csid1", "csid2", "csid3",
			"csid4", "ife0", "ife1", "ife2", "ife3", "ife4",
			"ipe0", "cam-cdm-intf0","ife-cdm0", "ife-cdm1",
			"ife-cdm2", "cpas-cdm0", "bps0", "icp0", "jpeg-dma0",
			"jpeg-enc0", "tpg13", "tpg14";

		camera-bus-nodes {
			level3-nodes {
				level-index = <3>;
				level3_rt0_rd_wr_sum: level3-rt0-rd-wr-sum {
					cell-index = <0>;
					node-name = "level3-rt0-rd-wr-sum";
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
					ib-bw-voting-needed;
					qcom,axi-port-mnoc {
						interconnect-names = "cam_hf_0";
						interconnects =
						<&mmss_noc MASTER_CAMNOC_HF
						&mc_virt SLAVE_EBI1>;
					};
				};

				level3_nrt0_rd_wr_sum: level3-nrt0-rd-wr-sum {
					cell-index = <1>;
					node-name = "level3-nrt0-rd-wr-sum";
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
					qcom,axi-port-mnoc {
						interconnect-names = "cam_sf_0";
						interconnects =
						<&mmss_noc MASTER_CAMNOC_SF
						&mc_virt SLAVE_EBI1>;
					};
				};

				level3_nrt1_rd_wr_sum: level3-nrt1-rd-wr-sum {
					cell-index = <2>;
					node-name = "level3-nrt1-rd-wr-sum";
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
					qcom,axi-port-mnoc {
						interconnect-names =
							"cam_sf_icp";
						interconnects =
						<&mmss_noc MASTER_CAMNOC_ICP
						&mc_virt SLAVE_EBI1>;
					};
				};
			};

			level2-nodes {
				level-index = <2>;
				camnoc-max-needed;
				level2_rt0_wr: level2-rt0-wr {
					cell-index = <3>;
					node-name = "level2-rt0-wr";
					parent-node = <&level3_rt0_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM_INTERLEAVE>;
				};

				level2_rt0_rd: level2-rt0-rd {
					cell-index = <4>;
					node-name = "level2-rt0-rd";
					parent-node = <&level3_rt0_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM_INTERLEAVE>;
				};

				level2_nrt0_wr: level2-nrt0-wr {
					cell-index = <5>;
					node-name = "level2-nrt0-wr";
					parent-node = <&level3_nrt0_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM_INTERLEAVE>;
				};

				level2_nrt0_rd: level2-nrt0-rd {
					cell-index = <6>;
					node-name = "level2-nrt0-rd";
					parent-node = <&level3_nrt0_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM_INTERLEAVE>;
				};

				level2_nrt1_rd: level2-nrt1-rd {
					cell-index = <7>;
					node-name = "level2-nrt1-rd";
					parent-node = <&level3_nrt1_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
					bus-width-factor = <4>;
				};
			};

			level1-nodes {
				level-index = <1>;
				camnoc-max-needed;
				level1_rt0_wr0: level1-rt0-wr0 {
					cell-index = <8>;
					node-name = "level1-rt0-wr0";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_wr1: level1-rt0-wr1 {
					cell-index = <9>;
					node-name = "level1-rt0-wr1";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_rd0: level1-rt0-rd0 {
					cell-index = <10>;
					node-name = "level1-rt0-rd0";
					parent-node = <&level2_rt0_rd>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_wr2: level1-rt0-wr2 {
					cell-index = <11>;
					node-name = "level1-rt0-wr2";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_nrt0_wr0: level1-nrt0-wr0 {
					cell-index = <12>;
					node-name = "level1-nrt0-wr0";
					parent-node = <&level2_nrt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_nrt0_rd0: level1-nrt0-rd0 {
					cell-index = <13>;
					node-name = "level1-nrt0-rd0";
					parent-node = <&level2_nrt0_rd>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_nrt0_wr1: level1-nrt0-wr1 {
					cell-index = <14>;
					node-name = "level1-nrt0-wr1";
					parent-node = <&level2_nrt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_nrt0_rd1: level1-nrt0-rd1 {
					cell-index = <15>;
					node-name = "level1-nrt0-rd2";
					parent-node = <&level2_nrt0_rd>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};
			};

			level0-nodes {
				level-index = <0>;
				ife2_ubwc_stats_wr: ife2-ubwc-stats-wr {
					cell-index = <16>;
					node-name = "ife2-ubwc-stats-wr";
					client-name = "ife2";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_UBWC_STATS>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_VID
					CAM_CPAS_PATH_DATA_IFE_DISP
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr0>;
				};

				ife0_ubwc_stats_wr: ife0-ubwc-stats-wr {
					cell-index = <17>;
					node-name = "ife0-ubwc-stats-wr";
					client-name = "ife0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_UBWC_STATS>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_VID
					CAM_CPAS_PATH_DATA_IFE_DISP
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr0>;
				};

				ife1_ubwc_stats_wr: ife1-ubwc-stats-wr {
					cell-index = <18>;
					node-name = "ife1-ubwc-stats-wr";
					client-name = "ife1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_UBWC_STATS>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_VID
					CAM_CPAS_PATH_DATA_IFE_DISP
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr0>;
				};

				ife0_linear_pdaf_wr: ife0-linear-pdaf-wr {
					cell-index = <19>;
					node-name = "ife0-linear-pdaf-wr";
					client-name = "ife0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR_PDAF>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR
					CAM_CPAS_PATH_DATA_IFE_PDAF>;
					parent-node = <&level1_rt0_wr1>;
				};

				ife1_linear_pdaf_wr: ife1-linear-pdaf-wr {
					cell-index = <20>;
					node-name = "ife1-linear-pdaf-wr";
					client-name = "ife1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR_PDAF>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR
					CAM_CPAS_PATH_DATA_IFE_PDAF>;
					parent-node = <&level1_rt0_wr1>;
				};

				ife2_linear_pdaf_wr: ife2-linear-pdaf-wr {
					cell-index = <21>;
					node-name = "ife2-linear-pdaf-wr";
					client-name = "ife2";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR_PDAF>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR
					CAM_CPAS_PATH_DATA_IFE_PDAF>;
					parent-node = <&level1_rt0_wr1>;
				};

				ife0_rdi_all_rd: ife0-rdi-all-rd {
					cell-index = <22>;
					node-name = "ife0-rdi-all-rd";
					client-name = "ife0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3>;
					parent-node = <&level1_rt0_rd0>;
				};

				ife1_rdi_all_rd: ife1-rdi-all-rd {
					cell-index = <23>;
					node-name = "ife1-rdi-all-rd";
					client-name = "ife1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3>;
					parent-node = <&level1_rt0_rd0>;
				};

				ife2_rdi_all_rd: ife2-rdi-all-rd {
					cell-index = <24>;
					node-name = "ife2-rdi-all-rd";
					client-name = "ife2";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3>;
					parent-node = <&level1_rt0_rd0>;
				};

				ife0_rdi_pixel_raw_wr: ife0-rdi-pixel-raw-wr {
					cell-index = <25>;
					node-name = "ife0-rdi-pixel-raw-wr";
					client-name = "ife0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_PIXEL_RAW>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW>;
					parent-node = <&level1_rt0_wr2>;
				};

				ife1_rdi_pixel_raw_wr: ife1-rdi-pixel-raw-wr {
					cell-index = <26>;
					node-name = "ife1-rdi-pixel-raw-wr";
					client-name = "ife1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_PIXEL_RAW>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW>;
					parent-node = <&level1_rt0_wr2>;
				};

				ife2_rdi_pixel_raw_wr: ife2-rdi-pixel-raw-wr {
					cell-index = <27>;
					node-name = "ife2-rdi-pixel-raw-wr";
					client-name = "ife2";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW>;
					parent-node = <&level1_rt0_wr2>;
				};

				ife3_rdi_all_wr: ife3-rdi-all-wr {
					cell-index = <28>;
					node-name = "ife3-rdi-all-wr";
					client-name = "ife3";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3>;
					parent-node = <&level1_rt0_wr2>;
				};

				ife4_rdi_all_wr: ife4-rdi-all-wr {
					cell-index = <29>;
					node-name = "ife4-rdi-all-wr";
					client-name = "ife4";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3>;
					parent-node = <&level1_rt0_wr2>;
				};

				ipe0_all_wr: ipe0-all-wr {
					cell-index = <30>;
					node-name = "ipe0-all-wr";
					client-name = "ipe0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IPE_WR_VID
					CAM_CPAS_PATH_DATA_IPE_WR_DISP
					CAM_CPAS_PATH_DATA_IPE_WR_REF>;
					parent-node = <&level1_nrt0_wr0>;
				};

				bps0_all_wr: bps0-all-wr {
					cell-index = <31>;
					node-name = "bps0-all-wr";
					client-name = "bps0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_nrt0_wr0>;
				};

				ipe0_ref_rd: ipe0-ref-rd {
					cell-index = <32>;
					node-name = "ipe0-ref-rd";
					client-name = "ipe0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IPE_RD_REF>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd0>;
				};

				bps0_all_rd: bps0-all-rd {
					cell-index = <33>;
					node-name = "bps0-all-rd";
					client-name = "bps0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd0>;
				};

				ipe0_in_rd: ipe0-in-rd {
					cell-index = <34>;
					node-name = "ipe0-in-rd";
					client-name = "ipe0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IPE_RD_IN>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level2_nrt0_rd>;
				};

				jpeg_enc0_all_wr: jpeg-enc0-all-wr {
					cell-index = <35>;
					node-name = "jpeg-enc0-all-wr";
					client-name = "jpeg-enc0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_nrt0_wr1>;
				};

				jpeg_dma0_all_wr: jpeg-dma0-all-wr {
					cell-index = <36>;
					node-name = "jpeg-dma0-all-wr";
					client-name = "jpeg-dma0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_nrt0_wr1>;
				};

				jpeg_enc0_all_rd: jpeg-enc0-all-rd {
					cell-index = <37>;
					node-name = "jpeg-enc0-all-rd";
					client-name = "jpeg-enc0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd1>;
				};

				jpeg_dma0_all_rd: jpeg-dma0-all-rd {
					cell-index = <38>;
					node-name = "jpeg-dma0-all-rd";
					client-name = "jpeg-dma0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd1>;
				};

				cpas_cdm0_all_rd: cpas-cdm0-all-rd {
					cell-index = <39>;
					node-name = "cpas-cdm0-all-rd";
					client-name = "cpas-cdm0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level2_nrt0_rd>;
				};

				icp0_all_rd: icp0-all-rd {
					cell-index = <40>;
					node-name = "icp0-all-rd";
					client-name = "icp0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level2_nrt1_rd>;
				};
			};
		};
	};
};
