&soc {
	/* QUPv3_0  wrapper  instance */
	qupv3_0: qcom,qupv3_0_geni_se@9c0000 {
		compatible = "qcom,geni-se-qup";
		reg = <0x9c0000 0x6000>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		clock-names = "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		iommus = <&apps_smmu 0x403 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0x10000000>;
		qcom,iommu-geometry = <0x40000000 0x10000000>;
		qcom,iommu-dma = "fastmap";
		dma-coherent;
		status = "ok";

		qupv3_se0_i2c: i2c@980000 {
			compatible = "qcom,i2c-geni";
			reg = <0x980000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 550 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se0_i2c_active>;
			pinctrl-1 = <&qupv3_se0_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se0_spi: spi@980000 {
			compatible = "qcom,spi-geni";
			reg = <0x980000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 550 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se0_spi_active>;
			pinctrl-1 = <&qupv3_se0_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se1_i2c: i2c@984000 {
			compatible = "qcom,i2c-geni";
			reg = <0x984000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 551 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S1_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se1_i2c_active>;
			pinctrl-1 = <&qupv3_se1_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se1_spi: spi@984000 {
			compatible = "qcom,spi-geni";
			reg = <0x984000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 551 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S1_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se1_spi_active>;
			pinctrl-1 = <&qupv3_se1_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se2_i2c: i2c@988000 {
			compatible = "qcom,i2c-geni";
			reg = <0x988000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 529 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se2_i2c_active>;
			pinctrl-1 = <&qupv3_se2_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se2_spi: spi@988000 {
			compatible = "qcom,spi-geni";
			reg = <0x988000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 529 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se2_spi_active>;
			pinctrl-1 = <&qupv3_se2_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se3_i2c: i2c@98c000 {
			compatible = "qcom,i2c-geni";
			reg = <0x98c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 530 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se3_i2c_active>;
			pinctrl-1 = <&qupv3_se3_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se3_spi: spi@98c000 {
			compatible = "qcom,spi-geni";
			reg = <0x98c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 530 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se3_spi_active>;
			pinctrl-1 = <&qupv3_se3_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se4_i2c: i2c@990000 {
			compatible = "qcom,i2c-geni";
			reg = <0x990000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 531 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S4_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se4_i2c_active>;
			pinctrl-1 = <&qupv3_se4_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se4_spi: spi@990000 {
			compatible = "qcom,spi-geni";
			reg = <0x990000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 531 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S4_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se4_spi_active>;
			pinctrl-1 = <&qupv3_se4_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se5_i2c: i2c@994000 {
			compatible = "qcom,i2c-geni";
			reg = <0x994000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 535 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se5_i2c_active>;
			pinctrl-1 = <&qupv3_se5_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se5_spi: spi@994000 {
			compatible = "qcom,spi-geni";
			reg = <0x994000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 535 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se5_spi_active>;
			pinctrl-1 = <&qupv3_se5_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se5_2uart: qcom,qup_uart@994000 {
			compatible = "qcom,msm-geni-serial-hs";
			reg = <0x994000 0x4000>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 535 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP0_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_0 &clk_virt SLAVE_QUP_CORE_0>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_0>,
			<&aggre2_noc MASTER_QUP_0  &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se5_2uart_active>;
			pinctrl-1 = <&qupv3_se5_2uart_sleep>;
			status = "disabled";
		};
	};

	/* QUPv3_1  wrapper  instance */
	qupv3_1: qcom,qupv3_1_geni_se@ac0000 {
		compatible = "qcom,geni-se-qup";
		reg = <0xac0000 0x6000>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		clock-names = "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		iommus = <&apps_smmu 0x443 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0x10000000>;
		qcom,iommu-geometry = <0x40000000 0x10000000>;
		qcom,iommu-dma = "fastmap";
		status = "ok";

		qupv3_se7_i2c: i2c@a80000 {
			compatible = "qcom,i2c-geni";
			reg = <0xa80000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 353 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se7_i2c_active>;
			pinctrl-1 = <&qupv3_se7_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se7_spi: spi@a80000 {
			compatible = "qcom,spi-geni";
			reg = <0xa80000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 353 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se7_spi_active>;
			pinctrl-1 = <&qupv3_se7_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se8_i2c: i2c@a84000 {
			compatible = "qcom,i2c-geni";
			reg = <0xa84000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 354 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S1_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se8_i2c_active>;
			pinctrl-1 = <&qupv3_se8_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se8_spi: spi@a84000 {
			compatible = "qcom,spi-geni";
			reg = <0xa84000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 354 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S1_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se8_spi_active>;
			pinctrl-1 = <&qupv3_se8_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se9_i2c: i2c@a88000 {
			compatible = "qcom,i2c-geni";
			reg = <0xa88000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 355 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se9_i2c_active>;
			pinctrl-1 = <&qupv3_se9_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se9_spi: spi@a88000 {
			compatible = "qcom,spi-geni";
			reg = <0xa88000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 355 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se9_spi_active>;
			pinctrl-1 = <&qupv3_se9_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		/* Debug UART Instance for RUMI*/
		qupv3_se9_2uart: qcom,qup_uart@a88000 {
			compatible = "qcom,geni-debug-uart";
			reg = <0xa88000 0x4000>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 355 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se";
			clocks = <&gcc GCC_QUPV3_WRAP1_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se9_2uart_active>;
			pinctrl-1 = <&qupv3_se9_2uart_sleep>;
			status = "disabled";
		};

		qupv3_se10_i2c: i2c@a8c000 {
			compatible = "qcom,i2c-geni";
			reg = <0xa8c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 356 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se10_i2c_active>;
			pinctrl-1 = <&qupv3_se10_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se10_spi: spi@a8c000 {
			compatible = "qcom,spi-geni";
			reg = <0xa8c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 356 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se10_spi_active>;
			pinctrl-1 = <&qupv3_se10_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		/* Debug UART Instance */
		qupv3_se10_2uart: qcom,qup_uart@a8c000 {
			compatible = "qcom,geni-debug-uart";
			reg = <0xa8c000 0x4000>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 356 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se";
			clocks = <&gcc GCC_QUPV3_WRAP1_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se10_2uart_active>;
			pinctrl-1 = <&qupv3_se10_2uart_sleep>;
			status = "disabled";
		};

		qupv3_se11_i2c: i2c@a90000 {
			compatible = "qcom,i2c-geni";
			reg = <0xa90000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 357 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S4_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se11_i2c_active>;
			pinctrl-1 = <&qupv3_se11_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se11_spi: spi@a90000 {
			compatible = "qcom,spi-geni";
			reg = <0xa90000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 357 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S4_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se11_spi_active>;
			pinctrl-1 = <&qupv3_se11_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se12_i2c: i2c@a94000 {
			compatible = "qcom,i2c-geni";
			reg = <0xa94000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 358 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se12_i2c_active>;
			pinctrl-1 = <&qupv3_se12_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se12_spi: spi@a94000 {
			compatible = "qcom,spi-geni";
			reg = <0xa94000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 358 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se12_spi_active>;
			pinctrl-1 = <&qupv3_se12_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se12_4uart: qcom,qup_uart@a94000 {
			compatible = "qcom,msm-geni-serial-hs";
			reg = <0xa94000 0x4000>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 585 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "active", "sleep", "shutdown";
			pinctrl-0 = <&qupv3_se12_default_cts>,
					<&qupv3_se12_default_rtsrx>, <&qupv3_se12_default_tx>;
			pinctrl-1 = <&qupv3_se12_ctsrx>, <&qupv3_se12_rts>,
					<&qupv3_se12_tx>;
			pinctrl-2 = <&qupv3_se12_ctsrx>, <&qupv3_se12_rts>,
					<&qupv3_se12_tx>;
			pinctrl-3 = <&qupv3_se12_default_cts>,
					<&qupv3_se12_default_rtsrx>, <&qupv3_se12_default_tx>;
			status = "disabled";
		};

		qupv3_se13_i2c: i2c@a98000 {
			compatible = "qcom,i2c-geni";
			reg = <0xa98000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 836 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP1_S6_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_1 &clk_virt SLAVE_QUP_CORE_1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_1>,
			<&aggre2_noc MASTER_QUP_1 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se13_i2c_active>;
			pinctrl-1 = <&qupv3_se13_i2c_sleep>;
			status = "disabled";
		};
	};

	/* QUPv3_2  wrapper  instance */
	qupv3_2: qcom,qupv3_2_geni_se@8c0000 {
		compatible = "qcom,geni-se-qup";
		reg = <0x8c0000 0x6000>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		clock-names = "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		iommus = <&apps_smmu 0x5a3  0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0x10000000>;
		qcom,iommu-geometry = <0x40000000 0x10000000>;
		qcom,iommu-dma = "fastmap";
		status = "ok";

		qupv3_se14_i2c: i2c@880000 {
			compatible = "qcom,i2c-geni";
			reg = <0x880000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 373 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se14_i2c_active>;
			pinctrl-1 = <&qupv3_se14_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se14_spi: spi@880000 {
			compatible = "qcom,spi-geni";
			reg = <0x880000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 373 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se14_spi_active>;
			pinctrl-1 = <&qupv3_se14_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se15_i2c: i2c@884000 {
			compatible = "qcom,i2c-geni";
			reg = <0x884000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 583 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S1_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se15_i2c_active>;
			pinctrl-1 = <&qupv3_se15_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se15_spi: spi@884000 {
			compatible = "qcom,spi-geni";
			reg = <0x884000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 583 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S1_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se15_spi_active>;
			pinctrl-1 = <&qupv3_se15_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se16_i2c: i2c@888000 {
			compatible = "qcom,i2c-geni";
			reg = <0x888000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 584 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se16_i2c_active>;
			pinctrl-1 = <&qupv3_se16_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se16_spi: spi@888000 {
			compatible = "qcom,spi-geni";
			reg = <0x888000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 584 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S2_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se16_spi_active>;
			pinctrl-1 = <&qupv3_se16_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se17_i2c: i2c@88c000 {
			compatible = "qcom,i2c-geni";
			reg = <0x88c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 585 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se17_i2c_active>;
			pinctrl-1 = <&qupv3_se17_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se17_spi: spi@88c000 {
			compatible = "qcom,spi-geni";
			reg = <0x88c000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 585 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se17_spi_active>;
			pinctrl-1 = <&qupv3_se17_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		/* BT UART Instance */
		qupv3_se17_4uart: qcom,qup_uart@88c000 {
			compatible = "qcom,msm-geni-serial-hs";
			reg = <0x88c000 0x4000>;
			reg-names = "se_phys";
			interrupts-extended = <&intc GIC_SPI 585 IRQ_TYPE_LEVEL_HIGH>,
					<&tlmm 94 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S3_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "active", "sleep", "shutdown";
			pinctrl-0 = <&qupv3_se17_default_cts>,
					<&qupv3_se17_default_rtsrx>, <&qupv3_se17_default_tx>;
			pinctrl-1 = <&qupv3_se17_ctsrx>, <&qupv3_se17_rts>,
					<&qupv3_se17_tx>;
			pinctrl-2 = <&qupv3_se17_ctsrx>, <&qupv3_se17_rts>,
					<&qupv3_se17_tx>;
			pinctrl-3 = <&qupv3_se17_default_cts>,
					<&qupv3_se17_default_rtsrx>, <&qupv3_se17_default_tx>;
			qcom,wakeup-byte = <0xFD>;
			status = "disabled";
		};

		qupv3_se18_i2c: i2c@890000 {
			compatible = "qcom,i2c-geni";
			reg = <0x890000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 586 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S4_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se18_i2c_active>;
			pinctrl-1 = <&qupv3_se18_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se18_spi: spi@890000 {
			compatible = "qcom,spi-geni";
			reg = <0x890000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 586 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S4_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se18_spi_active>;
			pinctrl-1 = <&qupv3_se18_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se19_i2c: i2c@894000 {
			compatible = "qcom,i2c-geni";
			reg = <0x894000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 587 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se19_i2c_active>;
			pinctrl-1 = <&qupv3_se19_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se19_spi: spi@894000 {
			compatible = "qcom,spi-geni";
			reg = <0x894000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 587 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S5_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se19_spi_active>;
			pinctrl-1 = <&qupv3_se19_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};

		qupv3_se20_i2c: i2c@898000 {
			compatible = "qcom,i2c-geni";
			reg = <0x898000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 834 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S6_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se20_i2c_active>;
			pinctrl-1 = <&qupv3_se20_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se20_spi: spi@898000 {
			compatible = "qcom,spi-geni";
			reg = <0x898000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 834 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP2_S6_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_2 &clk_virt SLAVE_QUP_CORE_2>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_2>,
			<&aggre2_noc MASTER_QUP_2 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se20_spi_active>;
			pinctrl-1 = <&qupv3_se20_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};
	};

	/* QUPv3_3  wrapper  instance */
	qupv3_3: qcom,qupv3_3_geni_se@bc0000 {
		compatible = "qcom,geni-se-qup";
		reg = <0xbc0000 0x6000>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		clock-names = "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP_3_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_3_S_AHB_CLK>;
		iommus = <&apps_smmu 0x43 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0x10000000>;
		qcom,iommu-geometry = <0x40000000 0x10000000>;
		qcom,iommu-dma = "fastmap";
		dma-coherent;
		status = "ok";

		qupv3_se21_i2c: i2c@b80000 {
			compatible = "qcom,i2c-geni";
			reg = <0xb80000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 831 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP3_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_3 &clk_virt SLAVE_QUP_CORE_3>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_3>,
			<&aggre1_noc MASTER_QUP_3 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se21_i2c_active>;
			pinctrl-1 = <&qupv3_se21_i2c_sleep>;
			status = "disabled";
		};

		qupv3_se21_spi: spi@b80000 {
			compatible = "qcom,spi-geni";
			reg = <0xb80000 0x4000>;
			#address-cells = <1>;
			#size-cells = <0>;
			reg-names = "se_phys";
			interrupts = <GIC_SPI 831 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "se-clk";
			clocks = <&gcc GCC_QUPV3_WRAP3_S0_CLK>;
			interconnect-names = "qup-core", "qup-config", "qup-memory";
			interconnects =
			<&clk_virt MASTER_QUP_CORE_3 &clk_virt SLAVE_QUP_CORE_3>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_QUP_3>,
			<&aggre1_noc MASTER_QUP_3 &mc_virt  SLAVE_EBI1>;
			pinctrl-names = "default", "sleep";
			pinctrl-0 = <&qupv3_se21_spi_active>;
			pinctrl-1 = <&qupv3_se21_spi_sleep>;
			spi-max-frequency = <50000000>;
			status = "disabled";
		};
	};
};
