Qualcomm Technologies, Inc. Audio devices for ALSA sound SoC

* msm-pcm

Required properties:

 - compatible : "qcom,msm-pcm-dsp"

 - qcom,msm-pcm-dsp-id : device node id

* msm-pcm-low-latency

Required properties:

 - compatible : "qcom,msm-pcm-dsp"

 - qcom,msm-pcm-dsp-id : device node id

Optional properties:

 - qcom,msm-pcm-low-latency : Flag indicating whether
   the device node is of type low latency.

 - qcom,latency-level : Flag indicating whether the device node
                        is of type regular low latency or ultra
                        low latency.
                        regular : regular low latency stream
                        ultra : ultra low latency stream
                        ull-pp : ultra low latency stream with post-processing capability

* msm-pcm-dsp-noirq

Required properties:

 - compatible : "qcom,msm-pcm-dsp-noirq";

Optional properties:

 - qcom,msm-pcm-low-latency : Flag indicating whether
                              the device node is of type low latency.

 - qcom,latency-level : Flag indicating whether the device node
                        is of type low latency or ultra low latency
                        ultra : ultra low latency stream
                        ull-pp : ultra low latency stream with post-processing capability
* msm-pcm-routing

Required properties:

 - compatible : "qcom,msm-pcm-routing"

* msm-pcm-lpa

Required properties:

 - compatible : "qcom,msm-pcm-lpa"

* msm-compr-dsp

Required properties:

 - compatible : "qcom,msm-compr-dsp"

* msm-compress-dsp

Required properties:

 - compatible : "qcom,msm-compress-dsp"

Optional properties:
 - qcom,adsp-version:
        This property can be used to specify the ADSP version/name.
        Based on ADSP version, we decide if we have to use older
        ADSP APIs or newer. Right now we are adding "MDSP 1.2" for
        8909 purpose. If the ADSP version is anything other than this
        we use new ADSP APIs.

* msm-voip-dsp

Required properties:

 - compatible : "qcom,msm-voip-dsp"

* msm-pcm-voice

Required properties:

 - compatible : "qcom,msm-pcm-voice"
 - qcom,destroy-cvd : Flag indicating whether to destroy cvd at
                      the end of call for low memory targets

* msm-voice-host-pcm

Required properties:

 - compatible : "qcom,msm-voice-host-pcm"

* msm-voice-svc

Required properties:

 - compatible : "qcom,msm-voice-svc"

* msm-stub-codec

Required properties:

 - compatible : "qcom,msm-stub-codec"

* msm-hdmi-dba-codec-rx

Required properties:

 - compatible : "qcom,msm-hdmi-dba-codec-rx"
 - qcom,dba-bridge-chip: String info to indicate which bridge-chip
                         is used for HDMI using DBA.

* msm-dai-fe

Required properties:

 - compatible : "qcom,msm-dai-fe"

* msm-pcm-afe

Required properties:

 - compatible : "qcom,msm-pcm-afe"

* msm-pcm-dtmf

Required properties:

 - compatible : "qcom,msm-pcm-dtmf"
 - qcom,msm-pcm-dtmf : Enable DTMF driver in Audio. DTMF driver is
   used for generation and detection of DTMF tones, when user is in
   active voice call. APR commands are sent from DTMF driver to ADSP.

* msm-dai-stub

[First Level Nodes]

Required properties:

 - compatible : "msm-dai-stub"

[Second Level Nodes]

Required properties:

 - compatible : "qcom,msm-dai-stub-dev"
 - qcom,msm-dai-stub-dev-id : Stub dai port ID value is from 0 to 3.
   This enables stub CPU dai in Audio. The stub dai is used when
   there is no real backend in Audio.

* msm-dai-q6-spdif

Optional properties:

 - compatible : "msm-dai-q6-spdif"

* msm-dai-q6-hdmi

Required properties:
 - compatible : "msm-dai-q6-hdmi"
 - qcom,msm-dai-q6-dev-id : The hdmi multi channel port ID.
   It is passed onto the dsp from the apps to form an audio
   path to the HDMI device. Currently the only supported value
   is 8, which indicates the rx path used for audio playback
   on HDMI device.

* msm-lsm-client

Required properties:

 - compatible : "qcom,msm-lsm-client"

* msm-pcm-loopback

Required properties:

 - compatible : "qcom,msm-pcm-loopback"

Optional properties:

 - qcom,msm-pcm-loopback-low-latency : Flag indicating whether
   the device node is of type low latency.

* msm-transcode-loopback

Required properties:

 - compatible : "qcom,msm-transcode-loopback"

* msm-dai-q6

[First Level Nodes]

Required properties:

 - compatible : "msm-dai-q6"

Optional properties:

 - qcom,ext-spk-amp-supply : External speaker amplifier power supply.
 - qcom,ext-spk-amp-gpio : External speaker amplifier enable signal.

[Second Level Nodes]

Required properties:

 - compatible : "qcom,msm-dai-q6-dev"
 - qcom,msm-dai-q6-dev-id : The slimbus multi channel port ID
                            Value is from 16384 to 16397.
                            BT SCO port ID value from 12288 to 12289.
                            RT Proxy port ID values from 224 to 225 and 240 to
                            241.
                            FM Rx and TX port ID values from 12292 to 12293.
                            incall record Rx and TX port ID values from 32771 to 32772.
                            inCall Music Delivery port ID is 32773.
                            incall Music 2 Delivery port ID is 32770.

Optional properties:

 - qcom,msm-dai-q6-slim-dev-id : The Slimbus HW device (instance) ID associated
                                 with Slimbus ports.
                                 0 - Slimbus HW device ID 0 (first instance)
                                 1 - Slimbus HW device ID 1 (second instance)

* msm_dai_cdc_dma

[First Level Nodes]

Required properties:

 - compatible : "qcom,msm-dai-cdc-dma"

[Second Level Nodes]

Required properties:

 - compatible : "qcom,msm-dai-cdc-dma-dev"
 - qcom,msm-dai-cdc-dma-dev-id : WSA codec dma port ID
                            Value is from 45056 to 45061.
                            VA codec dma port ID Value is from 45089 to 45091.
                            RX and TX codec dma port ID values from 45120
                            to 45135.

Optional properties:

- qcom,msm-dai-is-island-supported:       Defines whether this dai supported in
                                          island mode or not.
                                          0 - Unsupported
                                          1 - Supported

- qcom,msm-dai-cdc-dma-dev-id:            Indicate how data is packed within
                                          codec DMA.
                                          0 - MSB
                                          1 - LSB
* msm-auxpcm

Required properties:

 - compatible :                           "qcom,msm-auxpcm-dev"

 - qcom,msm-cpudai-auxpcm-mode:           mode information. The first value is
                                          for 8khz mode, the second is for
                                          16khz
                                          0 - for PCM

 - qcom,msm-cpudai-auxpcm-sync:           sync information. The first value is
                                          for 8khz mode, the second is for
                                          16khz

 - qcom,msm-cpudai-auxpcm-frame:          No.of bytes per frame. The first
                                          value is for 8khz mode, the second
                                          is for 16khz
                                          5 - 256BPF
                                          4 - 128BPF

 - qcom,msm-cpudai-auxpcm-quant:          Type of quantization. The first
                                          value is for 8khz mode, the second
                                          is for 16khz
                                          2 - Linear quantization

 - qcom,msm-cpudai-auxpcm-num-slots:      Number of slots per mode in the
                                          msm-cpudai-auxpcm-slot-mapping
                                          array.
                                          The first value is for 8khz mode, the
                                          second is for 16khz. Max number of
                                          slots supported by DSP is 4, anything
                                          above 4 will be truncated to 4 when
                                          sent to DSP.

 - qcom,msm-cpudai-auxpcm-slot-mapping:   Array of slot numbers for multi
                                          slot scenario. The first array
                                          is for 8khz mode, the second is
                                          for 16khz. The size of the array
                                          is determined by the value in
                                          qcom,msm-cpudai-auxpcm-num-slots

 - qcom,msm-cpudai-auxpcm-data:           Data field - 0. The first value is
                                          for 8khz mode, the second is for
                                          16khz

 - qcom,msm-cpudai-auxpcm-pcm-clk-rate:   Clock rate for pcm - 2048000. The
                                          first value is for 8khz mode, the
                                          second is for 16KHz mode. When clock
                                          rate is set to zero, then external
                                          clock is assumed.

 - qcom,msm-auxpcm-interface:             name of AUXPCM interface "primary"
                                          indicates primary AUXPCM interface
                                          "secondary" indicates secondary
                                          AUXPCM interface
Optional properties:

- pinctrl-names:                          Pinctrl state names for each pin
                                          group configuration.
- pinctrl-x:                              Defines pinctrl state for each pin
                                          group
- qcom,msm-cpudai-afe-clk-ver:            Indicates version of AFE clock
                                          interface to be used for enabling
                                          PCM clock. If not defined, selects
                                          default AFE clock interface.
- qcom,msm-dai-is-island-supported:       Defines whether this dai supported in
                                          island mode or not.
                                          0 - Unsupported
                                          1 - Supported

* msm-pcm-hostless

Required properties:

 - compatible : "qcom,msm-pcm-hostless"

* msm-audio-apr

Required properties:

 - compatible : "qcom,msm-audio-apr"
		This device is added to represent APR module.

 - qcom,subsys-name: This value provides the subsystem name where codec
		is present. It can be "apr_modem" or "apr_adsp". This
		property enable apr driver to receive subsystem up/down
		notification from modem/adsp.

* Bolero codec

Required properties:

 - compatible : "qcom,bolero-codec"
		This device is added to represent bolero codec.

Optional properties:
 - qcom,bolero-version: Provides info relating to bolero version.

* LPASS digital codec

Required properties:

 - compatible : "qcom,lpass-cdc"
		This device is added to represent LPASS digital codec.

Optional properties:
 - qcom,lpass-cdc-version: Provides info relating to LPASS codec version.

* msm-ocmem-audio

Required properties:

 - compatible :                            "qcom,msm-ocmem-audio"

 - qcom,msm_bus,name:                      Client name

 - qcom,msm_bus,num_cases:                 Total number of use cases

 - qcom,msm_bus,active_only:               Context flag for requests in active
                                           or dual (active & sleep) contex

 - qcom,msm_bus,num_paths:                 Total number of master-slave pairs

 - qcom,msm_bus,vectors:                   Arrays of unsigned integers
                                           representing:
                                               master-id, slave-id, arbitrated
                                               bandwidth,
                                               instantaneous bandwidth
* wcd9xxx_intc

Required properties:

 - compatible :                            "qcom,wcd9xxx-irq"

 - interrupt-controller :                  Mark this device node as an
                                           interrupt controller

 - #interrupt-cells :                      Should be 1

 - interrupt-parent :                      Parent interrupt controller

 - qcom,gpio-connect                       Gpio that connects to parent
                                           interrupt controller

* audio-ext-clk-up

Required properties:

 - compatible :                            "qcom,audio-ref-clk"

 - qcom,codec-ext-clk-src:                  Clock source type like PMIC, LPASS
                                            requested to enable reference
                                            or external clock.

Optional properties:

 - qcom,codec-lpass-ext-clk-freq:           Property used to specify frequency.

 - qcom,codec-lpass-clk-id:                 Property used to specify LPASS clock
                                            ID value.

 - clock-names:                             Name of the PMIC clock that needs
                                            to be enabled for audio ref clock.
                                            This clock is set as parent.

 - clocks:                                  phandle reference to the parent
                                            clock.

 - qcom,mclk-clk-reg:                       Indicate the register address for mclk.

 - qcom,use-pinctrl:                        Indicates pinctrl required or not for this
                                            clock node.

* audio_slimslave

Required properties:

 - compatible :                            "qcom,audio-slimslave"

 - elemental-addr:                         slimbus slave enumeration address.

* msm-cpe-lsm

Required properties:

 - compatible : "qcom,msm-cpe-lsm"
 - qcom,msm-cpe-lsm-id : lsm afe port ID. CPE lsm driver uses
   this property to find out the input afe port ID. Currently
   only supported values are 1 and 3.

* wcd_us_euro_gpio

Required properties:

 - compatible : "qcom,msm-cdc-pinctrl"

Optional properties:
 - qcom,lpi-gpios : This boolean property is added if GPIOs are under
                    LPI TLMM.
 - qcom,chip-wakeup-reg : This lists registers related to control interrupt mask
			for respective LPI TLMM GPIOs.
 - qcom,chip-wakeup-maskbit : This gives info on maskbit for given list of registers.
 - qcom,chip-wakeup-default-val : This gives info on default value to be updated
			for given chip regs.

* msm-dai-slim

Required properties:

 - compatible :                            "qcom,msm-dai-slim"

 - elemental-addr:                         slimbus slave enumeration address.

* wcd_gpio_ctrl

Required properties:

 - compatible :                            "qcom,msm-cdc-pinctrl"

 - qcom,cdc-rst-n-gpio :                   TLMM GPIO number

 - pinctrl-names:                          Pinctrl state names for each pin
                                           group configuration.
 - pinctrl-x:                              Defines pinctrl state for each pin
                                           group.
* msm_cdc_pinctrl

Required properties:

 - compatible :                            "qcom,msm-cdc-pinctrl"

 - pinctrl-names:                          Pinctrl state names for each pin
                                           group configuration.
 - pinctrl-x:                              Defines pinctrl state for each pin
                                           group.

* wcd_dsp_glink

Required properties:

 - compatible :                            "qcom,wcd-dsp-glink"
 - qcom,wdsp-channels:                      List of wdsp supported channel names.

* msm_ext_disp_audio_codec_rx

Required properties:

 - compatible :                            "qcom,msm-ext-disp-audio-codec-rx"

Example:

	qcom,msm-pcm {
		compatible = "qcom,msm-pcm-dsp";
		qcom,msm-pcm-dsp-id = <0>;
	};

	qcom,msm-pcm-low-latency {
		compatible = "qcom,msm-pcm-dsp";
		qcom,msm-pcm-dsp-id = <1>;
		qcom,msm-pcm-low-latency;
	};

	qcom,msm-pcm-loopback-low-latency {
		compatible = "qcom,msm-pcm-loopback";
		qcom,msm-pcm-loopback-low-latency;
	};

	qcom,msm-pcm-routing {
		compatible = "qcom,msm-pcm-routing";
	};

	qcom,msm-pcm-lpa {
		compatible = "qcom,msm-pcm-lpa";
	};

	qcom,msm-compr-dsp {
		compatible = "qcom,msm-compr-dsp";
	};

	qcom,msm-compress-dsp {
		compatible = "qcom,msm-compress-dsp";
	};

	qcom,msm-voip-dsp {
		compatible = "qcom,msm-voip-dsp";
	};

	qcom,msm-pcm-voice {
		compatible = "qcom,msm-pcm-voice";
		qcom,destroy-cvd;
	};

	qcom,msm-voice-host-pcm {
		compatible = "qcom,msm-voice-host-pcm";
	};

	qcom,msm-stub-codec {
		compatible = "qcom,msm-stub-codec";
	};

	qcom,msm-dai-fe {
		compatible = "qcom,msm-dai-fe";
	};

	qcom,msm-pcm-dtmf {
		compatible = "qcom,msm-pcm-dtmf";
	};

	qcom,msm-dai-stub {
		compatible = "qcom,msm-dai-stub";
	};

	qcom,msm-dai-q6-spdif {
		compatible = "qcom,msm-dai-q6-spdif";
	};

	qcom,msm-dai-q6-hdmi {
		compatible = "qcom,msm-dai-q6-hdmi";
		qcom,msm-dai-q6-dev-id = <8>;
	};

	dai_dp: qcom,msm-dai-q6-dp {
		compatible = "qcom,msm-dai-q6-hdmi";
		qcom,msm-dai-q6-dev-id = <24608>;
	};

	qcom,msm-dai-q6 {
		compatible = "qcom,msm-dai-q6";
		qcom,msm-dai-q6-sb-0-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16384>;
			qcom,msm-dai-q6-slim-dev-id = <0>;
		};

		qcom,msm-dai-q6-sb-0-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16385>;
		};

		qcom,msm-dai-q6-sb-1-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16386>;
		};

		qcom,msm-dai-q6-sb-1-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16387>;
		};

		qcom,msm-dai-q6-sb-3-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16390>;
		};

		qcom,msm-dai-q6-sb-3-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16391>;
		};

		qcom,msm-dai-q6-sb-4-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16392>;
		};

		qcom,msm-dai-q6-sb-4-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16393>;
		};

		qcom,msm-dai-q6-sb-5-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16395>;
		};

		qcom,msm-dai-q6-sb-6-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16396>;
		};

		qcom,msm-dai-q6-sb-6-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <16397>;
		};

		qcom,msm-dai-q6-bt-sco-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <12288>;
		};

		qcom,msm-dai-q6-bt-sco-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <12289>;
		};

		qcom,msm-dai-q6-int-fm-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <12292>;
		};

		qcom,msm-dai-q6-int-fm-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <12293>;
		};

		qcom,msm-dai-q6-be-afe-pcm-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <224>;
		};

		qcom,msm-dai-q6-be-afe-pcm-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <225>;
		};

		qcom,msm-dai-q6-afe-proxy-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <241>;
		};

		qcom,msm-dai-q6-afe-proxy-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <240>;
		};

		qcom,msm-dai-q6-incall-record-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <32771>;
		};

		qcom,msm-dai-q6-incall-record-tx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <32772>;
		};

		qcom,msm-dai-q6-incall-music-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <32773>;
		};

		qcom,msm-dai-q6-incall-music-2-rx {
			compatible = "qcom,msm-dai-q6-dev";
			qcom,msm-dai-q6-dev-id = <32770>;
		};
	};

	qcom,msm-pri-auxpcm {
		qcom,msm-cpudai-auxpcm-mode = <1>, <1>;
		qcom,msm-cpudai-auxpcm-sync = <1>, <1>;
		qcom,msm-cpudai-auxpcm-frame = <5>, <4>;
		qcom,msm-cpudai-auxpcm-quant = <2>, <2>;
		qcom,msm-cpudai-auxpcm-num-slots = <4>, <4>;
		qcom,msm-cpudai-auxpcm-slot-mapping = <1 0 0 0>, <1 3 0 0>;
		qcom,msm-cpudai-auxpcm-data = <0>, <0>;
		qcom,msm-cpudai-auxpcm-pcm-clk-rate = <2048000>, <2048000>;
		qcom,msm-auxpcm-interface = "primary";
		compatible = "qcom,msm-auxpcm-dev";
		pinctrl-names = "default", "idle";
		pinctrl-0 = <&pri_aux_pcm_active &pri_aux_pcm_din_active>;
		pinctrl-1 = <&pri_aux_pcm_sleep &pri_aux_pcm_din_sleep>;
	};

	qcom,msm-pcm-hostless {
		compatible = "qcom,msm-pcm-hostless";
	};

	audio_apr: qcom,msm-audio-apr {
		compatible = "qcom,msm-audio-apr";
		qcom,subsys-name = "apr_adsp";
                q6core {
                        compatible = "qcom,q6core-audio";
                        bolero: bolero-cdc {
                                compatible = "qcom,bolero-codec";
                        };
                };
	};

	qcom,msm-ocmem-audio {
		compatible = "qcom,msm-ocmem-audio";
		qcom,msm_bus,name = "audio-ocmem";
		qcom,msm_bus,num_cases = <2>;
		qcom,msm_bus,active_only = <0>;
		qcom,msm_bus,num_paths = <1>;
		qcom,msm_bus,vectors =
			<11 604 0 0>,
			<11 604 32505856 325058560>;
	};

	wcd9xxx_intc: wcd9xxx-irq {
		compatible = "qcom,wcd9xxx-irq";
		interrupt-controller;
		#interrupt-cells = <1>;
		interrupt-parent = <&msmgpio>;
		interrupts = <72 0>;
		interrupt-names = "cdc-int";
	};

	clock_audio: audio_ext_clk {
		compatible = "qcom,audio-ref-clk";
		qcom,codec-ext-clk-src = <2>;
		qcom,codec-lpass-ext-clk-freq = <19200000>;
		qcom,codec-lpass-clk-id = <1>;
		clock-names = "osr_clk";
		clocks = <&clock_rpm clk_div_clk1>;
		#clock-cells = <1>;
		pinctrl-names = "sleep", "active";
		pinctrl-0 = <&spkr_i2s_clk_sleep>;
		pinctrl-1 = <&spkr_i2s_clk_active>;
	};

	audio_slimslave {
		compatible = "qcom,audio-slimslave";
		elemental-addr = [ff ff ff ff 17 02];
	};

	msm_dai_slim {
		compatible = "qcom,msm_dai_slim";
		elemental-addr = [ff ff ff fe 17 02];
	};

	wcd_gpio_ctrl {
		compatible = "qcom,msm-cdc-pinctrl";
		qcom,cdc-rst-n-gpio = <&tlmm 64 0>;
		pinctrl-names = "aud_active", "aud_sleep";
		pinctrl-0 = <&cdc_reset_active>;
		pinctrl-1 = <&cdc_reset_sleep>;
	};

	msm_cdc_pinctrl {
		compatible = "qcom,msm-cdc-pinctrl";
		pinctrl-names = "aud_active", "aud_sleep";
		pinctrl-0 = <&cdc_reset_active>;
		pinctrl-1 = <&cdc_reset_sleep>;
	};

	wcd_dsp_glink {
		compatible = "qcom,wcd-dsp-glink";
	};

	msm_ext_disp_audio_codec_rx {
		compatible = "qcom,msm-ext-disp-audio-codec-rx";
	};

* msm-dai-mi2s

[First Level Nodes]

Required properties:

 - compatible : "msm-dai-mi2s"

 [Second Level Nodes]

Required properties:

 - compatible : "qcom,msm-dai-q6-mi2s"
 - qcom,msm-dai-q6-mi2s-dev-id: MSM or MDM can use Slimbus or I2S interface to
				transfer data to (WCD9XXX) codec.
				If slimbus interface is used then "msm-dai-q6"
				needs to be filled with correct data for
				slimbus interface.
				The sections "msm-dai-mi2s" is used by MDM or
				MSM to use I2S interface with codec.
				This section is used by CPU driver in ASOC MSM
				to configure MI2S interface. MSM internally
				has multiple MI2S namely Primary, Secondary,
				Tertiary and Quaternary MI2S.
				They are represented with id 0, 1, 2, 3
				respectively.
				The field "qcom,msm-dai-q6-mi2s-dev-id"
				represents which of the MI2S block is used.
				These MI2S are connected to I2S interface.

 - qcom,msm-mi2s-rx-lines:	Each MI2S interface in MSM has one or more SD
				lines. These lines are used for data transfer
				between codec and MSM.
				This element in indicates which output RX lines
				are used in the MI2S interface.

 - qcom,msm-mi2s-tx-lines:  	Each MI2S interface in MSM has one or more SD
				lines. These lines are used for data transfer
				between codec and MSM.
				This element in indicates which input TX lines
				are used in the MI2S interface.

Optional properties:

- pinctrl-names:		          Pinctrl state names for each pin group
				          configuration.
- pinctrl-x: 			          Defines pinctrl state for each pin group
- qcom,msm-dai-is-island-supported:       Defines whether this dai supported in
                                          island mode or not.
                                          0 - Unsupported
                                          1 - Supported

Example:

qcom,msm-dai-mi2s {
		compatible = "qcom,msm-dai-mi2s";
		qcom,msm-dai-q6-mi2s-prim {
			compatible = "qcom,msm-dai-q6-mi2s";
			qcom,msm-dai-q6-mi2s-dev-id = <0>;
			qcom,msm-mi2s-rx-lines = <2>;
			qcom,msm-mi2s-tx-lines = <1>;
			pinctrl-names = "default", "idle";
			pinctrl-0 = <&tert_mi2s_active &tert_mi2s_sd0_active>;
			pinctrl-1 = <&tert_mi2s_sleep &tert_mi2s_sd0_sleep>;
		};
};

* msm-dai-spdif

[First Level Nodes]

Required properties:

 - compatible : "msm-dai-spdif"

 [Second Level Nodes]

Required properties:

 - compatible : "qcom,msm-dai-q6-spdif"
 - qcom,msm-dai-q6-dev-id: The SPDIF port ID
                            Value is from 20480 to 20483.

Example:

qcom,msm-dai-spdif {
	compatible = "qcom,msm-dai-spdif";
	qcom,msm-dai-q6-spdif-pri-rx {
		compatible = "qcom,msm-dai-q6-spdif";
		qcom,msm-dai-q6-dev-id = <20480>;
	};
};

* msm-adsp-loader

Required properties:
 - compatible : "qcom,adsp-loader"
 - qcom,rproc-handle:
	remoteproc handler is used to load ADSP image at boot.
 - qcom,adsp-state:
	It is possible that some MSM use PIL to load the ADSP image. While
	other MSM may use SBL to load the ADSP image at boot. Audio APR needs
	state of ADSP to register and enable APR to be used for sending commands
	to ADSP. so adsp-state represents the state of ADSP to ADSP loader.
	Value of 0 indicates ADSP loader needs to use PIL and value of 2 means
	ADSP image is already loaded by SBL.

Example:

qcom,msm-adsp-loader {
	status = "ok";
	compatible = "qcom,adsp-loader";
	qcom,rproc-handle = <&adsp_pas>;
	qcom,adsp-state = <0>;
};

* msm-adsp_notify

Required properties:
 - compatible : "qcom,adsp_notify"
 - qcom,rproc-handle:
	remoteproc handler is used to get subsystem domain name.

Example:

adsp_notify: qcom,msm-adsp-notify {
	status = "ok";
	compatible = "qcom,adsp-notify";
	qcom,rproc-handle = <&adsp_pas>;
};

* msm-audio-ion

Required properties:
 - compatible : "qcom,msm-audio-ion"

Optional properties:
 - qcom,smmu-version:
	version ID to provide info regarding smmu version
	used in chipset. If ARM SMMU HW - use id value as 1,
	If QSMMU HW - use id value as 2.

 - qcom,smmu-sid-mask:
	Mask for the Stream ID part of SMMU SID.

 - qcom,smmu-enabled:
        It is possible that some MSM have SMMU in ADSP.  While other MSM use
	no SMMU. Audio lib introduce wrapper for ION APIs. The wrapper needs
        presence of SMMU in ADSP to handle ION APIs differently.
        Presence of this property means ADSP has SMMU in it.
 - iommus:
	A phandle parsed by smmu driver. Number of entries will vary across
	targets.

Example:

	qcom,msm-audio-ion {
		compatible = "qcom,msm-audio-ion;
		qcom,smmu-enabled;
	};

* msm-audio-ion-cma

Required properties:
 - compatible : "qcom,msm-audio-ion-cma"

Example:
	qcom,msm-audio-ion-cma {
		compatible = "qcom,msm-audio-ion-cma";
	};

* msm-dai-tdm

[First Level Nodes]

Required properties:

 - compatible : "qcom,msm-dai-tdm"
 - qcom,msm-cpudai-tdm-group-id: ID of the group device. TDM interface
				supports up to 8 groups:
				Primary RX: 	37120
				Primary TX: 	37121
				Secondary RX: 	37136
				Secondary TX: 	37137
				Tertiary RX: 	37152
				Tertiary TX: 	37153
				Quaternary RX: 	37168
				Quaternary TX: 	37169

 - qcom,msm-cpudai-tdm-group-num-ports:	Number of ports in
				msm-cpudai-tdm-group-port-id array.
				Max number of ports supported by DSP is 8.

 - qcom,msm-cpudai-tdm-group-port-id: Array of TDM port IDs of the group.
				The size of the array is determined by
				the value in msm-cpudai-tdm-group-num-ports.
				Each group supports up to 8 ports:
				Primary RX: 	36864, 36866, 36868, 36870,
								36872, 36874, 36876, 36878
				Primary TX: 	36865, 36867, 36869, 36871,
								36873, 36875, 36877, 36879
				Secondary RX: 	36880, 36882, 36884, 36886,
								36888, 36890, 36892, 36894
				Secondary TX:	36881, 36883, 36885, 36887,
								36889, 36891, 36893, 36895
				Tertiary RX: 	36896, 36898, 36900, 36902,
								36904, 36906, 36908, 36910
				Tertiary TX: 	36897, 36899, 36901, 36903,
								36905, 36907, 36909, 36911
				Quaternary RX:	36912, 36914, 36916, 36918,
								36920, 36922, 36924, 36926
				Quaternary TX:	36913, 36915, 36917, 36919,
								36921, 36923, 36925, 36927

 - qcom,msm-cpudai-tdm-clk-rate: Clock rate for tdm - 12288000.
				When clock rate is set to zero,
				then external clock is assumed.

 - qcom,msm-cpudai-tdm-clk-internal: Clock Source.
				0 - EBIT clock from clk tree
				1 - IBIT clock from clk tree

 - qcom,msm-cpudai-tdm-sync-mode: Synchronization setting.
				0 - Short sync bit mode
				1 - Long sync mode
				2 - Short sync slot mode

 - qcom,msm-cpudai-tdm-sync-src: Synchronization source.
				0 - External source
				1 - Internal source

 - qcom,msm-cpudai-tdm-data-out: Data out signal to drive with other masters.
				0 - Disable
				1 - Enable

 - qcom,msm-cpudai-tdm-invert-sync: Invert the sync.
				0 - Normal
				1 - Invert

 - qcom,msm-cpudai-tdm-data-delay: Number of bit clock to delay data
				with respect to sync edge.
				0 - 0 bit clock cycle
				1 - 1 bit clock cycle
				2 - 2 bit clock cycle

 [Second Level Nodes]

Required properties:

 - compatible : "qcom,msm-dai-q6-tdm"
 - qcom,msm-dai-q6-mi2s-dev-id: TDM port ID.

 - qcom,msm-cpudai-tdm-data-align: Indicate how data is packed
				within the slot. For example, 32 slot width in case of
				sample bit width is 24.
				0 - MSB
				1 - LSB

Optional properties:

 - qcom,msm-cpudai-tdm-header-start-offset: TDM Custom header start offset
				in bytes from this sub-frame. The bytes is counted from 0.
				0 is mapped to the 1st byte in or out of
				the digital serial data line this sub-frame belong to.
				Supported value: 0, 4, 8.

 - qcom,msm-cpudai-tdm-header-width: Header width per frame followed.
				2 bytes for MOST/TDM case.
				Supported value: 2.

 - qcom,msm-cpudai-tdm-header-num-frame-repeat: Number of header followed.
				Supported value: 8.

 - pinctrl-names: Pinctrl state names for each pin group
				configuration.

 - pinctrl-x: Defines pinctrl state for each pin group.

 - qcom,msm-dai-is-island-supported:      Defines whether this dai supported in
                                          island mode or not.
                                          0 - Unsupported
                                          1 - Supported

Example:

	qcom,msm-dai-tdm-quat-rx {
		compatible = "qcom,msm-dai-tdm";
		qcom,msm-cpudai-tdm-group-id = <37168>;
		qcom,msm-cpudai-tdm-group-num-ports = <1>;
		qcom,msm-cpudai-tdm-group-port-id = <36912>;
		qcom,msm-cpudai-tdm-clk-rate = <12288000>;
		qcom,msm-cpudai-tdm-clk-internal = <1>;
		qcom,msm-cpudai-tdm-sync-mode = <0>;
		qcom,msm-cpudai-tdm-sync-src = <1>;
		qcom,msm-cpudai-tdm-data-out = <0>;
		qcom,msm-cpudai-tdm-invert-sync = <0>;
		qcom,msm-cpudai-tdm-data-delay = <0>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&quat_tdm_active &quat_tdm_dout_active>;
		pinctrl-1 = <&quat_tdm_sleep &quat_tdm_dout_sleep>;
		dai_quat_tdm_rx_0: qcom,msm-dai-q6-tdm-quat-rx-0 {
			compatible = "qcom,msm-dai-q6-tdm";
			qcom,msm-cpudai-tdm-dev-id = <36912>;
			qcom,msm-cpudai-tdm-data-align = <0>;
			qcom,msm-cpudai-tdm-header-start-offset = <0>;
			qcom,msm-cpudai-tdm-header-width = <2>;
			qcom,msm-cpudai-tdm-header-num-frame-repeat = <8>;
		};
	};

* MSMSTUB ASoC Machine driver

Required properties:
- compatible : "qcom,sm8150-asoc-snd-stub" for SM8150 target.
- compatible : "qcom,kona-asoc-snd-stub" for Kona target.
- qcom,model : The user-visible name of this sound card.
- qcom,tasha-mclk-clk-freq : MCLK frequency value for tasha codec
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
Optional properties:
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target

Example:

	sound_stub {
		compatible = "qcom,sm8150-asoc-snd-stub";
		qcom,model = "sm8150-stub-snd-card";

		qcom,tasha-mclk-clk-freq = <9600000>;
		asoc-platform = <&pcm0>;
		asoc-platform-names = "msm-pcm-dsp.0";
		asoc-cpu = <&sb_0_rx>, <&sb_0_tx>;
		asoc-cpu-names = "msm-dai-q6-dev.16384", "msm-dai-q6-dev.16385";
		asoc-codec = <&stub_codec>;
		asoc-codec-names = "msm-stub-codec.1";
		qcom,wsa-max-devs = <0>;
	};

* WCD DSP manager driver

Required properties:
- compatible : "qcom,wcd-dsp-mgr"
- qcom,wdsp-components : This is phandle list containing the references to the
			 components of the manager driver. Manager driver will
			 register to component framework with these phandles.
- qcom,img-filename : String property to provide the dsp image file name that is
		     to be read from file system and downloaded to dsp memory
Optional properties:
- qcom,wdsp-cmpnt-dev-name : Property that manager driver will parse, but defined
			     in the child's DT entry that is given to manager driver
			     with phandle. This property will be used by the manager
			     driver in case the manager driver cannot match child's
			     of_node pointer to registered phandle.

Example:

	qcom,wcd-dsp-mgr {
		compatible = "qcom,wcd-dsp-mgr";
		qcom,wdsp-components = <&wcd934x_cdc 0>,
				       <&wcd_spi_0 1>,
				       <&glink_spi 2>;
		qcom,img-filename = "cpe_9340";
	};

Example of child node that would have qcom,wdsp-cmpnt-dev-name property

	wcd934x_cdc: tavil_codec {
		qcom,wdsp-cmpnt-dev-name = "tavil_codec";
	};

* msm-mdf

Required properties:
 - compatible : "qcom,msm-mdf"

Optional subnodes:
 - qcom,msm_mdf_cb : Child nodes representing the compute context banks.

Subnode Required properties:
 - compatible : "qcom,msm-mdf-cb"
 - label: Label describing the subsystem this context bank belongs to.

Subnode Optional properties:
 - qcom,smmu-enabled:
		It is possible that some MSM subsystems have SMMU, while other MSM
		subsystems do not. MDF platform driver needs to handle SMMU APIs
		differently according to the availability of SMMU.
		Presence of this property means the subsystem has SMMU in it.
 - iommus : A list of phandle and IOMMU specifier pairs that describe the
		IOMMU master interfaces of the device.

Example:
	qcom,msm-mdf {
		compatible = "qcom,msm-mdf";

		qcom,msm_mdf_cb1 {
			compatible = "qcom,msm-mdf-cb";
			label = "adsp";
			qcom,smmu-enabled;
		};
		qcom,msm_mdf_cb2 {
			compatible = "qcom,msm-mdf-cb";
			label = "dsps";
		};
		qcom,msm_mdf_cb3 {
			compatible = "qcom,msm-mdf-cb";
			label = "modem";
		};
	};

* msm-mdf-mem

Required properties:
 - compatible : "qcom,msm-mdf-mem-region"
 - qcom,msm-mdf-mem-data-size: indicates the size of memory
				for MDF purpose
 - memory-region : CMA region which is owned by this device.

Example:
	qcom,msm-mdf-mem {
		compatible = "qcom,msm-mdf-mem-region";
		memory-region = <&mdf_mem>;
	};

* SM8150 ASoC Machine driver

Required properties:
- compatible : "qcom,sm8150-asoc-snd-pahu-aqt" for pahu codec and
               "qcom,sm8150-asoc-snd-tavil" for tavil codec.
- qcom,model : The user-visible name of this sound card.
- qcom,pahu-ext-clk-freq : External CLK frequency value for pahu codec
- qcom,audio-routing : A list of the connections between audio components.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
Optional properties:
- clock-names : clock name defined for external clock.
- clocks : external clock defined for codec clock.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target

Example:

	sound-pahu {
		compatible = "qcom,sm8150-asoc-snd-pahu-aqt";
		qcom,model = "sm8150-pahu-aqt-snd-card";
		qcom,ext-disp-audio-rx;
		qcom,wcn-btfm;
		qcom,mi2s-audio-intf;
		qcom,auxpcm-audio-intf;
		qcom,msm-mi2s-master = <1>, <1>, <1>, <1>;

		reg = <0x1711a000 0x4>,
		      <0x1711b000 0x4>,
		      <0x1711c000 0x4>,
		      <0x1711d000 0x4>;
		reg-names = "lpaif_pri_mode_muxsel",
			    "lpaif_sec_mode_muxsel",
			    "lpaif_tert_mode_muxsel",
			    "lpaif_quat_mode_muxsel";

		qcom,audio-routing =
			"MADINPUT", "MCLK",
			"AMIC2", "MIC BIAS2",
			"AMIC3", "MIC BIAS2",
			"AMIC4", "MIC BIAS2",
			"AMIC5", "MIC BIAS3",
			"MIC BIAS3", "Handset Mic",
			"DMIC0", "MIC BIAS1",
			"MIC BIAS1", "Digital Mic0",
			"DMIC1", "MIC BIAS1",
			"MIC BIAS1", "Digital Mic1",
			"DMIC2", "MIC BIAS3",
			"MIC BIAS3", "Digital Mic2",
			"DMIC3", "MIC BIAS3",
			"MIC BIAS3", "Digital Mic3",
			"DMIC4", "MIC BIAS4",
			"MIC BIAS4", "Digital Mic4",
			"DMIC5", "MIC BIAS4",
			"MIC BIAS4", "Digital Mic5",
			"SpkrLeft IN", "SPK1 OUT",
			"SpkrRight IN", "SPK2 OUT";

		qcom,pahu-ext-clk-freq = <19200000>;
		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&cpe>, <&compr>,
				<&pcm_noirq>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-cpe-lsm",
				"msm-compr-dsp", "msm-pcm-dsp-noirq";
		asoc-cpu = <&dai_hdmi>, <&dai_dp>,
				<&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_pri_auxpcm>, <&dai_sec_auxpcm>,
				<&dai_tert_auxpcm>, <&dai_quat_auxpcm>,
				<&sb_0_rx>, <&sb_0_tx>, <&sb_1_rx>, <&sb_1_tx>,
				<&sb_2_rx>, <&sb_2_tx>, <&sb_3_rx>, <&sb_3_tx>,
				<&sb_4_rx>, <&sb_4_tx>, <&sb_5_tx>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>, <&sb_5_rx>, <&sb_6_rx>,
				<&sb_7_rx>, <&sb_7_tx>, <&sb_8_tx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_tx_0>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_tx_0>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_tx_0>,
				<&dai_quat_tdm_rx_0>, <&dai_quat_tdm_tx_0>;
		asoc-cpu-names = "msm-dai-q6-hdmi.8",  "msm-dai-q6-dp.24608",
				"msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-auxpcm.1", "msm-dai-q6-auxpcm.2",
				"msm-dai-q6-auxpcm.3", "msm-dai-q6-auxpcm.4",
				"msm-dai-q6-dev.16384", "msm-dai-q6-dev.16385",
				"msm-dai-q6-dev.16386", "msm-dai-q6-dev.16387",
				"msm-dai-q6-dev.16388", "msm-dai-q6-dev.16389",
				"msm-dai-q6-dev.16390", "msm-dai-q6-dev.16391",
				"msm-dai-q6-dev.16392", "msm-dai-q6-dev.16393",
				"msm-dai-q6-dev.16395", "msm-dai-q6-dev.224",
				"msm-dai-q6-dev.225", "msm-dai-q6-dev.241",
				"msm-dai-q6-dev.240", "msm-dai-q6-dev.32771",
				"msm-dai-q6-dev.32772", "msm-dai-q6-dev.32773",
				"msm-dai-q6-dev.32770", "msm-dai-q6-dev.16394",
				"msm-dai-q6-dev.16396", "msm-dai-q6-dev.16398",
				"msm-dai-q6-dev.16399", "msm-dai-q6-dev.16401",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36865",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36881",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36912", "msm-dai-q6-tdm.36913";
		asoc-codec = <&stub_codec>, <&ext_disp_audio_codec>;
		asoc-codec-names = "msm-stub-codec.1",
				   "msm-ext-disp-audio-codec-rx";
		qcom,wsa-max-devs = <2>;
		qcom,wsa-devs = <&wsa881x_0211>, <&wsa881x_0212>,
				<&wsa881x_0213>, <&wsa881x_0214>;
		qcom,wsa-aux-dev-prefix = "SpkrLeft", "SpkrRight",
					  "SpkrLeft", "SpkrRight";
	};


* QCS405 ASoC Machine driver

Required properties:
- compatible : "qcom,qcs405-asoc-snd".
- qcom,model : The user-visible name of this sound card.
- qcom,audio-routing : A list of the connections between audio components.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
Optional properties:
- clock-names : clock name defined for external clock.
- clocks : external clock defined for codec clock.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target
- qcom,wsa_bolero_codec : Property to specify if WSA macro in Bolero codec is used for this target
- qcom,va_bolero_codec : Property to specify if VA macro in Bolero codec is used for this target
- qcom,tasha_codec : Property to specify if Tasha codec is used for this target
- qcom,cdc-dmic-gpios : phandle for Digital mic clk and data gpios.
- qcom,csra-codec : Property to specify if CSRA66x0 is used for this target
- qcom,csra-max-devs : Maximum number of CSRA66x0 devices present in the target
- qcom,csra-devs : List of phandles of all possible CSRA66x0 devices supported for the target
- qcom,csra-aux-dev-prefix : Name prefix in multi-channel configuration for CSRA66x0 device
Example:

	qcs405_snd {
		compatible = "qcom,qcs405-asoc-snd";
		qcom,wsa_bolero_codec =  <1>;
		qcom,va_bolero_codec = <1>;
		qcom,tasha_codec = <1>;
		qcom,ext-disp-audio-rx = <1>;
		qcom,wcn-btfm = <1>;
		qcom,mi2s-audio-intf = <1>;
		qcom,auxpcm-audio-intf = <1>;
		qcom,msm-mi2s-master = <1>, <1>, <1>, <1>;

		qcom,audio-routing =
			"MADINPUT", "MCLK",
			"AMIC2", "MIC BIAS2",
			"AMIC3", "MIC BIAS2",
			"AMIC4", "MIC BIAS2",
			"AMIC5", "MIC BIAS3",
			"MIC BIAS3", "Handset Mic",
			"DMIC0", "MIC BIAS1",
			"MIC BIAS1", "Digital Mic0",
			"DMIC1", "MIC BIAS1",
			"MIC BIAS1", "Digital Mic1",
			"DMIC2", "MIC BIAS3",
			"MIC BIAS3", "Digital Mic2",
			"DMIC3", "MIC BIAS3",
			"MIC BIAS3", "Digital Mic3",
			"DMIC4", "MIC BIAS4",
			"MIC BIAS4", "Digital Mic4",
			"DMIC5", "MIC BIAS4",
			"MIC BIAS4", "Digital Mic5",
			"SpkrLeft IN", "SPK1 OUT",
			"SpkrRight IN", "SPK2 OUT";

		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&cpe>, <&compr>,
				<&pcm_noirq>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-cpe-lsm",
				"msm-compr-dsp", "msm-pcm-dsp-noirq";
		asoc-cpu = <&dai_hdmi>, <&dai_dp>,
				<&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_pri_auxpcm>, <&dai_sec_auxpcm>,
				<&dai_tert_auxpcm>, <&dai_quat_auxpcm>,
				<&sb_0_rx>, <&sb_0_tx>, <&sb_1_rx>, <&sb_1_tx>,
				<&sb_2_rx>, <&sb_2_tx>, <&sb_3_rx>, <&sb_3_tx>,
				<&sb_4_rx>, <&sb_4_tx>, <&sb_5_tx>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>, <&sb_5_rx>, <&sb_6_rx>,
				<&sb_7_rx>, <&sb_7_tx>, <&sb_8_tx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_tx_0>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_tx_0>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_tx_0>,
				<&dai_quat_tdm_rx_0>, <&dai_quat_tdm_tx_0>,
				<&wsa_cdc_dma_0_rx>, <&wsa_cdc_dma_0_tx>,
				<&wsa_cdc_dma_1_rx>, <&wsa_cdc_dma_1_tx>,
				<&wsa_cdc_dma_2_tx>, <&va_cdc_dma_0_tx>,
				<&va_cdc_dma_1_tx>;
		asoc-cpu-names = "msm-dai-q6-hdmi.8",  "msm-dai-q6-dp.24608",
				"msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-auxpcm.1", "msm-dai-q6-auxpcm.2",
				"msm-dai-q6-auxpcm.3", "msm-dai-q6-auxpcm.4",
				"msm-dai-q6-dev.16384", "msm-dai-q6-dev.16385",
				"msm-dai-q6-dev.16386", "msm-dai-q6-dev.16387",
				"msm-dai-q6-dev.16388", "msm-dai-q6-dev.16389",
				"msm-dai-q6-dev.16390", "msm-dai-q6-dev.16391",
				"msm-dai-q6-dev.16392", "msm-dai-q6-dev.16393",
				"msm-dai-q6-dev.16395", "msm-dai-q6-dev.224",
				"msm-dai-q6-dev.225", "msm-dai-q6-dev.241",
				"msm-dai-q6-dev.240", "msm-dai-q6-dev.32771",
				"msm-dai-q6-dev.32772", "msm-dai-q6-dev.32773",
				"msm-dai-q6-dev.32770", "msm-dai-q6-dev.16394",
				"msm-dai-q6-dev.16396", "msm-dai-q6-dev.16398",
				"msm-dai-q6-dev.16399", "msm-dai-q6-dev.16401",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36865",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36881",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36912", "msm-dai-q6-tdm.36913",
				"msm-dai-q6-cdc-dma-dev.45056",
				"msm-dai-q6-cdc-dma-dev.45057",
				"msm-dai-q6-cdc-dma-dev.45058",
				"msm-dai-q6-cdc-dma-dev.45059",
				"msm-dai-q6-cdc-dma-dev.45061",
				"msm-dai-q6-cdc-dma-dev.45089",
				"msm-dai-q6-cdc-dma-dev.45091";
		asoc-codec = <&stub_codec>, <&ext_disp_audio_codec>,
				<&bolero>;;
		asoc-codec-names = "msm-stub-codec.1",
				   "msm-ext-disp-audio-codec-rx",
				   "bolero_codec";
		qcom,wsa-max-devs = <2>;
		qcom,wsa-devs = <&wsa881x_0211>, <&wsa881x_0212>,
				<&wsa881x_0213>, <&wsa881x_0214>;
		qcom,wsa-aux-dev-prefix = "SpkrLeft", "SpkrRight",
					  "SpkrLeft", "SpkrRight";
		qcom,cdc-dmic-gpios = <&cdc_dmic12_gpios>, <&cdc_dmic34_gpios>,
					<&cdc_dmic56_gpios>, <&cdc_dmic78_gpios>;
	};

* SM6150 ASoC Machine driver

Required properties:
- compatible : "qcom,sm6150-asoc-snd".
- qcom,model : The user-visible name of this sound card.
- qcom,audio-routing : A list of the connections between audio components.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
- qcom,codec-aux-devs: This is phandle list containing the references to Auxilary
		       codec devices.

Optional properties:
- qcom,msm-mi2s-master: This property is used to inform machine driver
  if MSM is the clock master of mi2s. 1 means master and 0 means slave. The
  first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,msm-mbhc-hphl-swh: This property is used to distinguish headset HPHL
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,msm-mbhc-gnd-swh: This property is used to distinguish headset GND
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,ext-disp-audio-rx: Property to specify if Audio over Display port is supported for the target
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target
- qcom,mi2s-audio-intf: Property to specify if MI2S interface is used for the target
- qcom,auxpcm-audio-intf: Property to specify if Aux PCM interface is used for the target
- qcom,tavil_codec : Property to specify if Tavil codec is used for this target
- qcom,cdc-dmic-gpios : phandle for Digital mic clk and data gpios.
- qcom,msm_audio_ssr_devs: List the snd event framework clients

Example:
	sm6150_snd: sound {
		status = "okay";
		compatible = "qcom,sm6150-asoc-snd";
		qcom,ext-disp-audio-rx = <1>;
		qcom,wcn-btfm = <1>;
		qcom,mi2s-audio-intf = <1>;
		qcom,auxpcm-audio-intf = <1>;

		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&compr>,
				<&pcm_noirq>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-compr-dsp",
				"msm-pcm-dsp-noirq";
		asoc-cpu = <&dai_dp>,
				<&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_mi2s4>, <&dai_pri_auxpcm>,
				<&dai_sec_auxpcm>, <&dai_tert_auxpcm>,
				<&dai_quat_auxpcm>, <&dai_quin_auxpcm>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>,
				<&sb_7_rx>, <&sb_7_tx>, <&sb_8_tx>, <&sb_8_rx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_tx_0>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_tx_0>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_tx_0>,
				<&dai_quat_tdm_rx_0>, <&dai_quat_tdm_tx_0>,
				<&dai_quin_tdm_rx_0>, <&dai_quin_tdm_tx_0>,
				<&wsa_cdc_dma_0_rx>, <&wsa_cdc_dma_0_tx>,
				<&wsa_cdc_dma_1_rx>, <&wsa_cdc_dma_1_tx>,
				<&wsa_cdc_dma_2_tx>,
				<&va_cdc_dma_0_tx>, <&va_cdc_dma_1_tx>,
				<&rx_cdc_dma_0_rx>, <&tx_cdc_dma_0_tx>,
				<&rx_cdc_dma_1_rx>, <&tx_cdc_dma_1_tx>,
				<&rx_cdc_dma_2_rx>, <&tx_cdc_dma_2_tx>,
				<&rx_cdc_dma_3_rx>, <&tx_cdc_dma_3_tx>,
				<&rx_cdc_dma_4_rx>, <&tx_cdc_dma_4_tx>,
				<&rx_cdc_dma_5_rx>, <&tx_cdc_dma_5_tx>,
				<&tx_cdc_dma_6_tx>, <&tx_cdc_dma_7_tx>;
		asoc-cpu-names = "msm-dai-q6-dp.24608",
				"msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-mi2s.4", "msm-dai-q6-auxpcm.1",
				"msm-dai-q6-auxpcm.2", "msm-dai-q6-auxpcm.3",
				"msm-dai-q6-auxpcm.4", "msm-dai-q6-auxpcm.5",
				"msm-dai-q6-dev.224",
				"msm-dai-q6-dev.225", "msm-dai-q6-dev.241",
				"msm-dai-q6-dev.240", "msm-dai-q6-dev.32771",
				"msm-dai-q6-dev.32772", "msm-dai-q6-dev.32773",
				"msm-dai-q6-dev.32770", "msm-dai-q6-dev.16398",
				"msm-dai-q6-dev.16399", "msm-dai-q6-dev.16401",
				"msm-dai-q6-dev.16400",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36865",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36881",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36912", "msm-dai-q6-tdm.36913",
				"msm-dai-q6-tdm.36928", "msm-dai-q6-tdm.36929",
				"msm-dai-cdc-dma-dev.45056",
				"msm-dai-cdc-dma-dev.45057",
				"msm-dai-cdc-dma-dev.45058",
				"msm-dai-cdc-dma-dev.45059",
				"msm-dai-cdc-dma-dev.45061",
				"msm-dai-cdc-dma-dev.45089",
				"msm-dai-cdc-dma-dev.45091",
				"msm-dai-cdc-dma-dev.45120",
				"msm-dai-cdc-dma-dev.45121",
				"msm-dai-cdc-dma-dev.45122",
				"msm-dai-cdc-dma-dev.45123",
				"msm-dai-cdc-dma-dev.45124",
				"msm-dai-cdc-dma-dev.45125",
				"msm-dai-cdc-dma-dev.45126",
				"msm-dai-cdc-dma-dev.45127",
				"msm-dai-cdc-dma-dev.45128",
				"msm-dai-cdc-dma-dev.45129",
				"msm-dai-cdc-dma-dev.45130",
				"msm-dai-cdc-dma-dev.45131",
				"msm-dai-cdc-dma-dev.45133",
				"msm-dai-cdc-dma-dev.45135";
		qcom,msm-mi2s-master = <1>, <1>, <1>, <1>, <1>;
		qcom,msm-mbhc-hphl-swh = <1>;
		qcom,msm-mbhc-gnd-swh = <1>;
		qcom,cdc-dmic-gpios = <&cdc_dmic12_gpios>, <&cdc_dmic34_gpios>;
		asoc-codec  = <&stub_codec>, <&bolero>,
			      <&ext_disp_audio_codec>;
		asoc-codec-names = "msm-stub-codec.1", "bolero-codec",
				   "msm-ext-disp-audio-codec-rx";
		qcom,wsa-max-devs = <2>;
		qcom,wsa-devs = <&wsa881x_0211>, <&wsa881x_0212>,
				<&wsa881x_0213>, <&wsa881x_0214>;
		qcom,wsa-aux-dev-prefix = "SpkrLeft", "SpkrRight",
					  "SpkrLeft", "SpkrRight";
		qcom,codec-aux-devs = <&wcd937x_codec>;
		qcom,msm_audio_ssr_devs = <&audio_apr>, <&q6core>;
	};
};

* SA8155 ASoC Machine driver

Required properties:
- compatible : "qcom,sa8155-asoc-snd-auto" for auto adp codec and
               "qcom,sa8155-asoc-snd-auto-custom" for auto custom codec.
- qcom,model : The user-visible name of this sound card.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
Optional properties:
- qcom,mi2s-audio-intf : Property to specify if MI2S interface is used for the target
- qcom,auxpcm-audio-intf : Property to specify if AUX PCM interface is used for the target
- qcom,msm-mi2s-master : List of master/slave configuration for MI2S interfaces

Example:

	sound-adp-star {
		compatible = "qcom,sa8155-asoc-snd-adp-star";
		qcom,model = "sa8155-adp-star-snd-card";
		qcom,mi2s-audio-intf;
		qcom,auxpcm-audio-intf;
		qcom,msm-mi2s-master = <1>, <1>, <1>, <1>, <1>;

		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&compr>,
				<&pcm_noirq>, <&loopback1>, <&pcm_dtmf>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-compr-dsp",
				"msm-pcm-dsp-noirq", "msm-pcm-loopback.1",
				"msm-pcm-dtmf";
		asoc-cpu = <&dai_hdmi>, <&dai_dp>,
				<&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_mi2s4>, <&dai_pri_auxpcm>,
				<&dai_sec_auxpcm>, <&dai_tert_auxpcm>,
				<&dai_quat_auxpcm>, <&dai_quin_auxpcm>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_rx_1>,
				<&dai_pri_tdm_rx_2>, <&dai_pri_tdm_rx_3>,
				<&dai_pri_tdm_tx_0>, <&dai_pri_tdm_tx_1>,
				<&dai_pri_tdm_tx_2>, <&dai_pri_tdm_tx_3>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_rx_1>,
				<&dai_sec_tdm_rx_2>, <&dai_sec_tdm_rx_3>,
				<&dai_sec_tdm_tx_0>, <&dai_sec_tdm_tx_1>,
				<&dai_sec_tdm_tx_2>, <&dai_sec_tdm_tx_3>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_rx_1>,
				<&dai_tert_tdm_rx_2>, <&dai_tert_tdm_rx_3>,
				<&dai_tert_tdm_rx_4>, <&dai_tert_tdm_tx_0>,
				<&dai_tert_tdm_tx_1>, <&dai_tert_tdm_tx_2>,
				<&dai_tert_tdm_tx_3>, <&dai_quat_tdm_rx_0>,
				<&dai_quat_tdm_rx_1>, <&dai_quat_tdm_rx_2>,
				<&dai_quat_tdm_rx_3>, <&dai_quat_tdm_tx_0>,
				<&dai_quat_tdm_tx_1>, <&dai_quat_tdm_tx_2>,
				<&dai_quat_tdm_tx_3>, <&dai_quin_tdm_rx_0>,
				<&dai_quin_tdm_rx_1>, <&dai_quin_tdm_rx_2>,
				<&dai_quin_tdm_rx_3>, <&dai_quin_tdm_tx_0>,
				<&dai_quin_tdm_tx_1>, <&dai_quin_tdm_tx_2>,
				<&dai_quin_tdm_tx_3>;
		asoc-cpu-names = "msm-dai-q6-hdmi.8",  "msm-dai-q6-dp.24608",
				"msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-mi2s.4", "msm-dai-q6-auxpcm.1",
				"msm-dai-q6-auxpcm.2", "msm-dai-q6-auxpcm.3",
				"msm-dai-q6-auxpcm.4", "msm-dai-q6-auxpcm.5",
				"msm-dai-q6-dev.224", "msm-dai-q6-dev.225",
				"msm-dai-q6-dev.241", "msm-dai-q6-dev.240",
				"msm-dai-q6-dev.32771", "msm-dai-q6-dev.32772",
				"msm-dai-q6-dev.32773", "msm-dai-q6-dev.32770",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36866",
				"msm-dai-q6-tdm.36868", "msm-dai-q6-tdm.36870",
				"msm-dai-q6-tdm.36865", "msm-dai-q6-tdm.36867",
				"msm-dai-q6-tdm.36869", "msm-dai-q6-tdm.36871",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36882",
				"msm-dai-q6-tdm.36884", "msm-dai-q6-tdm.36886",
				"msm-dai-q6-tdm.36881", "msm-dai-q6-tdm.36883",
				"msm-dai-q6-tdm.36885", "msm-dai-q6-tdm.36887",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36898",
				"msm-dai-q6-tdm.36900", "msm-dai-q6-tdm.36902",
				"msm-dai-q6-tdm.36904", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36899", "msm-dai-q6-tdm.36901",
				"msm-dai-q6-tdm.36903", "msm-dai-q6-tdm.36912",
				"msm-dai-q6-tdm.36914", "msm-dai-q6-tdm.36916",
				"msm-dai-q6-tdm.36918", "msm-dai-q6-tdm.36913",
				"msm-dai-q6-tdm.36915", "msm-dai-q6-tdm.36917",
				"msm-dai-q6-tdm.36919", "msm-dai-q6-tdm.36928",
				"msm-dai-q6-tdm.36930", "msm-dai-q6-tdm.36932",
				"msm-dai-q6-tdm.36934", "msm-dai-q6-tdm.36929",
				"msm-dai-q6-tdm.36931", "msm-dai-q6-tdm.36933",
				"msm-dai-q6-tdm.36935";
		asoc-codec = <&stub_codec>;
		asoc-codec-names = "msm-stub-codec.1";
	};

* BENGAL ASoC Machine driver

Required properties:
- compatible : "qcom,bengal-asoc-snd".
- qcom,model : The user-visible name of this sound card.
- qcom,audio-routing : A list of the connections between audio components.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
- qcom,codec-aux-devs: This is phandle list containing the references to Auxilary
		       codec devices.

Optional properties:
- qcom,msm-mi2s-master: This property is used to inform machine driver
  if MSM is the clock master of mi2s. 1 means master and 0 means slave. The
  first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,msm-mbhc-hphl-swh: This property is used to distinguish headset HPHL
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,msm-mbhc-gnd-swh: This property is used to distinguish headset GND
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,ext-disp-audio-rx: Property to specify if Audio over Display port is supported for the target
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target
- qcom,mi2s-audio-intf: Property to specify if MI2S interface is used for the target
- qcom,auxpcm-audio-intf: Property to specify if Aux PCM interface is used for the target
- qcom,cdc-dmic-gpios : phandle for Digital mic clk and data gpios.
- qcom,msm_audio_ssr_devs: List the snd event framework clients
- qcom,afe-rxtx-lb: AFE RX to TX loopback.
- qcom,tlmm-gpio: TLMM gpio number for corresponding LPASS gpio
- qcom,va-bolero-codec: Property to specify VA macro supported.
- qcom,rxtx-bolero-codec: Property to specify RX-TX macros supported.
- qcom,wsa-bolero-codec: Property to specify WSA macro supported.

Example:
	bengal_snd: sound {
		status = "okay";
		compatible = "qcom,bengal-asoc-snd";
		qcom,wcn-btfm = <1>;
		qcom,mi2s-audio-intf = <1>;
		qcom,auxpcm-audio-intf = <1>;
		qcom,afe-rxtx-lb = <1>;
		qcom,va-bolero-codec = <1>;
		qcom,rxtx-bolero-codec = <1>;

		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&compr>,
				<&pcm_noirq>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-compr-dsp",
				"msm-pcm-dsp-noirq";
		asoc-cpu = <&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_mi2s4>, <&dai_pri_auxpcm>,
				<&dai_sec_auxpcm>, <&dai_tert_auxpcm>,
				<&dai_quat_auxpcm>, <&dai_quin_auxpcm>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_tx_0>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_tx_0>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_tx_0>,
				<&dai_quat_tdm_rx_0>, <&dai_quat_tdm_tx_0>,
				<&dai_quin_tdm_rx_0>, <&dai_quin_tdm_tx_0>,
				<&wsa_cdc_dma_0_rx>, <&wsa_cdc_dma_0_tx>,
				<&wsa_cdc_dma_1_rx>, <&wsa_cdc_dma_1_tx>,
				<&wsa_cdc_dma_2_tx>,
				<&va_cdc_dma_0_tx>, <&va_cdc_dma_1_tx>,
				<&rx_cdc_dma_0_rx>, <&tx_cdc_dma_0_tx>,
				<&rx_cdc_dma_1_rx>, <&tx_cdc_dma_1_tx>,
				<&rx_cdc_dma_2_rx>, <&tx_cdc_dma_2_tx>,
				<&rx_cdc_dma_3_rx>, <&tx_cdc_dma_3_tx>,
				<&rx_cdc_dma_4_rx>, <&tx_cdc_dma_4_tx>,
				<&rx_cdc_dma_5_rx>, <&tx_cdc_dma_5_tx>,
				<&tx_cdc_dma_6_tx>, <&tx_cdc_dma_7_tx>;
		asoc-cpu-names = "msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-mi2s.4", "msm-dai-q6-auxpcm.1",
				"msm-dai-q6-auxpcm.2", "msm-dai-q6-auxpcm.3",
				"msm-dai-q6-auxpcm.4", "msm-dai-q6-auxpcm.5",
				"msm-dai-q6-dev.224",
				"msm-dai-q6-dev.225", "msm-dai-q6-dev.241",
				"msm-dai-q6-dev.240", "msm-dai-q6-dev.32771",
				"msm-dai-q6-dev.32772", "msm-dai-q6-dev.32773",
				"msm-dai-q6-dev.32770", "msm-dai-q6-dev.16398",
				"msm-dai-q6-dev.16399", "msm-dai-q6-dev.16401",
				"msm-dai-q6-dev.16400",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36865",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36881",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36912", "msm-dai-q6-tdm.36913",
				"msm-dai-q6-tdm.36928", "msm-dai-q6-tdm.36929",
				"msm-dai-cdc-dma-dev.45056",
				"msm-dai-cdc-dma-dev.45057",
				"msm-dai-cdc-dma-dev.45058",
				"msm-dai-cdc-dma-dev.45059",
				"msm-dai-cdc-dma-dev.45061",
				"msm-dai-cdc-dma-dev.45089",
				"msm-dai-cdc-dma-dev.45091",
				"msm-dai-cdc-dma-dev.45120",
				"msm-dai-cdc-dma-dev.45121",
				"msm-dai-cdc-dma-dev.45122",
				"msm-dai-cdc-dma-dev.45123",
				"msm-dai-cdc-dma-dev.45124",
				"msm-dai-cdc-dma-dev.45125",
				"msm-dai-cdc-dma-dev.45126",
				"msm-dai-cdc-dma-dev.45127",
				"msm-dai-cdc-dma-dev.45128",
				"msm-dai-cdc-dma-dev.45129",
				"msm-dai-cdc-dma-dev.45130",
				"msm-dai-cdc-dma-dev.45131",
				"msm-dai-cdc-dma-dev.45133",
				"msm-dai-cdc-dma-dev.45135";
		qcom,msm-mi2s-master = <1>, <1>, <1>, <1>;
		qcom,msm-mbhc-hphl-swh = <1>;
		qcom,msm-mbhc-gnd-swh = <1>;
		qcom,cdc-dmic-gpios = <&cdc_dmic12_gpios>, <&cdc_dmic34_gpios>;
		asoc-codec  = <&stub_codec>, <&bolero>;
		asoc-codec-names = "msm-stub-codec.1", "bolero-codec";
		qcom,wsa-max-devs = <1>;
		qcom,wsa-devs = <&wsa881x_i2c_f>;
		qcom,wsa-aux-dev-prefix = "SpkrMono";
		qcom,codec-aux-devs = <&wcd937x_codec>;
		qcom,msm_audio_ssr_devs = <&audio_apr>, <&q6core>;
	};

* KONA ASoC Machine driver

Required properties:
- compatible : "qcom,kona-asoc-snd".
- qcom,model : The user-visible name of this sound card.
- qcom,audio-routing : A list of the connections between audio components.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
- qcom,codec-aux-devs: This is phandle list containing the references to Auxilary
		       codec devices.

Optional properties:
- qcom,msm-mi2s-master: This property is used to inform machine driver
  if MSM is the clock master of mi2s. 1 means master and 0 means slave. The
  first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,msm-mbhc-hphl-swh: This property is used to distinguish headset HPHL
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,msm-mbhc-gnd-swh: This property is used to distinguish headset GND
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,ext-disp-audio-rx: Property to specify if Audio over Display port is supported for the target
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target
- qcom,mi2s-audio-intf: Property to specify if MI2S interface is used for the target
- qcom,auxpcm-audio-intf: Property to specify if Aux PCM interface is used for the target
- qcom,cdc-dmic-gpios : phandle for Digital mic clk and data gpios.
- qcom,msm_audio_ssr_devs: List the snd event framework clients
- qcom,afe-rxtx-lb: AFE RX to TX loopback.
- qcom,tlmm-gpio: TLMM gpio number for corresponding LPASS gpio

Example:
	kona_snd: sound {
		status = "okay";
		compatible = "qcom,kona-asoc-snd";
		qcom,ext-disp-audio-rx = <1>;
		qcom,wcn-btfm = <1>;
		qcom,mi2s-audio-intf = <1>;
		qcom,auxpcm-audio-intf = <1>;
		qcom,afe-rxtx-lb = <1>;

		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&compr>,
				<&pcm_noirq>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-compr-dsp",
				"msm-pcm-dsp-noirq";
		asoc-cpu = <&dai_dp>,
				<&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_mi2s4>, <&dai_pri_auxpcm>,
				<&dai_sec_auxpcm>, <&dai_tert_auxpcm>,
				<&dai_quat_auxpcm>, <&dai_quin_auxpcm>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_tx_0>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_tx_0>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_tx_0>,
				<&dai_quat_tdm_rx_0>, <&dai_quat_tdm_tx_0>,
				<&dai_quin_tdm_rx_0>, <&dai_quin_tdm_tx_0>,
				<&wsa_cdc_dma_0_rx>, <&wsa_cdc_dma_0_tx>,
				<&wsa_cdc_dma_1_rx>, <&wsa_cdc_dma_1_tx>,
				<&wsa_cdc_dma_2_tx>,
				<&va_cdc_dma_0_tx>, <&va_cdc_dma_1_tx>,
				<&rx_cdc_dma_0_rx>, <&tx_cdc_dma_0_tx>,
				<&rx_cdc_dma_1_rx>, <&tx_cdc_dma_1_tx>,
				<&rx_cdc_dma_2_rx>, <&tx_cdc_dma_2_tx>,
				<&rx_cdc_dma_3_rx>, <&tx_cdc_dma_3_tx>,
				<&rx_cdc_dma_4_rx>, <&tx_cdc_dma_4_tx>,
				<&rx_cdc_dma_5_rx>, <&tx_cdc_dma_5_tx>,
				<&tx_cdc_dma_6_tx>, <&tx_cdc_dma_7_tx>;
		asoc-cpu-names = "msm-dai-q6-dp.24608",
				"msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-mi2s.4", "msm-dai-q6-auxpcm.1",
				"msm-dai-q6-auxpcm.2", "msm-dai-q6-auxpcm.3",
				"msm-dai-q6-auxpcm.4", "msm-dai-q6-auxpcm.5",
				"msm-dai-q6-dev.224",
				"msm-dai-q6-dev.225", "msm-dai-q6-dev.241",
				"msm-dai-q6-dev.240", "msm-dai-q6-dev.32771",
				"msm-dai-q6-dev.32772", "msm-dai-q6-dev.32773",
				"msm-dai-q6-dev.32770", "msm-dai-q6-dev.16398",
				"msm-dai-q6-dev.16399", "msm-dai-q6-dev.16401",
				"msm-dai-q6-dev.16400",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36865",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36881",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36912", "msm-dai-q6-tdm.36913",
				"msm-dai-q6-tdm.36928", "msm-dai-q6-tdm.36929",
				"msm-dai-cdc-dma-dev.45056",
				"msm-dai-cdc-dma-dev.45057",
				"msm-dai-cdc-dma-dev.45058",
				"msm-dai-cdc-dma-dev.45059",
				"msm-dai-cdc-dma-dev.45061",
				"msm-dai-cdc-dma-dev.45089",
				"msm-dai-cdc-dma-dev.45091",
				"msm-dai-cdc-dma-dev.45120",
				"msm-dai-cdc-dma-dev.45121",
				"msm-dai-cdc-dma-dev.45122",
				"msm-dai-cdc-dma-dev.45123",
				"msm-dai-cdc-dma-dev.45124",
				"msm-dai-cdc-dma-dev.45125",
				"msm-dai-cdc-dma-dev.45126",
				"msm-dai-cdc-dma-dev.45127",
				"msm-dai-cdc-dma-dev.45128",
				"msm-dai-cdc-dma-dev.45129",
				"msm-dai-cdc-dma-dev.45130",
				"msm-dai-cdc-dma-dev.45131",
				"msm-dai-cdc-dma-dev.45133",
				"msm-dai-cdc-dma-dev.45135";
		qcom,msm-mi2s-master = <1>, <1>, <1>, <1>, <1>;
		qcom,msm-mbhc-hphl-swh = <1>;
		qcom,msm-mbhc-gnd-swh = <1>;
		qcom,cdc-dmic-gpios = <&cdc_dmic12_gpios>, <&cdc_dmic34_gpios>;
		asoc-codec  = <&stub_codec>, <&bolero>,
			      <&ext_disp_audio_codec>;
		asoc-codec-names = "msm-stub-codec.1", "bolero-codec",
				   "msm-ext-disp-audio-codec-rx";
		qcom,wsa-max-devs = <2>;
		qcom,wsa-devs = <&wsa881x_0211>, <&wsa881x_0212>,
				<&wsa881x_0213>, <&wsa881x_0214>;
		qcom,wsa-aux-dev-prefix = "SpkrLeft", "SpkrRight",
					  "SpkrLeft", "SpkrRight";
		qcom,codec-aux-devs = <&wcd937x_codec>;
		qcom,msm_audio_ssr_devs = <&audio_apr>, <&q6core>;
	};

* voice-mhi-audio

Required properties:
 - compatible : "qcom,voice-mhi-audio"
 - memory-region : CMA region owned by this device

Optional properties:
 - voice_mhi_voting : Property that defines whether voting is needed or not for this device

Example:

	qcom,voice-mhi-audio {
		compatible = "qcom,voice-mhi-audio";
		memory-region = <&mailbox_mem>;
		voice_mhi_voting;
	};

};

* LAHAINA ASoC Machine driver

Required properties:
- compatible : "qcom,lahaina-asoc-snd".
- qcom,model : The user-visible name of this sound card.
- qcom,audio-routing : A list of the connections between audio components.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
- qcom,codec-aux-devs: This is phandle list containing the references to Auxilary
		       codec devices.

Optional properties:
- qcom,msm-mi2s-master: This property is used to inform machine driver
  if MSM is the clock master of mi2s. 1 means master and 0 means slave. The
  first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,msm-mbhc-hphl-swh: This property is used to distinguish headset HPHL
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,msm-mbhc-gnd-swh: This property is used to distinguish headset GND
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,ext-disp-audio-rx: Property to specify if Audio over Display port is supported for the target
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target
- qcom,mi2s-audio-intf: Property to specify if MI2S interface is used for the target
- qcom,auxpcm-audio-intf: Property to specify if Aux PCM interface is used for the target
- qcom,cdc-dmic-gpios : phandle for Digital mic clk and data gpios.
- qcom,msm_audio_ssr_devs: List the snd event framework clients
- qcom,afe-rxtx-lb: AFE RX to TX loopback.
- qcom,tlmm-gpio: TLMM gpio number for corresponding LPASS gpio
- qcom,wcd-disabled : Property to specify if wcd codec is disabled for the target

Example:
	lahaina_snd: sound {
		compatible = "qcom,lahaina-asoc-snd";
		qcom,mi2s-audio-intf = <1>;
		qcom,auxpcm-audio-intf = <1>;
		qcom,wcn-bt = <0>;
		qcom,ext-disp-audio-rx = <0>;
		qcom,afe-rxtx-lb = <0>;
		qcom,wcd-disabled = <0>;

		clock-names = "lpass_audio_hw_vote";
		clocks = <&lpass_audio_hw_vote 0>;

		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&compr>,
				<&pcm_noirq>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-compr-dsp",
				"msm-pcm-dsp-noirq";
		asoc-cpu = <&dai_dp>, <&dai_dp1>,
				<&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_mi2s4>, <&dai_mi2s5>, <&dai_pri_auxpcm>,
				<&dai_sec_auxpcm>, <&dai_tert_auxpcm>,
				<&dai_quat_auxpcm>, <&dai_quin_auxpcm>,
				<&dai_sen_auxpcm>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&sb_7_rx>, <&sb_7_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_tx_0>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_tx_0>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_tx_0>,
				<&dai_quat_tdm_rx_0>, <&dai_quat_tdm_tx_0>,
				<&dai_quin_tdm_rx_0>, <&dai_quin_tdm_tx_0>,
				<&dai_sen_tdm_rx_0>, <&dai_sen_tdm_tx_0>,
				<&wsa_cdc_dma_0_rx>, <&wsa_cdc_dma_0_tx>,
				<&wsa_cdc_dma_1_rx>, <&wsa_cdc_dma_1_tx>,
				<&wsa_cdc_dma_2_tx>,
				<&va_cdc_dma_0_tx>, <&va_cdc_dma_1_tx>,
				<&va_cdc_dma_2_tx>,
				<&rx_cdc_dma_0_rx>, <&tx_cdc_dma_0_tx>,
				<&rx_cdc_dma_1_rx>, <&tx_cdc_dma_1_tx>,
				<&rx_cdc_dma_2_rx>, <&tx_cdc_dma_2_tx>,
				<&rx_cdc_dma_3_rx>, <&tx_cdc_dma_3_tx>,
				<&rx_cdc_dma_4_rx>, <&tx_cdc_dma_4_tx>,
				<&rx_cdc_dma_5_rx>, <&tx_cdc_dma_5_tx>,
				<&rx_cdc_dma_6_rx>, <&rx_cdc_dma_7_rx>,
				<&afe_loopback_tx>;
		asoc-cpu-names = "msm-dai-q6-dp.0", "msm-dai-q6-dp.1",
				"msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-mi2s.4", "msm-dai-q6-mi2s.5",
				"msm-dai-q6-auxpcm.1",
				"msm-dai-q6-auxpcm.2", "msm-dai-q6-auxpcm.3",
				"msm-dai-q6-auxpcm.4", "msm-dai-q6-auxpcm.5",
				"msm-dai-q6-auxpcm.6", "msm-dai-q6-dev.224",
				"msm-dai-q6-dev.225", "msm-dai-q6-dev.241",
				"msm-dai-q6-dev.240", "msm-dai-q6-dev.32771",
				"msm-dai-q6-dev.32772", "msm-dai-q6-dev.32773",
				"msm-dai-q6-dev.32770",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-dev.16398", "msm-dai-q6-dev.16399",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36865",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36881",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36912", "msm-dai-q6-tdm.36913",
				"msm-dai-q6-tdm.36928", "msm-dai-q6-tdm.36929",
				"msm-dai-q6-tdm.36944", "msm-dai-q6-tdm.36945",
				"msm-dai-cdc-dma-dev.45056",
				"msm-dai-cdc-dma-dev.45057",
				"msm-dai-cdc-dma-dev.45058",
				"msm-dai-cdc-dma-dev.45059",
				"msm-dai-cdc-dma-dev.45061",
				"msm-dai-cdc-dma-dev.45089",
				"msm-dai-cdc-dma-dev.45091",
				"msm-dai-cdc-dma-dev.45093",
				"msm-dai-cdc-dma-dev.45104",
				"msm-dai-cdc-dma-dev.45105",
				"msm-dai-cdc-dma-dev.45106",
				"msm-dai-cdc-dma-dev.45107",
				"msm-dai-cdc-dma-dev.45108",
				"msm-dai-cdc-dma-dev.45109",
				"msm-dai-cdc-dma-dev.45110",
				"msm-dai-cdc-dma-dev.45111",
				"msm-dai-cdc-dma-dev.45112",
				"msm-dai-cdc-dma-dev.45113",
				"msm-dai-cdc-dma-dev.45114",
				"msm-dai-cdc-dma-dev.45115",
				"msm-dai-cdc-dma-dev.45116",
				"msm-dai-cdc-dma-dev.45118",
				"msm-dai-q6-dev.24577";
		fsa4480-i2c-handle = <&fsa4480>;
	};
};

* HOLI ASoC Machine driver

Required properties:
- compatible : "qcom,holi-asoc-snd".
>>>>>>> kernel.lnx.5.4-200915
- qcom,model : The user-visible name of this sound card.
- qcom,audio-routing : A list of the connections between audio components.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
- qcom,codec-aux-devs: This is phandle list containing the references to Auxilary
		       codec devices.

Optional properties:
- qcom,msm-mi2s-master: This property is used to inform machine driver
  if MSM is the clock master of mi2s. 1 means master and 0 means slave. The
  first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,msm-mbhc-hphl-swh: This property is used to distinguish headset HPHL
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,msm-mbhc-gnd-swh: This property is used to distinguish headset GND
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,ext-disp-audio-rx: Property to specify if Audio over Display port is supported for the target
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target
- qcom,mi2s-audio-intf: Property to specify if MI2S interface is used for the target
- qcom,auxpcm-audio-intf: Property to specify if Aux PCM interface is used for the target
- qcom,cdc-dmic-gpios : phandle for Digital mic clk and data gpios.
- qcom,msm_audio_ssr_devs: List the snd event framework clients
- qcom,afe-rxtx-lb: AFE RX to TX loopback.
- qcom,tlmm-gpio: TLMM gpio number for corresponding LPASS gpio

Example:
	holi_snd: sound {
		compatible = "qcom,holi-asoc-snd";
		qcom,mi2s-audio-intf = <1>;
		qcom,auxpcm-audio-intf = <1>;
		qcom,wcn-bt = <0>;
		qcom,afe-rxtx-lb = <0>;
		qcom,is-wcd937x-codec = <1>;

		clock-names = "lpass_audio_hw_vote";
		clocks = <&lpass_audio_hw_vote 0>;

		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&compr>,
				<&pcm_noirq>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-compr-dsp",
				"msm-pcm-dsp-noirq";
		asoc-cpu = <&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_pri_auxpcm>,
				<&dai_sec_auxpcm>, <&dai_tert_auxpcm>,
				<&dai_quat_auxpcm>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>,
				<&afe_proxy_tx_1>,
				<&proxy_rx>, <&proxy_tx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&sb_7_rx>, <&sb_7_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_tx_0>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_tx_0>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_tx_0>,
				<&dai_quat_tdm_rx_0>, <&dai_quat_tdm_tx_0>,
				<&va_cdc_dma_0_tx>, <&va_cdc_dma_1_tx>,
				<&va_cdc_dma_2_tx>,
				<&rx_cdc_dma_0_rx>, <&tx_cdc_dma_0_tx>,
				<&rx_cdc_dma_1_rx>, <&tx_cdc_dma_1_tx>,
				<&rx_cdc_dma_2_rx>, <&tx_cdc_dma_2_tx>,
				<&rx_cdc_dma_3_rx>, <&tx_cdc_dma_3_tx>,
				<&rx_cdc_dma_4_rx>, <&tx_cdc_dma_4_tx>,
				<&rx_cdc_dma_5_rx>, <&tx_cdc_dma_5_tx>,
				<&rx_cdc_dma_7_rx>,<&afe_loopback_tx>;
		asoc-cpu-names = "msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-auxpcm.1",
				"msm-dai-q6-auxpcm.2", "msm-dai-q6-auxpcm.3",
				"msm-dai-q6-auxpcm.4",
				"msm-dai-q6-dev.224",
				"msm-dai-q6-dev.225", "msm-dai-q6-dev.241",
				"msm-dai-q6-dev.240", "msm-dai-q6-dev.32771",
				"msm-dai-q6-dev.32772", "msm-dai-q6-dev.32773",
				"msm-dai-q6-dev.32770",
				"msm-dai-q6-dev.242",
				"msm-dai-q6-dev.8194", "msm-dai-q6-dev.8195",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-dev.16398", "msm-dai-q6-dev.16399",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36865",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36881",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36912", "msm-dai-q6-tdm.36913",
				"msm-dai-cdc-dma-dev.45089",
				"msm-dai-cdc-dma-dev.45091",
				"msm-dai-cdc-dma-dev.45093",
				"msm-dai-cdc-dma-dev.45104",
				"msm-dai-cdc-dma-dev.45105",
				"msm-dai-cdc-dma-dev.45106",
				"msm-dai-cdc-dma-dev.45107",
				"msm-dai-cdc-dma-dev.45108",
				"msm-dai-cdc-dma-dev.45109",
				"msm-dai-cdc-dma-dev.45110",
				"msm-dai-cdc-dma-dev.45111",
				"msm-dai-cdc-dma-dev.45112",
				"msm-dai-cdc-dma-dev.45113",
				"msm-dai-cdc-dma-dev.45114",
				"msm-dai-cdc-dma-dev.45115",
				"msm-dai-cdc-dma-dev.45118",
				"msm-dai-q6-dev.24577";
	};
};


* Waipio ASoC Machine driver

Required properties:
- compatible : "qcom,waipio-asoc-snd".
- compatible : "qcom,waipio-asoc-snd-stub" for waipio rumi target.
- qcom,model : The user-visible name of this sound card.
- qcom,audio-routing : A list of the connections between audio components.
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".
- qcom,codec-aux-devs: This is phandle list containing the references to Auxilary
		       codec devices.

Optional properties:
- qcom,msm-mi2s-master: This property is used to inform machine driver
  if MSM is the clock master of mi2s. 1 means master and 0 means slave. The
  first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,tdm-clk-attribute: This property is used to set the clock attribute for tdm.
  The first entry is primary tdm; the second entry is secondary tdm, and so on.
- qcom,mi2s-clk-attribute: This property is used to set the clock attribute for mi2s.
  The first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,msm-mbhc-hphl-swh: This property is used to distinguish headset HPHL
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,msm-mbhc-gnd-swh: This property is used to distinguish headset GND
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,ext-disp-audio-rx: Property to specify if Audio over Display port is supported for the target
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target
- qcom,mi2s-audio-intf: Property to specify if MI2S interface is used for the target
- qcom,auxpcm-audio-intf: Property to specify if Aux PCM interface is used for the target
- qcom,cdc-dmic-gpios : phandle for Digital mic clk and data gpios.
- qcom,msm_audio_ssr_devs: List the snd event framework clients
- qcom,afe-rxtx-lb: AFE RX to TX loopback.
- qcom,tlmm-gpio: TLMM gpio number for corresponding LPASS gpio

Example:
	waipio_snd: sound {
		compatible = "qcom,waipio-asoc-snd";
		qcom,mi2s-audio-intf = <1>;
		qcom,auxpcm-audio-intf = <1>;
		qcom,tdm-clk-attribute = <0x1>, <0x1>, <0x1>, <0x1>, <0x1>, <0x1>;
		qcom,mi2s-clk-attribute = <0x1>, <0x1>, <0x1>, <0x1>, <0x1>, <0x1>;
		qcom,wcn-bt = <0>;
		qcom,ext-disp-audio-rx = <0>;
		qcom,afe-rxtx-lb = <0>;

		clock-names = "lpass_audio_hw_vote";
		clocks = <&lpass_audio_hw_vote 0>;

		asoc-platform = <&pcm0>, <&pcm1>, <&pcm2>, <&voip>, <&voice>,
				<&loopback>, <&compress>, <&hostless>,
				<&afe>, <&lsm>, <&routing>, <&compr>,
				<&pcm_noirq>;
		asoc-platform-names = "msm-pcm-dsp.0", "msm-pcm-dsp.1",
				"msm-pcm-dsp.2", "msm-voip-dsp",
				"msm-pcm-voice", "msm-pcm-loopback",
				"msm-compress-dsp", "msm-pcm-hostless",
				"msm-pcm-afe", "msm-lsm-client",
				"msm-pcm-routing", "msm-compr-dsp",
				"msm-pcm-dsp-noirq";
		asoc-cpu = <&dai_dp>, <&dai_dp1>,
				<&dai_mi2s0>, <&dai_mi2s1>,
				<&dai_mi2s2>, <&dai_mi2s3>,
				<&dai_mi2s4>, <&dai_mi2s5>, <&dai_pri_auxpcm>,
				<&dai_sec_auxpcm>, <&dai_tert_auxpcm>,
				<&dai_quat_auxpcm>, <&dai_quin_auxpcm>,
				<&dai_sen_auxpcm>,
				<&afe_pcm_rx>, <&afe_pcm_tx>, <&afe_proxy_rx>,
				<&afe_proxy_tx>, <&incall_record_rx>,
				<&incall_record_tx>, <&incall_music_rx>,
				<&incall_music_2_rx>,
				<&usb_audio_rx>, <&usb_audio_tx>,
				<&sb_7_rx>, <&sb_7_tx>,
				<&dai_pri_tdm_rx_0>, <&dai_pri_tdm_tx_0>,
				<&dai_sec_tdm_rx_0>, <&dai_sec_tdm_tx_0>,
				<&dai_tert_tdm_rx_0>, <&dai_tert_tdm_tx_0>,
				<&dai_quat_tdm_rx_0>, <&dai_quat_tdm_tx_0>,
				<&dai_quin_tdm_rx_0>, <&dai_quin_tdm_tx_0>,
				<&dai_sen_tdm_rx_0>, <&dai_sen_tdm_tx_0>,
				<&wsa_cdc_dma_0_rx>, <&wsa_cdc_dma_0_tx>,
				<&wsa_cdc_dma_1_rx>, <&wsa_cdc_dma_1_tx>,
				<&wsa_cdc_dma_2_tx>,
				<&va_cdc_dma_0_tx>, <&va_cdc_dma_1_tx>,
				<&va_cdc_dma_2_tx>,
				<&rx_cdc_dma_0_rx>, <&tx_cdc_dma_0_tx>,
				<&rx_cdc_dma_1_rx>, <&tx_cdc_dma_1_tx>,
				<&rx_cdc_dma_2_rx>, <&tx_cdc_dma_2_tx>,
				<&rx_cdc_dma_3_rx>, <&tx_cdc_dma_3_tx>,
				<&rx_cdc_dma_4_rx>, <&tx_cdc_dma_4_tx>,
				<&rx_cdc_dma_5_rx>, <&tx_cdc_dma_5_tx>,
				<&rx_cdc_dma_6_rx>, <&rx_cdc_dma_7_rx>,
				<&afe_loopback_tx>;
		asoc-cpu-names = "msm-dai-q6-dp.0", "msm-dai-q6-dp.1",
				"msm-dai-q6-mi2s.0", "msm-dai-q6-mi2s.1",
				"msm-dai-q6-mi2s.2", "msm-dai-q6-mi2s.3",
				"msm-dai-q6-mi2s.4", "msm-dai-q6-mi2s.5",
				"msm-dai-q6-auxpcm.1",
				"msm-dai-q6-auxpcm.2", "msm-dai-q6-auxpcm.3",
				"msm-dai-q6-auxpcm.4", "msm-dai-q6-auxpcm.5",
				"msm-dai-q6-auxpcm.6", "msm-dai-q6-dev.224",
				"msm-dai-q6-dev.225", "msm-dai-q6-dev.241",
				"msm-dai-q6-dev.240", "msm-dai-q6-dev.32771",
				"msm-dai-q6-dev.32772", "msm-dai-q6-dev.32773",
				"msm-dai-q6-dev.32770",
				"msm-dai-q6-dev.28672", "msm-dai-q6-dev.28673",
				"msm-dai-q6-dev.16398", "msm-dai-q6-dev.16399",
				"msm-dai-q6-tdm.36864", "msm-dai-q6-tdm.36865",
				"msm-dai-q6-tdm.36880", "msm-dai-q6-tdm.36881",
				"msm-dai-q6-tdm.36896", "msm-dai-q6-tdm.36897",
				"msm-dai-q6-tdm.36912", "msm-dai-q6-tdm.36913",
				"msm-dai-q6-tdm.36928", "msm-dai-q6-tdm.36929",
				"msm-dai-q6-tdm.36944", "msm-dai-q6-tdm.36945",
				"msm-dai-cdc-dma-dev.45056",
				"msm-dai-cdc-dma-dev.45057",
				"msm-dai-cdc-dma-dev.45058",
				"msm-dai-cdc-dma-dev.45059",
				"msm-dai-cdc-dma-dev.45061",
				"msm-dai-cdc-dma-dev.45089",
				"msm-dai-cdc-dma-dev.45091",
				"msm-dai-cdc-dma-dev.45093",
				"msm-dai-cdc-dma-dev.45104",
				"msm-dai-cdc-dma-dev.45105",
				"msm-dai-cdc-dma-dev.45106",
				"msm-dai-cdc-dma-dev.45107",
				"msm-dai-cdc-dma-dev.45108",
				"msm-dai-cdc-dma-dev.45109",
				"msm-dai-cdc-dma-dev.45110",
				"msm-dai-cdc-dma-dev.45111",
				"msm-dai-cdc-dma-dev.45112",
				"msm-dai-cdc-dma-dev.45113",
				"msm-dai-cdc-dma-dev.45114",
				"msm-dai-cdc-dma-dev.45115",
				"msm-dai-cdc-dma-dev.45116",
				"msm-dai-cdc-dma-dev.45118",
				"msm-dai-q6-dev.24577";
		fsa4480-i2c-handle = <&fsa4480>;
	};
};


* Kalama ASoC Machine driver

Required properties:
- compatible : "qcom,kalama-asoc-snd".
- compatible : "qcom,kalama-asoc-snd-stub" for kalama rumi target.
- qcom,model : The user-visible name of this sound card.
- qcom,audio-routing : A list of the connections between audio components.
- asoc-codec: This is phandle list containing the references to codec dai device
	      nodes that are used as part of the sound card dai-links.
- asoc-codec-names: This property contains list of codec dai names. The order of the
		    codec dai names should match to that of the phandle order given
		    in "asoc-codec".

Optional properties:
- asoc-platform: This is phandle list containing the references to platform device
		 nodes that are used as part of the sound card dai-links.
- asoc-platform-names: This property contains list of platform names. The order of
		       the platform names should match to that of the phandle order
		       given in "asoc-platform".
- asoc-cpu: This is phandle list containing the references to cpu dai device nodes
	    that are used as part of the sound card dai-links.
- asoc-cpu-names: This property contains list of cpu dai names. The order of the
		  cpu dai names should match to that of the phandle order given
		  in "asoc-cpu". The cpu names are in the form of "%s.%d" form,
		  where the id (%d) field represents the back-end AFE port id that
		  this CPU dai is associated with.
- qcom,msm-mi2s-master: This property is used to inform machine driver
  if MSM is the clock master of mi2s. 1 means master and 0 means slave. The
  first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,tdm-clk-attribute: This property is used to set the clock attribute for tdm.
  The first entry is primary tdm; the second entry is secondary tdm, and so on.
- qcom,mi2s-clk-attribute: This property is used to set the clock attribute for mi2s.
  The first entry is primary mi2s; the second entry is secondary mi2s, and so on.
- qcom,msm-mbhc-hphl-swh: This property is used to distinguish headset HPHL
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,msm-mbhc-gnd-swh: This property is used to distinguish headset GND
  switch type on target typically the switch type will be normally open or
  normally close, value for this property 0 for normally close and 1 for
  normally open.
- qcom,codec-aux-devs: This is phandle list containing the references to Auxilary
		       codec devices.
- qcom,wsa-max-devs : Maximum number of WSA881x devices present in the target
- qcom,wsa-devs : List of phandles for all possible WSA881x devices supported for the target
- qcom,wsa-aux-dev-prefix : Name prefix with Left/Right configuration for WSA881x device
- qcom,ext-disp-audio-rx: Property to specify if Audio over Display port is supported for the target
- qcom,wcn-btfm : Property to specify if WCN BT/FM chip is used for the target
- qcom,mi2s-audio-intf: Property to specify if MI2S interface is used for the target
- qcom,auxpcm-audio-intf: Property to specify if Aux PCM interface is used for the target
- qcom,cdc-dmic-gpios : phandle for Digital mic clk and data gpios.
- qcom,msm_audio_ssr_devs: List the snd event framework clients
- qcom,afe-rxtx-lb: AFE RX to TX loopback.
- qcom,tlmm-gpio: TLMM gpio number for corresponding LPASS gpio

Example:
	kalama_snd: sound {
		compatible = "qcom,kalama-asoc-snd";
		qcom,mi2s-audio-intf = <1>;
		qcom,auxpcm-audio-intf = <1>;
		qcom,tdm-clk-attribute = <0x1>, <0x1>, <0x1>, <0x1>, <0x1>, <0x1>;
		qcom,mi2s-clk-attribute = <0x1>, <0x1>, <0x1>, <0x1>, <0x1>, <0x1>;
		qcom,wcn-bt = <0>;
		qcom,ext-disp-audio-rx = <0>;
		qcom,afe-rxtx-lb = <0>;

		clock-names = "lpass_audio_hw_vote";
		clocks = <&lpass_audio_hw_vote 0>;

		asoc-codec  = <&stub_codec>, <&lpass_cdc>,
			      <&wcd938x_codec>, <&swr_haptics>,
		      	<&wsa884x_0220>, <&wsa884x_0221>;
		asoc-codec-names = "msm-stub-codec.1", "lpass-cdc",
				   "wcd938x_codec", "swr-haptics",
			   	"wsa-codec1", "wsa-codec2";
	};
};

Required properties:
- compatible : "qcom,spf-core-platform"

Required properties:
- compatible : "qcom,audio-pkt-core-platform"

Required properties:
- compatible : "qcom,swr-wcd"

Required properties:
- compatible : "qcom,tavil-i2c"

Required properties:
- compatible : "qcom,wcd-pinctrl"

Required properties:
- compatible : "qcom,gpr"

Required properties:
- compatible : "qcom,spf_core"

Required properties:
- compatible : "qcom,audio-pkt"

Required properties:
- compatible : "qcom,audio_prm"
