#include <dt-bindings/regulator/qcom,rpmh-regulator-levels.h>

&apps_rsc_drv2 {
	rpmh-regulator-gfxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "gfx.lvl";
		VDD_GFX_LEVEL: S5B_LEVEL:
		pm8350_s5_level: regulator-pm8350-s5-level {
			regulator-name = "pm8350_s5_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-lcxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "lcx.lvl";
		VDD_LPI_CX_LEVEL: L8B_LEVEL:
		pm8350_l8_level: regulator-pm8350-l8-level {
			regulator-name = "pm8350_l8_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-msslvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mss.lvl";
		VDD_MODEM_LEVEL: S4C_LEVEL:
		pm8350c_s4_level: regulator-pm8350c-s4-level {
			regulator-name = "pm8350c_s4_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-cxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "cx.lvl";
		proxy-supply = <&VDD_CX_LEVEL>;

		VDD_CX_LEVEL: S6C_LEVEL:
		pm8350c_s6_level: regulator-pm8350c-s6-level {
			regulator-name = "pm8350c_s6_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_CX_LEVEL_AO: S6C_LEVEL_AO:
		pm8350c_s6_level_ao: regulator-pm8350c-s6-level-ao {
			regulator-name = "pm8350c_s6_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};

		VDD_CX_MMCX_SUPPLY_LEVEL: regulator-pm8350c-s6-mmcx-sup-level {
			regulator-name = "pm8350c_s6_mmcx_sup_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
		};
	};

	rpmh-regulator-ebilvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "ebi.lvl";
		VDD_EBI_LEVEL: S2H_LEVEL:
		pm8450_s2_level: regulator-pm8450-s2-level {
			regulator-name = "pm8450_s2_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-mmcxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mmcx.lvl";
		proxy-supply = <&VDD_MMCX_LEVEL>;

		VDD_MMCX_LEVEL: VDD_MM_LEVEL: S4H_LEVEL:
		pm8450_s4_level: regulator-pm8450-s4-level {
			regulator-name = "pm8450_s4_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			pm8450_s4_level-parent-supply =
				<&VDD_CX_MMCX_SUPPLY_LEVEL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MMCX_LEVEL_AO: VDD_MM_LEVEL_AO: S4H_LEVEL_AO:
		pm8450_s4_level_ao: regulator-pm8450-s4-level-ao {
			regulator-name = "pm8450_s4_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
		};

		regulator-pm8450-s4-level-so {
			regulator-name = "pm8450_s4_level_so";
			qcom,set = <RPMH_REGULATOR_SET_SLEEP>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
		};
	};

	rpmh-regulator-mxclvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mxc.lvl";
		proxy-supply = <&VDD_MXC_LEVEL>;

		VDD_MXC_LEVEL: S2C_LEVEL:
		pm8350c_s2_level: regulator-pm8350c-s2-level {
			regulator-name = "pm8350c_s2_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MXC_LEVEL_AO: S2C_LEVEL_AO:
		pm8350c_s2_level_ao: regulator-pm8350c-s2-level-ao {
			regulator-name = "pm8350c_s2_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};

		VDD_MXC_MMCX_VOTER_LEVEL: VDD_MXC_MM_VOTER_LEVEL:
		VDD_MM_MXC_VOTER_LEVEL:
		regulator-pm8350c-s2-mmcx-voter-level {
			regulator-name = "pm8350c_s2_mmcx_voter_level";
			vin-supply = <&VDD_MMCX_LEVEL>;
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
		};

		VDD_MXC_GFX_VOTER_LEVEL: VDD_GFX_MXC_VOTER_LEVEL:
		regulator-pm8350c-s2-gfx-voter-level {
			regulator-name = "pm8350c_s2_gfx_voter_level";
			pm8350c_s2_gfx_voter_level-parent-supply =
				<&VDD_GFX_LEVEL>;
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
		};
	};

	rpmh-regulator-mxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mx.lvl";
		proxy-supply = <&VDD_MXA_LEVEL>;

		VDD_MXA_LEVEL: S6H_LEVEL:
		pm8450_s6_level: regulator-pm8450-s6-level {
			regulator-name = "pm8450_s6_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MXA_LEVEL_AO: S6H_LEVEL_AO:
		pm8450_s6_level_ao: regulator-pm8450-s6-level-ao {
			regulator-name = "pm8450_s6_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-lmxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "lmx.lvl";
		VDD_LPI_MX_LEVEL: L1H_LEVEL:
		pm8450_l1_level: regulator-pm8450-l1-level {
			regulator-name = "pm8450_l1_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-smpb10 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb10";
		S10B: pm8350_s10: regulator-pm8350-s10 {
			regulator-name = "pm8350_s10";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
		};
	};

	rpmh-regulator-smpb11 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb11";
		S11B: pm8350_s11: regulator-pm8350-s11 {
			regulator-name = "pm8350_s11";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <848000>;
			regulator-max-microvolt = <1104000>;
			qcom,init-voltage = <952000>;
		};
	};

	rpmh-regulator-smpb12 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb12";
		S12B: pm8350_s12: regulator-pm8350-s12 {
			regulator-name = "pm8350_s12";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1224000>;
			regulator-max-microvolt = <1400000>;
			qcom,init-voltage = <1256000>;
		};
	};

	rpmh-regulator-ldob1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L1B: pm8350_l1: regulator-pm8350-l1 {
			regulator-name = "pm8350_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <912000>;
			regulator-max-microvolt = <920000>;
			qcom,init-voltage = <912000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L2B: pm8350_l2: regulator-pm8350-l2 {
			regulator-name = "pm8350_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3072000>;
			regulator-max-microvolt = <3072000>;
			qcom,init-voltage = <3072000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L3B: pm8350_l3: regulator-pm8350-l3 {
			regulator-name = "pm8350_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <904000>;
			regulator-max-microvolt = <904000>;
			qcom,init-voltage = <904000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L5B: pm8350_l5: regulator-pm8350-l5 {
			regulator-name = "pm8350_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <912000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};

		L5B_AO: pm8350_l5_ao: regulator-pm8350-l5-ao {
			regulator-name = "pm8350_l5_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <880000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_LPM>;
		};

		regulator-pm8350-l5-so {
			regulator-name = "pm8350_l5_so";
			qcom,set = <RPMH_REGULATOR_SET_SLEEP>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <880000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_LPM>;
			qcom,init-enable = <0>;
		};
	};

	rpmh-regulator-ldob6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L6B: pm8350_l6: regulator-pm8350-l6 {
			regulator-name = "pm8350_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};

		L6B_AO: pm8350_l6_ao: regulator-pm8350-l6-ao {
			regulator-name = "pm8350_l6_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_LPM>;
		};

		regulator-pm8350-l6-so {
			regulator-name = "pm8350_l6_so";
			qcom,set = <RPMH_REGULATOR_SET_SLEEP>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_LPM>;
			qcom,init-enable = <0>;
		};
	};

	rpmh-regulator-ldob7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L7B: pm8350_l7: regulator-pm8350-l7 {
			regulator-name = "pm8350_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2504000>;
			regulator-max-microvolt = <2504000>;
			qcom,init-voltage = <2504000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob9";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L9B: pm8350_l9: regulator-pm8350-l9 {
			regulator-name = "pm8350_l9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-smpc1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpc1";
		S1C: pm8350c_s1: regulator-pm8350c-s1 {
			regulator-name = "pm8350c_s1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <2024000>;
			qcom,init-voltage = <1856000>;
		};
	};

	rpmh-regulator-smpc10 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpc10";
		S10C: pm8350c_s10: regulator-pm8350c-s10 {
			regulator-name = "pm8350c_s10";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1000000>;
			regulator-max-microvolt = <1100000>;
			qcom,init-voltage = <1052000>;
		};
	};

	rpmh-regulator-ldoc1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L1C: pm8350c_l1: regulator-pm8350c-l1 {
			regulator-name = "pm8350c_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L2C: pm8350c_l2: regulator-pm8350c-l2 {
			regulator-name = "pm8350c_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L3C: pm8350c_l3: regulator-pm8350c-l3 {
			regulator-name = "pm8350c_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3296000>;
			regulator-max-microvolt = <3304000>;
			qcom,init-voltage = <3296000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L4C: pm8350c_l4: regulator-pm8350c-l4 {
			regulator-name = "pm8350c_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1704000>;
			regulator-max-microvolt = <3000000>;
			qcom,init-voltage = <1808000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L5C: pm8350c_l5: regulator-pm8350c-l5 {
			regulator-name = "pm8350c_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1704000>;
			regulator-max-microvolt = <3000000>;
			qcom,init-voltage = <1808000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L6C: pm8350c_l6: regulator-pm8350c-l6 {
			regulator-name = "pm8350c_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <3008000>;
			qcom,init-voltage = <2960000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L7C: pm8350c_l7: regulator-pm8350c-l7 {
			regulator-name = "pm8350c_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3008000>;
			regulator-max-microvolt = <3008000>;
			qcom,init-voltage = <3008000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc8";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L8C: pm8350c_l8: regulator-pm8350c-l8 {
			regulator-name = "pm8350c_l8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc9";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L9C: pm8350c_l9: regulator-pm8350c-l9 {
			regulator-name = "pm8350c_l9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2960000>;
			regulator-max-microvolt = <3008000>;
			qcom,init-voltage = <2960000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc10 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc10";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L10C: pm8350c_l10: regulator-pm8350c-l10 {
			regulator-name = "pm8350c_l10";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc12 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc12";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L12C: pm8350c_l12: regulator-pm8350c-l12 {
			regulator-name = "pm8350c_l12";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1968000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc13 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc13";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L13C: pm8350c_l13: regulator-pm8350c-l13 {
			regulator-name = "pm8350c_l13";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3000000>;
			regulator-max-microvolt = <3000000>;
			qcom,init-voltage = <3000000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-bobc1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "bobc1";
		qcom,regulator-type = "pmic5-bob";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_PASS
			 RPMH_REGULATOR_MODE_AUTO>;
		qcom,mode-threshold-currents = <0 1000000>;
		qcom,send-defaults;

		BOB: pm8350c_bob: regulator-pm8350c-bob {
			regulator-name = "pm8350c_bob";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3008000>;
			regulator-max-microvolt = <3960000>;
			qcom,init-voltage = <3296000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_PASS>;
		};

		BOB_AO: pm8350c_bob_ao: regulator-pm8350c-bob-ao {
			regulator-name = "pm8350c_bob_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt = <3008000>;
			regulator-max-microvolt = <3960000>;
			qcom,init-voltage = <3008000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_AUTO>;
		};
	};

	rpmh-regulator-ldod1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldod1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L1D: pm8350b_l1: regulator-pm8350b-l1 {
			regulator-name = "pm8350b_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1296000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-smpe1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe1";
		S1E: pmr735a_s1: regulator-pmr735a-s1 {
			regulator-name = "pmr735a_s1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1296000>;
			qcom,init-voltage = <1256000>;
		};
	};

	rpmh-regulator-smpe2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe2";
		S2E: pmr735a_s2: regulator-pmr735a-s2 {
			regulator-name = "pmr735a_s2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <500000>;
			regulator-max-microvolt = <1040000>;
			qcom,init-voltage = <852000>;
		};
	};

	rpmh-regulator-smpe3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe3";
		S3E: pmr735a_s3: regulator-pmr735a-s3 {
			regulator-name = "pmr735a_s3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2200000>;
			regulator-max-microvolt = <2352000>;
			qcom,init-voltage = <2200000>;
		};
	};

	rpmh-regulator-ldoe1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L1E: pmr735a_l1: regulator-pmr735a-l1 {
			regulator-name = "pmr735a_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <800000>;
			regulator-max-microvolt = <800000>;
			qcom,init-voltage = <800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L2E: pmr735a_l2: regulator-pmr735a-l2 {
			regulator-name = "pmr735a_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <480000>;
			regulator-max-microvolt = <912000>;
			qcom,init-voltage = <800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L3E: pmr735a_l3: regulator-pmr735a-l3 {
			regulator-name = "pmr735a_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L4E: pmr735a_l4: regulator-pmr735a-l4 {
			regulator-name = "pmr735a_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1776000>;
			regulator-max-microvolt = <1776000>;
			qcom,init-voltage = <1776000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L5E: pmr735a_l5: regulator-pmr735a-l5 {
			regulator-name = "pmr735a_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <880000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L6E: pmr735a_l6: regulator-pmr735a-l6 {
			regulator-name = "pmr735a_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L7E: pmr735a_l7: regulator-pmr735a-l7 {
			regulator-name = "pmr735a_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2800000>;
			regulator-max-microvolt = <2800000>;
			qcom,init-voltage = <2800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldof1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldof1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L1F: pmr735b_l1: regulator-pmr735b-l1 {
			regulator-name = "pmr735b_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <912000>;
			regulator-max-microvolt = <912000>;
			qcom,init-voltage = <912000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldof2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldof2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L2F: pmr735b_l2: regulator-pmr735b-l2 {
			regulator-name = "pmr735b_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldof4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldof4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L4F: pmr735b_l4: regulator-pmr735b-l4 {
			regulator-name = "pmr735b_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldof5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldof5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L5F: pmr735b_l5: regulator-pmr735b-l5 {
			regulator-name = "pmr735b_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <800000>;
			regulator-max-microvolt = <800000>;
			qcom,init-voltage = <800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldof6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldof6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L6F: pmr735b_l6: regulator-pmr735b-l6 {
			regulator-name = "pmr735b_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <480000>;
			regulator-max-microvolt = <904000>;
			qcom,init-voltage = <768000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-smph3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smph3";
		S3H: pm8450_s3: regulator-pm8450-s3 {
			regulator-name = "pm8450_s3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <500000>;
			regulator-max-microvolt = <600000>;
			qcom,init-voltage = <504000>;
		};
	};

	rpmh-regulator-ldoh2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoh2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L2H: pm8450_l2: regulator-pm8450-l2 {
			regulator-name = "pm8450_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <912000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoh3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoh3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L3H: pm8450_l3: regulator-pm8450-l3 {
			regulator-name = "pm8450_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <912000>;
			regulator-max-microvolt = <912000>;
			qcom,init-voltage = <912000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};
};
