MSM HDCP driver

Standalone driver managing HDCP related communications
between TZ and HLOS for MSM chipset.

Required properties:

compatible = "qcom,msm-hdcp";

Example:

qcom_msmhdcp: qcom,msm_hdcp {
       compatible = "qcom,msm-hdcp";
};
