&cam_cci0 {
/delete-node/ qcom,cam-sensor0;
/delete-node/ qcom,cam-sensor1;

	qcom,cam-sensor0 {
		cell-index = <5>;
		compatible = "qcom,cam-sensor";
		csiphy-sd-index = <0>;
		sensor-position-roll = <0>;
		sensor-position-pitch = <0>;
		sensor-position-yaw = <180>;
		eeprom-src = <&eeprom_triple_tele>;
		actuator-src = <&actuator_triple_tele>;
		led-flash-src = <&led_flash_triple_rear_aux>;
		cam_vio-supply = <&pm8008j_l3>;
		cam_vana-supply = <&pm8008i_l4>;
		cam_vdig-supply = <&pm8008i_l2>;
		cam_clk-supply = <&cam_cc_titan_top_gdsc>;
		cam_bob-supply = <&pm8350c_bob>;
		regulator-names = "cam_vio", "cam_vana", "cam_vdig",
			"cam_clk", "cam_bob";
		rgltr-cntrl-support;
		rgltr-min-voltage = <1800000 2700000 1000000 0 3200000>;
		rgltr-max-voltage = <1800000 2900000 1150000 0 3960000>;
		rgltr-load-current = <10000 52000 140000 0 2000000>;
		gpio-no-mux = <0>;
		pinctrl-names = "cam_default", "cam_suspend";
		pinctrl-0 = <&cam_sensor_mclk0_active
				&cam_sensor_active_rst0>;
		pinctrl-1 = <&cam_sensor_mclk0_suspend
				&cam_sensor_suspend_rst0>;
		gpios = <&tlmm 100 0>,
			<&tlmm 17 0>;
		gpio-reset = <1>;
		gpio-req-tbl-num = <0 1>;
		gpio-req-tbl-flags = <1 0>;
		gpio-req-tbl-label = "CAMIF_MCLK0",
					"CAM_RESET0";
		cci-master = <0>;
		status = "ok";
		clocks = <&clock_camcc CAM_CC_MCLK0_CLK>;
		clock-names = "cam_clk";
		clock-cntl-level = "nominal";
		clock-rates = <24000000>;
	};

	qcom,cam-sensor1 {
		cell-index = <4>;
		compatible = "qcom,cam-sensor";
		csiphy-sd-index = <1>;
		sensor-position-roll = <0>;
		sensor-position-pitch = <0>;
		sensor-position-yaw = <180>;
		actuator-src = <&actuator_triple_wide>;
		eeprom-src = <&eeprom_triple_wide>;
		led-flash-src = <&led_flash_triple_rear>;
		cam_vio-supply = <&pm8008j_l3>;
		cam_vana-supply = <&pm8008i_l3>;
		cam_v_custom1-supply = <&pm8008i_l5>;
		cam_vdig-supply = <&pm8008i_l1>;
		cam_clk-supply = <&cam_cc_titan_top_gdsc>;
		cam_bob-supply = <&pm8350c_bob>;
		regulator-names = "cam_vio", "cam_vana", "cam_v_custom1",
			"cam_vdig","cam_clk", "cam_bob";
		rgltr-cntrl-support;
		rgltr-min-voltage = <1800000 2700000 1700000 1050000 0 3200000>;
		rgltr-max-voltage = <1800000 3000000 1900000 1200000 0 3960000>;
		rgltr-load-current = <5000 68000 74000 805000 0 2000000>;
		gpio-no-mux = <0>;
		pinctrl-names = "cam_default", "cam_suspend";
		pinctrl-0 = <&cam_sensor_mclk1_active
				&cam_sensor_active_rst1>;
		pinctrl-1 = <&cam_sensor_mclk1_suspend
				&cam_sensor_suspend_rst1>;
		gpios = <&tlmm 101 0>,
			<&tlmm 16 0>;
		gpio-reset = <1>;
		gpio-req-tbl-num = <0 1>;
		gpio-req-tbl-flags = <1 0>;
		gpio-req-tbl-label = "CAMIF_MCLK1",
					"CAM_RESET1";
		cci-master = <1>;
		status = "ok";
		clocks = <&clock_camcc CAM_CC_MCLK1_CLK>;
		clock-names = "cam_clk";
		clock-cntl-level = "nominal";
		clock-rates = <24000000>;
	};
};

&cam_cci1 {
/delete-node/ qcom,cam-sensor2;
/delete-node/ qcom,cam-sensor5;

	qcom,cam-sensor2 {
		cell-index = <6>;
		compatible = "qcom,cam-sensor";
		csiphy-sd-index = <2>;
		sensor-position-roll = <0>;
		sensor-position-pitch = <0>;
		sensor-position-yaw = <180>;
		eeprom-src = <&eeprom_triple_uw>;
		actuator-src = <&actuator_triple_uw>;
		led-flash-src = <&led_flash_triple_rear_aux2>;
		cam_vio-supply = <&pm8008j_l3>;
		cam_vana-supply = <&pm8008i_l6>;
		cam_vdig-supply = <&pm8008i_l2>;
		cam_clk-supply = <&cam_cc_titan_top_gdsc>;
		cam_bob-supply = <&pm8350c_bob>;
		regulator-names = "cam_vio", "cam_vana", "cam_vdig",
			"cam_clk", "cam_bob";
		rgltr-cntrl-support;
		rgltr-min-voltage = <1800000 2700000 1000000 0 3200000>;
		rgltr-max-voltage = <1800000 2900000 1150000 0 3960000>;
		rgltr-load-current = <3000 52000 257000 0 2000000>;
		gpio-no-mux = <0>;
		pinctrl-names = "cam_default", "cam_suspend";
		pinctrl-0 = <&cam_sensor_mclk2_active
				 &cam_sensor_active_rst2>;
		pinctrl-1 = <&cam_sensor_mclk2_suspend
				 &cam_sensor_suspend_rst2>;
		gpios = <&tlmm 102 0>,
			<&tlmm 106 0>;
		gpio-reset = <1>;
		gpio-req-tbl-num = <0 1>;
		gpio-req-tbl-flags = <1 0>;
		gpio-req-tbl-label = "CAMIF_MCLK2",
					"CAM_RESET2";
		cci-master = <0>;
		status = "ok";
		clocks = <&clock_camcc CAM_CC_MCLK2_CLK>;
		clock-names = "cam_clk";
		clock-cntl-level = "nominal";
		clock-rates = <24000000>;
	};

	qcom,cam-sensor5 {
		cell-index = <2>;
		compatible = "qcom,cam-sensor";
		csiphy-sd-index = <5>;
		sensor-position-roll = <0>;
		sensor-position-pitch = <0>;
		sensor-position-yaw = <0>;
		eeprom-src = <&eeprom_front>;
		cam_vio-supply = <&pm8008j_l3>;
		cam_vana-supply = <&pm8008j_l5>;
		cam_vdig-supply = <&pm8008j_l1>;
		cam_clk-supply = <&cam_cc_titan_top_gdsc>;
		cam_bob-supply = <&pm8350c_bob>;
		regulator-names = "cam_vio", "cam_vana", "cam_vdig",
			"cam_clk", "cam_bob";
		rgltr-cntrl-support;
		rgltr-min-voltage = <1800000 2700000 1000000 0 3200000>;
		rgltr-max-voltage = <1800000 2900000 1150000 0 3960000>;
		rgltr-load-current = <5000 35000 301000 0 2000000>;
		gpio-no-mux = <0>;
		pinctrl-names = "cam_default", "cam_suspend";
		pinctrl-0 = <&cam_sensor_mclk5_active
				 &cam_sensor_active_rst5>;
		pinctrl-1 = <&cam_sensor_mclk5_suspend
				 &cam_sensor_suspend_rst5>;
		gpios = <&tlmm 105 0>,
			<&tlmm 115 0>;
		gpio-reset = <1>;
		gpio-req-tbl-num = <0 1>;
		gpio-req-tbl-flags = <1 0>;
		gpio-req-tbl-label = "CAMIF_MCLK5",
					"CAM_RESET5";
		cci-master = <1>;
		status = "ok";
		clocks = <&clock_camcc CAM_CC_MCLK5_CLK>;
		clock-names = "cam_clk";
		clock-cntl-level = "nominal";
		clock-rates = <24000000>;
	};
};
