&soc {
	tlmm: pinctrl@f000000 {
		compatible = "qcom,kona-pinctrl";
		reg = <0x0F000000 0x1000000>;
		interrupts = <GIC_SPI 208 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
		wakeup-parent = <&pdc>;
		qcom,gpios-reserved = <28 29 30 31 40 41 42 43>;

		trigout_a: trigout_a {
			mux {
				pins = "gpio2";
				function = "qdss_cti";
			};

			config {
				pins = "gpio2";
				drive-strength = <2>;
				bias-disable;
			};
		};

		qupv3_se2_2uart_pins: qupv3_se2_2uart_pins {
			qupv3_se2_2uart_active: qupv3_se2_2uart_active {
				mux {
					pins = "gpio117", "gpio118";
					function = "qup2";
				};

				config {
					pins = "gpio117", "gpio118";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se2_2uart_sleep: qupv3_se2_2uart_sleep {
				mux {
					pins = "gpio117", "gpio118";
					function = "gpio";
				};

				config {
					pins = "gpio117", "gpio118";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		qupv3_se6_4uart_pins: qupv3_se6_4uart_pins {
			qupv3_se6_default_cts:
				qupv3_se6_default_cts {
				mux {
					pins = "gpio16";
					function = "gpio";
				};

				config {
					pins = "gpio16";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se6_default_rtsrx:
				qupv3_se6_default_rtsrx {
				mux {
					pins = "gpio17", "gpio19";
					function = "gpio";
				};

				config {
					pins = "gpio17", "gpio19";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			qupv3_se6_default_tx:
				qupv3_se6_default_tx {
				mux {
					pins = "gpio18";
					function = "gpio";
				};

				config {
					pins = "gpio18";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			qupv3_se6_ctsrx: qupv3_se6_ctsrx {
				mux {
					pins = "gpio16", "gpio19";
					function = "qup6";
				};

				config {
					pins = "gpio16", "gpio19";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se6_rts: qupv3_se6_rts {
				mux {
					pins = "gpio17";
					function = "qup6";
				};

				config {
					pins = "gpio17";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			qupv3_se6_tx: qupv3_se6_tx {
				mux {
					pins = "gpio18";
					function = "qup6";
				};

				config {
					pins = "gpio18";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se12_2uart_pins: qupv3_se12_2uart_pins {
			qupv3_se12_2uart_active: qupv3_se12_2uart_active {
				mux {
					pins = "gpio34", "gpio35";
					function = "qup12";
				};

				config {
					pins = "gpio34", "gpio35";
					drive-strength = <2>;
				};
			};

			qupv3_se12_2uart_sleep: qupv3_se12_2uart_sleep {
				mux {
					pins = "gpio34", "gpio35";
					drive-strength = <2>;
					bias-pull-down;
				};

				config {
					pins = "gpio34", "gpio35";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		qupv3_se17_4uart_pins: qupv3_se17_4uart_pins {
			qupv3_se17_ctsrx: qupv3_se17_ctsrx {
				mux {
					pins = "gpio52", "gpio55";
					function = "qup17";
				};

				config {
					pins = "gpio52", "gpio55";
					drive-strength = <2>;
					bias-no-pull;
				};
			};

			qupv3_se17_rts: qupv3_se17_rts {
				mux {
					pins = "gpio53";
					function = "qup17";
				};

				config {
					pins = "gpio53";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			qupv3_se17_tx: qupv3_se17_tx {
				mux {
					pins = "gpio54";
					function = "qup17";
				};

				config {
					pins = "gpio54";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se18_2uart_pins: qupv3_se18_2uart_pins {
			qupv3_se18_rx: qupv3_se18_rx {
				mux {
					pins = "gpio59";
					function = "qup18";
				};

				config {
					pins = "gpio59";
					drive-strength = <2>;
					bias-no-pull;
				};
			};

			qupv3_se18_tx: qupv3_se18_tx {
				mux {
					pins = "gpio58";
					function = "qup18";
				};

				config {
					pins = "gpio58";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		pmx_ts_active {
			ts_active: ts_active {
					mux {
						pins = "gpio38", "gpio39";
						function = "gpio";
					};

					config {
						pins = "gpio38", "gpio39";
						drive-strength = <8>;
						bias-pull-up;
					};
			};
		};

		pmx_ts_int_suspend {
			ts_int_suspend: ts_int_suspend {
				mux {
					pins = "gpio39";
					function = "gpio";
				};

				config {
					pins = "gpio39";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		pmx_ts_reset_suspend {
			ts_reset_suspend: ts_reset_suspend {
				mux {
					pins = "gpio38";
					function = "gpio";
				};

				config {
					pins = "gpio38";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		pmx_ts_release {
			pmx_ts_release: pmx_ts_release {
				mux {
					pins = "gpio38", "gpio39";
					function = "gpio";
				};

				config {
					pins = "gpio38", "gpio39";
					drive-strength = <2>;
					bias-disable;
				};
			};
		};

		ufs_dev_reset_assert: ufs_dev_reset_assert {
			config {
				pins = "ufs_reset";
				bias-pull-down;		/* default: pull down */
				/*
				 * UFS_RESET driver strengths are having
				 * different values/steps compared to typical
				 * GPIO drive strengths.
				 *
				 * Following table clarifies:
				 *
				 * HDRV value | UFS_RESET | Typical GPIO
				 *   (dec)    |   (mA)    |    (mA)
				 *     0      |   0.8     |    2
				 *     1      |   1.55    |    4
				 *     2      |   2.35    |    6
				 *     3      |   3.1     |    8
				 *     4      |   3.9     |    10
				 *     5      |   4.65    |    12
				 *     6      |   5.4     |    14
				 *     7      |   6.15    |    16
				 *
				 * POR value for UFS_RESET HDRV is 3 which means
				 * 3.1mA and we want to use that. Hence just
				 * specify 8mA to "drive-strength" binding and
				 * that should result into writing 3 to HDRV
				 * field.
				 */
				drive-strength = <8>;	/* default: 3.1 mA */
				output-low; /* active low reset */
			};
		};

		ufs_dev_reset_deassert: ufs_dev_reset_deassert {
			config {
				pins = "ufs_reset";
				bias-pull-down;		/* default: pull down */
				/*
				 * default: 3.1 mA
				 * check comments under ufs_dev_reset_assert
				 */
				drive-strength = <8>;
				output-high; /* active low reset */
			};
		};

		sdc2_on: sdc2_on {
			clk {
				pins = "sdc2_clk";
				bias-disable;		/* NO pull */
				drive-strength = <16>;	/* 16 MA */
			};

			cmd {
				pins = "sdc2_cmd";
				bias-pull-up;		/* pull up */
				drive-strength = <16>;	/* 16 MA */
			};

			data {
				pins = "sdc2_data";
				bias-pull-up;		/* pull up */
				drive-strength = <16>;	/* 16 MA */
			};

			sd-cd {
				pins = "gpio77";
				drive-strength = <2>;
				bias-pull-up;
			};
		};

		sdc2_off: sdc2_off {
			clk {
				pins = "sdc2_clk";
				bias-disable;		/* NO pull */
				drive-strength = <2>;	/* 2 MA */
			};

			cmd {
				pins = "sdc2_cmd";
				bias-pull-up;		/* pull up */
				drive-strength = <2>;	/* 2 MA */
			};

			data {
				pins = "sdc2_data";
				bias-pull-up;		/* pull up */
				drive-strength = <2>;	/* 2 MA */
			};

			sd_cd {
				pins = "gpio77";
				drive-strength = <2>;
				bias-disable;
			};
		};

		/* add pins for DisplayPort */
		sde_dp_usbplug_cc_active: sde_dp_usbplug_cc_active {
			mux {
				pins = "gpio65";
				function = "gpio";
			};

			config {
				pins = "gpio65";
				bias-disable;
				drive-strength = <16>;
			};
		};

		sde_dp_usbplug_cc_suspend: sde_dp_usbplug_cc_suspend {
			mux {
				pins = "gpio65";
				function = "gpio";
			};

			config {
				pins = "gpio65";
				bias-pull-down;
				drive-strength = <2>;
			};
		};

		ap2mdm {
			ap2mdm_active: ap2mdm_active {
				mux {
					/* ap2mdm-status
					 * ap2mdm-errfatal
					 * ap2mdm-vddmin
					 */
					pins = "gpio56", "gpio57";
					function = "gpio";
				};

				config {
					pins = "gpio56", "gpio57";
					drive-strength = <16>;
					bias-disable;
				};
			};

			ap2mdm_sleep: ap2mdm_sleep {
				mux {
					/* ap2mdm-status
					 * ap2mdm-errfatal
					 * ap2mdm-vddmin
					 */
					pins = "gpio56", "gpio57";
					function = "gpio";
				};

				config {
					pins = "gpio56", "gpio57";
					drive-strength = <8>;
					bias-disable;
				};

			};
		};

		mdm2ap {
			mdm2ap_active: mdm2ap_active {
				mux {
					/* mdm2ap-status
					 * mdm2ap-errfatal
					 * mdm2ap-vddmin
					 */
					pins = "gpio1", "gpio3";
					function = "gpio";
				};

				config {
					pins = "gpio1", "gpio3";
					drive-strength = <8>;
					bias-disable;
				};
			};

			mdm2ap_sleep: mdm2ap_sleep {
				mux {
					/* mdm2ap-status
					 * mdm2ap-errfatal
					 * mdm2ap-vddmin
					 */
					pins = "gpio1", "gpio3";
					function = "gpio";
				};

				config {
					pins = "gpio1", "gpio3";
					drive-strength = <8>;
					bias-disable;
				};
			};
		};

		pcie0 {
			pcie0_perst_default: pcie0_perst_default {
				mux {
					pins = "gpio79";
					function = "gpio";
				};

				config {
					pins = "gpio79";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			pcie0_clkreq_default: pcie0_clkreq_default {
				mux {
					pins = "gpio80";
					function = "pci_e0";
				};

				config {
					pins = "gpio80";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			pcie0_wake_default: pcie0_wake_default {
				mux {
					pins = "gpio81";
					function = "gpio";
				};

				config {
					pins = "gpio81";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			pcie0_clkreq_sleep: pcie0_clkreq_sleep {
				mux {
					pins = "gpio80";
					function = "gpio";
				};

				config {
					pins = "gpio80";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		pcie1 {
			pcie1_perst_default: pcie1_perst_default {
				mux {
					pins = "gpio82";
					function = "gpio";
				};

				config {
					pins = "gpio82";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			pcie1_clkreq_default: pcie1_clkreq_default {
				mux {
					pins = "gpio83";
					function = "pci_e1";
				};

				config {
					pins = "gpio83";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			pcie1_wake_default: pcie1_wake_default {
				mux {
					pins = "gpio84";
					function = "gpio";
				};

				config {
					pins = "gpio84";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		pcie2 {
			pcie2_perst_default: pcie2_perst_default {
				mux {
					pins = "gpio85";
					function = "gpio";
				};

				config {
					pins = "gpio85";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			pcie2_clkreq_default: pcie2_clkreq_default {
				mux {
					pins = "gpio86";
					function = "pci_e2";
				};

				config {
					pins = "gpio86";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			pcie2_wake_default: pcie2_wake_default {
				mux {
					pins = "gpio87";
					function = "gpio";
				};

				config {
					pins = "gpio87";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		cnss_pins {
			cnss_wlan_en_active: cnss_wlan_en_active {
				mux {
					pins = "gpio20";
					function = "gpio";
				};

				config {
					pins = "gpio20";
					drive-strength = <16>;
					output-high;
					bias-pull-up;
				};
			};

			cnss_wlan_en_sleep: cnss_wlan_en_sleep {
				mux {
					pins = "gpio20";
					function = "gpio";
				};

				config {
					pins = "gpio20";
					drive-strength = <2>;
					output-low;
					bias-pull-down;
				};
			};
		};

		pmx_sde: pmx_sde {
			sde_dsi_active: sde_dsi_active {
				mux {
					pins = "gpio75", "gpio60";
					function = "gpio";
				};

				config {
					pins = "gpio75", "gpio60";
					drive-strength = <8>;   /* 8 mA */
					bias-disable = <0>;   /* no pull */
				};
			};

			sde_dsi_suspend: sde_dsi_suspend {
				mux {
					pins = "gpio75", "gpio60";
					function = "gpio";
				};

				config {
					pins = "gpio75", "gpio60";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_dsi1_active: sde_dsi1_active {
				mux {
					pins = "gpio128";
					function = "gpio";
				};

				config {
					pins = "gpio128";
					drive-strength = <8>;   /* 8 mA */
					bias-disable = <0>;   /* no pull */
				};
			};

			sde_dsi1_suspend: sde_dsi1_suspend {
				mux {
					pins = "gpio128";
					function = "gpio";
				};

				config {
					pins = "gpio128";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};
		};

		pmx_sde_te {
			sde_te_active: sde_te_active {
				mux {
					pins = "gpio66";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio66";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_te_suspend: sde_te_suspend {
				mux {
					pins = "gpio66";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio66";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_te1_active: sde_te1_active {
				mux {
					pins = "gpio67";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio67";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_te1_suspend: sde_te1_suspend {
				mux {
					pins = "gpio67";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio67";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};
		};

		pri_aux_pcm_clk {
			pri_aux_pcm_clk_sleep: pri_aux_pcm_clk_sleep {
				mux {
					pins = "gpio138";
					function = "gpio";
				};

				config {
					pins = "gpio138";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_aux_pcm_clk_active: pri_aux_pcm_clk_active {
				mux {
					pins = "gpio138";
					function = "mi2s0_sck";
				};

				config {
					pins = "gpio138";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_aux_pcm_sync {
			pri_aux_pcm_sync_sleep: pri_aux_pcm_sync_sleep {
				mux {
					pins = "gpio141";
					function = "gpio";
				};

				config {
					pins = "gpio141";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_aux_pcm_sync_active: pri_aux_pcm_sync_active {
				mux {
					pins = "gpio141";
					function = "mi2s0_ws";
				};

				config {
					pins = "gpio141";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_aux_pcm_din {
			pri_aux_pcm_din_sleep: pri_aux_pcm_din_sleep {
				mux {
					pins = "gpio139";
					function = "gpio";
				};

				config {
					pins = "gpio139";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_aux_pcm_din_active: pri_aux_pcm_din_active {
				mux {
					pins = "gpio139";
					function = "mi2s0_data0";
				};

				config {
					pins = "gpio139";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_aux_pcm_dout {
			pri_aux_pcm_dout_sleep: pri_aux_pcm_dout_sleep {
				mux {
					pins = "gpio140";
					function = "gpio";
				};

				config {
					pins = "gpio140";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_aux_pcm_dout_active: pri_aux_pcm_dout_active {
				mux {
					pins = "gpio140";
					function = "mi2s0_data1";
				};

				config {
					pins = "gpio140";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_aux_pcm {
			sec_aux_pcm_clk_sleep: sec_aux_pcm_clk_sleep {
				mux {
					pins = "gpio142";
					function = "gpio";
				};

				config {
					pins = "gpio142";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_aux_pcm_clk_active: sec_aux_pcm_clk_active {
				mux {
					pins = "gpio142";
					function = "mi2s1_sck";
				};

				config {
					pins = "gpio142";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};

			sec_aux_pcm_ws_sleep: sec_aux_pcm_ws_sleep {
				mux {
					pins = "gpio145";
					function = "gpio";
				};

				config {
					pins = "gpio145";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_aux_pcm_ws_active: sec_aux_pcm_ws_active {
				mux {
					pins = "gpio145";
					function = "mi2s1_ws";
				};

				config {
					pins = "gpio145";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_aux_pcm_din {
			sec_aux_pcm_din_sleep: sec_aux_pcm_din_sleep {
				mux {
					pins = "gpio143";
					function = "gpio";
				};

				config {
					pins = "gpio143";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_aux_pcm_din_active: sec_aux_pcm_din_active {
				mux {
					pins = "gpio143";
					function = "mi2s1_data0";
				};

				config {
					pins = "gpio143";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_aux_pcm_dout {
			sec_aux_pcm_dout_sleep: sec_aux_pcm_dout_sleep {
				mux {
					pins = "gpio144";
					function = "gpio";
				};

				config {
					pins = "gpio144";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_aux_pcm_dout_active: sec_aux_pcm_dout_active {
				mux {
					pins = "gpio144";
					function = "mi2s1_data1";
				};

				config {
					pins = "gpio144";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_aux_pcm {
			tert_aux_pcm_clk_sleep: tert_aux_pcm_clk_sleep {
				mux {
					pins = "gpio133";
					function = "gpio";
				};

				config {
					pins = "gpio133";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_aux_pcm_clk_active: tert_aux_pcm_clk_active {
				mux {
					pins = "gpio133";
					function = "mi2s2_sck";
				};

				config {
					pins = "gpio133";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};

			tert_aux_pcm_ws_sleep: tert_aux_pcm_ws_sleep {
				mux {
					pins = "gpio135";
					function = "gpio";
				};

				config {
					pins = "gpio135";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_aux_pcm_ws_active: tert_aux_pcm_ws_active {
				mux {
					pins = "gpio135";
					function = "mi2s2_ws";
				};

				config {
					pins = "gpio135";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		tert_aux_pcm_din {
			tert_aux_pcm_din_sleep: tert_aux_pcm_din_sleep {
				mux {
					pins = "gpio134";
					function = "gpio";
				};

				config {
					pins = "gpio134";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_aux_pcm_din_active: tert_aux_pcm_din_active {
				mux {
					pins = "gpio134";
					function = "mi2s2_data0";
				};

				config {
					pins = "gpio134";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_aux_pcm_dout {
			tert_aux_pcm_dout_sleep: tert_aux_pcm_dout_sleep {
				mux {
					pins = "gpio137";
					function = "gpio";
				};

				config {
					pins = "gpio137";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_aux_pcm_dout_active: tert_aux_pcm_dout_active {
				mux {
					pins = "gpio137";
					function = "mi2s2_data1";
				};

				config {
					pins = "gpio137";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_tdm_clk {
			pri_tdm_clk_sleep: pri_tdm_clk_sleep {
				mux {
					pins = "gpio138";
					function = "gpio";
				};

				config {
					pins = "gpio138";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_tdm_clk_active: pri_tdm_clk_active {
				mux {
					pins = "gpio138";
					function = "mi2s0_sck";
				};

				config {
					pins = "gpio138";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_tdm_sync {
			pri_tdm_sync_sleep: pri_tdm_sync_sleep {
				mux {
					pins = "gpio141";
					function = "gpio";
				};

				config {
					pins = "gpio141";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_tdm_sync_active: pri_tdm_sync_active {
				mux {
					pins = "gpio141";
					function = "mi2s0_ws";
				};

				config {
					pins = "gpio141";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_tdm_din {
			pri_tdm_din_sleep: pri_tdm_din_sleep {
				mux {
					pins = "gpio139";
					function = "gpio";
				};

				config {
					pins = "gpio139";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_tdm_din_active: pri_tdm_din_active {
				mux {
					pins = "gpio139";
					function = "mi2s0_data0";
				};

				config {
					pins = "gpio139";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_tdm_dout {
			pri_tdm_dout_sleep: pri_tdm_dout_sleep {
				mux {
					pins = "gpio140";
					function = "gpio";
				};

				config {
					pins = "gpio140";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_tdm_dout_active: pri_tdm_dout_active {
				mux {
					pins = "gpio140";
					function = "mi2s0_data1";
				};

				config {
					pins = "gpio140";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_tdm {
			sec_tdm_sck_sleep: sec_tdm_sck_sleep {
				mux {
					pins = "gpio142";
					function = "gpio";
				};

				config {
					pins = "gpio142";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_tdm_sck_active: sec_tdm_sck_active {
				mux {
					pins = "gpio142";
					function = "mi2s1_sck";
				};

				config {
					pins = "gpio142";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};

			sec_tdm_ws_sleep: sec_tdm_ws_sleep {
				mux {
					pins = "gpio145";
					function = "gpio";
				};

				config {
					pins = "gpio145";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_tdm_ws_active: sec_tdm_ws_active {
				mux {
					pins = "gpio145";
					function = "mi2s1_ws";
				};

				config {
					pins = "gpio145";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_tdm_din {
			sec_tdm_din_sleep: sec_tdm_din_sleep {
				mux {
					pins = "gpio143";
					function = "gpio";
				};

				config {
					pins = "gpio143";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_tdm_din_active: sec_tdm_din_active {
				mux {
					pins = "gpio143";
					function = "mi2s1_data0";
				};

				config {
					pins = "gpio143";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_tdm_dout {
			sec_tdm_dout_sleep: sec_tdm_dout_sleep {
				mux {
					pins = "gpio144";
					function = "gpio";
				};

				config {
					pins = "gpio144";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_tdm_dout_active: sec_tdm_dout_active {
				mux {
					pins = "gpio144";
					function = "mi2s1_data1";
				};

				config {
					pins = "gpio144";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_tdm {
			tert_tdm_clk_sleep: tert_tdm_clk_sleep {
				mux {
					pins = "gpio133";
					function = "gpio";
				};

				config {
					pins = "gpio133";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_tdm_clk_active: tert_tdm_clk_active {
				mux {
					pins = "gpio133";
					function = "mi2s2_sck";
				};

				config {
					pins = "gpio133";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};

			tert_tdm_ws_sleep: tert_tdm_ws_sleep {
				mux {
					pins = "gpio135";
					function = "gpio";
				};

				config {
					pins = "gpio135";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_tdm_ws_active: tert_tdm_ws_active {
				mux {
					pins = "gpio135";
					function = "mi2s2_ws";
				};

				config {
					pins = "gpio135";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		tert_tdm_din {
			tert_tdm_din_sleep: tert_tdm_din_sleep {
				mux {
					pins = "gpio134";
					function = "gpio";
				};

				config {
					pins = "gpio134";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_tdm_din_active: tert_tdm_din_active {
				mux {
					pins = "gpio134";
					function = "mi2s2_data0";
				};

				config {
					pins = "gpio134";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_tdm_dout {
			tert_tdm_dout_sleep: tert_tdm_dout_sleep {
				mux {
					pins = "gpio137";
					function = "gpio";
				};

				config {
					pins = "gpio137";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_tdm_dout_active: tert_tdm_dout_active {
				mux {
					pins = "gpio137";
					function = "mi2s2_data1";
				};

				config {
					pins = "gpio137";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		pri_mi2s_mclk {
			pri_mi2s_mclk_sleep: pri_mi2s_mclk_sleep {
				mux {
					pins = "gpio136";
					function = "gpio";
				};

				config {
					pins = "gpio136";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_mclk_active: pri_mi2s_mclk_active {
				mux {
					pins = "gpio136";
					function = "pri_mi2s";
				};

				config {
					pins = "gpio136";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_mi2s_sck {
			pri_mi2s_sck_sleep: pri_mi2s_sck_sleep {
				mux {
					pins = "gpio138";
					function = "gpio";
				};

				config {
					pins = "gpio138";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_sck_active: pri_mi2s_sck_active {
				mux {
					pins = "gpio138";
					function = "mi2s0_sck";
				};

				config {
					pins = "gpio138";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_mi2s_ws {
			pri_mi2s_ws_sleep: pri_mi2s_ws_sleep {
				mux {
					pins = "gpio141";
					function = "gpio";
				};

				config {
					pins = "gpio141";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_ws_active: pri_mi2s_ws_active {
				mux {
					pins = "gpio141";
					function = "mi2s0_ws";
				};

				config {
					pins = "gpio141";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_mi2s_sd0 {
			pri_mi2s_sd0_sleep: pri_mi2s_sd0_sleep {
				mux {
					pins = "gpio139";
					function = "gpio";
				};

				config {
					pins = "gpio139";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_sd0_active: pri_mi2s_sd0_active {
				mux {
					pins = "gpio139";
					function = "mi2s0_data0";
				};

				config {
					pins = "gpio139";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		pri_mi2s_sd1 {
			pri_mi2s_sd1_sleep: pri_mi2s_sd1_sleep {
				mux {
					pins = "gpio140";
					function = "gpio";
				};

				config {
					pins = "gpio140";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			pri_mi2s_sd1_active: pri_mi2s_sd1_active {
				mux {
					pins = "gpio140";
					function = "mi2s0_data1";
				};

				config {
					pins = "gpio140";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		sec_mi2s_mclk {
			sec_mi2s_mclk_sleep: sec_mi2s_mclk_sleep {
				mux {
					pins = "gpio137";
					function = "gpio";
				};

				config {
					pins = "gpio137";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_mi2s_mclk_active: sec_mi2s_mclk_active {
				mux {
					pins = "gpio137";
					function = "sec_mi2s";
				};

				config {
					pins = "gpio137";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
					output-high;
				};
			};
		};

		sec_mi2s_sck {
			sec_mi2s_sck_sleep: sec_mi2s_sck_sleep {
				mux {
					pins = "gpio142";
					function = "gpio";
				};

				config {
					pins = "gpio142";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_mi2s_sck_active: sec_mi2s_sck_active {
				mux {
					pins = "gpio142";
					function = "mi2s1_sck";
				};

				config {
					pins = "gpio142";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_mi2s_ws {
			sec_mi2s_ws_sleep: sec_mi2s_ws_sleep {
				mux {
					pins = "gpio145";
					function = "gpio";
				};

				config {
					pins = "gpio145";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_mi2s_ws_active: sec_mi2s_ws_active {
				mux {
					pins = "gpio145";
					function = "mi2s1_ws";
				};

				config {
					pins = "gpio145";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_mi2s_sd0 {
			sec_mi2s_sd0_sleep: sec_mi2s_sd0_sleep {
				mux {
					pins = "gpio143";
					function = "gpio";
				};

				config {
					pins = "gpio143";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_mi2s_sd0_active: sec_mi2s_sd0_active {
				mux {
					pins = "gpio143";
					function = "mi2s1_data0";
				};

				config {
					pins = "gpio143";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		sec_mi2s_sd1 {
			sec_mi2s_sd1_sleep: sec_mi2s_sd1_sleep {
				mux {
					pins = "gpio144";
					function = "gpio";
				};

				config {
					pins = "gpio144";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			sec_mi2s_sd1_active: sec_mi2s_sd1_active {
				mux {
					pins = "gpio144";
					function = "mi2s1_data1";
				};

				config {
					pins = "gpio144";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_mi2s_sck {
			tert_mi2s_sck_sleep: tert_mi2s_sck_sleep {
				mux {
					pins = "gpio133";
					function = "gpio";
				};

				config {
					pins = "gpio133";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_mi2s_sck_active: tert_mi2s_sck_active {
				mux {
					pins = "gpio133";
					function = "mi2s2_sck";
				};

				config {
					pins = "gpio133";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_mi2s_ws {
			tert_mi2s_ws_sleep: tert_mi2s_ws_sleep {
				mux {
					pins = "gpio135";
					function = "gpio";
				};

				config {
					pins = "gpio135";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_mi2s_ws_active: tert_mi2s_ws_active {
				mux {
					pins = "gpio135";
					function = "mi2s2_ws";
				};

				config {
					pins = "gpio135";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_mi2s_sd0 {
			tert_mi2s_sd0_sleep: tert_mi2s_sd0_sleep {
				mux {
					pins = "gpio134";
					function = "gpio";
				};

				config {
					pins = "gpio134";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_mi2s_sd0_active: tert_mi2s_sd0_active {
				mux {
					pins = "gpio134";
					function = "mi2s2_data0";
				};

				config {
					pins = "gpio134";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		tert_mi2s_sd1 {
			tert_mi2s_sd1_sleep: tert_mi2s_sd1_sleep {
				mux {
					pins = "gpio137";
					function = "gpio";
				};

				config {
					pins = "gpio137";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
					input-enable;
				};
			};

			tert_mi2s_sd1_active: tert_mi2s_sd1_active {
				mux {
					pins = "gpio137";
					function = "mi2s2_data1";
				};

				config {
					pins = "gpio137";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;           /* NO PULL */
				};
			};
		};

		/* WSA speaker reset pins */
		spkr_1_sd_n {
			spkr_1_sd_n_sleep: spkr_1_sd_n_sleep {
				mux {
					pins = "gpio26";
					function = "gpio";
				};

				config {
					pins = "gpio26";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;
					input-enable;
				};
			};

			spkr_1_sd_n_active: spkr_1_sd_n_active {
				mux {
					pins = "gpio26";
					function = "gpio";
				};

				config {
					pins = "gpio26";
					drive-strength = <16>;   /* 16 mA */
					bias-disable;
					output-high;
				};
			};
		};

		spkr_2_sd_n {
			spkr_2_sd_n_sleep: spkr_2_sd_n_sleep {
				mux {
					pins = "gpio127";
					function = "gpio";
				};

				config {
					pins = "gpio127";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;
					input-enable;
				};
			};

			spkr_2_sd_n_active: spkr_2_sd_n_active {
				mux {
					pins = "gpio127";
					function = "gpio";
				};

				config {
					pins = "gpio127";
					drive-strength = <16>;   /* 16 mA */
					bias-disable;
					output-high;
				};
			};
		};

		wcd938x_reset_active: wcd938x_reset_active {
			mux {
				pins = "gpio32";
				function = "func2";
			};

			config {
				pins = "gpio32";
				drive-strength = <16>;
				output-high;
			};
		};

		wcd938x_reset_sleep: wcd938x_reset_sleep {
			mux {
				pins = "gpio32";
				function = "func2";
			};

			config {
				pins = "gpio32";
				drive-strength = <16>;
				bias-disable;
				output-low;
			};
		};

		cam_sensor_mclk0_active: cam_sensor_mclk0_active {
			/* MCLK0 */
			mux {
				pins = "gpio94";
				function = "cam_mclk";
			};

			config {
				pins = "gpio94";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk0_suspend: cam_sensor_mclk0_suspend {
			/* MCLK0 */
			mux {
				pins = "gpio94";
				function = "cam_mclk";
			};

			config {
				pins = "gpio94";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk1_active: cam_sensor_mclk1_active {
			/* MCLK1 */
			mux {
				pins = "gpio95";
				function = "cam_mclk";
			};

			config {
				pins = "gpio95";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk1_suspend: cam_sensor_mclk1_suspend {
			/* MCLK1 */
			mux {
				pins = "gpio95";
				function = "cam_mclk";
			};

			config {
				pins = "gpio95";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk2_active: cam_sensor_mclk2_active {
			/* MCLK2 */
			mux {
				pins = "gpio96";
				function = "cam_mclk";
			};

			config {
				pins = "gpio96";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk2_suspend: cam_sensor_mclk2_suspend {
			/* MCLK2 */
			mux {
				pins = "gpio96";
				function = "cam_mclk";
			};

			config {
				pins = "gpio96";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk3_active: cam_sensor_mclk3_active {
			/* MCLK3 */
			mux {
				pins = "gpio97";
				function = "cam_mclk";
			};

			config {
				pins = "gpio97";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk3_suspend: cam_sensor_mclk3_suspend {
			/* MCLK3 */
			mux {
				pins = "gpio97";
				function = "cam_mclk";
			};

			config {
				pins = "gpio97";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk4_active: cam_sensor_mclk4_active {
			/* MCLK4 */
			mux {
				pins = "gpio98";
				function = "cam_mclk";
			};

			config {
				pins = "gpio98";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk4_suspend: cam_sensor_mclk4_suspend {
			/* MCLK4 */
			mux {
				pins = "gpio98";
				function = "cam_mclk";
			};

			config {
				pins = "gpio98";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk5_active: cam_sensor_mclk5_active {
			/* MCLK5 */
			mux {
				pins = "gpio99";
				function = "cam_mclk";
			};

			config {
				pins = "gpio99";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk5_suspend: cam_sensor_mclk5_suspend {
			/* MCLK5 */
			mux {
				pins = "gpio99";
				function = "cam_mclk";
			};

			config {
				pins = "gpio99";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk6_active: cam_sensor_mclk6_active {
			/* MCLK6 */
			mux {
				pins = "gpio100";
				function = "cam_mclk";
			};

			config {
				pins = "gpio100";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk6_suspend: cam_sensor_mclk6_suspend {
			/* MCLK6 */
			mux {
				pins = "gpio100";
				function = "cam_mclk";
			};

			config {
				pins = "gpio100";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_active_rear: cam_sensor_active_rear {
			/* RESET REAR */
			mux {
				pins = "gpio93";
				function = "gpio";
			};

			config {
				pins = "gpio93";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rear: cam_sensor_suspend_rear {
			/* RESET REAR */
			mux {
				pins = "gpio93";
				function = "gpio";
			};

			config {
				pins = "gpio93";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_rear_aux: cam_sensor_active_rear_aux {
			/* RESET REARAUX */
			mux {
				pins = "gpio92";
				function = "gpio";
			};

			config {
				pins = "gpio92";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rear_aux: cam_sensor_suspend_rear_aux {
			/* RESET REARAUX */
			mux {
				pins = "gpio92";
				function = "gpio";
			};

			config {
				pins = "gpio92";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_rst2: cam_sensor_active_rst2 {
			/* RESET 2 */
			mux {
				pins = "gpio78";
				function = "gpio";
			};

			config {
				pins = "gpio78";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rst2: cam_sensor_suspend_rst2 {
			/* RESET 2 */
			mux {
				pins = "gpio78";
				function = "gpio";
			};

			config {
				pins = "gpio78";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_3: cam_sensor_active_3 {
			/* RESET 3 */
			mux {
				pins = "gpio109";
				function = "gpio";
			};

			config {
				pins = "gpio109";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_3: cam_sensor_suspend_3 {
			/* RESET 3 */
			mux {
				pins = "gpio109";
				function = "gpio";
			};

			config {
				pins = "gpio109";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_rst4: cam_sensor_active_rst4 {
			/* RESET 2 */
			mux {
				pins = "gpio25";
				function = "gpio";
			};

			config {
				pins = "gpio25";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rst4: cam_sensor_suspend_rst4 {
			/* RESET 2 */
			mux {
				pins = "gpio25";
				function = "gpio";
			};

			config {
				pins = "gpio25";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_rst3: cam_sensor_active_rst3 {
			/* RESET 2 */
			mux {
				pins = "gpio144";
				function = "gpio";
			};

			config {
				pins = "gpio144";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rst3: cam_sensor_suspend_rst3 {
			/* RESET 2 */
			mux {
				pins = "gpio144";
				function = "gpio";
			};

			config {
				pins = "gpio144";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_4: cam_sensor_active_4 {
			/* RESET 4 */
			mux {
				pins = "gpio130";
				function = "gpio";
			};

			config {
				pins = "gpio130";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_4: cam_sensor_suspend_4 {
			/* RESET 4 */
			mux {
				pins = "gpio130";
				function = "gpio";
			};

			config {
				pins = "gpio130";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_5: cam_sensor_active_5 {
			/* RESET 5 */
			mux {
				pins = "gpio131";
				function = "gpio";
			};

			config {
				pins = "gpio131";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_5: cam_sensor_suspend_5 {
			/* RESET 5 */
			mux {
				pins = "gpio131";
				function = "gpio";
			};

			config {
				pins = "gpio131";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_6: cam_sensor_active_6 {
			/* RESET 6 */
			mux {
				pins = "gpio114";
				function = "gpio";
			};

			config {
				pins = "gpio114";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_6: cam_sensor_suspend_6 {
			/* RESET 6 */
			mux {
				pins = "gpio114";
				function = "gpio";
			};

			config {
				pins = "gpio114";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cci0_active: cci0_active {
			mux {
				/* CLK, DATA */
				pins = "gpio101","gpio102"; // Only 2
				function = "cci_i2c";
			};

			config {
				pins = "gpio101","gpio102";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci0_suspend: cci0_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio101","gpio102";
				function = "cci_i2c";
			};

			config {
				pins = "gpio101","gpio102";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci1_active: cci1_active {
			mux {
				/* CLK, DATA */
				pins = "gpio103","gpio104";
				function = "cci_i2c";
			};

			config {
				pins = "gpio103","gpio104";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci1_suspend: cci1_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio103","gpio104";
				function = "cci_i2c";
			};

			config {
				pins = "gpio103","gpio104";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci2_active: cci2_active {
			mux {
				/* CLK, DATA */
				pins = "gpio105","gpio106";
				function = "cci_i2c";
			};

			config {
				pins = "gpio105","gpio106";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci2_suspend: cci2_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio105","gpio106";
				function = "cci_i2c";
			};

			config {
				pins = "gpio105","gpio106";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci3_active: cci3_active {
			mux {
				/* CLK, DATA */
				pins = "gpio107","gpio108";
				function = "cci_i2c";
			};

			config {
				pins = "gpio107","gpio108";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci3_suspend: cci3_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio107","gpio108";
				function = "cci_i2c";
			};

			config {
				pins = "gpio107","gpio108";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		tsif0_signals_active: tsif0_signals_active {
			tsif1_clk {
				pins = "gpio69"; /* TSIF0 CLK */
				function = "tsif0_clk";
			};

			tsif1_en {
				pins = "gpio70"; /* TSIF0 Enable */
				function = "tsif0_en";
			};

			tsif1_data {
				pins = "gpio71"; /* TSIF0 DATA */
				function = "tsif0_data";
			};

			signals_cfg {
				pins = "gpio69", "gpio70", "gpio71";
				drive_strength = <2>;	/* 2 mA */
				bias-pull-down;		/* pull down */
			};
		};

		/* sync signal is only used if configured to mode-2 */
		tsif0_sync_active: tsif0_sync_active {
			tsif1_sync {
				pins = "gpio72";	/* TSIF0 SYNC */
				function = "tsif0_sync";
				drive_strength = <2>;	/* 2 mA */
				bias-pull-down;		/* pull down */
			};
		};

		tsif1_signals_active: tsif1_signals_active {
			tsif2_clk {
				pins = "gpio73"; /* TSIF1 CLK */
				function = "tsif1_clk";
			};

			tsif2_en {
				pins = "gpio74"; /* TSIF1 Enable */
				function = "tsif1_en";
			};

			tsif2_data {
				pins = "gpio75"; /* TSIF1 DATA */
				function = "tsif1_data";
			};

			signals_cfg {
				pins = "gpio73", "gpio74", "gpio75";
				drive_strength = <2>;	/* 2 mA */
				bias-pull-down;		/* pull down */
			};
		};

		/* sync signal is only used if configured to mode-2 */
		tsif1_sync_active: tsif1_sync_active {
			tsif2_sync {
				pins = "gpio76";	/* TSIF1 SYNC */
				function = "tsif1_sync";
				drive_strength = <2>;	/* 2 mA */
				bias-pull-down;		/* pull down */
			};
		};

		sde_led_driver_en1_gpio: sde_led_driver_en1_gpio {
			mux {
				pins = "gpio144";
				function = "gpio";
			};

			config {
				pins = "gpio144";
				bias-pull-down;
				drive-strength = <16>;
			};
		};

		sde_led_driver_en2_gpio: sde_led_driver_en2_gpio {
			mux {
				pins = "gpio140";
				function = "gpio";
			};

			config {
				pins = "gpio140";
				bias-pull-down;
				drive-strength = <16>;
			};
		};

		sde_led_5v_en_gpio: sde_led_5v_en_gpio {
			mux {
				pins = "gpio134";
				function = "gpio";
			};

			config {
				pins = "gpio134";
				bias-pull-down;
				drive-strength = <16>;
			};
		};

		sde_display_1p8_en_gpio: sde_display_1p8_en_gpio {
			mux {
				pins = "gpio133";
				function = "gpio";
			};

			config {
				pins = "gpio133";
				bias-pull-down;
				drive-strength = <16>;
			};
		};

		cam_sensor_6dof_vana_active: cam_sensor_6dof_vana_active {
			/*  AVDD LDO */
			mux {
				pins = "gpio84";
				function = "gpio";
			};

			config {
				pins = "gpio84";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_6dof_vana_suspend: cam_sensor_6dof_vana_suspend {
			/*  AVDD LDO */
			mux {
				pins = "gpio84";
				function = "gpio";
			};

			config {
				pins = "gpio84";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_6dof_vdig_active: cam_sensor_6dof_vdig_active {
			/*  VDIG LDO */
			mux {
				pins = "gpio82";
				function = "gpio";
			};

			config {
				pins = "gpio82";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_6dof_vdig_suspend: cam_sensor_6dof_vdig_suspend {
			/*  VDIG LDO */
			mux {
				pins = "gpio82";
				function = "gpio";
			};

			config {
				pins = "gpio82";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_6dof_vio_active: cam_sensor_6dof_vio_active {
			/*  VIO LDO */
			mux {
				pins = "gpio83";
				function = "gpio";
			};

			config {
				pins = "gpio83";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_6dof_vio_suspend: cam_sensor_6dof_vio_suspend {
			/*  VIO LDO */
			mux {
				pins = "gpio83";
				function = "gpio";
			};

			config {
				pins = "gpio83";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_et_vana_active: cam_sensor_et_vana_active {
			/*  AVDD LDO */
			mux {
				pins = "gpio114";
				function = "gpio";
			};

			config {
				pins = "gpio114";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_et_vana_suspend: cam_sensor_et_vana_suspend {
			/*  AVDD LDO */
			mux {
				pins = "gpio114";
				function = "gpio";
			};

			config {
				pins = "gpio114";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_et_vio_active: cam_sensor_et_vio_active {
			/*  VIO LDO */
			mux {
				pins = "gpio145";
				function = "gpio";
			};

			config {
				pins = "gpio145";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_et_vio_suspend: cam_sensor_et_vio_suspend {
			/*  VIO LDO */
			mux {
				pins = "gpio145";
				function = "gpio";
			};

			config {
				pins = "gpio145";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rgb_vana_active: cam_sensor_rgb_vana_active {
			mux {
				pins = "gpio117";
				function = "gpio";
			};

			config {
				pins = "gpio117";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rgb_vana_suspend: cam_sensor_rgb_vana_suspend {
			mux {
				pins = "gpio117";
				function = "gpio";
			};

			config {
				pins = "gpio117";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rgb_vio_active: cam_sensor_rgb_vio_active {
			mux {
				pins = "gpio116";
				function = "gpio";
			};

			config {
				pins = "gpio116";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rgb_vio_suspend: cam_sensor_rgb_vio_suspend {
			mux {
				pins = "gpio116";
				function = "gpio";
			};

			config {
				pins = "gpio116";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rgb_vdig_active: cam_sensor_rgb_vdig_active {
			mux {
				pins = "gpio115";
				function = "gpio";
			};

			config {
				pins = "gpio115";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rgb_vdig_suspend: cam_sensor_rgb_vdig_suspend {
			mux {
				pins = "gpio115";
				function = "gpio";
			};

			config {
				pins = "gpio115";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_active_etleft: cam_sensor_active_etleft {
			/* RESET REAR */
			mux {
				pins = "gpio93";
				function = "gpio";
			};

			config {
				pins = "gpio93";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_etleft: cam_sensor_suspend_etleft {
			/* RESET REAR */
			mux {
				pins = "gpio93";
				function = "gpio";
			};

			config {
				pins = "gpio93";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_etright: cam_sensor_active_etright {
			/* RESET REAR */
			mux {
				pins = "gpio92";
				function = "gpio";
			};

			config {
				pins = "gpio92";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_etright: cam_sensor_suspend_etright {
			/* RESET REAR */
			mux {
				pins = "gpio92";
				function = "gpio";
			};

			config {
				pins = "gpio92";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_6dofleft: cam_sensor_active_6dofleft {
			/* RESET REAR */
			mux {
				pins = "gpio130";
				function = "gpio";
			};

			config {
				pins = "gpio130";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_6dofleft: cam_sensor_suspend_6dofleft {
			/* RESET REAR */
			mux {
				pins = "gpio130";
				function = "gpio";
			};

			config {
				pins = "gpio130";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_6dofright: cam_sensor_active_6dofright {
			/* RESET REAR */
			mux {
				pins = "gpio131";
				function = "gpio";
			};

			config {
				pins = "gpio131";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_6dofright: cam_sensor_suspend_6dofright {
			/* RESET REAR */
			mux {
				pins = "gpio131";
				function = "gpio";
			};

			config {
				pins = "gpio131";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_rgbright: cam_sensor_active_rgbright {
			/* RESET REAR */
			mux {
				pins = "gpio109";
				function = "gpio";
			};

			config {
				pins = "gpio109";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rgbright: cam_sensor_suspend_rgbright {
			/* RESET REAR */
			mux {
				pins = "gpio109";
				function = "gpio";
			};

			config {
				pins = "gpio109";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_active_rgbleft: cam_sensor_active_rgbleft {
			/* RESET REAR */
			mux {
				pins = "gpio78";
				function = "gpio";
			};

			config {
				pins = "gpio78";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_suspend_rgbleft: cam_sensor_suspend_rgbleft {
			/* RESET REAR */
			mux {
				pins = "gpio78";
				function = "gpio";
			};

			config {
				pins = "gpio78";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		bt_en_sleep: bt_en_sleep {
			mux {
			pins = "gpio21";
			function = "gpio";
			};

			config {
			pins = "gpio21";
			drive-strength = <2>;
			output-low;
			bias-pull-down;
			};
		};

		/* QUPv3_0 North SE0 mappings */
		qupv3_se0_i3c_pins: qupv3_se0_i3c_pins {
			qupv3_se0_i3c_active: qupv3_se0_i3c_active {
				mux {
					pins = "gpio28", "gpio29";
					function = "ibi_i3c";
				};

				config {
					pins = "gpio28", "gpio29";
					drive-strength = <16>;
					bias-pull-up;
				};
			};

			qupv3_se0_i3c_sleep: qupv3_se0_i3c_sleep {
				mux {
					pins = "gpio28", "gpio29";
					function = "ibi_i3c";
				};

				config {
					pins = "gpio28", "gpio29";
					drive-strength = <16>;
					bias-pull-up;
				};
			};
		};

		/* QUPv3_0 North SE1 mappings */
		qupv3_se1_i3c_pins: qupv3_se1_i3c_pins {
			qupv3_se1_i3c_active: qupv3_se1_i3c_active {
				mux {
					pins = "gpio4", "gpio5";
					function = "ibi_i3c";
				};

				config {
					pins = "gpio4", "gpio5";
					drive-strength = <16>;
					bias-pull-up;
				};
			};

			qupv3_se1_i3c_sleep: qupv3_se1_i3c_sleep {
				mux {
					pins = "gpio4", "gpio5";
					function = "ibi_i3c";
				};

				config {
					pins = "gpio4", "gpio5";
					drive-strength = <16>;
					bias-pull-up;
				};
			};
		};

		/* SE 0 pin mappings */
		qupv3_se0_i2c_pins: qupv3_se0_i2c_pins {
			qupv3_se0_i2c_active: qupv3_se0_i2c_active {
				mux {
					pins = "gpio28", "gpio29";
					function = "qup0";
				};

				config {
					pins = "gpio28", "gpio29";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se0_i2c_sleep: qupv3_se0_i2c_sleep {
				mux {
					pins = "gpio28", "gpio29";
					function = "gpio";
				};

				config {
					pins = "gpio28", "gpio29";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 1 pin mappings */
		qupv3_se1_i2c_pins: qupv3_se1_i2c_pins {
			qupv3_se1_i2c_active: qupv3_se1_i2c_active {
				mux {
					pins = "gpio4", "gpio5";
					function = "qup1";
				};

				config {
					pins = "gpio4", "gpio5";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se1_i2c_sleep: qupv3_se1_i2c_sleep {
				mux {
					pins = "gpio4", "gpio5";
					function = "gpio";
				};

				config {
					pins = "gpio4", "gpio5";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		lt9611_pins: lt9611_pins {
			mux {
				pins = "gpio2", "gpio1";
				function = "gpio";
			};

			config {
				pins = "gpio2", "gpio1";
				drive-strength = <8>;
				bias-disable = <0>;
			};
		};

		nfc {
			nfc_int_active: nfc_int_active {
				/* active state */
				mux {
					/* GPIO 111 NFC Read Interrupt */
					pins = "gpio111";
					function = "gpio";
				};

				config {
					pins = "gpio111";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_int_suspend: nfc_int_suspend {
				/* sleep state */
				mux {
					/* GPIO 111 NFC Read Interrupt */
					pins = "gpio111";
					function = "gpio";
				};

				config {
					pins = "gpio111";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_enable_active: nfc_enable_active {
				/* active state */
				mux {
					/* 6: Enable 110: Firmware */
					pins = "gpio6", "gpio110";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio110";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_enable_suspend: nfc_enable_suspend {
				/* sleep state */
				mux {
					/* 6: Enable 110: Firmware */
					pins = "gpio6", "gpio110";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio110";
					drive-strength = <2>; /* 2 MA */
					bias-disable;
				};
			};

			nfc_clk_req_active: nfc_clk_req_active {
				/* active state */
				mux {
					/* GPIO 7: NFC CLOCK REQUEST */
					pins = "gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio7";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_clk_req_suspend: nfc_clk_req_suspend {
				/* sleep state */
				mux {
					/* GPIO 7: NFC CLOCK REQUEST */
					pins = "gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio7";
					drive-strength = <2>; /* 2 MA */
					bias-disable;
				};
			};
		};

		/* SE 2 pin mappings */
		qupv3_se2_i2c_pins: qupv3_se2_i2c_pins {
			qupv3_se2_i2c_active: qupv3_se2_i2c_active {
				mux {
					pins = "gpio115", "gpio116";
					function = "qup2";
				};

				config {
					pins = "gpio115", "gpio116";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se2_i2c_sleep: qupv3_se2_i2c_sleep {
				mux {
					pins = "gpio115", "gpio116";
					function = "gpio";
				};

				config {
					pins = "gpio115", "gpio116";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 3 pin mappings */
		qupv3_se3_i2c_pins: qupv3_se3_i2c_pins {
			qupv3_se3_i2c_active: qupv3_se3_i2c_active {
				mux {
					pins = "gpio119", "gpio120";
					function = "qup3";
				};

				config {
					pins = "gpio119", "gpio120";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se3_i2c_sleep: qupv3_se3_i2c_sleep {
				mux {
					pins = "gpio119", "gpio120";
					function = "gpio";
				};

				config {
					pins = "gpio119", "gpio120";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 4 pin mappings */
		qupv3_se4_i2c_pins: qupv3_se4_i2c_pins {
			qupv3_se4_i2c_active: qupv3_se4_i2c_active {
				mux {
					pins = "gpio8", "gpio9";
					function = "qup4";
				};

				config {
					pins = "gpio8", "gpio9";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se4_i2c_sleep: qupv3_se4_i2c_sleep {
				mux {
					pins = "gpio8", "gpio9";
					function = "gpio";
				};

				config {
					pins = "gpio8", "gpio9";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 5 pin mappings */
		qupv3_se5_i2c_pins: qupv3_se5_i2c_pins {
			qupv3_se5_i2c_active: qupv3_se5_i2c_active {
				mux {
					pins = "gpio12", "gpio13";
					function = "qup5";
				};

				config {
					pins = "gpio12", "gpio13";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se5_i2c_sleep: qupv3_se5_i2c_sleep {
				mux {
					pins = "gpio12", "gpio13";
					function = "gpio";
				};

				config {
					pins = "gpio12", "gpio13";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 6 pin mappings */
		qupv3_se6_i2c_pins: qupv3_se6_i2c_pins {
			qupv3_se6_i2c_active: qupv3_se6_i2c_active {
				mux {
					pins = "gpio16", "gpio17";
					function = "qup6";
				};

				config {
					pins = "gpio16", "gpio17";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se6_i2c_sleep: qupv3_se6_i2c_sleep {
				mux {
					pins = "gpio16", "gpio17";
					function = "gpio";
				};

				config {
					pins = "gpio16", "gpio17";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 7 pin mappings */
		qupv3_se7_i2c_pins: qupv3_se7_i2c_pins {
			qupv3_se7_i2c_active: qupv3_se7_i2c_active {
				mux {
					pins = "gpio20", "gpio21";
					function = "qup7";
				};

				config {
					pins = "gpio20", "gpio21";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se7_i2c_sleep: qupv3_se7_i2c_sleep {
				mux {
					pins = "gpio20", "gpio21";
					function = "gpio";
				};

				config {
					pins = "gpio20", "gpio21";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		qupv3_se0_spi_pins: qupv3_se0_spi_pins {
			qupv3_se0_spi_active: qupv3_se0_spi_active {
				mux {
					pins = "gpio28", "gpio29", "gpio30",
								"gpio31";
					function = "qup0";
				};

				config {
					pins = "gpio28", "gpio29", "gpio30",
								"gpio31";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se0_spi_sleep: qupv3_se0_spi_sleep {
				mux {
					pins = "gpio28", "gpio29", "gpio30",
								"gpio31";
					function = "gpio";
				};

				config {
					pins = "gpio28", "gpio29", "gpio30",
								"gpio31";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se1_spi_pins: qupv3_se1_spi_pins {
			qupv3_se1_spi_active: qupv3_se1_spi_active {
				mux {
					pins = "gpio4", "gpio5", "gpio6",
								"gpio7";
					function = "qup1";
				};

				config {
					pins = "gpio4", "gpio5", "gpio6",
								"gpio7";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se1_spi_sleep: qupv3_se1_spi_sleep {
				mux {
					pins = "gpio4", "gpio5", "gpio6",
								"gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio4", "gpio5", "gpio6",
								"gpio7";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se2_spi_pins: qupv3_se2_spi_pins {
			qupv3_se2_spi_active: qupv3_se2_spi_active {
				mux {
					pins = "gpio115", "gpio116", "gpio117",
								"gpio118";
					function = "qup2";
				};

				config {
					pins = "gpio115", "gpio116", "gpio117",
								"gpio118";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se2_spi_sleep: qupv3_se2_spi_sleep {
				mux {
					pins = "gpio115", "gpio116", "gpio117",
								"gpio118";
					function = "gpio";
				};

				config {
					pins = "gpio115", "gpio116", "gpio117",
								"gpio118";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se3_spi_pins: qupv3_se3_spi_pins {
			qupv3_se3_spi_active: qupv3_se3_spi_active {
				mux {
					pins = "gpio119", "gpio120", "gpio121",
								"gpio122";
					function = "qup3";
				};

				config {
					pins = "gpio119", "gpio120", "gpio121",
								"gpio122";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se3_spi_sleep: qupv3_se3_spi_sleep {
				mux {
					pins = "gpio119", "gpio120", "gpio121",
							"gpio122";
					function = "gpio";
				};

				config {
					pins = "gpio119", "gpio120", "gpio121",
							"gpio122";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se4_spi_pins: qupv3_se4_spi_pins {
			qupv3_se4_spi_active: qupv3_se4_spi_active {
				mux {
					pins = "gpio8", "gpio9", "gpio10",
								"gpio11";
					function = "qup4";
				};

				config {
					pins = "gpio8", "gpio9", "gpio10",
								"gpio11";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se4_spi_sleep: qupv3_se4_spi_sleep {
				mux {
					pins = "gpio8", "gpio9", "gpio10",
								"gpio11";
					function = "gpio";
				};

				config {
					pins = "gpio8", "gpio9", "gpio10",
								"gpio11";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se5_spi_pins: qupv3_se5_spi_pins {
			qupv3_se5_spi_active: qupv3_se5_spi_active {
				mux {
					pins = "gpio12", "gpio13", "gpio14",
								"gpio15";
					function = "qup5";
				};

				config {
					pins = "gpio12", "gpio13", "gpio14",
								"gpio15";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se5_spi_sleep: qupv3_se5_spi_sleep {
				mux {
					pins = "gpio12", "gpio13", "gpio14",
								"gpio15";
					function = "gpio";
				};

				config {
					pins = "gpio12", "13", "gpio14",
								"gpio15";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se6_spi_pins: qupv3_se6_spi_pins {
			qupv3_se6_spi_active: qupv3_se6_spi_active {
				mux {
					pins = "gpio16", "gpio17", "gpio18",
								"gpio19";
					function = "qup6";
				};

				config {
					pins = "gpio16", "gpio17", "gpio18",
								"gpio19";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se6_spi_sleep: qupv3_se6_spi_sleep {
				mux {
					pins = "gpio16", "gpio17", "gpio18",
								"gpio19";
					function = "gpio";
				};

				config {
					pins = "gpio16", "gpio17", "gpio18",
								"gpio19";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se7_spi_pins: qupv3_se7_spi_pins {
			qupv3_se7_spi_active: qupv3_se7_spi_active {
				mux {
					pins = "gpio20", "gpio21", "gpio22",
								"gpio23";
					function = "qup7";
				};

				config {
					pins = "gpio20", "gpio21", "gpio22",
								"gpio23";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se7_spi_sleep: qupv3_se7_spi_sleep {
				mux {
					pins = "gpio20", "gpio21", "gpio22",
								"gpio23";
					function = "gpio";
				};

				config {
					pins = "gpio20", "gpio21", "gpio22",
								"gpio23";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* QUPv3_1 South_1 SE mappings */
		/* SE 8 pin mappings */
		qupv3_se8_i2c_pins: qupv3_se8_i2c_pins {
			qupv3_se8_i2c_active: qupv3_se8_i2c_active {
				mux {
					pins = "gpio24", "gpio25";
					function = "qup8";
				};

				config {
					pins = "gpio24", "gpio25";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se8_i2c_sleep: qupv3_se8_i2c_sleep {
				mux {
					pins = "gpio24", "gpio25";
					function = "gpio";
				};

				config {
					pins = "gpio24", "gpio25";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 9 pin mappings */
		qupv3_se9_i2c_pins: qupv3_se9_i2c_pins {
			qupv3_se9_i2c_active: qupv3_se9_i2c_active {
				mux {
					pins = "gpio125", "gpio126";
					function = "qup9";
				};

				config {
					pins = "gpio125", "gpio126";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se9_i2c_sleep: qupv3_se9_i2c_sleep {
				mux {
					pins = "gpio125", "gpio126";
					function = "gpio";
				};

				config {
					pins = "gpio125", "gpio126";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 10 pin mappings */
		qupv3_se10_i2c_pins: qupv3_se10_i2c_pins {
			qupv3_se10_i2c_active: qupv3_se10_i2c_active {
				mux {
					pins = "gpio129", "gpio130";
					function = "qup10";
				};

				config {
					pins = "gpio129", "gpio130";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se10_i2c_sleep: qupv3_se10_i2c_sleep {
				mux {
					pins = "gpio129", "gpio130";
					function = "gpio";
				};

				config {
					pins = "gpio129", "gpio130";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 11 pin mappings */
		qupv3_se11_i2c_pins: qupv3_se11_i2c_pins {
			qupv3_se11_i2c_active: qupv3_se11_i2c_active {
				mux {
					pins = "gpio60", "gpio61";
					function = "qup11";
				};

				config {
					pins = "gpio60", "gpio61";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se11_i2c_sleep: qupv3_se11_i2c_sleep {
				mux {
					pins = "gpio60", "gpio61";
					function = "gpio";
				};

				config {
					pins = "gpio60", "gpio61";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 12 pin mappings */
		qupv3_se12_i2c_pins: qupv3_se12_i2c_pins {
			qupv3_se12_i2c_active: qupv3_se12_i2c_active {
				mux {
					pins = "gpio32", "gpio33";
					function = "qup12";
				};

				config {
					pins = "gpio32", "gpio33";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se12_i2c_sleep: qupv3_se12_i2c_sleep {
				mux {
					pins = "gpio32", "gpio33";
					function = "gpio";
				};

				config {
					pins = "gpio32", "gpio33";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 13 pin mappings */
		qupv3_se13_i2c_pins: qupv3_se13_i2c_pins {
			qupv3_se13_i2c_active: qupv3_se13_i2c_active {
				mux {
					pins = "gpio36", "gpio37";
					function = "qup13";
				};

				config {
					pins = "gpio36", "gpio37";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se13_i2c_sleep: qupv3_se13_i2c_sleep {
				mux {
					pins = "gpio36", "gpio37";
					function = "gpio";
				};

				config {
					pins = "gpio36", "gpio37";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		qupv3_se8_spi_pins: qupv3_se8_spi_pins {
			qupv3_se8_spi_active: qupv3_se8_spi_active {
				mux {
					pins = "gpio24", "gpio25", "gpio26",
								"gpio27";
					function = "qup8";
				};

				config {
					pins = "gpio24", "gpio25", "gpio26",
								"gpio27";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se8_spi_sleep: qupv3_se8_spi_sleep {
				mux {
					pins = "gpio24", "gpio25", "gpio26",
								"gpio27";
					function = "gpio";
				};

				config {
					pins = "gpio24", "gpio25", "gpio26",
								"gpio27";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se9_spi_pins: qupv3_se9_spi_pins {
			qupv3_se9_spi_active: qupv3_se9_spi_active {
				mux {
					pins = "gpio125", "gpio126", "gpio127",
								"gpio128";
					function = "qup9";
				};

				config {
					pins = "gpio125", "gpio126", "gpio127",
								"gpio128";
					drive-strength = <6>;
					bias-disable;
				};
		};

			qupv3_se9_spi_sleep: qupv3_se9_spi_sleep {
				mux {
					pins = "gpio125", "gpio126", "gpio127",
								"gpio128";
					function = "gpio";
				};

				config {
					pins = "gpio125", "gpio126", "gpio127",
								"gpio128";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se10_spi_pins: qupv3_se10_spi_pins {
			qupv3_se10_spi_active: qupv3_se10_spi_active {
				mux {
					pins = "gpio129", "gpio130", "gpio131",
								"gpio132";
					function = "qup10";
				};

				config {
					pins = "gpio129", "gpio130", "gpio131",
								"gpio132";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se10_spi_sleep: qupv3_se10_spi_sleep {
				mux {
					pins = "gpio129", "gpio130", "gpio131",
								"gpio132";
					function = "gpio";
				};

				config {
					pins = "gpio129", "gpio130", "gpio131",
								"gpio132";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se11_spi_pins: qupv3_se11_spi_pins {
			qupv3_se11_spi_active: qupv3_se11_spi_active {
				mux {
					pins = "gpio60", "gpio61", "gpio62",
								"gpio63";
					function = "qup11";
				};

				config {
					pins = "gpio60", "gpio61", "gpio62",
								"gpio63";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se11_spi_sleep: qupv3_se11_spi_sleep {
				mux {
					pins = "gpio60", "gpio61", "gpio62",
								"gpio63";
					function = "gpio";
				};

				config {
					pins = "gpio60", "gpio61", "gpio62",
								"gpio63";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se12_spi_pins: qupv3_se12_spi_pins {
			qupv3_se12_spi_active: qupv3_se12_spi_active {
				mux {
					pins = "gpio32", "gpio33", "gpio34",
								"gpio35";
					function = "qup12";
				};

				config {
					pins = "gpio32", "gpio33", "gpio34",
								"gpio35";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se12_spi_sleep: qupv3_se12_spi_sleep {
				mux {
					pins = "gpio32", "gpio33", "gpio34",
								"gpio35";
					function = "gpio";
				};

				config {
					pins = "gpio32", "gpio33", "gpio34",
								"gpio35";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se13_spi_pins: qupv3_se13_spi_pins {
			qupv3_se13_spi_active: qupv3_se13_spi_active {
				mux {
					pins = "gpio36", "gpio37", "gpio38",
								"gpio39";
					function = "qup13";
				};

				config {
					pins = "gpio36", "gpio37", "gpio38",
								"gpio39";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se13_spi_sleep: qupv3_se13_spi_sleep {
				mux {
					pins = "gpio36", "gpio37", "gpio38",
								"gpio39";
					function = "gpio";
				};

				config {
					pins = "gpio36", "gpio37", "gpio38",
								"gpio39";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		/* QUPv3_2 South_2 SE mappings */
		/* SE 14 pin mappings */
		qupv3_se14_i2c_pins: qupv3_se14_i2c_pins {
			qupv3_se14_i2c_active: qupv3_se14_i2c_active {
				mux {
					pins = "gpio40", "gpio41";
					function = "qup14";
				};

				config {
					pins = "gpio40", "gpio41";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se14_i2c_sleep: qupv3_se14_i2c_sleep {
				mux {
					pins = "gpio40", "gpio41";
					function = "gpio";
				};

				config {
					pins = "gpio40", "gpio41";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 15 pin mappings */
		qupv3_se15_i2c_pins: qupv3_se15_i2c_pins {
			qupv3_se15_i2c_active: qupv3_se15_i2c_active {
				mux {
					pins = "gpio44", "gpio45";
					function = "qup15";
				};

				config {
					pins = "gpio44", "gpio45";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se15_i2c_sleep: qupv3_se15_i2c_sleep {
				mux {
					pins = "gpio44", "gpio45";
					function = "gpio";
				};

				config {
					pins = "gpio44", "gpio45";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 16 pin mappings */
		qupv3_se16_i2c_pins: qupv3_se16_i2c_pins {
			qupv3_se16_i2c_active: qupv3_se16_i2c_active {
				mux {
					pins = "gpio48", "gpio49";
					function = "qup16";
				};

				config {
					pins = "gpio48", "gpio49";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se16_i2c_sleep: qupv3_se16_i2c_sleep {
				mux {
					pins = "gpio48", "gpio49";
					function = "gpio";
				};

				config {
					pins = "gpio48", "gpio49";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 17 pin mappings */
		qupv3_se17_i2c_pins: qupv3_se17_i2c_pins {
			qupv3_se17_i2c_active: qupv3_se17_i2c_active {
				mux {
					pins = "gpio52", "gpio53";
					function = "qup17";
				};

				config {
					pins = "gpio52", "gpio53";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se17_i2c_sleep: qupv3_se17_i2c_sleep {
				mux {
					pins = "gpio52", "gpio53";
					function = "gpio";
				};

				config {
					pins = "gpio52", "gpio53";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 18 pin mappings */
		qupv3_se18_i2c_pins: qupv3_se18_i2c_pins {
			qupv3_se18_i2c_active: qupv3_se18_i2c_active {
				mux {
					pins = "gpio56", "gpio57";
					function = "qup18";
				};

				config {
					pins = "gpio56", "gpio57";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se18_i2c_sleep: qupv3_se18_i2c_sleep {
				mux {
					pins = "gpio56", "gpio57";
					function = "gpio";
				};

				config {
					pins = "gpio56", "gpio57";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 19 pin mappings */
		qupv3_se19_i2c_pins: qupv3_se19_i2c_pins {
			qupv3_se19_i2c_active: qupv3_se19_i2c_active {
				mux {
					pins = "gpio0", "gpio1";
					function = "qup19";
				};

				config {
					pins = "gpio0", "gpio1";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se19_i2c_sleep: qupv3_se19_i2c_sleep {
				mux {
					pins = "gpio0", "gpio1";
					function = "gpio";
				};

				config {
					pins = "gpio0", "gpio1";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		qupv3_se14_spi_pins: qupv3_se14_spi_pins {
			qupv3_se14_spi_active: qupv3_se14_spi_active {
				mux {
					pins = "gpio40", "gpio41", "gpio42",
								"gpio43";
					function = "qup14";
				};

				config {
					pins = "gpio40", "gpio41", "gpio42",
								"gpio43";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se14_spi_sleep: qupv3_se14_spi_sleep {
				mux {
					pins = "gpio40", "gpio41", "gpio42",
								"gpio43";
					function = "gpio";
				};

				config {
					pins = "gpio40", "gpio41", "gpio42",
								"gpio43";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se15_spi_pins: qupv3_se15_spi_pins {
			qupv3_se15_spi_active: qupv3_se15_spi_active {
				mux {
					pins = "gpio44", "gpio45", "gpio46",
								"gpio47";
					function = "qup15";
				};

				config {
					pins = "gpio44", "gpio45", "gpio46",
								"gpio47";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se15_spi_sleep: qupv3_se15_spi_sleep {
				mux {
					pins = "gpio44", "gpio45", "gpio46",
								"gpio47";
					function = "gpio";
				};

				config {
					pins = "gpio44", "gpio45", "gpio46",
								"gpio47";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se16_spi_pins: qupv3_se16_spi_pins {
			qupv3_se16_spi_active: qupv3_se16_spi_active {
				mux {
					pins = "gpio48", "gpio49", "gpio50",
								"gpio51";
					function = "qup16";
				};

				config {
					pins = "gpio48", "gpio49", "gpio50",
								"gpio51";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se16_spi_sleep: qupv3_se16_spi_sleep {
				mux {
					pins = "gpio48", "gpio49", "gpio50",
								"gpio51";
					function = "gpio";
				};

				config {
					pins = "gpio48", "gpio49", "gpio50",
								"gpio51";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se17_spi_pins: qupv3_se17_spi_pins {
			qupv3_se17_spi_active: qupv3_se17_spi_active {
				mux {
					pins = "gpio52", "gpio53", "gpio54",
								"gpio55";
					function = "qup17";
				};

				config {
					pins = "gpio52", "gpio53", "gpio54",
								"gpio55";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se17_spi_sleep: qupv3_se17_spi_sleep {
				mux {
					pins = "gpio52", "gpio53", "gpio54",
								"gpio55";
					function = "gpio";
				};

				config {
					pins = "gpio52", "gpio53", "gpio54",
								"gpio55";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se18_spi_pins: qupv3_se18_spi_pins {
			qupv3_se18_spi_active: qupv3_se18_spi_active {
				mux {
					pins = "gpio56", "gpio57", "gpio58",
								"gpio59";
					function = "qup18";
				};

				config {
					pins = "gpio56", "gpio57", "gpio58",
								"gpio59";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se18_spi_sleep: qupv3_se18_spi_sleep {
				mux {
					pins = "gpio56", "gpio57", "gpio58",
								"gpio59";
					function = "gpio";
				};

				config {
					pins = "gpio56", "gpio57", "gpio58",
								"gpio59";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se19_spi_pins: qupv3_se19_spi_pins {
			qupv3_se19_spi_active: qupv3_se19_spi_active {
				mux {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					function = "qup19";
				};

				config {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se19_spi_sleep: qupv3_se19_spi_sleep {
				mux {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					function = "gpio";
				};

				config {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		usb2_id_det_default: usb2_id_det_default {
			config {
				pins = "gpio91";
				function = "gpio";
				input-enable;
				bias-pull-up;
			};
		};

		wil6210_refclk_en_pin: wil6210_refclk_en_pin {
			mux {
				pins = "gpio14";
				function = "gpio";
			};

			config {
				pins = "gpio14";
				bias-pull-down;         /* PULL DOWN */
				drive-strength = <2>;   /* 2 MA */
			};
		};
	};
};
