&soc {
	tlmm: pinctrl@03000000 {
		compatible = "qcom,sm6150-pinctrl";
		reg = <0x03000000 0xdc2000>, <0x17c000f0 0x50>;
		reg-names = "pinctrl", "spi_cfg";
		interrupts = <GIC_SPI 208 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 209 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 210 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 211 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 212 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 213 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 214 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 215 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 216 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;

		ufs_dev_reset_assert: ufs_dev_reset_assert {
			config {
				pins = "ufs_reset";
				bias-pull-down;		/* default: pull down */
				/*
				 * UFS_RESET driver strengths are having
				 * different values/steps compared to typical
				 * GPIO drive strengths.
				 *
				 * Following table clarifies:
				 *
				 * HDRV value | UFS_RESET | Typical GPIO
				 *   (dec)    |   (mA)    |    (mA)
				 *     0      |   0.8     |    2
				 *     1      |   1.55    |    4
				 *     2      |   2.35    |    6
				 *     3      |   3.1     |    8
				 *     4      |   3.9     |    10
				 *     5      |   4.65    |    12
				 *     6      |   5.4     |    14
				 *     7      |   6.15    |    16
				 *
				 * POR value for UFS_RESET HDRV is 3 which means
				 * 3.1mA and we want to use that. Hence just
				 * specify 8mA to "drive-strength" binding and
				 * that should result into writing 3 to HDRV
				 * field.
				 */
				drive-strength = <8>;	/* default: 3.1 mA */
				output-low; /* active low reset */
			};
		};

		ufs_dev_reset_deassert: ufs_dev_reset_deassert {
			config {
				pins = "ufs_reset";
				bias-pull-down;		/* default: pull down */
				/*
				 * default: 3.1 mA
				 * check comments under ufs_dev_reset_assert
				 */
				drive-strength = <8>;
				output-high; /* active low reset */
			};
		};

		/* QUPv3_0 South SE mappings */
		/* SE 0 pin mappings */
		qupv3_se0_2uart_pins: qupv3_se0_2uart_pins {
			qupv3_se0_2uart_active: qupv3_se0_2uart_active {
				mux {
					pins = "gpio16", "gpio17";
					function = "qup00";
				};

				config {
					pins = "gpio16", "gpio17";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se0_2uart_sleep: qupv3_se0_2uart_sleep {
				mux {
					pins = "gpio16", "gpio17";
					function = "gpio";
				};

				config {
					pins = "gpio16", "gpio17";
					drive-strength = <2>;
					bias-disable;
				};
			};
		};

		/* SE 1 pin mappings */
		qupv3_se1_i2c_pins: qupv3_se1_i2c_pins {
			qupv3_se1_i2c_active: qupv3_se1_i2c_active {
				mux {
					pins = "gpio4", "gpio5";
					function = "qup01";
				};

				config {
					pins = "gpio4", "gpio5";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se1_i2c_sleep: qupv3_se1_i2c_sleep {
				mux {
					pins = "gpio4", "gpio5";
					function = "gpio";
				};

				config {
					pins = "gpio4", "gpio5";
					drive-strength = <2>;
					bias-no-pull;
				};
			};
		};

		/* SE 2 pin mappings */
		qupv3_se2_i2c_pins: qupv3_se2_i2c_pins {
			qupv3_se2_i2c_active: qupv3_se2_i2c_active {
				mux {
					pins = "gpio0", "gpio1";
					function = "qup02";
				};

				config {
					pins = "gpio0", "gpio1";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se2_i2c_sleep: qupv3_se2_i2c_sleep {
				mux {
					pins = "gpio0", "gpio1";
					function = "gpio";
				};

				config {
					pins = "gpio0", "gpio1";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se2_spi_pins: qupv3_se2_spi_pins {
			qupv3_se2_spi_active: qupv3_se2_spi_active {
				mux {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					function = "qup02";
				};

				config {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se2_spi_sleep: qupv3_se2_spi_sleep {
				mux {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					function = "gpio";
				};

				config {
					pins = "gpio0", "gpio1", "gpio2",
								"gpio3";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		fpc_reset_int {
			fpc_reset_low: reset_low {
				mux {
					pins = "gpio101";
					function = "gpio";
				};

				config {
					pins = "gpio101";
					drive-strength = <2>;
					bias-disable;
					output-low;
				};
			};

			fpc_reset_high: reset_high {
				mux {
					pins = "gpio101";
					function = "gpio";
				};

				config {
					pins = "gpio101";
					drive-strength = <2>;
					bias-disable;
					output-high;
				};
			};

			fpc_int_low: int_low {
				mux {
					pins = "gpio93";
					function = "gpio";
				};

				config {
					pins = "gpio93";
					drive-strength = <2>;
					bias-pull-down;
					input-enable;
				};
			};
		};

		/* SE 3 pin mappings */
		qupv3_se3_i2c_pins: qupv3_se3_i2c_pins {
			qupv3_se3_i2c_active: qupv3_se3_i2c_active {
				mux {
					pins = "gpio18", "gpio19";
					function = "qup03";
				};

				config {
					pins = "gpio18", "gpio19";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se3_i2c_sleep: qupv3_se3_i2c_sleep {
				mux {
					pins = "gpio18", "gpio19";
					function = "gpio";
				};

				config {
					pins = "gpio18", "gpio19";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		ss5_pwr_ctrl_pins: ss5_pwr_ctrl_pins {
			ss5_pwr_ctrl_rst_on: ss5_pwr_ctrl_rst_on {
				mux {
					pins = "gpio87", "gpio20", "gpio21";
					function = "gpio";
				};

				config {
					pins = "gpio87", "gpio20", "gpio21";
					drive-strength = <16>; /* 16 mA */
					bias-pull-up;
					output-high;
				};
			};

			ss5_pwr_ctrl_rst_off: ss5_pwr_ctrl_off {
				mux {
					pins = "gpio87", "gpio20", "gpio21";
					function = "gpio";
				};

				config {
					pins = "gpio87", "gpio20", "gpio21";
					drive-strength = <16>; /* 16 mA */
					bias-pull-up;
					output-high;
				};
			};
		};

		/* QUPv3_1 North instances */
		/* SE 4 pin mappings */
		qupv3_se4_i2c_pins: qupv3_se4_i2c_pins {
			qupv3_se4_i2c_active: qupv3_se4_i2c_active {
				mux {
					pins = "gpio20", "gpio21";
					function = "qup10";
				};

				config {
					pins = "gpio20", "gpio21";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se4_i2c_sleep: qupv3_se4_i2c_sleep {
				mux {
					pins = "gpio20", "gpio21";
					function = "gpio";
				};

				config {
					pins = "gpio20", "gpio21";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se4_spi_pins: qupv3_se4_spi_pins {
			qupv3_se4_spi_active: qupv3_se4_spi_active {
				mux {
					pins = "gpio20", "gpio21", "gpio22",
								"gpio23";
					function = "qup10";
				};

				config {
					pins = "gpio20", "gpio21", "gpio22",
								"gpio23";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se4_spi_sleep: qupv3_se4_spi_sleep {
				mux {
					pins = "gpio20", "gpio21", "gpio22",
								"gpio23";
					function = "gpio";
				};

				config {
					pins = "gpio20", "gpio21", "gpio22",
								"gpio23";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se4_2uart_pins: qupv3_se4_2uart_pins {
			qupv3_se4_2uart_active: qupv3_se4_2uart_active {
				mux {
					pins = "gpio22", "gpio23";
					function = "qup10";
				};

				config {
					pins = "gpio22", "gpio23";
					drive-strength = <16>;
					bias-disable;
				};
			};

			qupv3_se4_2uart_sleep: qupv3_se4_2uart_sleep {
				mux {
					pins = "gpio22", "gpio23";
					function = "gpio";
				};

				config {
					pins = "gpio22", "gpio23";
					drive-strength = <16>;
					bias-disable;
				};
			};
		};

		/* SE 5 pin mappings */
		qupv3_se5_i2c_pins: qupv3_se5_i2c_pins {
			qupv3_se5_i2c_active: qupv3_se5_i2c_active {
				mux {
					pins = "gpio14", "gpio15";
					function = "qup11";
				};

				config {
					pins = "gpio14", "gpio15";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se5_i2c_sleep: qupv3_se5_i2c_sleep {
				mux {
					pins = "gpio14", "gpio15";
					function = "gpio";
				};

				config {
					pins = "gpio14", "gpio15";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		nfc {
			nfc_int_active: nfc_int_active {
				/* active state */
				mux {
					/* GPIO 86 NFC Read Interrupt */
					pins = "gpio86";
					function = "gpio";
				};

				config {
					pins = "gpio86";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_int_suspend: nfc_int_suspend {
				/* sleep state */
				mux {
					/* GPIO 86 NFC Read Interrupt */
					pins = "gpio86";
					function = "gpio";
				};

				config {
					pins = "gpio86";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_enable_active: nfc_enable_active {
				/* active state */
				mux {
					/* 84: Enable 85: Firmware */
					pins = "gpio84", "gpio85";
					function = "gpio";
				};

				config {
					pins = "gpio84", "gpio85";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_enable_suspend: nfc_enable_suspend {
				/* sleep state */
				mux {
					/* 84: Enable 85: Firmware */
					pins = "gpio84", "gpio85";
					function = "gpio";
				};

				config {
					pins = "gpio84", "gpio85";
					drive-strength = <2>; /* 2 MA */
					bias-disable;
				};
			};

			nfc_clk_req_active: nfc_clk_req_active {
				/* active state */
				mux {
					/* GPIO 50: NFC CLOCK REQUEST */
					pins = "gpio50";
					function = "gpio";
				};

				config {
					pins = "gpio50";
					drive-strength = <2>; /* 2 MA */
					bias-pull-up;
				};
			};

			nfc_clk_req_suspend: nfc_clk_req_suspend {
				/* sleep state */
				mux {
					/* GPIO 50: NFC CLOCK REQUEST */
					pins = "gpio50";
					function = "gpio";
				};

				config {
					pins = "gpio50";
					drive-strength = <2>; /* 2 MA */
					bias-disable;
				};
			};
		};

		/* SE 6 pin mappings */
		qupv3_se6_i2c_pins: qupv3_se6_i2c_pins {
			qupv3_se6_i2c_active: qupv3_se6_i2c_active {
				mux {
					pins = "gpio6", "gpio7";
					function = "qup12";
				};

				config {
					pins = "gpio6", "gpio7";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se6_i2c_sleep: qupv3_se6_i2c_sleep {
				mux {
					pins = "gpio6", "gpio7";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio7";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se6_spi_pins: qupv3_se6_spi_pins {
			qupv3_se6_spi_active: qupv3_se6_spi_active {
				mux {
					pins = "gpio6", "gpio7", "gpio8",
								"gpio9";
					function = "qup12";
				};

				config {
					pins = "gpio6", "gpio7", "gpio8",
								"gpio9";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se6_spi_sleep: qupv3_se6_spi_sleep {
				mux {
					pins = "gpio6", "gpio7", "gpio8",
								"gpio9";
					function = "gpio";
				};

				config {
					pins = "gpio6", "gpio7", "gpio8",
								"gpio9";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		/* SE 7 pin mappings */
		qupv3_se7_i2c_pins: qupv3_se7_i2c_pins {
			qupv3_se7_i2c_active: qupv3_se7_i2c_active {
				mux {
					pins = "gpio10", "gpio11";
					function = "qup13";
				};

				config {
					pins = "gpio10", "gpio11";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se7_i2c_sleep: qupv3_se7_i2c_sleep {
				mux {
					pins = "gpio10", "gpio11";
					function = "gpio";
				};

				config {
					pins = "gpio10", "gpio11";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		qupv3_se7_spi_pins: qupv3_se7_spi_pins {
			qupv3_se7_spi_active: qupv3_se7_spi_active {
				mux {
					pins = "gpio10", "gpio11", "gpio12",
								"gpio13";
					function = "qup13";
				};

				config {
					pins = "gpio10", "gpio11", "gpio12",
								"gpio13";
					drive-strength = <6>;
					bias-disable;
				};
			};

			qupv3_se7_spi_sleep: qupv3_se7_spi_sleep {
				mux {
					pins = "gpio10", "gpio11", "gpio12",
								"gpio13";
					function = "gpio";
				};

				config {
					pins = "gpio10", "gpio11", "gpio12",
								"gpio13";
					drive-strength = <6>;
					bias-disable;
				};
			};
		};

		qupv3_se7_4uart_pins: qupv3_se7_4uart_pins {
			qupv3_se7_ctsrx: qupv3_se7_ctsrx {
				mux {
					pins = "gpio10", "gpio13";
					function = "qup13";
				};

				config {
					pins = "gpio10", "gpio13";
					drive-strength = <2>;
					bias-disable;
				};
			};

			qupv3_se7_rts: qupv3_se7_rts {
				mux {
					pins = "gpio11";
					function = "qup13";
				};

				config {
					pins = "gpio11";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			qupv3_se7_tx: qupv3_se7_tx {
				mux {
					pins = "gpio12";
					function = "qup13";
				};

				config {
					pins = "gpio12";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		lt9611_pins: lt9611_pins {
			mux {
				pins = "gpio26", "gpio20", "gpio79";
				function = "gpio";
			};

			config {
				pins = "gpio26", "gpio20", "gpio79";
				drive-strength = <8>;
				bias-disable = <0>;   /* no pull */
			};
		};

		pmx_sde: pmx_sde {
			sde_dsi_active: sde_dsi_active {
				mux {
					pins = "gpio91";
					function = "gpio";
				};

				config {
					pins = "gpio91";
					drive-strength = <8>;   /* 8 mA */
					bias-disable = <0>;   /* no pull */
				};
			};

			sde_dsi_suspend: sde_dsi_suspend {
				mux {
					pins = "gpio91";
					function = "gpio";
				};

				config {
					pins = "gpio91";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};
		};

		fsa_usbc_ana_en_n@114 {
			fsa_usbc_ana_en: fsa_usbc_ana_en {
				mux {
					pins = "gpio114";
					function = "gpio";
				};

				config {
					pins = "gpio114";
					drive-strength = <2>;
					bias-disable;
					output-low;
				};
			};
		};

		pmx_sde_te {
			sde_te_active: sde_te_active {
				mux {
					pins = "gpio90";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio90";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};

			sde_te_suspend: sde_te_suspend {
				mux {
					pins = "gpio90";
					function = "mdp_vsync";
				};

				config {
					pins = "gpio90";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;         /* PULL DOWN */
				};
			};
		};

		sde_dp_usbplug_cc_active: sde_dp_usbplug_cc_active {
			mux {
				pins = "gpio104";
				function = "gpio";
			};

			config {
				pins = "gpio104";
				bias-disable;
				drive-strength = <16>;
			};
		};

		sde_dp_usbplug_cc_suspend: sde_dp_usbplug_cc_suspend {
			mux {
				pins = "gpio104";
				function = "gpio";
			};

			config {
				pins = "gpio104";
				bias-pull-down;
				drive-strength = <2>;
			};
		};

		sde_dp_switch_active: sde_dp_switch_active {
			mux {
				pins = "gpio49";
				function = "gpio";
			};

			config {
				pins = "gpio49";
				bias-pull-up;		/* pull up */
				output-high;
				drive-strength = <2>;
			};
		};

		sde_dp_switch_suspend: sde_dp_switch_suspend {
			mux {
				pins = "gpio49";
				function = "gpio";
			};

			config {
				pins = "gpio49";
				bias-pull-down;
				output-low;
				drive-strength = <2>;
			};
		};

		sde_dp_connector_enable: sde_dp_connector_enable {
			mux {
				pins = "gpio44";
				function = "gpio";
			};

			config {
				pins = "gpio44";
				bias-pull-up;
				output-high;
				drive-strength = <2>;
			};
		};

		sde_dp_hotplug_ctrl: sde_dp_hotplug_ctrl {
			mux {
				pins = "gpio103";
				function = "debug_hot";
			};

			config {
				pins = "gpio103";
				bias-disable;
				input-enable;
				drive-strength = <2>;
			};
		};

		sde_dp_hotplug_tlmm: sde_dp_hotplug_tlmm {
			mux {
				pins = "gpio103";
				function = "gpio";
			};

			config {
				pins = "gpio103";
				bias-disable;
				input-enable;
				drive-strength = <2>;
			};
		};

		sdc1_on: sdc1_on {
			clk {
				pins = "sdc1_clk";
				bias-disable;
				drive-strength = <16>;
			};

			cmd {
				pins = "sdc1_cmd";
				bias-pull-up;
				drive-strength = <10>;
			};

			data {
				pins = "sdc1_data";
				bias-pull-up;
				drive-strength = <10>;
			};

			rclk {
				pins = "sdc1_rclk";
				bias-pull-down;
			};
		};

		sdc1_off: sdc1_off {
			clk {
				pins = "sdc1_clk";
				bias-disable;
				drive-strength = <2>;
			};

			cmd {
				pins = "sdc1_cmd";
				bias-pull-up;
				drive-strength = <2>;
			};

			data {
				pins = "sdc1_data";
				bias-pull-up;
				drive-strength = <2>;
			};

			rclk {
				pins = "sdc1_rclk";
				bias-pull-down;
			};
		};

		sdc2_on: sdc2_on {
			clk {
				pins = "sdc2_clk";
				bias-disable;		/* NO pull */
				drive-strength = <16>;	/* 16 MA */
			};

			cmd {
				pins = "sdc2_cmd";
				bias-pull-up;		/* pull up */
				drive-strength = <10>;	/* 10 MA */
			};

			data {
				pins = "sdc2_data";
				bias-pull-up;		/* pull up */
				drive-strength = <10>;	/* 10 MA */
			};

			sd-cd {
				pins = "gpio99";
				bias-pull-up;           /* pull up */
				drive-strength = <2>;   /* 2 MA */
			};
		};

		sdc2_off: sdc2_off {
			clk {
				pins = "sdc2_clk";
				bias-disable;		/* NO pull */
				drive-strength = <2>;	/* 2 MA */
			};

			cmd {
				pins = "sdc2_cmd";
				bias-pull-up;		/* pull up */
				drive-strength = <2>;	/* 2 MA */
			};

			data {
				pins = "sdc2_data";
				bias-pull-up;		/* pull up */
				drive-strength = <2>;	/* 2 MA */
			};

			sd-cd {
				pins = "gpio99";
				bias-disable;           /* pull up */
				drive-strength = <2>;   /* 2 MA */
			};
		};

		cnss_pins {
			cnss_wlan_en_active: cnss_wlan_en_active {
				mux {
					pins = "gpio98";
					function = "gpio";
				};

				config {
					pins = "gpio98";
					drive-strength = <16>;
					output-high;
					bias-pull-up;
				};
			};

			cnss_wlan_en_sleep: cnss_wlan_en_sleep {
				mux {
					pins = "gpio98";
					function = "gpio";
				};

				config {
					pins = "gpio98";
					drive-strength = <2>;
					output-low;
					bias-pull-down;
				};
			};
		};

		wsa_swr_clk_pin {
			wsa_swr_clk_sleep: wsa_swr_clk_sleep {
				mux {
					pins = "gpio111";
					function = "WSA_CLK";
				};

				config {
					pins = "gpio111";
					drive-strength = <2>;
					bias-bus-hold;
				};
			};

			wsa_swr_clk_active: wsa_swr_clk_active {
				mux {
					pins = "gpio111";
					function = "WSA_CLK";
				};

				config {
					pins = "gpio111";
					drive-strength = <2>;
					bias-bus-hold;
				};
			};
		};

		wsa_swr_data_pin {
			wsa_swr_data_sleep: wsa_swr_data_sleep {
				mux {
					pins = "gpio110";
					function = "WSA_DATA";
				};

				config {
					pins = "gpio110";
					drive-strength = <4>;
					bias-bus-hold;
				};
			};

			wsa_swr_data_active: wsa_swr_data_active {
				mux {
					pins = "gpio110";
					function = "WSA_DATA";
				};

				config {
					pins = "gpio110";
					drive-strength = <4>;
					bias-bus-hold;
				};
			};
		};

		/* WSA speaker reset pins */
		spkr_1_sd_n {
			spkr_1_sd_n_sleep: spkr_1_sd_n_sleep {
				mux {
					pins = "gpio108";
					function = "gpio";
				};

				config {
					pins = "gpio108";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;
					input-enable;
				};
			};

			spkr_1_sd_n_active: spkr_1_sd_n_active {
				mux {
					pins = "gpio108";
					function = "gpio";
				};

				config {
					pins = "gpio108";
					drive-strength = <16>;   /* 16 mA */
					bias-disable;
					output-high;
				};
			};
		};

		spkr_2_sd_n {
			spkr_2_sd_n_sleep: spkr_2_sd_n_sleep {
				mux {
					pins = "gpio109";
					function = "gpio";
				};

				config {
					pins = "gpio109";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-down;
					input-enable;
				};
			};

			spkr_2_sd_n_active: spkr_2_sd_n_active {
				mux {
					pins = "gpio109";
					function = "gpio";
				};

				config {
					pins = "gpio109";
					drive-strength = <16>;   /* 16 mA */
					bias-disable;
					output-high;
				};
			};
		};

		wcd9xxx_intr {
			wcd_intr_default: wcd_intr_default {
				mux {
					pins = "gpio122";
					function = "gpio";
				};

				config {
					pins = "gpio122";
					drive-strength = <2>; /* 2 mA */
					bias-pull-down; /* pull down */
					input-enable;
				};
			};
		};

		tert_i2s_sck_ws_d0 {
			tert_i2s_sck_ws_d0_sleep: tert_i2s_sck_ws_do_sleep {
				mux {
					pins = "gpio115", "gpio116", "gpio117";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio115", "gpio116", "gpio117";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			tert_i2s_sck_ws_d0_active: tert_i2s_sck_ws_do_active {
				mux {
					pins = "gpio115", "gpio116", "gpio117";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio115", "gpio116", "gpio117";
					drive-strength = <8>;   /* 8 mA */
					bias-disable;
					output-high;
					input-enable;
				};
			};
		};

		ter_i2s_sck_ws {
			ter_i2s_sck_sleep: ter_i2s_sck_sleep {
				mux {
					pins = "gpio115", "gpio116";
					function = "gpio";
				};

				config {
					pins = "gpio115", "gpio116";
					drive-strength = <2>;   /* 2 mA */
					bias-disable;
				};
			};

			ter_i2s_sck_active: ter_i2s_sck_active {
				mux {
					pins = "gpio115", "gpio116";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio115", "gpio116";
					drive-strength = <8>;   /* 8 mA */
					output-high;
					bias-disable;
				};
			};
		};

		ter_i2s_data0 {
			ter_i2s_data0_sleep: ter_i2s_data0_sleep {
				mux {
					pins = "gpio117";
					function = "gpio";
				};

				config {
					pins = "gpio117";
					drive-strength = <2>;   /* 2 mA */
					bias-pull-up;
				};
			};

			ter_i2s_data0_active: ter_i2s_data0_active {
				mux {
					pins = "gpio117";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio117";
					drive-strength = <2>;   /* 8 mA */
					input-enable;
					bias-disable;
				};
			};
		};

		ter_i2s_data1 {
			ter_i2s_data1_sleep: ter_i2s_data1_sleep {
				mux {
					pins = "gpio118";
					function = "gpio";
				};

				config {
					pins = "gpio118";
					drive-strength = <2>;   /* 2 mA */
					bias-disable;
				};
			};

			ter_i2s_data1_active: ter_i2s_data1_active {
				mux {
					pins = "gpio118";
					function = "ter_mi2s";
				};

				config {
					pins = "gpio118";
					drive-strength = <8>;   /* 8 mA */
					output-high;
					bias-disable;
				};
			};
		};

		pcie0 {
			pcie0_clkreq_default: pcie0_clkreq_default {
				mux {
					pins = "gpio90";
					function = "pcie_clk";
				};

				config {
					pins = "gpio90";
					drive-strength = <2>;
					bias-pull-up;
				};
			};

			pcie0_perst_default: pcie0_perst_default {
				mux {
					pins = "gpio101";
					function = "gpio";
				};

				config {
					pins = "gpio101";
					drive-strength = <2>;
					bias-pull-down;
				};
			};

			pcie0_wake_default: pcie0_wake_default {
				mux {
					pins = "gpio100";
					function = "gpio";
				};

				config {
					pins = "gpio100";
					drive-strength = <2>;
					bias-pull-up;
				};
			};
		};

		pri_aux_pcm_sck {
			pri_aux_pcm_sck_sleep: pri_aux_pcm_sck_sleep {
				mux {
					pins = "gpio108";
					function = "mi2s_1";
				};

				config {
					pins = "gpio108";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			pri_aux_pcm_sck_active: pri_aux_pcm_sck_active {
				mux {
					pins = "gpio108";
					function = "mi2s_1";
				};

				config {
					pins = "gpio108";
					drive-strength = <8>;   /* 8 mA */
					input-enable;
				};
			};
		};

		pri_aux_pcm_ws {
			pri_aux_pcm_ws_sleep: pri_aux_pcm_ws_sleep {
				mux {
					pins = "gpio109";
					function = "mi2s_1";
				};

				config {
					pins = "gpio109";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			pri_aux_pcm_ws_active: pri_aux_pcm_ws_active {
				mux {
					pins = "gpio109";
					function = "mi2s_1";
				};

				config {
					pins = "gpio109";
					drive-strength = <8>;   /* 8 mA */
					input-enable;
				};
			};
		};

		pri_aux_pcm_data0 {
			pri_aux_pcm_data0_sleep: pri_aux_pcm_data0_sleep {
				mux {
					pins = "gpio110";
					function = "mi2s_1";
				};

				config {
					pins = "gpio110";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			pri_aux_pcm_data0_active: pri_aux_pcm_data0_active {
				mux {
					pins = "gpio110";
					function = "mi2s_1";
				};

				config {
					pins = "gpio110";
					drive-strength = <8>;   /* 8 mA */
					input-enable;
				};
			};
		};

		pri_aux_pcm_data1 {
			pri_aux_pcm_data1_sleep: pri_aux_pcm_data1_sleep {
				mux {
					pins = "gpio111";
					function = "mi2s_1";
				};

				config {
					pins = "gpio111";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			pri_aux_pcm_data1_active: pri_aux_pcm_data1_active {
				mux {
					pins = "gpio111";
					function = "mi2s_1";
				};

				config {
					pins = "gpio111";
					drive-strength = <8>;   /* 8 mA */
					output-high;
				};
			};
		};

		audio_internal_mclk2_active: audio_internal_mclk2_active {
			mux {
				pins = "gpio122";
				function = "mclk2";
			};

			config {
				pins = "gpio122";
				drive-strength = <2>;
				bias-disable;
			};
		};

		audio_internal_mclk2_sleep: audio_internal_mclk2_sleep {
			mux {
				pins = "gpio122";
				function = "mclk2";
			};

			config {
				pins = "gpio122";
				drive-strength = <2>;
				bias-pull-down;
			};
		};

		pmx_ts_int_active {
			ts_int_active: ts_int_active {
				mux {
					pins = "gpio89";
					function = "gpio";
				};

				config {
					pins = "gpio89";
					drive-strength = <8>;
					bias-pull-up;
				};
			};
		};

		pmx_ts_int_suspend {
			ts_int_suspend: ts_int_suspend {
				mux {
					pins = "gpio89";
					function = "gpio";
				};

				config {
					pins = "gpio89";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		pmx_ts_reset_active {
			ts_reset_active: ts_reset_active {
				mux {
					pins = "gpio88";
					function = "gpio";
				};

				config {
					pins = "gpio88";
					drive-strength = <8>;
					bias-pull-up;
				};
			};
		};

		pmx_ts_reset_suspend {
			ts_reset_suspend: ts_reset_suspend {
				mux {
					pins = "gpio88";
					function = "gpio";
				};

				config {
					pins = "gpio88";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		pmx_ts_release {
			ts_release: ts_release {
				mux {
					pins = "gpio89", "gpio88";
					function = "gpio";
				};

				config {
					pins = "gpio89", "gpio88";
					drive-strength = <2>;
					bias-pull-down;
				};
			};
		};

		cci0_active: cci0_active {
			mux {
				/* CLK, DATA */
				pins = "gpio32", "gpio33";
				function = "cci_i2c";
			};

			config {
				pins = "gpio32", "gpio33";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci0_suspend: cci0_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio32", "gpio33";
				function = "cci_i2c";
			};

			config {
				pins = "gpio32", "gpio33";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci1_active: cci1_active {
			mux {
				/* CLK, DATA */
				pins = "gpio34", "gpio35";
				function = "cci_i2c";
			};

			config {
				pins = "gpio34", "gpio35";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cci1_suspend: cci1_suspend {
			mux {
				/* CLK, DATA */
				pins = "gpio34", "gpio35";
				function = "cci_i2c";
			};

			config {
				pins = "gpio34", "gpio35";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk0_active: cam_sensor_mclk0_active {
			/* MCLK0 */
			mux {
				pins = "gpio28";
				function = "cam_mclk";
			};

			config {
				pins = "gpio28";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk0_suspend: cam_sensor_mclk0_suspend {
			/* MCLK0 */
			mux {
				pins = "gpio28";
				function = "cam_mclk";
			};

			config {
				pins = "gpio28";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rear_active: cam_sensor_rear_active {
			/* RESET */
			mux {
				pins = "gpio47";
				function = "gpio";
			};

			config {
				pins = "gpio47";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rear_suspend: cam_sensor_rear_suspend {
			/* RESET */
			mux {
				pins = "gpio47";
				function = "gpio";
			};

			config {
				pins = "gpio47";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_front_active: cam_sensor_front_active {
			/* RESET  */
			mux {
				pins = "gpio37";
				function = "gpio";
			};

			config {
				pins = "gpio37";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_front_suspend: cam_sensor_front_suspend {
			/* RESET */
			mux {
				pins = "gpio37";
				function = "gpio";
			};

			config {
				pins = "gpio37";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_rear2_active: cam_sensor_rear2_active {
			/* RESET */
			mux {
				pins = "gpio45";
				function = "gpio";
			};

			config {
				pins = "gpio45";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_rear2_suspend: cam_sensor_rear2_suspend {
			/* RESET */
			mux {
				pins = "gpio45";
				function = "gpio";
			};

			config {
				pins = "gpio45";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
				output-low;
			};
		};

		cam_sensor_mclk1_active: cam_sensor_mclk1_active {
			/* MCLK1 */
			mux {
				pins = "gpio29";
				function = "cam_mclk";
			};

			config {
				pins = "gpio29";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk1_suspend: cam_sensor_mclk1_suspend {
			/* MCLK1 */
			mux {
				pins = "gpio29";
				function = "cam_mclk";
			};

			config {
				pins = "gpio29";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk2_active: cam_sensor_mclk2_active {
			/* MCLK2 */
			mux {
				pins = "gpio30";
				function = "cam_mclk";
			};

			config {
				pins = "gpio30";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk2_suspend: cam_sensor_mclk2_suspend {
			/* MCLK2 */
			mux {
				pins = "gpio30";
				function = "cam_mclk";
			};

			config {
				pins = "gpio30";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk3_active: cam_sensor_mclk3_active {
			/* MCLK3 */
			mux {
				pins = "gpio31";
				function = "cam_mclk";
			};

			config {
				pins = "gpio31";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_mclk3_suspend: cam_sensor_mclk3_suspend {
			/* MCLK3 */
			mux {
				pins = "gpio31";
				function = "cam_mclk";
			};

			config {
				pins = "gpio31";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};


		cam_sensor0_active: cam_sensor0_active {
			/* intr gpio for bridge chip 0 */
			mux {
				pins = "gpio43";
				function = "gpio";
			};

			config {
				pins = "gpio43";
				bias-pull-up; /* PULL UP */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor0_suspend: cam_sensor0_suspend {
			/* intr gpio for bridge chip 0 */
			mux {
				pins = "gpio43";
				function = "gpio";
			};

			config {
				pins = "gpio43";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor1_active: cam_sensor1_active {
			/* intr gpio for bridge chip 1 */
			mux {
				pins = "gpio31";
				function = "gpio";
			};

			config {
				pins = "gpio31";
				bias-pull-up; /* PULL UP*/
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor1_suspend: cam_sensor1_suspend {
			/* intr gpio for bridge chip 1 */
			mux {
				pins = "gpio31";
				function = "gpio";
			};

			config {
				pins = "gpio31";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		flash_led3_front {
			flash_led3_front_en: flash_led3_front_en {
				mux {
					pins = "gpio38";
					function = "gpio";
				};

				config {
					pins = "gpio38";
					drive_strength = <2>;
					output-high;
					bias-disable;
				};
			};

			flash_led3_front_dis: flash_led3_front_dis {
				mux {
					pins = "gpio38";
					function = "gpio";
				};

				config {
					pins = "gpio38";
					drive_strength = <2>;
					output-low;
					bias-disable;
				};
			};
		};

		cam_sensor_ir_cut_on: cam_sensor_ir_led_on {
			/*IR_LED*/
			mux {
				pins = "gpio73", "gpio74";
				function = "gpio";
			};

			config {
				pins = "gpio73", "gpio74";
				bias-disable; /* No PULL */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_ir_cut_off: cam_sensor_ir_led_off {
			/*IR_LED*/
			mux {
				pins = "gpio73", "gpio74";
				function = "gpio";
			};

			config {
				pins = "gpio73", "gpio74";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		cam_sensor_dvdd_en: cam_sensor_dvdd_en {
			mux {
				pins = "gpio9";
				function = "gpio";
			};

			config {
				pins = "gpio9";
				bias-pull-down; /* PULL DOWN */
				drive-strength = <2>; /* 2 MA */
			};
		};

		hs0_i2s_sck_ws {
			hs0_i2s_sck_sleep: hs0_i2s_sck_sleep {
				mux {
					pins = "gpio36", "gpio37";
					function = "hs0_mi2s";
				};

				config {
					pins = "gpio36", "gpio37";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			hs0_i2s_sck_active: hs0_i2s_sck_active {
				mux {
					pins = "gpio36", "gpio37";
					function = "hs0_mi2s";
				};

				config {
					pins = "gpio36", "gpio37";
					drive-strength = <4>;   /* 4 mA */
					bias-no-pull;
					input-enable;
				};
			};
		};

		hs0_i2s_data0 {
			hs0_i2s_data0_sleep: hs0_i2s_data0_sleep {
				mux {
					pins = "gpio38";
					function = "hs0_mi2s";
				};

				config {
					pins = "gpio38";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			hs0_i2s_data0_active: hs0_i2s_data0_active {
				mux {
					pins = "gpio38";
					function = "hs0_mi2s";
				};

				config {
					pins = "gpio38";
					drive-strength = <4>;   /* 4 mA */
					bias-no-pull;
					input-enable;
				};
			};
		};

		hs0_i2s_data1 {
			hs0_i2s_data1_sleep: hs0_i2s_data1_sleep {
				mux {
					pins = "gpio39";
					function = "hs0_mi2s";
				};

				config {
					pins = "gpio39";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			hs0_i2s_data1_active: hs0_i2s_data1_active {
				mux {
					pins = "gpio39";
					function = "hs0_mi2s";
				};

				config {
					pins = "gpio39";
					drive-strength = <4>;   /* 4 mA */
					bias-no-pull;
					input-enable;
				};
			};
		};

		hs1_i2s_sck_ws {
			hs1_i2s_sck_sleep: hs1_i2s_sck_sleep {
				mux {
					pins = "gpio24", "gpio25";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio24", "gpio25";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			hs1_i2s_sck_active: hs1_i2s_sck_active {
				mux {
					pins = "gpio24", "gpio25";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio24", "gpio25";
					drive-strength = <4>;   /* 4 mA */
					bias-no-pull;
					input-enable;
				};
			};
		};

		hs1_i2s_data0 {
			hs1_i2s_data0_sleep: hs1_i2s_data0_sleep {
				mux {
					pins = "gpio26";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio26";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			hs1_i2s_data0_active: hs1_i2s_data0_active {
				mux {
					pins = "gpio26";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio26";
					drive-strength = <4>;   /* 4 mA */
					bias-no-pull;
					input-enable;
				};
			};
		};

		hs1_i2s_data1 {
			hs1_i2s_data1_sleep: hs1_i2s_data1_sleep {
				mux {
					pins = "gpio27";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio27";
					drive-strength = <2>;   /* 2 mA */
				};
			};

			hs1_i2s_data1_active: hs1_i2s_data1_active {
				mux {
					pins = "gpio27";
					function = "hs1_mi2s";
				};

				config {
					pins = "gpio27";
					drive-strength = <4>;   /* 4 mA */
					bias-no-pull;
					input-enable;
				};
			};
		};

		emac {
			emac_mdc: emac_mdc {
				mux {
					pins = "gpio113";
					function = "rgmii_mdc";
				};

				config {
					pins = "gpio113";
					bias-pull-up;
				};
			};

			emac_mdio: emac_mdio {
				mux {
					pins = "gpio114";
					function = "rgmii_mdio";
				};

				config {
					pins = "gpio114";
					bias-pull-up;
				};
			};

			emac_rgmii_txd0: emac_rgmii_txd0 {
				mux {
					pins = "gpio96";
					function = "rgmii_txd0";
				};

				config {
					pins = "gpio96";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_txd1: emac_rgmii_txd1 {
				mux {
					pins = "gpio95";
					function = "rgmii_txd1";
				};

				config {
					pins = "gpio95";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_txd2: emac_rgmii_txd2 {
				mux {
					pins = "gpio94";
					function = "rgmii_txd2";
				};

				config {
					pins = "gpio94";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_txd3: emac_rgmii_txd3 {
				mux {
					pins = "gpio93";
					function = "rgmii_txd3";
				};

				config {
					pins = "gpio93";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_txc: emac_rgmii_txc {
				mux {
					pins = "gpio92";
					function = "rgmii_txc";
				};

				config {
					pins = "gpio92";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_rgmii_tx_ctl: emac_rgmii_tx_ctl {
				mux {
					pins = "gpio97";
					function = "rgmii_tx";
				};

				config {
					pins = "gpio97";
					bias-pull-up;
					drive-strength = <16>;
				};
			};


			emac_rgmii_rxd0: emac_rgmii_rxd0 {
				mux {
					pins = "gpio83";
					function = "rgmii_rxd0";
				};

				config {
					pins = "gpio83";
					bias-disable;  /* NO pull */
					drive-strength = <2>;  /* 2MA */
				};
			};

			emac_rgmii_rxd1: emac_rgmii_rxd1 {
				mux {
					pins = "gpio82";
					function = "rgmii_rxd1";
				};

				config {
					pins = "gpio82";
					bias-disable;  /* NO pull */
					drive-strength = <2>;
				};
			};

			emac_rgmii_rxd2: emac_rgmii_rxd2 {
				mux {
					pins = "gpio81";
					function = "rgmii_rxd2";
				};

				config {
					pins = "gpio81";
					bias-disable;	/* NO pull */
					drive-strength = <2>;
				};
			};

			emac_rgmii_rxd3: emac_rgmii_rxd3 {
				mux {
					pins = "gpio103";
					function = "rgmii_rxd3";
				};

				config {
					pins = "gpio103";
					bias-disable;	/* NO pull */
					drive-strength = <2>;
				};
			};

			emac_rgmii_rxc: emac_rgmii_rxc {
				mux {
					pins = "gpio102";
					function = "rgmii_rxc";
				};

				config {
					pins = "gpio102";
					bias-disable;	/* NO pull */
					drive-strength = <2>;
				};
			};

			emac_rgmii_rxc_suspend: emac_rgmii_rxc_suspend {
				mux {
					pins = "gpio102";
					function = "rgmii_rxc";
				};

				config {
					pins = "gpio102";
					input-disable;
				};
			};

			emac_rgmii_rxc_resume: emac_rgmii_rxc_resume {
				mux {
					pins = "gpio102";
					function = "rgmii_rxc";
				};

				config {
					pins = "gpio102";
					input-enable;
					bias-disable;/* NO pull */
				};
			};

			emac_rgmii_rx_ctl: emac_rgmii_rx_ctl {
				mux {
					pins = "gpio112";
					function = "rgmii_rx";
				};

				config {
					pins = "gpio112";
					bias-disable;  /* NO pull */
					drive-strength = <2>;
				};
			};

			emac_phy_intr: emac_phy_intr {
				mux {
					pins = "gpio121";
					function = "emac_phy";
				};

				config {
					pins = "gpio121";
					bias-disable;  /* NO pull */
					drive-strength = <2>;
				};
			};

			emac_phy_reset_state: emac_phy_reset_state {
				mux {
					pins = "gpio104";
					function = "gpio";
				};

				config {
					pins = "gpio104";
					bias-pull-up;
					drive-strength = <16>;
				};
			};

			emac_pin_pps_0: emac_pin_pps_0 {
				mux {
					pins = "gpio91";
					function = "rgmii_sync";
				};

				config {
					pins = "gpio91";
					bias-pull-up;
					drive-strength = <16>;
				};
			};
		};

		bt_en_active: bt_en_active {
			mux {
				pins = "gpio85";
				function = "gpio";
			};

			config {
				pins = "gpio85";
				drive-strength = <2>;
				output-low;
				bias-pull-down;
			};
		};

		usb0_hs_ac_en_default: usb0_hs_ac_en_default {
			mux {
				pins = "gpio88";
				function = "usb0_hs_ac";
			};

			config {
				pins = "gpio88";
				drive-strength = <2>;
				bias-disable;
			};
		};

		usb1_hs_ac_en_default: usb1_hs_ac_en_default {
			mux {
				pins = "gpio89";
				function = "usb1_hs_ac";
			};

			config {
				pins = "gpio89";
				drive-strength = <2>;
				bias-disable;
			};
		};
	};
};
