Qualcomm Technologies, Inc. ISL97900 Driver

ISL97900 Device

This device is used to support the current adjustment for R/G/B LED.
By changing the current through I2C registers, user can see different
brightness of R/G/B LED device.

Required properties:
 - compatible:          "qcom,isl97900-led"
 - reg:                 I2C address of the device

Example:
        isl97900_left: isl97900_left@28 {
                compatible = "qcom,isl97900-led";
                reg = <0x28>;
        };
