&lpi_tlmm {
	quat_mi2s_sck {
		quat_mi2s_sck_sleep: quat_mi2s_sck_sleep {
			mux {
				pins = "gpio0";
				function = "func2";
			};

			config {
				pins = "gpio0";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_mi2s_sck_active: quat_mi2s_sck_active {
			mux {
				pins = "gpio0";
				function = "func2";
			};

			config {
				pins = "gpio0";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_mi2s_ws {
		quat_mi2s_ws_sleep: quat_mi2s_ws_sleep {
			mux {
				pins = "gpio1";
				function = "func2";
			};

			config {
				pins = "gpio1";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_mi2s_ws_active: quat_mi2s_ws_active {
			mux {
				pins = "gpio1";
				function = "func2";
			};

			config {
				pins = "gpio1";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_mi2s_sd0 {
		quat_mi2s_sd0_sleep: quat_mi2s_sd0_sleep {
			mux {
				pins = "gpio2";
				function = "func2";
			};

			config {
				pins = "gpio2";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_mi2s_sd0_active: quat_mi2s_sd0_active {
			mux {
				pins = "gpio2";
				function = "func2";
			};

			config {
				pins = "gpio2";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_mi2s_sd1 {
		quat_mi2s_sd1_sleep: quat_mi2s_sd1_sleep {
			mux {
				pins = "gpio3";
				function = "func2";
			};

			config {
				pins = "gpio3";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_mi2s_sd1_active: quat_mi2s_sd1_active {
			mux {
				pins = "gpio3";
				function = "func2";
			};

			config {
				pins = "gpio3";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_mi2s_sd2 {
		quat_mi2s_sd2_sleep: quat_mi2s_sd2_sleep {
			mux {
				pins = "gpio4";
				function = "func2";
			};

			config {
				pins = "gpio4";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_mi2s_sd2_active: quat_mi2s_sd2_active {
			mux {
				pins = "gpio4";
				function = "func2";
			};

			config {
				pins = "gpio4";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_mi2s_sd3 {
		quat_mi2s_sd3_sleep: quat_mi2s_sd3_sleep {
			mux {
				pins = "gpio5";
				function = "func3";
			};

			config {
				pins = "gpio5";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_mi2s_sd3_active: quat_mi2s_sd3_active {
			mux {
				pins = "gpio5";
				function = "func3";
			};

			config {
				pins = "gpio5";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_i2s1_sck {
		lpi_i2s1_sck_sleep: lpi_i2s1_sck_sleep {
			mux {
				pins = "gpio6";
				function = "func2";
			};

			config {
				pins = "gpio6";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_i2s1_sck_active: lpi_i2s1_sck_active {
			mux {
				pins = "gpio6";
				function = "func2";
			};

			config {
				pins = "gpio6";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_i2s1_ws {
		lpi_i2s1_ws_sleep: lpi_i2s1_ws_sleep {
			mux {
				pins = "gpio7";
				function = "func2";
			};

			config {
				pins = "gpio7";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_i2s1_ws_active: lpi_i2s1_ws_active {
			mux {
				pins = "gpio7";
				function = "func2";
			};

			config {
				pins = "gpio7";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_i2s1_sd0 {
		lpi_i2s1_sd0_sleep: lpi_i2s1_sd0_sleep {
			mux {
				pins = "gpio8";
				function = "func2";
			};

			config {
				pins = "gpio8";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_i2s1_sd0_active: lpi_i2s1_sd0_active {
			mux {
				pins = "gpio8";
				function = "func2";
			};

			config {
				pins = "gpio8";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_i2s1_sd1 {
		lpi_i2s1_sd1_sleep: lpi_i2s1_sd1_sleep {
			mux {
				pins = "gpio9";
				function = "func2";
			};

			config {
				pins = "gpio9";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_i2s1_sd1_active: lpi_i2s1_sd1_active {
			mux {
				pins = "gpio9";
				function = "func2";
			};

			config {
				pins = "gpio9";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_i2s2_sck {
		lpi_i2s2_sck_sleep: lpi_i2s2_sck_sleep {
			mux {
				pins = "gpio10";
				function = "func1";
			};

			config {
				pins = "gpio10";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_i2s2_sck_active: lpi_i2s2_sck_active {
			mux {
				pins = "gpio10";
				function = "func1";
			};

			config {
				pins = "gpio10";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_i2s2_ws {
		lpi_i2s2_ws_sleep: lpi_i2s2_ws_sleep {
			mux {
				pins = "gpio11";
				function = "func1";
			};

			config {
				pins = "gpio11";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_i2s2_ws_active: lpi_i2s2_ws_active {
			mux {
				pins = "gpio11";
				function = "func1";
			};

			config {
				pins = "gpio11";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_i2s2_sd0 {
		lpi_i2s2_sd0_sleep: lpi_i2s2_sd0_sleep {
			mux {
				pins = "gpio12";
				function = "func2";
			};

			config {
				pins = "gpio12";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_i2s2_sd0_active: lpi_i2s2_sd0_active {
			mux {
				pins = "gpio12";
				function = "func2";
			};

			config {
				pins = "gpio12";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_i2s2_sd1 {
		lpi_i2s2_sd1_sleep: lpi_i2s2_sd1_sleep {
			mux {
				pins = "gpio13";
				function = "func2";
			};

			config {
				pins = "gpio13";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_i2s2_sd1_active: lpi_i2s2_sd1_active {
			mux {
				pins = "gpio13";
				function = "func2";
			};

			config {
				pins = "gpio13";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_tdm_sck {
		quat_tdm_sck_sleep: quat_tdm_sck_sleep {
			mux {
				pins = "gpio0";
				function = "func2";
			};

			config {
				pins = "gpio0";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_tdm_sck_active: quat_tdm_sck_active {
			mux {
				pins = "gpio0";
				function = "func2";
			};

			config {
				pins = "gpio0";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_tdm_ws {
		quat_tdm_ws_sleep: quat_tdm_ws_sleep {
			mux {
				pins = "gpio1";
				function = "func2";
			};

			config {
				pins = "gpio1";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_tdm_ws_active: quat_tdm_ws_active {
			mux {
				pins = "gpio1";
				function = "func2";
			};

			config {
				pins = "gpio1";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_tdm_sd0 {
		quat_tdm_sd0_sleep: quat_tdm_sd0_sleep {
			mux {
				pins = "gpio2";
				function = "func2";
			};

			config {
				pins = "gpio2";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_tdm_sd0_active: quat_tdm_sd0_active {
			mux {
				pins = "gpio2";
				function = "func2";
			};

			config {
				pins = "gpio2";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_tdm_sd1 {
		quat_tdm_sd1_sleep: quat_tdm_sd1_sleep {
			mux {
				pins = "gpio3";
				function = "func2";
			};

			config {
				pins = "gpio3";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_tdm_sd1_active: quat_tdm_sd1_active {
			mux {
				pins = "gpio3";
				function = "func2";
			};

			config {
				pins = "gpio3";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_tdm_sd2 {
		quat_tdm_sd2_sleep: quat_tdm_sd2_sleep {
			mux {
				pins = "gpio4";
				function = "func2";
			};

			config {
				pins = "gpio4";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_tdm_sd2_active: quat_tdm_sd2_active {
			mux {
				pins = "gpio4";
				function = "func2";
			};

			config {
				pins = "gpio4";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_tdm_sd3 {
		quat_tdm_sd3_sleep: quat_tdm_sd3_sleep {
			mux {
				pins = "gpio5";
				function = "func3";
			};

			config {
				pins = "gpio5";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_tdm_sd3_active: quat_tdm_sd3_active {
			mux {
				pins = "gpio5";
				function = "func3";
			};

			config {
				pins = "gpio5";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_tdm1_sck {
		lpi_tdm1_sck_sleep: lpi_tdm1_sck_sleep {
			mux {
				pins = "gpio6";
				function = "func2";
			};

			config {
				pins = "gpio6";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_tdm1_sck_active: lpi_tdm1_sck_active {
			mux {
				pins = "gpio6";
				function = "func2";
			};

			config {
				pins = "gpio6";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_tdm1_ws {
		lpi_tdm1_ws_sleep: lpi_tdm1_ws_sleep {
			mux {
				pins = "gpio7";
				function = "func2";
			};

			config {
				pins = "gpio7";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_tdm1_ws_active: lpi_tdm1_ws_active {
			mux {
				pins = "gpio7";
				function = "func2";
			};

			config {
				pins = "gpio7";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_tdm1_sd0 {
		lpi_tdm1_sd0_sleep: lpi_tdm1_sd0_sleep {
			mux {
				pins = "gpio8";
				function = "func2";
			};

			config {
				pins = "gpio8";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_tdm1_sd0_active: lpi_tdm1_sd0_active {
			mux {
				pins = "gpio8";
				function = "func2";
			};

			config {
				pins = "gpio8";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_tdm1_sd1 {
		lpi_tdm1_sd1_sleep: lpi_tdm1_sd1_sleep {
			mux {
				pins = "gpio9";
				function = "func2";
			};

			config {
				pins = "gpio9";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_tdm1_sd1_active: lpi_tdm1_sd1_active {
			mux {
				pins = "gpio9";
				function = "func2";
			};

			config {
				pins = "gpio9";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_tdm2_sck {
		lpi_tdm2_sck_sleep: lpi_tdm2_sck_sleep {
			mux {
				pins = "gpio10";
				function = "func1";
			};

			config {
				pins = "gpio10";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_tdm2_sck_active: lpi_tdm2_sck_active {
			mux {
				pins = "gpio10";
				function = "func1";
			};

			config {
				pins = "gpio10";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_tdm2_ws {
		lpi_tdm2_ws_sleep: lpi_tdm2_ws_sleep {
			mux {
				pins = "gpio11";
				function = "func1";
			};

			config {
				pins = "gpio11";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_tdm2_ws_active: lpi_tdm2_ws_active {
			mux {
				pins = "gpio11";
				function = "func1";
			};

			config {
				pins = "gpio11";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_tdm2_sd0 {
		lpi_tdm2_sd0_sleep: lpi_tdm2_sd0_sleep {
			mux {
				pins = "gpio12";
				function = "func2";
			};

			config {
				pins = "gpio12";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_tdm2_sd0_active: lpi_tdm2_sd0_active {
			mux {
				pins = "gpio12";
				function = "func2";
			};

			config {
				pins = "gpio12";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_tdm2_sd1 {
		lpi_tdm2_sd1_sleep: lpi_tdm2_sd1_sleep {
			mux {
				pins = "gpio13";
				function = "func2";
			};

			config {
				pins = "gpio13";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_tdm2_sd1_active: lpi_tdm2_sd1_active {
			mux {
				pins = "gpio13";
				function = "func2";
			};

			config {
				pins = "gpio13";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_aux_sck {
		quat_aux_sck_sleep: quat_aux_sck_sleep {
			mux {
				pins = "gpio0";
				function = "func2";
			};

			config {
				pins = "gpio0";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_aux_sck_active: quat_aux_sck_active {
			mux {
				pins = "gpio0";
				function = "func2";
			};

			config {
				pins = "gpio0";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_aux_ws {
		quat_aux_ws_sleep: quat_aux_ws_sleep {
			mux {
				pins = "gpio1";
				function = "func2";
			};

			config {
				pins = "gpio1";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_aux_ws_active: quat_aux_ws_active {
			mux {
				pins = "gpio1";
				function = "func2";
			};

			config {
				pins = "gpio1";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_aux_sd0 {
		quat_aux_sd0_sleep: quat_aux_sd0_sleep {
			mux {
				pins = "gpio2";
				function = "func2";
			};

			config {
				pins = "gpio2";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_aux_sd0_active: quat_aux_sd0_active {
			mux {
				pins = "gpio2";
				function = "func2";
			};

			config {
				pins = "gpio2";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_aux_sd1 {
		quat_aux_sd1_sleep: quat_aux_sd1_sleep {
			mux {
				pins = "gpio3";
				function = "func2";
			};

			config {
				pins = "gpio3";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_aux_sd1_active: quat_aux_sd1_active {
			mux {
				pins = "gpio3";
				function = "func2";
			};

			config {
				pins = "gpio3";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_aux_sd2 {
		quat_aux_sd2_sleep: quat_aux_sd2_sleep {
			mux {
				pins = "gpio4";
				function = "func2";
			};

			config {
				pins = "gpio4";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_aux_sd2_active: quat_aux_sd2_active {
			mux {
				pins = "gpio4";
				function = "func2";
			};

			config {
				pins = "gpio4";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	quat_aux_sd3 {
		quat_aux_sd3_sleep: quat_aux_sd3_sleep {
			mux {
				pins = "gpio5";
				function = "func3";
			};

			config {
				pins = "gpio5";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		quat_aux_sd3_active: quat_aux_sd3_active {
			mux {
				pins = "gpio5";
				function = "func3";
			};

			config {
				pins = "gpio5";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_aux1_sck {
		lpi_aux1_sck_sleep: lpi_aux1_sck_sleep {
			mux {
				pins = "gpio6";
				function = "func2";
			};

			config {
				pins = "gpio6";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_aux1_sck_active: lpi_aux1_sck_active {
			mux {
				pins = "gpio6";
				function = "func2";
			};

			config {
				pins = "gpio6";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_aux1_ws {
		lpi_aux1_ws_sleep: lpi_aux1_ws_sleep {
			mux {
				pins = "gpio7";
				function = "func2";
			};

			config {
				pins = "gpio7";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_aux1_ws_active: lpi_aux1_ws_active {
			mux {
				pins = "gpio7";
				function = "func2";
			};

			config {
				pins = "gpio7";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_aux1_sd0 {
		lpi_aux1_sd0_sleep: lpi_aux1_sd0_sleep {
			mux {
				pins = "gpio8";
				function = "func2";
			};

			config {
				pins = "gpio8";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_aux1_sd0_active: lpi_aux1_sd0_active {
			mux {
				pins = "gpio8";
				function = "func2";
			};

			config {
				pins = "gpio8";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_aux1_sd1 {
		lpi_aux1_sd1_sleep: lpi_aux1_sd1_sleep {
			mux {
				pins = "gpio9";
				function = "func2";
			};

			config {
				pins = "gpio9";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_aux1_sd1_active: lpi_aux1_sd1_active {
			mux {
				pins = "gpio9";
				function = "func2";
			};

			config {
				pins = "gpio9";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_aux2_sck {
		lpi_aux2_sck_sleep: lpi_aux2_sck_sleep {
			mux {
				pins = "gpio10";
				function = "func1";
			};

			config {
				pins = "gpio10";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_aux2_sck_active: lpi_aux2_sck_active {
			mux {
				pins = "gpio10";
				function = "func1";
			};

			config {
				pins = "gpio10";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_aux2_ws {
		lpi_aux2_ws_sleep: lpi_aux2_ws_sleep {
			mux {
				pins = "gpio11";
				function = "func1";
			};

			config {
				pins = "gpio11";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_aux2_ws_active: lpi_aux2_ws_active {
			mux {
				pins = "gpio11";
				function = "func1";
			};

			config {
				pins = "gpio11";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_aux2_sd0 {
		lpi_aux2_sd0_sleep: lpi_aux2_sd0_sleep {
			mux {
				pins = "gpio12";
				function = "func2";
			};

			config {
				pins = "gpio12";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_aux2_sd0_active: lpi_aux2_sd0_active {
			mux {
				pins = "gpio12";
				function = "func2";
			};

			config {
				pins = "gpio12";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	lpi_aux2_sd1 {
		lpi_aux2_sd1_sleep: lpi_aux2_sd1_sleep {
			mux {
				pins = "gpio13";
				function = "func2";
			};

			config {
				pins = "gpio13";
				drive-strength = <2>;   /* 2 mA */
				bias-pull-down;         /* PULL DOWN */
				input-enable;
			};
		};

		lpi_aux2_sd1_active: lpi_aux2_sd1_active {
			mux {
				pins = "gpio13";
				function = "func2";
			};

			config {
				pins = "gpio13";
				drive-strength = <8>;   /* 8 mA */
				bias-disable;           /* NO PULL */
				output-high;
			};
		};
	};

	tx_swr_clk_sleep: tx_swr_clk_sleep {
		mux {
			pins = "gpio0";
			function = "func1";
			input-enable;
			bias-pull-down;
		};

		config {
			pins = "gpio0";
			drive-strength = <10>;
		};
	};

	tx_swr_clk_active: tx_swr_clk_active {
		mux {
			pins = "gpio0";
			function = "func1";
		};

		config {
			pins = "gpio0";
			drive-strength = <10>;
			slew-rate = <1>;
			bias-disable;
		};
	};

	tx_swr_data0_sleep: tx_swr_data0_sleep {
		mux {
			pins = "gpio1";
			function = "func1";
		};

		config {
			pins = "gpio1";
			drive-strength = <10>;
			input-enable;
			bias-bus-hold;
		};
	};

	tx_swr_data0_active: tx_swr_data0_active {
		mux {
			pins = "gpio1";
			function = "func1";
		};

		config {
			pins = "gpio1";
			drive-strength = <10>;
			slew-rate = <1>;
			bias-bus-hold;
		};
	};

	tx_swr_data1_sleep: tx_swr_data1_sleep {
		mux {
			pins = "gpio2";
			function = "func1";
		};

		config {
			pins = "gpio2";
			drive-strength = <10>;
			input-enable;
			bias-pull-down;
		};
	};

	tx_swr_data1_active: tx_swr_data1_active {
		mux {
			pins = "gpio2";
			function = "func1";
		};

		config {
			pins = "gpio2";
			drive-strength = <10>;
			slew-rate = <1>;
			bias-bus-hold;
		};
	};

	tx_swr_data2_sleep: tx_swr_data2_sleep {
		mux {
			pins = "gpio18";
			function = "func2";
		};

		config {
			pins = "gpio18";
			drive-strength = <10>;
			input-enable;
			bias-pull-down;
		};
	};

	tx_swr_data2_active: tx_swr_data2_active {
		mux {
			pins = "gpio18";
			function = "func2";
		};

		config {
			pins = "gpio18";
			drive-strength = <10>;
			slew-rate = <1>;
			bias-bus-hold;
		};
	};

	rx_swr_clk_sleep: rx_swr_clk_sleep {
		mux {
			pins = "gpio3";
			function = "func1";
		};

		config {
			pins = "gpio3";
			drive-strength = <10>;
			input-enable;
			bias-pull-down;
		};
	};

	rx_swr_clk_active: rx_swr_clk_active {
		mux {
			pins = "gpio3";
			function = "func1";
		};

		config {
			pins = "gpio3";
			drive-strength = <10>;
			slew-rate = <1>;
			bias-disable;
		};
	};

	rx_swr_data_sleep: rx_swr_data_sleep {
		mux {
			pins = "gpio4";
			function = "func1";
		};

		config {
			pins = "gpio4";
			drive-strength = <10>;
			input-enable;
			bias-pull-down;
		};
	};

	rx_swr_data_active: rx_swr_data_active {
		mux {
			pins = "gpio4";
			function = "func1";
		};

		config {
			pins = "gpio4";
			drive-strength = <10>;
			slew-rate = <1>;
			bias-bus-hold;
		};
	};

	rx_swr_data1_sleep: rx_swr_data1_sleep {
		mux {
			pins = "gpio5";
			function = "func1";
		};

		config {
			pins = "gpio5";
			drive-strength = <10>;
			input-enable;
			bias-pull-down;
		};
	};

	rx_swr_data1_active: rx_swr_data1_active {
		mux {
			pins = "gpio5";
			function = "func1";
		};

		config {
			pins = "gpio5";
			drive-strength = <10>;
			slew-rate = <1>;
			bias-bus-hold;
		};
	};

	cdc_dmic01_clk_active: dmic01_clk_active {
		mux {
			pins = "gpio6";
			function = "func1";
		};

		config {
			pins = "gpio6";
			drive-strength = <8>;
			output-high;
		};
	};

	cdc_dmic01_clk_sleep: dmic01_clk_sleep {
		mux {
			pins = "gpio6";
			function = "func1";
		};

		config {
			pins = "gpio6";
			drive-strength = <2>;
			bias-disable;
			output-low;
		};
	};

	cdc_dmic01_data_active: dmic01_data_active {
		mux {
			pins = "gpio7";
			function = "func1";
		};

		config {
			pins = "gpio7";
			drive-strength = <8>;
			input-enable;
		};
	};

	cdc_dmic01_data_sleep: dmic01_data_sleep {
		mux {
			pins = "gpio7";
			function = "func1";
		};

		config {
			pins = "gpio7";
			drive-strength = <2>;
			pull-down;
			input-enable;
		};
	};

	cdc_dmic23_clk_active: dmic23_clk_active {
		mux {
			pins = "gpio8";
			function = "func1";
		};

		config {
			pins = "gpio8";
			drive-strength = <8>;
			output-high;
		};
	};

	cdc_dmic23_clk_sleep: dmic23_clk_sleep {
		mux {
			pins = "gpio8";
			function = "func1";
		};

		config {
			pins = "gpio8";
			drive-strength = <2>;
			bias-disable;
			output-low;
		};
	};

	cdc_dmic23_data_active: dmic23_data_active {
		mux {
			pins = "gpio9";
			function = "func1";
		};

		config {
			pins = "gpio9";
			drive-strength = <8>;
			input-enable;
		};
	};

	cdc_dmic23_data_sleep: dmic23_data_sleep {
		mux {
			pins = "gpio9";
			function = "func1";
		};

		config {
			pins = "gpio9";
			drive-strength = <2>;
			pull-down;
			input-enable;
		};
	};

	cdc_dmic45_clk_active: dmic45_clk_active {
		mux {
			pins = "gpio12";
			function = "func1";
		};

		config {
			pins = "gpio12";
			drive-strength = <8>;
			output-high;
		};
	};

	cdc_dmic45_clk_sleep: dmic45_clk_sleep {
		mux {
			pins = "gpio12";
			function = "func1";
		};

		config {
			pins = "gpio12";
			drive-strength = <2>;
			bias-disable;
			output-low;
		};
	};

	cdc_dmic45_data_active: dmic45_data_active {
		mux {
			pins = "gpio13";
			function = "func1";
		};

		config {
			pins = "gpio13";
			drive-strength = <8>;
			input-enable;
		};
	};

	cdc_dmic45_data_sleep: dmic45_data_sleep {
		mux {
			pins = "gpio13";
			function = "func1";
		};

		config {
			pins = "gpio13";
			drive-strength = <2>;
			pull-down;
			input-enable;
		};
	};

	wsa_mclk_active: wsa_mclk_active {
		mux {
			pins = "gpio17";
			function = "func2";
		};

		config {
			pins = "gpio17";
			drive-strength = <16>;   /* 16 mA */
			bias-disable;
			output-high;
		};
	};

	wsa_mclk_sleep: wsa_mclk_sleep {
		mux {
			pins = "gpio17";
			function = "func2";
		};

		config {
			pins = "gpio17";
			drive-strength = <2>;   /* 2 mA */
			bias-pull-down;
		};
	};
};
