Qualcomm's SPMI PMIC ADC

- SPMI PMIC voltage ADC (VADC) provides interface to clients to read
  voltage. The VADC is a 15-bit sigma-delta ADC.
- SPMI PMIC5 voltage ADC (ADC) provides interface to clients to read
  voltage. The VADC is a 16-bit sigma-delta ADC.

VADC node:

- compatible:
    Usage: required
    Value type: <string>
    Definition: Should contain "qcom,spmi-vadc".
                Should contain "qcom,spmi-adc5-gen3" for PMIC5 Gen3 ADC driver.
                Should contain "qcom,spmi-adc7" for PMIC7 ADC driver.
                Should contain "qcom,spmi-adc5" for PMIC5 ADC driver.
                Should contain "qcom,spmi-adc-rev2" for PMIC rev2 ADC driver.
                Should contain "qcom,pms405-adc" for PMS405 PMIC
		Should contain "qcom,spmi-adc5-lite" for PMIC5 ADC-lite driver.
- reg:
    Usage: required
    Value type: <prop-encoded-array>
    Definition: VADC base address in the SPMI PMIC register map.

- qcom,debug-base:
    Usage: optional
    Value type: <u32>
    Definition: Debug ADC peripheral base address in the SPMI PMIC
            register map. Only applicable for devices with compatible
            property "qcom,spmi-adc5-gen3".

- #address-cells:
    Usage: required
    Value type: <u32>
    Definition: Must be one. Child node 'reg' property should define ADC
            channel number.

- #size-cells:
    Usage: required
    Value type: <u32>
    Definition: Must be zero.

- #io-channel-cells:
    Usage: required
    Value type: <u32>
    Definition: Must be one. For details about IIO bindings see:
            Documentation/devicetree/bindings/iio/iio-bindings.txt

- interrupts:
    Usage: optional
    Value type: <prop-encoded-array>
    Definition: End of conversion interrupt.

- interrupt-names:
    Usage: optional
    Value type: <string-array>
    Definition: Specifies the interrupt names for ADC SDAMs. Names should
        be defined as "adc-sdam<N>" where <N> represents the SDAM index.

Channel node properties:

- reg:
    Usage: required
    Value type: <u32>
    Definition: ADC channel number.
            See include/dt-bindings/iio/qcom,spmi-vadc.h

- label:
    Usage: required for "qcom,spmi-adc5", "qcom,spmi-adc7", "qcom,spmi-adc5-gen3"
    and "qcom,spmi-adc-rev2"
    Value type: <empty>
    Definition: ADC input of the platform as seen in the schematics.
            For thermistor inputs connected to generic AMUX or GPIO inputs
            these can vary across platform for the same pins. Hence select
            the platform schematics name for this channel.

- qcom,decimation:
    Usage: optional
    Value type: <u32>
    Definition: This parameter is used to decrease ADC sampling rate.
            Quicker measurements can be made by reducing decimation ratio.
            - For compatible property "qcom,spmi-vadc", valid values are
              512, 1024, 2048, 4096. If property is not found, default value
              of 512 will be used.
            - For compatible property "qcom,spmi-adc5", valid values are
              250, 420 and 840. If property is not found, default value of
              840 is used.
            - For compatible property "qcom,spmi-adc7" and "qcom,spmi-adc5-gen3",
              valid values are 85, 340 and 1360. If property is not found, default
              value of 1360 is used.
            - For compatible property "qcom,spmi-adc-rev2", valid values are 256,
              512 and 1024. If property is not present, default value is 1024.

- qcom,pre-scaling:
    Usage: optional
    Value type: <u32 array>
    Definition: Used for scaling the channel input signal before the signal is
            fed to VADC. The configuration for this node is to know the
            pre-determined ratio and use it for post scaling. Select one from
            the following options.
            <1 1>, <1 3>, <1 4>, <1 6>, <1 20>, <1 8>, <10 81>, <1 10>, <1 16>,
            <32 100>, <14, 100>, <28, 100>, <1000 305185>, <1000 610370>

            If property is not found default value depending on chip will be used.

- qcom,ratiometric:
    Usage: optional
    Value type: <empty>
    Definition: Channel calibration type.
            - For compatible property "qcom,spmi-vadc", if this property is
              specified VADC will use the VDD reference (1.8V) and GND for
              channel calibration. If property is not found, channel will be
              calibrated with 0.625V and 1.25V reference channels, also
              known as absolute calibration.
            - For compatible property "qcom,spmi-adc5", "qcom,spmi-adc7",
              "qcom,spmi-adc5-gen3" and "qcom,spmi-adc-rev2", if this property
              is specified VADC will use the VDD reference (1.875V) and GND for
              channel calibration.
              If property is not found, channel will be calibrated with 0V
              and 1.25V reference channels, also known as absolute calibration.

- qcom,hw-settle-time:
    Usage: optional
    Value type: <u32>
    Definition: Time between AMUX getting configured and the ADC starting
            conversion. The 'hw_settle_time' is an index used from valid values
            and programmed in hardware to achieve the hardware settling delay.
            - For compatible property "qcom,spmi-vadc" and "qcom,spmi-adc-rev2",
              Delay = 100us * (hw_settle_time) for hw_settle_time < 11,
              and 2ms * (hw_settle_time - 10) otherwise.
              Valid values are: 0, 100, 200, 300, 400, 500, 600, 700, 800,
              900 us and 1, 2, 4, 6, 8, 10 ms.
              If property is not found, channel will use 0us.
            - For compatible property "qcom,spmi-adc5", delay = 15us for
              value 0, 100us * (value) for values < 11,
              and 2ms * (value - 10) otherwise.
              Valid values are: 15, 100, 200, 300, 400, 500, 600, 700, 800,
              900 us and 1, 2, 4, 6, 8, 10 ms
              Certain controller digital versions have valid values of
              15, 100, 200, 300, 400, 500, 600, 700, 1, 2, 4, 8, 16, 32, 64, 128 ms
              If property is not found, channel will use 15us.
            - For compatible property "qcom,spmi-adc7" or "qcom,spmi-adc5-gen3",
              delay = 15us for value 0, 100us * (value) for values < 8, 1ms for value 8
              and 2ms * (value - 8) otherwise.
              Valid values are: 15, 100, 200, 300, 400, 500, 600, 700, 1000, 2000,
              4000, 8000, 16000, 32000, 64000, 128000 us.
              If property is not found, channel will use 15us.

- qcom,avg-samples:
    Usage: optional
    Value type: <u32>
    Definition: Number of samples to be used for measurement.
            Averaging provides the option to obtain a single measurement
            from the ADC that is an average of multiple samples. The value
            selected is 2^(value).
            - For compatible property "qcom,spmi-vadc", valid values
              are: 1, 2, 4, 8, 16, 32, 64, 128, 256, 512
              If property is not found, 1 sample will be used.
            - For compatible property "qcom,spmi-adc5", "qcom,spmi-adc7",
              "qcom,spmi-adc5-gen3" and "qcom,spmi-adc-rev2",
              valid values are: 1, 2, 4, 8, 16.
              If property is not found, 1 sample will be used.

- qcom,scale-fn-type:
    Usage: optional
    Value type: <u32>
    Definition: The index of the VADC scale function used to convert raw ADC
            code to physical scaled units for the channel. Defined for compatible
            properties "qcom,spmi-adc5", "qcom,spmi-adc5-gen3" and "qcom,spmi-adc7".
            See include/dt-bindings/iio/qcom,spmi-vadc.h.

- qcom,adc-tm-type:
    Usage: optional
    Value type: <u32>
    Definition: Type of ADC_TM usage defined for a given channel. Valid values
            are 0-3. Defined for compatible property "qcom,spmi-adc5-gen3".
            - Value 0 indicates it will not be used for ADC_TM.
            - Value 1 indicates it will be used for thermistors, for detecting
              temperature threshold violations and temperature reads.
            - Value 2 indicates it will be used for thermistors, for temperature
              reads alone.
            - Value 3 indicates it will be used for non-thermal clients, for
              detecting threshold violations for that channel.

- qcom,rscale-type:
    Usage: optional
    Value type: <u32>
    Definition: Type of reverse scaling function used for ADC_TM channels. Valid only
            for the case of non-thermal ADC_TM client. Valid value at present is only
            0 for reverse scaling of default voltage scaling function. Defined for
            compatible property "qcom,spmi-adc5-gen3".

NOTE:

For compatible property "qcom,spmi-vadc" following channels, also known as
reference point channels, are used for result calibration and their channel
configuration nodes should be defined:
VADC_REF_625MV and/or VADC_SPARE1(based on PMIC version) VADC_REF_1250MV,
VADC_GND_REF and VADC_VDD_VADC.

Example1:

#include <dt-bindings/iio/qcom,spmi-vadc.h>
#include <linux/irq.h>
/* ... */

	/* VADC node */
	pmic_vadc: vadc@3100 {
		compatible = "qcom,spmi-vadc";
		reg = <0x3100>;
		interrupts = <0x0 0x31 0x0 IRQ_TYPE_EDGE_RISING>;
		#address-cells = <1>;
		#size-cells = <0>;
		#io-channel-cells = <1>;
		io-channel-ranges;

		/* Channel node */
		adc-chan@VADC_LR_MUX10_USB_ID {
			reg = <VADC_LR_MUX10_USB_ID>;
			qcom,decimation = <512>;
			qcom,ratiometric;
			qcom,hw-settle-time = <200>;
			qcom,avg-samples = <1>;
			qcom,pre-scaling = <1 3>;
		};
	};

	/* IIO client node */
	usb {
		io-channels = <&pmic_vadc VADC_LR_MUX10_USB_ID>;
		io-channel-names = "vadc";
	};

Example2:

#include <dt-bindings/iio/qcom,spmi-adc5-gen3-pm5100.h>
#include <linux/irq.h>
/* ... */

	/* VADC node */
	pm5100_adc: adc@8000 {
		compatible = "qcom,spmi-adc-gen3";
		reg = <0x8000>;
		#address-cells = <1>;
		#size-cells = <0>;
		interrupts = <0x0 0x80 0x0 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "adc";
		#io-channel-cells = <1>;
		io-channel-ranges;
		#thermal-sensor-cells = <1>;

		pm5100_die_temp {
			reg = <PM5100_ADC5_GEN3_DIE_TEMP>;
			label = "pm5100_die_temp";
			qcom,pre-scaling = <1 1>;
		};

		pm5100_xo_therm {
			reg = <PM5100_ADC5_GEN3_XO_THERM>;
			label = "pm5100_xo_therm";
			qcom,ratiometric;
			qcom,hw-settle-time = <200>;
			qcom,pre-scaling = <1 1>;
			qcom,adc-tm-type = <1>;
		};

		pm5100_vph_pwr {
			reg = <PM5100_ADC5_GEN3_VPH_PWR>;
			label = "pm5100_vph_pwr";
			qcom,pre-scaling = <1 3>;
		};
	};

	/* IIO client node */
	batt {
		io-channels = <&pm5100_adc PM5100_ADC5_GEN3_VPH_PWR>;
		io-channel-names = "vph_pwr";
	};
