Bindings for the Maxim MAX31760 Intelligent Fan Controller
==========================================================

The Maxim MAX31760 is a i2c device providing closed-loop, multi-channel fan
management with temperature. Various fan control features are provided,
including PWM frequency control, temperature hysteresis, dual tachometer
measurements, and fan health monitoring.

Required properties:
- compatible         : should be "maxim,max31760".
- reg                : I2C address, 0x50.

Optional properties:
- maxim,driver-en-gpio : fan driver enable gpio
- maxim,pwr-en-gpio  : fan pwr enable gpio

Example:
	max31760@50 {
		compatible = "maxim,max31760";
		reg = <0x50>;
		pinctrl-names = "default";
		pinctrl-0 = <&pwr_en_gpio_default
			&driver_en_gpio_default>;

		maxim,driver-en-gpio = <&pm8550ve_f_gpios 5 GPIO_ACTIVE_LOW>;
		maxim,pwr-en-gpio = <&pm8550ve_f_gpios 6 GPIO_ACTIVE_LOW>;
	};
