#include "holi-audio-overlay.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/linux-event-codes.h>
#include "holi-pmic-overlay.dtsi"
#include <dt-bindings/iio/qti_power_supply_iio.h>

&sdhc_1 {
	status = "ok";

	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&sdc1_on>;
	pinctrl-1 = <&sdc1_off>;

	vdd-supply = <&L7E>;
	qcom,vdd-voltage-level = <2960000 2960000>;
	qcom,vdd-current-level = <0 570000>;

	vdd-io-supply = <&L12A>;
	qcom,vdd-io-always-on;
	qcom,vdd-io-lpm-sup;
	qcom,vdd-io-voltage-level = <1800000 1800000>;
	qcom,vdd-io-current-level = <0 325000>;
};

&sdhc_2 {
	status = "ok";

	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&sdc2_on>;
	pinctrl-1 = <&sdc2_off>;

	vdd-supply = <&L9E>;
	qcom,vdd-voltage-level = <2960000 2960000>;
	qcom,vdd-current-level = <0 800000>;

	vdd-io-supply = <&L6E>;
	qcom,vdd-io-voltage-level = <1800000 2960000>;
	qcom,vdd-io-current-level = <0 22000>;

	cd-gpios = <&tlmm 94 GPIO_ACTIVE_LOW>;
};

&ufsphy_mem {
		compatible = "qcom,ufs-phy-qmp-v3";

		vdda-phy-supply = <&L18A>;
		vdda-pll-supply = <&L22A>;
		vdda-phy-max-microamp = <62900>;
		vdda-pll-max-microamp = <18300>;

		status = "ok";
};

&ufshc_mem {
		vdd-hba-supply = <&gcc_ufs_phy_gdsc>;
		vdd-hba-fixed-regulator;

		vcc-supply = <&L7E>;
		vcc-voltage-level = <2950000 2960000>;
		vcc-max-microamp = <800000>;

		vccq2-supply = <&L12A>;
		vccq2-max-microamp = <800000>;
		vccq2-voltage-level = <1800000 1800000>;

		qcom,vddp-ref-clk-supply = <&L22A>;
		qcom,vddp-ref-clk-max-microamp = <100>;

		status = "ok";
};

&holi_snd {
	qcom,msm-mbhc-usbc-audio-supported = <1>;
	qcom,msm-mbhc-hphl-swh = <0>;
	qcom,msm-mbhc-gnd-swh = <0>;
};

&soc {
	gpio_keys {
		compatible = "gpio-keys";
		label = "gpio-keys";

		pinctrl-names = "default";
		pinctrl-0 = <&key_vol_up_default>;

		vol_up {
			label = "volume_up";
			gpios = <&pm6350_gpios 2 GPIO_ACTIVE_LOW>;
			linux,input-type = <1>;
			linux,code = <KEY_VOLUMEUP>;
			gpio-key,wakeup;
			debounce-interval = <15>;
			linux,can-disable;
		};
	};

	mtp_batterydata: qcom,battery-data {
		qcom,batt-id-range-pct = <15>;
		#include "qg-batterydata-alium-3600mah.dtsi"
		#include "qg-batterydata-atl466271_3300mAh.dtsi"
		#include "qg-batterydata-atl436186020H_3780mAh.dtsi"
	};
};

&pm7250b_charger {
	status = "ok";
	#io-channel-cells = <1>;
	io-channels = <&pm7250b_vadc ADC5_USB_IN_V_16>,
		      <&pm7250b_vadc ADC5_USB_IN_I>,
		      <&pm7250b_vadc ADC5_CHG_TEMP>,
		      <&pm7250b_vadc ADC5_DIE_TEMP>,
		      <&pm7250b_vadc ADC5_AMUX_THM3_100K_PU>,
		      <&pm7250b_vadc ADC5_SBUx>,
		      <&pm7250b_vadc ADC5_VPH_PWR>,
		      <&pm7250b_vadc ADC5_AMUX_THM1_100K_PU>,
		      <&pm7250b_qg PSY_IIO_RESISTANCE_ID>,
		      <&pm7250b_qg PSY_IIO_VOLTAGE_NOW>,
		      <&pm7250b_qg PSY_IIO_TEMP>,
		      <&pm7250b_qg PSY_IIO_CAPACITY>,
		      <&pm7250b_qg PSY_IIO_VOLTAGE_OCV>,
		      <&pm7250b_qg PSY_IIO_VOLTAGE_AVG>,
		      <&pm7250b_qg PSY_IIO_DEBUG_BATTERY>,
		      <&pm7250b_qg PSY_IIO_REAL_CAPACITY>,
		      <&pm7250b_qg PSY_IIO_CC_SOC>,
		      <&pm7250b_qg PSY_IIO_CURRENT_NOW>,
		      <&pm7250b_qg PSY_IIO_VOLTAGE_MAX>,
		      <&pm7250b_qg PSY_IIO_CHARGE_FULL>,
		      <&pm7250b_qg PSY_IIO_CHARGE_COUNTER>,
		      <&pm7250b_qg PSY_IIO_CYCLE_COUNT>,
		      <&pm7250b_qg PSY_IIO_CHARGE_FULL_DESIGN>,
		      <&pm7250b_qg PSY_IIO_TIME_TO_FULL_NOW>,
		      <&smb1396_div2_cp_master PSY_IIO_PARALLEL_MODE>,
		      <&smb1396_div2_cp_master PSY_IIO_PARALLEL_OUTPUT_MODE>,
		      <&smb1396_div2_cp_master PSY_IIO_MIN_ICL>,
		      <&smb1396_div2_cp_master PSY_IIO_CP_SWITCHER_EN>,
		      <&smb1396_div2_cp_master PSY_IIO_CP_ENABLE>,
		      <&smb1396_div2_cp_master PSY_IIO_CP_ILIM>,
		      <&smb1396_div2_cp_master PSY_IIO_CP_DIE_TEMP>,
		      <&smb1396_div2_cp_slave PSY_IIO_CURRENT_CAPABILITY>;
	io-channel-names = "usb_in_voltage",
			   "usb_in_current",
			   "chg_temp",
			   "die_temp",
			   "conn_temp",
			   "sbux_res",
			   "vph_voltage",
			   "skin_temp",
			   "resistance_id",
			   "voltage_now",
			   "temp",
			   "capacity",
			   "voltage_ocv",
			   "voltage_avg",
			   "debug_battery",
			   "real_capacity",
			   "cc_soc",
			   "current_now",
			   "voltage_max",
			   "charge_full",
			   "charge_counter",
			   "cycle_count",
			   "charge_full_design",
			   "time_to_full_now",
			   "parallel_mode",
			   "parallel_output_mode",
			   "min_icl",
			   "cp_switcher_en",
			   "cp_enable",
			   "cp_ilim",
			   "cp_die_temp",
			   "current_capability";
	qcom,battery-data = <&mtp_batterydata>;
	qcom,sec-charger-config = <1>;
	qcom,auto-recharge-soc = <98>;
	qcom,step-charging-enable;
	qcom,sw-jeita-enable;
	qcom,charger-temp-max = <800>;
	qcom,smb-temp-max = <800>;
	qcom,suspend-input-on-debug-batt;
	qcom,fcc-stepping-enable;
	qcom,fcc-step-delay-ms = <100>;
	qcom,fcc-step-size-ua = <100000>;
	qcom,smb-internal-pull-kohm = <0>;
	qcom,en-skin-therm-mitigation;
	qcom,hvdcp3-standalone-config;
};

&pm7250b_qg {
	status = "ok";
	#io-channel-cells = <1>;
	io-channels = <&pm7250b_vadc ADC5_BAT_THERM_100K_PU>,
		      <&pm7250b_vadc ADC5_BAT_ID_100K_PU>,
		      <&pm7250b_charger PSY_IIO_INPUT_CURRENT_LIMITED>,
		      <&pm7250b_charger PSY_IIO_RECHARGE_SOC>,
		      <&pm7250b_charger PSY_IIO_FORCE_RECHARGE>,
		      <&pm7250b_charger PSY_IIO_CHARGE_DONE>,
		      <&smb1396_div2_cp_master PSY_IIO_CP_ENABLE>;
	io-channel-names = "batt-therm",
			   "batt-id",
			   "input_current_limited",
			   "recharge_soc",
			   "force_recharge",
			   "charge_done",
			   "cp_charging_enabled";
	qcom,battery-data = <&mtp_batterydata>;
	qcom,qg-iterm-ma = <150>;
	qcom,hold-soc-while-full;
	qcom,linearize-soc;
	qcom,cl-feedback-on;
	qcom,tcss-enable;
	qcom,fvss-enable;
	qcom,fvss-vbatt-mv = <3300>;
	qcom,bass-enable;
	qcom,use-cp-iin-sns;
};

&pm6150a_amoled {
	status = "ok";
};

&pm7250b_charger {
	dpdm-supply = <&qusb_phy0>;

	smb5_vbus: qcom,smb5-vbus {
		regulator-name = "smb5-vbus";
	};

	smb5_vconn: qcom,smb5-vconn {
		regulator-name = "smb5-vconn";
	};
};

&pm7250b_vadc {
	smb1390_therm@e {
		qcom,scale-fn-type = <ADC_SCALE_HW_CALIB_PM5_SMB1398_TEMP>;
	};
};

&pm7250b_gpios {
	smb_stat {
		smb_stat_default: smb_stat_default {
			pins = "gpio6";
			function = "normal";
			input-enable;
			bias-pull-up;
			qcom,pull-up-strength = <PMIC_GPIO_PULL_UP_30>;
			power-source = <0>;
		};
	};
};

&qupv3_se10_i2c {
	qcom,clk-freq-out = <100000>;
	status = "ok";
	#include "smb1398.dtsi"
};

&smb1396 {
	interrupts = <0x2 0xc5 0x0 IRQ_TYPE_LEVEL_LOW>;
	interrupt-parent = <&spmi_bus>;
	interrupt-names = "smb1396";
	pinctrl-names = "default";
	qcom,enable-toggle-stat;
	pinctrl-0 = <&smb_stat_default>;
	status = "ok";
};

&smb1396_div2_cp_master {
	io-channels = <&smb1396_div2_cp_slave PSY_IIO_CURRENT_CAPABILITY>,
		      <&smb1396_div2_cp_slave PSY_IIO_CP_ENABLE>,
		      <&smb1396_div2_cp_slave PSY_IIO_CP_INPUT_CURRENT_MAX>,
		      <&pm7250b_vadc ADC5_AMUX_THM2>,
		      <&pm7250b_charger PSY_IIO_USB_REAL_TYPE>,
		      <&pm7250b_charger PSY_IIO_ADAPTER_CC_MODE>,
		      <&pm7250b_charger PSY_IIO_PD_CURRENT_MAX>,
		      <&pm7250b_charger PSY_IIO_USB_INPUT_CURRENT_SETTLED>,
		      <&pm7250b_charger PSY_IIO_SMB_EN_MODE>,
		      <&pm7250b_charger PSY_IIO_SMB_EN_REASON>;
	io-channel-names = "current_capability",
			   "cp_enable",
			   "cp_input_current_max",
			   "die_temp",
			   "real_type",
			   "adapter_cc_mode",
			   "pd_current_max",
			   "input_current_settled",
			   "smb_en_mode",
			   "smb_en_reason";
	qcom,parallel-input-mode = <1>; /* USBIN */
	qcom,parallel-output-mode = <2>; /* VBAT */
	status = "ok";
};

&smb1396_slave {
	status = "ok";
};

&smb1396_div2_cp_slave {
	status = "ok";
};

&pm7250b_pdphy {
	vdd-pdphy-supply = <&L3A>;
	vbus-supply = <&smb5_vbus>;
	vconn-supply = <&smb5_vconn>;

	#io-channel-cells = <1>;
	io-channels = <&pm7250b_charger PSY_IIO_PD_ACTIVE>,
		      <&pm7250b_charger PSY_IIO_TYPEC_CC_ORIENTATION>,
		      <&pm7250b_charger PSY_IIO_CONNECTOR_TYPE>,
		      <&pm7250b_charger PSY_IIO_TYPEC_POWER_ROLE>,
		      <&pm7250b_charger PSY_IIO_PD_USB_SUSPEND_SUPPORTED>,
		      <&pm7250b_charger PSY_IIO_TYPEC_SRC_RP>,
		      <&pm7250b_charger PSY_IIO_PD_IN_HARD_RESET>,
		      <&pm7250b_charger PSY_IIO_PD_CURRENT_MAX>,
		      <&pm7250b_charger PSY_IIO_PR_SWAP>,
		      <&pm7250b_charger PSY_IIO_PD_VOLTAGE_MIN>,
		      <&pm7250b_charger PSY_IIO_PD_VOLTAGE_MAX>,
		      <&pm7250b_charger PSY_IIO_USB_REAL_TYPE>,
		      <&pm7250b_charger PSY_IIO_TYPEC_MODE>,
		      <&pm7250b_charger PSY_IIO_PE_START>;
	io-channel-names = "pd_active",
			   "typec_cc_orientation",
			   "connector_type",
			   "typec_power_role",
			   "pd_usb_suspend_supported",
			   "typec_src_rp",
			   "pd_in_hard_reset",
			   "pr_current_max",
			   "pr_swap",
			   "pd_voltage_min",
			   "pd_voltage_max",
			   "real_type",
			   "typec_mode",
			   "pe_start";
};

&usb0 {
	extcon = <&pm7250b_pdphy>, <&eud>;
};
