Diodes AP72200 voltage regulator

AP72200 is a high-current synchronous buck-boost converter providing
high efficiency, excellent transient response, and high DC output accuracy.
It operates with a 2.3-5.4V Input range and Outputs 2.6-5.14V.

Properties:
- compatible
	Usage:      required
	Value type: <string>
	Definition: Must be "diodes,ap72200".

- reg
	Usage:      required
	Value type: <u32>
	Definition: I2C slave address.

- enable-gpio:
	Usage:      required
	Value type: <phandle>
	Definition: Phandle to GPIO used to control enable status of regulator.

Example:
&qupv3_se2_i2c {
	itof_level: ap72200-regulator@43 {
		reg = <0x43>;
		compatible = "diodes,ap72200";
		enable-gpio = <&tlmm 87 GPIO_ACTIVE_HIGH>;
		regulator-name = "ap72200-vout";
		regulator-min-microvolt = <3600000>;
		regulator-max-microvolt = <3600000>;
	};
};

