#include <dt-bindings/interconnect/qcom,lahaina.h>

&soc {

	/* QUPv3 Instances
	 * North   0 : SE 0
	 * North   1 : SE 1
	 * North   2 : SE 2
	 * North   3 : SE 3
	 * North   4 : SE 4
	 * North   5 : SE 5
	 * North   6 : SE 6
	 * North   7 : SE 7
	 * South_1 0 : SE 8
	 * South_1 1 : SE 9
	 * South_1 2 : SE 10
	 * South_1 3 : SE 11
	 * South_1 4 : SE 12
	 * South_1 5 : SE 13
	 * South_2 0 : SE 14
	 * South_2 1 : SE 15
	 * South_2 2 : SE 16
	 * South_2 3 : SE 17
	 * South_2 4 : SE 18
	 * South_2 5 : SE 19
	 */

	/* QUPv3_0  wrapper  instance : North QUP*/
	qupv3_0: qcom,qupv3_0_geni_se@9c0000 {
		compatible = "qcom,qupv3-geni-se";
		reg = <0x9c0000 0x2000>;
		qcom,msm-bus,num-paths = <2>;
		qcom,msm-bus,vectors-bus-ids =
			<MASTER_QUP_CORE_0 SLAVE_QUP_CORE_0>,
			<MASTER_QUP_0 SLAVE_EBI1>;
		iommus = <&apps_smmu 0x5a3 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0xc0000000>;
		qcom,iommu-dma = "fastmap";
	};

	/* GPI */
	gpi_dma0: qcom,gpi-dma@900000 {
		compatible = "qcom,gpi-dma";
		#dma-cells = <5>;
		reg = <0x900000 0x60000>;
		reg-names = "gpi-top";
		interrupts = <GIC_SPI 244 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 245 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 246 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 247 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 248 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 249 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 250 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 251 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 252 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 253 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 254 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 255 IRQ_TYPE_LEVEL_HIGH>;
		qcom,max-num-gpii = <12>;
		qcom,static-gpii-mask = <0x1>;
		qcom,gpii-mask = <0x7e>;
		qcom,ev-factor = <2>;
		iommus = <&apps_smmu 0x5b6 0x0>;
		qcom,gpi-ee-offset = <0x10000>;
		qcom,iommu-dma-addr-pool = <0x100000 0x100000>;
		qcom,le-vm;
		status = "ok";
	};

	/* PORed Debug UART */
	qupv3_se3_2uart: qcom,qup_uart@98c000 {
		compatible = "qcom,msm-geni-console";
		reg = <0x98C000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S3_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se3_2uart_active>;
		pinctrl-1 = <&qupv3_se3_2uart_sleep>;
		interrupts = <GIC_SPI 604 IRQ_TYPE_LEVEL_HIGH>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "ok";
	};

	/* Debug UART Instance for RUMI */
	qupv3_se2_2uart: qcom,qup_uart@988000 {
		compatible = "qcom,msm-geni-console";
		reg = <0x988000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S2_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se2_2uart_active>;
		pinctrl-1 = <&qupv3_se2_2uart_sleep>;
		interrupts = <GIC_SPI 603 IRQ_TYPE_LEVEL_HIGH>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	/* Travel adapter over 2-wire HSUART, no wakeup */
	qupv3_se6_2uart: qcom,qup_uart@998000 {
		compatible = "qcom,msm-geni-serial-hs";
		reg = <0x998000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S6_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "active", "sleep";
		pinctrl-0 = <&qupv3_se6_default_txrx>;
		pinctrl-1 = <&qupv3_se6_2uart_active>;
		pinctrl-2 = <&qupv3_se6_2uart_sleep>;
		interrupts = <GIC_SPI 607 IRQ_TYPE_LEVEL_HIGH>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	/* SPI */
	qupv3_se0_spi: spi@980000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x980000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S0_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se0_spi_active>;
		pinctrl-1 = <&qupv3_se0_spi_sleep>;
		interrupts = <GIC_SPI 601 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		dmas = <&gpi_dma0 0 0 1 64 0>,
			<&gpi_dma0 1 0 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se1_spi: spi@984000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x984000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S1_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se1_spi_active>;
		pinctrl-1 = <&qupv3_se1_spi_sleep>;
		interrupts = <GIC_SPI 602 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		dmas = <&gpi_dma0 0 1 1 64 0>,
			<&gpi_dma0 1 1 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se2_spi: spi@988000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x988000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S2_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se2_spi_active>;
		pinctrl-1 = <&qupv3_se2_spi_sleep>;
		interrupts = <GIC_SPI 603 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		dmas = <&gpi_dma0 0 2 1 64 0>,
			<&gpi_dma0 1 2 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se4_spi: spi@990000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x990000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S4_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se4_spi_active>;
		pinctrl-1 = <&qupv3_se4_spi_sleep>;
		interrupts = <GIC_SPI 605 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		dmas = <&gpi_dma0 0 4 1 64 2>,
			<&gpi_dma0 1 4 1 64 2>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se5_spi: spi@994000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x994000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S5_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se5_spi_active>;
		pinctrl-1 = <&qupv3_se5_spi_sleep>;
		interrupts = <GIC_SPI 606 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		dmas = <&gpi_dma0 0 5 1 64 0>,
			<&gpi_dma0 1 5 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se6_spi: spi@998000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x998000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S6_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se6_spi_active>;
		pinctrl-1 = <&qupv3_se6_spi_sleep>;
		interrupts = <GIC_SPI 607 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		dmas = <&gpi_dma0 0 6 1 64 0>,
			<&gpi_dma0 1 6 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se7_spi: spi@99c000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x99c000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S7_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se7_spi_active>;
		pinctrl-1 = <&qupv3_se7_spi_sleep>;
		interrupts = <GIC_SPI 608 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		dmas = <&gpi_dma0 0 7 1 64 0>,
			<&gpi_dma0 1 7 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	/* I2C */
	qupv3_se0_i2c: i2c@980000 {
		compatible = "qcom,i2c-geni";
		reg = <0x980000 0x4000>;
		interrupts = <GIC_SPI 601 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S0_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		dmas = <&gpi_dma0 0 0 3 64 0>,
			<&gpi_dma0 1 0 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se0_i2c_active>;
		pinctrl-1 = <&qupv3_se0_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se1_i2c: i2c@984000 {
		compatible = "qcom,i2c-geni";
		reg = <0x984000 0x4000>;
		interrupts = <GIC_SPI 602 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S1_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		dmas = <&gpi_dma0 0 1 3 64 0>,
			<&gpi_dma0 1 1 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se1_i2c_active>;
		pinctrl-1 = <&qupv3_se1_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se2_i2c: i2c@988000 {
		compatible = "qcom,i2c-geni";
		reg = <0x988000 0x4000>;
		interrupts = <GIC_SPI 603 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S2_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		dmas = <&gpi_dma0 0 2 3 64 0>,
			<&gpi_dma0 1 2 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se2_i2c_active>;
		pinctrl-1 = <&qupv3_se2_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se4_i2c: i2c@990000 {
		compatible = "qcom,i2c-geni";
		reg = <0x990000 0x4000>;
		interrupts = <GIC_SPI 605 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S4_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		dmas = <&gpi_dma0 0 4 3 64 2>,
			<&gpi_dma0 1 4 3 64 2>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se4_i2c_active>;
		pinctrl-1 = <&qupv3_se4_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se5_i2c: i2c@994000 {
		compatible = "qcom,i2c-geni";
		reg = <0x994000 0x4000>;
		interrupts = <GIC_SPI 606 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S5_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		dmas = <&gpi_dma0 0 5 3 64 0>,
			<&gpi_dma0 1 5 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se5_i2c_active>;
		pinctrl-1 = <&qupv3_se5_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se6_i2c: i2c@998000 {
		compatible = "qcom,i2c-geni";
		reg = <0x998000 0x4000>;
		interrupts = <GIC_SPI 607 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S6_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		dmas = <&gpi_dma0 0 6 3 64 0>,
			<&gpi_dma0 1 6 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se6_i2c_active>;
		pinctrl-1 = <&qupv3_se6_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se7_i2c: i2c@99c000 {
		compatible = "qcom,i2c-geni";
		reg = <0x99c000 0x4000>;
		interrupts = <GIC_SPI 608 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP0_S7_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		dmas = <&gpi_dma0 0 7 3 64 0>,
			<&gpi_dma0 1 7 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se7_i2c_active>;
		pinctrl-1 = <&qupv3_se7_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	/* QUPv3_1  wrapper  instance : South 1 QUP */
	qupv3_1: qcom,qupv3_1_geni_se@ac0000 {
		compatible = "qcom,qupv3-geni-se";
		reg = <0xac0000 0x2000>;
		qcom,msm-bus,num-paths = <2>;
		qcom,msm-bus,vectors-bus-ids =
			<MASTER_QUP_CORE_1 SLAVE_QUP_CORE_1>,
			<MASTER_QUP_1 SLAVE_EBI1>;
		iommus = <&apps_smmu 0x43 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0xc0000000>;
		qcom,iommu-dma = "fastmap";
	};

	/* GPI */
	gpi_dma1: qcom,gpi-dma@a00000 {
		compatible = "qcom,gpi-dma";
		#dma-cells = <5>;
		reg = <0xa00000 0x60000>;
		reg-names = "gpi-top";
		interrupts = <GIC_SPI 279 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 280 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 281 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 282 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 283 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 284 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 293 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 294 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 295 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 296 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 297 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 298 IRQ_TYPE_LEVEL_HIGH>;
		qcom,max-num-gpii = <12>;
		qcom,gpii-mask = <0xff>;
		qcom,ev-factor = <2>;
		iommus = <&apps_smmu 0x56 0x0>;
		qcom,gpi-ee-offset = <0x10000>;
		qcom,iommu-dma-addr-pool = <0x100000 0x100000>;
		status = "ok";
	};

	/* I3C */
	i3c0: i3c-master@a80000 {
		compatible = "qcom,geni-i3c";
		reg = <0xa80000 0x4000>,
			<0xec90000 0x10000>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S0_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se8_i3c_active>;
		pinctrl-1 = <&qupv3_se8_i3c_sleep>;
		interrupts-extended  = <&intc GIC_SPI 353 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 31 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 30 IRQ_TYPE_LEVEL_HIGH>;
		qcom,ibi-ctrl-id = <8>;
		#address-cells = <3>;
		#size-cells = <0>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	i3c1: i3c-master@a84000 {
		compatible = "qcom,geni-i3c";
		reg = <0xa84000 0x4000>,
			<0xeca0000 0x10000>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S1_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se9_i3c_active>;
		pinctrl-1 = <&qupv3_se9_i3c_sleep>;
		interrupts-extended  = <&intc GIC_SPI 354 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 33 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 32 IRQ_TYPE_LEVEL_HIGH>;
		qcom,ibi-ctrl-id = <1>;
		#address-cells = <3>;
		#size-cells = <0>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	/* SPI */
	qupv3_se8_spi: spi@a80000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0xa80000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S0_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se8_spi_active>;
		pinctrl-1 = <&qupv3_se8_spi_sleep>;
		interrupts = <GIC_SPI 353 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_1>;
		dmas = <&gpi_dma1 0 0 1 64 0>,
			<&gpi_dma1 1 0 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se9_spi: spi@a84000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0xa84000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S1_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se9_spi_active>;
		pinctrl-1 = <&qupv3_se9_spi_sleep>;
		interrupts = <GIC_SPI 354 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_1>;
		dmas = <&gpi_dma1 0 1 1 64 0>,
			<&gpi_dma1 1 1 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se10_spi: spi@a88000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0xa88000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S2_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se10_spi_active>;
		pinctrl-1 = <&qupv3_se10_spi_sleep>;
		interrupts = <GIC_SPI 355 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_1>;
		dmas = <&gpi_dma1 0 2 1 64 0>,
			<&gpi_dma1 1 2 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se11_spi: spi@a8c000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0xa8c000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S3_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se11_spi_active>;
		pinctrl-1 = <&qupv3_se11_spi_sleep>;
		interrupts = <GIC_SPI 356 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_1>;
		dmas = <&gpi_dma1 0 3 1 64 0>,
			<&gpi_dma1 1 3 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se12_spi: spi@a90000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0xa90000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S4_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se12_spi_active>;
		pinctrl-1 = <&qupv3_se12_spi_sleep>;
		interrupts = <GIC_SPI 357 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_1>;
		dmas = <&gpi_dma1 0 4 1 64 0>,
			<&gpi_dma1 1 4 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se13_spi: spi@a94000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0xa94000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S5_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se13_spi_active>;
		pinctrl-1 = <&qupv3_se13_spi_sleep>;
		interrupts = <GIC_SPI 358 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_1>;
		dmas = <&gpi_dma1 0 5 1 64 0>,
			<&gpi_dma1 1 5 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	/* I2C */
	qupv3_se8_i2c: i2c@a80000 {
		compatible = "qcom,i2c-geni";
		reg = <0xa80000 0x4000>;
		interrupts = <GIC_SPI 353 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S0_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		dmas = <&gpi_dma1 0 0 3 64 0>,
			<&gpi_dma1 1 0 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se8_i2c_active>;
		pinctrl-1 = <&qupv3_se8_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se9_i2c: i2c@a84000 {
		compatible = "qcom,i2c-geni";
		reg = <0xa84000 0x4000>;
		interrupts = <GIC_SPI 354 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S1_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		dmas = <&gpi_dma1 0 1 3 64 0>,
			<&gpi_dma1 1 1 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se9_i2c_active>;
		pinctrl-1 = <&qupv3_se9_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se10_i2c: i2c@a88000 {
		compatible = "qcom,i2c-geni";
		reg = <0xa88000 0x4000>;
		interrupts = <GIC_SPI 355 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S2_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		dmas = <&gpi_dma1 0 2 3 64 0>,
			<&gpi_dma1 1 2 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se10_i2c_active>;
		pinctrl-1 = <&qupv3_se10_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se11_i2c: i2c@a8c000 {
		compatible = "qcom,i2c-geni";
		reg = <0xa8c000 0x4000>;
		interrupts = <GIC_SPI 356 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S3_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		dmas = <&gpi_dma1 0 3 3 64 0>,
			<&gpi_dma1 1 3 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se11_i2c_active>;
		pinctrl-1 = <&qupv3_se11_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se12_i2c: i2c@a90000 {
		compatible = "qcom,i2c-geni";
		reg = <0xa90000 0x4000>;
		interrupts = <GIC_SPI 357 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S4_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		dmas = <&gpi_dma1 0 4 3 64 0>,
			<&gpi_dma1 1 4 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se12_i2c_active>;
		pinctrl-1 = <&qupv3_se12_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se13_i2c: i2c@a94000 {
		compatible = "qcom,i2c-geni";
		reg = <0xa94000 0x4000>;
		interrupts = <GIC_SPI 358 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP1_S5_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		dmas = <&gpi_dma1 0 5 3 64 0>,
			<&gpi_dma1 1 5 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se13_i2c_active>;
		pinctrl-1 = <&qupv3_se13_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_1>;
		qcom,shared;
		status = "disabled";
	};

	/* QUPv3_2  wrapper  instance : South 2 QUP */
	qupv3_2: qcom,qupv3_2_geni_se@8c0000 {
		compatible = "qcom,qupv3-geni-se";
		reg = <0x8c0000 0x2000>;
		qcom,msm-bus,num-paths = <2>;
		qcom,msm-bus,vectors-bus-ids =
			<MASTER_QUP_CORE_2 SLAVE_QUP_CORE_2>,
			<MASTER_QUP_2 SLAVE_EBI1>;
		iommus = <&apps_smmu 0x5e3 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0xc0000000>;
		qcom,iommu-dma = "fastmap";
	};

	/* GPI */
	gpi_dma2: qcom,gpi-dma@800000 {
		compatible = "qcom,gpi-dma";
		#dma-cells = <5>;
		reg = <0x800000 0x60000>;
		reg-names = "gpi-top";
		interrupts = <GIC_SPI 588 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 589 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 590 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 591 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 592 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 593 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 594 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 595 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 596 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 597 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 598 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 599 IRQ_TYPE_LEVEL_HIGH>;
		qcom,max-num-gpii = <12>;
		qcom,gpii-mask = <0xff>;
		qcom,ev-factor = <2>;
		iommus = <&apps_smmu 0x5f6 0x0>;
		qcom,gpi-ee-offset = <0x10000>;
		qcom,iommu-dma-addr-pool = <0x100000 0x100000>;
		status = "ok";
	};

	/* I3C */
	i3c2: i3c-master@880000 {
		compatible = "qcom,geni-i3c";
		reg = <0x880000 0x4000>,
			<0xecb0000 0x10000>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S0_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se14_i3c_active>;
		pinctrl-1 = <&qupv3_se14_i3c_sleep>;
		interrupts-extended  = <&intc GIC_SPI 373 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 35 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 34 IRQ_TYPE_LEVEL_HIGH>;
		qcom,ibi-ctrl-id = <14>;
		#address-cells = <3>;
		#size-cells = <0>;
		qcom,wrapper-core = <&qupv3_2>;
		status = "disabled";
	};

	i3c3: i3c-master@884000 {
		compatible = "qcom,geni-i3c";
		reg = <0x884000 0x4000>,
			<0xecc0000 0x10000>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S1_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se15_i3c_active>;
		pinctrl-1 = <&qupv3_se15_i3c_sleep>;
		interrupts-extended  = <&intc GIC_SPI 583 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 37 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 36 IRQ_TYPE_LEVEL_HIGH>;
		qcom,ibi-ctrl-id = <15>;
		#address-cells = <3>;
		#size-cells = <0>;
		qcom,wrapper-core = <&qupv3_2>;
		status = "disabled";
	};

	/* HS UART Instance */
	qupv3_se18_4uart: qcom,qup_uart@890000 {
		compatible = "qcom,msm-geni-serial-hs";
		reg = <0x890000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S4_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		pinctrl-names = "default", "active", "sleep";
		pinctrl-0 = <&qupv3_se18_default_cts>,
			<&qupv3_se18_default_rtsrx>, <&qupv3_se18_default_tx>;
		pinctrl-1 = <&qupv3_se18_ctsrx>, <&qupv3_se18_rts>,
							<&qupv3_se18_tx>;
		pinctrl-2 = <&qupv3_se18_ctsrx>, <&qupv3_se18_rts>,
							<&qupv3_se18_tx>;
		interrupts-extended = <&intc GIC_SPI 586 IRQ_TYPE_LEVEL_HIGH>,
				<&tlmm 71 IRQ_TYPE_LEVEL_HIGH>;
		qcom,wrapper-core = <&qupv3_2>;
		qcom,wakeup-byte = <0xFD>;
		status = "disabled";
	};

	/* SPI */
	qupv3_se14_spi: spi@880000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x880000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S0_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se14_spi_active>;
		pinctrl-1 = <&qupv3_se14_spi_sleep>;
		interrupts = <GIC_SPI 373 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_2>;
		dmas = <&gpi_dma2 0 0 1 64 0>,
			<&gpi_dma2 1 0 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se15_spi: spi@884000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x884000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S1_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se15_spi_active>;
		pinctrl-1 = <&qupv3_se15_spi_sleep>;
		interrupts = <GIC_SPI 583 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_2>;
		dmas = <&gpi_dma2 0 1 1 64 0>,
			<&gpi_dma2 1 1 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se16_spi: spi@888000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x888000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S2_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se16_spi_active>;
		pinctrl-1 = <&qupv3_se16_spi_sleep>;
		interrupts = <GIC_SPI 584 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_2>;
		dmas = <&gpi_dma2 0 2 1 64 0>,
			<&gpi_dma2 1 2 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se17_spi: spi@88c000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x88c000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S3_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se17_spi_active>;
		pinctrl-1 = <&qupv3_se17_spi_sleep>;
		interrupts = <GIC_SPI 585 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_2>;
		dmas = <&gpi_dma2 0 3 1 64 0>,
			<&gpi_dma2 1 3 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	qupv3_se19_spi: spi@894000 {
		compatible = "qcom,spi-geni";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x894000 0x4000>;
		reg-names = "se_phys";
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S5_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se19_spi_active>;
		pinctrl-1 = <&qupv3_se19_spi_sleep>;
		interrupts = <GIC_SPI 587 IRQ_TYPE_LEVEL_HIGH>;
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_2>;
		dmas = <&gpi_dma2 0 5 1 64 0>,
			<&gpi_dma2 1 5 1 64 0>;
		dma-names = "tx", "rx";
		status = "disabled";
	};

	/* I2C */
	qupv3_se14_i2c: i2c@880000 {
		compatible = "qcom,i2c-geni";
		reg = <0x880000 0x4000>;
		interrupts = <GIC_SPI 373 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S0_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		dmas = <&gpi_dma2 0 0 3 64 0>,
			<&gpi_dma2 1 0 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se14_i2c_active>;
		pinctrl-1 = <&qupv3_se14_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_2>;
		status = "disabled";
	};

	qupv3_se15_i2c: i2c@884000 {
		compatible = "qcom,i2c-geni";
		reg = <0x884000 0x4000>;
		interrupts = <GIC_SPI 583 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S1_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		dmas = <&gpi_dma2 0 1 3 64 0>,
			<&gpi_dma2 1 1 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se15_i2c_active>;
		pinctrl-1 = <&qupv3_se15_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_2>;
		status = "disabled";
	};

	qupv3_se16_i2c: i2c@888000 {
		compatible = "qcom,i2c-geni";
		reg = <0x888000 0x4000>;
		interrupts = <GIC_SPI 584 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S2_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		dmas = <&gpi_dma2 0 2 3 64 0>,
			<&gpi_dma2 1 2 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se16_i2c_active>;
		pinctrl-1 = <&qupv3_se16_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_2>;
		status = "disabled";
	};

	qupv3_se17_i2c: i2c@88c000 {
		compatible = "qcom,i2c-geni";
		reg = <0x88c000 0x4000>;
		interrupts = <GIC_SPI 585 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S3_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		dmas = <&gpi_dma2 0 3 3 64 0>,
			<&gpi_dma2 1 3 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se17_i2c_active>;
		pinctrl-1 = <&qupv3_se17_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_2>;
		status = "disabled";
	};

	qupv3_se19_i2c: i2c@894000 {
		compatible = "qcom,i2c-geni";
		reg = <0x894000 0x4000>;
		interrupts = <GIC_SPI 587 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <0>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&clock_gcc GCC_QUPV3_WRAP2_S5_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_M_AHB_CLK>,
			<&clock_gcc GCC_QUPV3_WRAP_2_S_AHB_CLK>;
		dmas = <&gpi_dma2 0 5 3 64 0>,
			<&gpi_dma2 1 5 3 64 0>;
		dma-names = "tx", "rx";
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se19_i2c_active>;
		pinctrl-1 = <&qupv3_se19_i2c_sleep>;
		qcom,wrapper-core = <&qupv3_2>;
		status = "disabled";
	};

};
