#include <dt-bindings/regulator/qcom,rpmh-regulator-levels.h>


/ {
	L1B: pmxr2230_l1: regulator-pmxr2230-l1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l1";
		regulator-min-microvolt = <830000>;
		regulator-max-microvolt = <920000>;
		qcom,hpm-min-load = <10000>;
	};

	L2B: pmxr2230_l2: regulator-pmxr2230-l2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l2";
		regulator-min-microvolt = <1170000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <10000>;
	};

	L3B: pmxr2230_l3: regulator-pmxr2230-l3 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l3";
		regulator-min-microvolt = <1080000>;
		regulator-max-microvolt = <1320000>;
		qcom,hpm-min-load = <10000>;
	};

	L4B: pmxr2230_l4: regulator-pmxr2230-l4 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l4";
		regulator-min-microvolt = <1710000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <10000>;
	};

	L5B: pmxr2230_l5: regulator-pmxr2230-l5 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l5";
		regulator-min-microvolt = <1710000>;
		regulator-max-microvolt = <1890000>;
		qcom,hpm-min-load = <10000>;
	};

	L6B: pmxr2230_l6: regulator-pmxr2230-l6 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l6";
		regulator-min-microvolt = <1620000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <10000>;
	};

	L7B: pmxr2230_l7: regulator-pmxr2230-l7 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l7";
		regulator-min-microvolt = <512000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <10000>;
	};

	L8B: pmxr2230_l8: regulator-pmxr2230-l8 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l8";
		regulator-min-microvolt = <1700000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <10000>;
	};

	L9B: pmxr2230_l9: regulator-pmxr2230-l9 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l9";
		regulator-min-microvolt = <1700000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <10000>;
	};

	L10B: pmxr2230_l10: regulator-pmxr2230-l10 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l10";
		regulator-min-microvolt = <1620000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <10000>;
	};

	L11B: pmxr2230_l11: regulator-pmxr2230-l11 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l11";
		regulator-min-microvolt = <1620000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <10000>;
	};

	L12B: pmxr2230_l12: regulator-pmxr2230-l12 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l12";
		regulator-min-microvolt = <2504000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <10000>;
	};

	L13B: pmxr2230_l13: regulator-pmxr2230-l13 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l13";
		regulator-min-microvolt = <1504000>;
		regulator-max-microvolt = <3544000>;
		qcom,hpm-min-load = <10000>;
	};

	L14B: pmxr2230_l14: regulator-pmxr2230-l14 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l14";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3544000>;
		qcom,hpm-min-load = <10000>;
	};

	L15B: pmxr2230_l15: regulator-pmxr2230-l15 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l15";
		regulator-min-microvolt = <2700000>;
		regulator-max-microvolt = <3544000>;
		qcom,hpm-min-load = <10000>;
	};

	L16B: pmxr2230_l16: regulator-pmxr2230-l16 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l16";
		regulator-min-microvolt = <1504000>;
		regulator-max-microvolt = <3544000>;
		qcom,hpm-min-load = <10000>;
	};

	L17B: pmxr2230_l17: regulator-pmxr2230-l17 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l17";
		regulator-min-microvolt = <1504000>;
		regulator-max-microvolt = <3544000>;
		qcom,hpm-min-load = <10000>;
	};

	L18B: pmxr2230_l18: regulator-pmxr2230-l18 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l18";
		regulator-min-microvolt = <1760000>;
		regulator-max-microvolt = <3100000>;
		qcom,hpm-min-load = <10000>;
	};

	L19B: pmxr2230_l19: regulator-pmxr2230-l19 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_l19";
		regulator-min-microvolt = <1504000>;
		regulator-max-microvolt = <3544000>;
		qcom,hpm-min-load = <10000>;
	};

	BOB: pmxr2230_bob: regulator-pmxr2230-bob {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_bob";
		regulator-min-microvolt = <1504000>;
		regulator-max-microvolt = <3960000>;
	};

	VDD_MM_LEVEL:
	S4B_LEVEL:
	pmxr2230_s4_level: regulator-pmxr2230-s4-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_s4_level";
		regulator-min-microvolt = <RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	S1B: pmxr2230_s1: regulator-pmxr2230-s1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_s1";
		regulator-min-microvolt = <1816000>;
		regulator-max-microvolt = <2040000>;
	};

	S2B: pmxr2230_s2: regulator-pmxr2230-s2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_s2";
		regulator-min-microvolt = <1224000>;
		regulator-max-microvolt = <1518000>;
	};

	S3B: pmxr2230_s3: regulator-pmxr2230-s3 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_s3";
		regulator-min-microvolt = <880000>;
		regulator-max-microvolt = <1120000>;
	};

	S6B: pmxr2230_s6: regulator-pmxr2230-s6 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pmxr2230_s6";
		regulator-min-microvolt = <352000>;
		regulator-max-microvolt = <888000>;
	};

	VDD_LPI_CX_LEVEL:
	L1C_LEVEL:
	pm_v6c_l1_level: regulator-pm-v6c-l1-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6c_l1_level";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	L2C:
	pm_v6c_l2: regulator-pm-v6c-l2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6c_l2";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <1140000>;
		regulator-max-microvolt = <1260000>;
	};

	VDD_MXA_LEVEL:
	S3C_LEVEL:
	pm_v6c_s3_level: regulator-pm-v6c-s3-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6c_s3_level";
		regulator-min-microvolt = <RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
		qcom,hpm-min-load = <10000>;
	};

	L1D:
	pm_v6d_l1: regulator-pm-v6d-l1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6d_l1";
		regulator-min-microvolt = <720000>;
		regulator-max-microvolt = <950000>;
		qcom,hpm-min-load = <30000>;
	};

	L2D:
	pm_v6d_l2: regulator-pm-v6d-l2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6d_l2";
		regulator-min-microvolt = <870000>;
		regulator-max-microvolt = <970000>;
		qcom,hpm-min-load = <30000>;
	};

	L3D:
	pm_v6d_l3: regulator-pm-v6d-l3 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6d_l3";
		regulator-min-microvolt = <320000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <30000>;
	};

	VDD_EBI_LEVEL:
	S4D_LEVEL:
	pm_v6d_s4_level: regulator-pm-v6d-s4-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6d_s4_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	S5D:
	pm_v6d_s5: regulator-pm-v6d-s5 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6d_s5";
		regulator-min-microvolt = <300000>;
		regulator-max-microvolt = <570000>;
		qcom,hpm-min-load = <10000>;
	};

	VDD_CX_LEVEL:
	S6D_LEVEL:
	pm_v6d_s6_level: regulator-pm-v6d-s6-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v6d_s6_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_LPI_MX_LEVEL:
	L1F_LEVEL:
	pm_v8_l1_level: regulator-pm-v8-l1-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v8_l1_level";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	L2F:
	pm_v8_l2: regulator-pm-v8-l2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v8_l2";
		regulator-min-microvolt = <788000>;
		regulator-max-microvolt = <1050000>;
		qcom,hpm-min-load = <30000>;
	};

	L3F:
	pm_v8_l3: regulator-pm-v8-l3 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v8_l3";
		regulator-min-microvolt = <1700000>;
		regulator-max-microvolt = <1800000>;
		qcom,hpm-min-load = <30000>;
	};

	VDD_MXC_LEVEL:
	S2F_LEVEL:
	VDD_MM_MXC_VOTER_LEVEL:
	VDD_GFX_MXC_VOTER_LEVEL:
	pm_v8_s2_level: regulator-pm-v8-s2-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v8_s2_level";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	S4F:
	pm_v8_s4: regulator-pm-v8-s4 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v8_s4";
		regulator-min-microvolt = <806000>;
		regulator-max-microvolt = <2210000>;
		qcom,hpm-min-load = <10000>;
	};

	VDD_GFX_LEVEL:
	S5F_LEVEL:
	pm_v8_s5_level: regulator-pm-v8-s5-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm_v8_s5_level";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	L1I: pm8010i_l1: regulator-pm8010i-l1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010i_l1";
		regulator-min-microvolt = <1140000>;
		regulator-max-microvolt = <1260000>;
		qcom,hpm-min-load = <30000>;
	};

	L2I: pm8010i_l2: regulator-pm8010i-l2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010i_l2";
		regulator-min-microvolt = <528000>;
		regulator-max-microvolt = <1544000>;
		qcom,hpm-min-load = <30000>;
	};

	L3I: pm8010i_l3: regulator-pm8010i-l3 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010i_l3";
		regulator-min-microvolt = <2600000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <30000>;
	};

	L4I: pm8010i_l4: regulator-pm8010i-l4 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010i_l4";
		regulator-min-microvolt = <2600000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <30000>;
	};

	L5I: pm8010i_l5: regulator-pm8010i-l5 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010i_l5";
		regulator-min-microvolt = <2600000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <30000>;
	};

	L6I: pm8010i_l6: regulator-pm8010i-l6 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010i_l6";
		regulator-min-microvolt = <2600000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <30000>;
	};

	L1J: pm8010j_l1: regulator-pm8010j-l1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010j_l1";
		regulator-min-microvolt = <1140000>;
		regulator-max-microvolt = <1260000>;
		qcom,hpm-min-load = <30000>;
	};

	L2J: pm8010j_l2: regulator-pm8010j-l2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010j_l2";
		regulator-min-microvolt = <950000>;
		regulator-max-microvolt = <1150000>;
		qcom,hpm-min-load = <30000>;
	};

	L3J: pm8010j_l3: regulator-pm8010j-l3 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010j_l3";
		regulator-min-microvolt = <2700000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <30000>;
	};

	L4J: pm8010j_l4: regulator-pm8010j-l4 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010j_l4";
		regulator-min-microvolt = <2700000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <30000>;
	};

	L5J: pm8010j_l5: regulator-pm8010j-l5 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010j_l5";
		regulator-min-microvolt = <2600000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <30000>;
	};

	L7J: pm8010j_l7: regulator-pm8010j-l7 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8010j_l7";
		regulator-min-microvolt = <2600000>;
		regulator-max-microvolt = <3000000>;
		qcom,hpm-min-load = <30000>;
	};
};
