* Helioscom Interface Driver

helioscom_interface driver creates a helios_com_dev device
node for user space communication. Single user space
client can open device node for communication from hardware.
Hardware will provide access to read/write registers or AHB
memory in the device.

Required properties:
- compatible:	      Must be "qcom,helios-daemon"

Example:
	qcom,helios-daemon {
		compatible = "qcom,helios-daemon";
		};

