#include <dt-bindings/regulator/qcom,rpmh-regulator-levels.h>

&apps_rsc {
	rpmh-regulator-cxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "cx.lvl";
		proxy-supply = <&VDD_CX_LEVEL>;
		VDD_CX_LEVEL:
		S1B_LEVEL:
		pm6450_s1_level: regulator-pm6450-s1-level {
			regulator-name = "pm6450_s1_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_CX_LEVEL_AO:
		S1B_LEVEL_AO:
		pm6450_s1_level_ao: regulator-pm6450-s1-level-ao {
			regulator-name = "pm6450_s1_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};

		cx_cdev: regulator-cdev {
			compatible = "qcom,rpmh-reg-cdev";
			mboxes = <&qmp_aop 0>;
			qcom,reg-resource-name = "cx";
			#cooling-cells = <2>;
		};
	};

	rpmh-regulator-gfxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "gfx.lvl";
		VDD_GFX_LEVEL: S3B_LEVEL:
		pm6450_s3_level: regulator-pm6450-s3-level {
			regulator-name = "pm6450_s3_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-ebilvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "ebi.lvl";
		VDD_EBI_LEVEL:
		S5B_LEVEL:
		pm6450_s5_level: regulator-pm6450-s5-level {
			regulator-name = "pm6450_s5_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-smpb6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb6";
		S6B:
		pm6450_s6: regulator-pm6450-s6 {
			regulator-name = "pm6450_s6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1010000>;
			regulator-max-microvolt = <1170000>;
			qcom,init-voltage = <1052000>;
		};
	};

	rpmh-regulator-smpb7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb7";
		S7B:
		pm6450_s7: regulator-pm6450-s7 {
			regulator-name = "pm6450_s7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <1174000>;
			qcom,init-voltage = <972000>;
		};
	};

	rpmh-regulator-smpb8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb8";
		S8B:
		pm6450_s8: regulator-pm6450-s8 {
			regulator-name = "pm6450_s8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1224000>;
			regulator-max-microvolt = <1654000>;
			qcom,init-voltage = <1272000>;
		};
	};

	rpmh-regulator-smpb9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb9";
		S9B:
		pm6450_s9: regulator-pm6450-s9 {
			regulator-name = "pm6450_s9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <850000>;
			regulator-max-microvolt = <2208000>;
			qcom,init-voltage = <2208000>;
		};
	};

	rpmh-regulator-ldob1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L1B:
		pm6450_l1: regulator-pm6450-l1 {
			regulator-name = "pm6450_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <300000>;
			regulator-max-microvolt = <650000>;
			qcom,init-voltage = <504000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-lcxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "lcx.lvl";
		VDD_LPI_CX_LEVEL:
		L2B_LEVEL:
		pm6450_l2_level: regulator-pm6450-l2-level {
			regulator-name = "pm6450_l2_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-ldob3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L3B:
		pm6450_l3: regulator-pm6450-l3 {
			regulator-name = "pm6450_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <870000>;
			regulator-max-microvolt = <970000>;
			qcom,init-voltage = <904000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L4B:
		pm6450_l4: regulator-pm6450-l4 {
			regulator-name = "pm6450_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <530000>;
			regulator-max-microvolt = <864000>;
			qcom,init-voltage = <530000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L5B:
		pm6450_l5: regulator-pm6450-l5 {
			regulator-name = "pm6450_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <830000>;
			regulator-max-microvolt = <920000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L6B:
		pm6450_l6: regulator-pm6450-l6 {
			regulator-name = "pm6450_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <751000>;
			regulator-max-microvolt = <824000>;
			qcom,init-voltage = <751000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L7B:
		pm6450_l7: regulator-pm6450-l7 {
			regulator-name = "pm6450_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <830000>;
			regulator-max-microvolt = <920000>;
			qcom,init-voltage = <912000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob8";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L8B:
		pm6450_l8: regulator-pm6450-l8 {
			regulator-name = "pm6450_l8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <870000>;
			regulator-max-microvolt = <970000>;
			qcom,init-voltage = <870000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-lmxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "lmx.lvl";
		VDD_LPI_MX_LEVEL:
		L9B_LEVEL:
		pm6450_l9_level: regulator-pm6450-l9-level {
			regulator-name = "pm6450_l9_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-ldob10 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob10";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L10B:
		pm6450_l10: regulator-pm6450-l10 {
			regulator-name = "pm6450_l10";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <824000>;
			regulator-max-microvolt = <950000>;
			qcom,init-voltage = <824000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob11 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob11";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L11B:
		pm6450_l11: regulator-pm6450-l11 {
			regulator-name = "pm6450_l11";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <348000>;
			regulator-max-microvolt = <888000>;
			qcom,init-voltage = <348000>;
		};
	};

	rpmh-regulator-ldob12 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob12";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L12B:
		pm6450_l12: regulator-pm6450-l12 {
			regulator-name = "pm6450_l12";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1080000>;
			regulator-max-microvolt = <1240000>;
			qcom,init-voltage = <1080000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob13 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob13";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L13B:
		pm6450_l13: regulator-pm6450-l13 {
			regulator-name = "pm6450_l13";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1080000>;
			regulator-max-microvolt = <1304000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob14 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob14";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L14B:
		pm6450_l14: regulator-pm6450-l14 {
			regulator-name = "pm6450_l14";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1150000>;
			regulator-max-microvolt = <1304000>;
			qcom,init-voltage = <1150000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob16 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob16";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L16B:
		pm6450_l16: regulator-pm6450-l16 {
			regulator-name = "pm6450_l16";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1140000>;
			regulator-max-microvolt = <1260000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob17 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob17";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L17B:
		pm6450_l17: regulator-pm6450-l17 {
			regulator-name = "pm6450_l17";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob18 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob18";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L18B:
		pm6450_l18: regulator-pm6450-l18 {
			regulator-name = "pm6450_l18";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1504000>;
			regulator-max-microvolt = <2000000>;
			qcom,init-voltage = <1504000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob19 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob19";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L19B:
		pm6450_l19: regulator-pm6450-l19 {
			regulator-name = "pm6450_l19";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1620000>;
			regulator-max-microvolt = <1980000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob20 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob20";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L20B:
		pm6450_l20: regulator-pm6450-l20 {
			regulator-name = "pm6450_l20";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1700000>;
			regulator-max-microvolt = <1900000>;
			qcom,init-voltage = <1700000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob21 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob21";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L21B:
		pm6450_l21: regulator-pm6450-l21 {
			regulator-name = "pm6450_l21";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1950000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob22 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob22";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L22B:
		pm6450_l22: regulator-pm6450-l22 {
			regulator-name = "pm6450_l22";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <2000000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob23 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob23";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L23B:
		pm6450_l23: regulator-pm6450-l23 {
			regulator-name = "pm6450_l23";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1650000>;
			regulator-max-microvolt = <1950000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob24 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob24";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L24B:
		pm6450_l24: regulator-pm6450-l24 {
			regulator-name = "pm6450_l24";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			/*
			 * Remove min/max voltages for this regulator as initial
			 * voltage of  L24B is set to be 2.4v/2.96v during PON
			 * depending upon the UFS mode. UFS is the only client
			 * on this and this regulator will only be voted
			 * for enabling/disabling conditions.
			 */
		};
	};

	rpmh-regulator-ldob25 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob25";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L25B:
		pm6450_l25: regulator-pm6450-l25 {
			regulator-name = "pm6450_l25";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2700000>;
			regulator-max-microvolt = <3544000>;
			qcom,init-voltage = <3072000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob26 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob26";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L26B:
		pm6450_l26: regulator-pm6450-l26 {
			regulator-name = "pm6450_l26";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1620000>;
			regulator-max-microvolt = <3300000>;
			qcom,init-voltage = <1620000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob27 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob27";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L27B:
		pm6450_l27: regulator-pm6450-l27 {
			regulator-name = "pm6450_l27";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1620000>;
			regulator-max-microvolt = <3300000>;
			qcom,init-voltage = <1620000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob28 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob28";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L28B:
		pm6450_l28: regulator-pm6450-l28 {
			regulator-name = "pm6450_l28";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2700000>;
			regulator-max-microvolt = <3544000>;
			qcom,init-voltage = <2700000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-msslvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mss.lvl";
		VDD_MODEM_LEVEL:
		S1E_LEVEL:
		pm6150l_s1_level: regulator-pm6150l-s1-level {
			regulator-name = "pm6150l_s1_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-mxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mx.lvl";
		proxy-supply = <&VDD_MXA_LEVEL>;

		VDD_MXA_LEVEL:
		S3E_LEVEL:
		pm6150l_s3_level: regulator-pm6150l-s3-level {
			regulator-name = "pm6150l_s3_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MXA_LEVEL_AO: S10C_LEVEL_AO:
		pm6150l_s3_level_ao: regulator-pm6150l-s3-level-ao {
			regulator-name = "pm6150l_s3_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-smpe8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe8";
		S8E:
		pm6150l_s8: regulator-pm6150l-s8 {
			regulator-name = "pm6150l_s8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1816000>;
			regulator-max-microvolt = <2040000>;
			qcom,init-voltage = <1872000>;
		};
	};

	rpmh-regulator-ldoe1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L1E:
		pm6150l_l1: regulator-pm6150l-l1 {
			regulator-name = "pm6150l_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1620000>;
			regulator-max-microvolt = <1980000>;
			qcom,init-voltage = <1620000>;
		};
	};

	rpmh-regulator-ldoe4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L4E:
		pm6150l_l4: regulator-pm6150l-l4 {
			regulator-name = "pm6150l_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2700000>;
			regulator-max-microvolt = <3300000>;
			qcom,init-voltage = <2700000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L5E:
		pm6150l_l5: regulator-pm6150l-l5 {
			regulator-name = "pm6150l_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1504000>;
			regulator-max-microvolt = <3544000>;
			qcom,init-voltage = <1504000>;
		};
	};

	rpmh-regulator-ldoe6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L6E:
		pm6150l_l6: regulator-pm6150l-l6 {
			regulator-name = "pm6150l_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1650000>;
			regulator-max-microvolt = <3300000>;
			qcom,init-voltage = <1650000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L7E:
		pm6150l_l7: regulator-pm6150l-l7 {
			regulator-name = "pm6150l_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3000000>;
			regulator-max-microvolt = <3544000>;
			qcom,init-voltage = <3000000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe8";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L8E:
		pm6150l_l8: regulator-pm6150l-l8 {
			regulator-name = "pm6150l_l8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1620000>;
			regulator-max-microvolt = <2000000>;
			qcom,init-voltage = <1620000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe9";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L9E:
		pm6150l_l9: regulator-pm6150l-l9 {
			regulator-name = "pm6150l_l9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2700000>;
			regulator-max-microvolt = <3544000>;
			qcom,init-voltage = <2700000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe10 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe10";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L10E:
		pm6150l_l10: regulator-pm6150l-l10 {
			regulator-name = "pm6150l_l10";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3000000>;
			regulator-max-microvolt = <3400000>;
			qcom,init-voltage = <3000000>;
			/*
			 * Removed init-mode as it needs to be
			 * set from client votes alone.
			 */
		};
	};

	rpmh-regulator-ldoe11 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe11";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L11E:
		pm6150l_l11: regulator-pm6150l-l11 {
			regulator-name = "pm6150l_l11";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3000000>;
			regulator-max-microvolt = <3400000>;
			qcom,init-voltage = <3000000>;
		};
	};

	rpmh-regulator-ldog2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldog2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L2G:
		pmr735a_l2: regulator-pmr735a-l2 {
			regulator-name = "pmr735a_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1140000>;
			regulator-max-microvolt = <1236000>;
			qcom,init-voltage = <1140000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldog3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldog3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L3G:
		pmr735a_l3: regulator-pmr735a-l3 {
			regulator-name = "pmr735a_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <866000>;
			regulator-max-microvolt = <939000>;
			qcom,init-voltage = <866000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldog4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldog4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L4G:
		pmr735a_l4: regulator-pmr735a-l4 {
			regulator-name = "pmr735a_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1710000>;
			regulator-max-microvolt = <1854000>;
			qcom,init-voltage = <1710000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldog5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldog5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L5G:
		pmr735a_l5: regulator-pmr735a-l5 {
			regulator-name = "pmr735a_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <760000>;
			regulator-max-microvolt = <824000>;
			qcom,init-voltage = <760000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldog6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldog6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L6G:
		pmr735a_l6: regulator-pmr735a-l6 {
			regulator-name = "pmr735a_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <588000>;
			regulator-max-microvolt = <800000>;
			qcom,init-voltage = <588000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-bobe1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "bobe1";
		qcom,regulator-type = "pmic5-bob";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_PASS
			 RPMH_REGULATOR_MODE_AUTO>;
		qcom,mode-threshold-currents = <0 1000000>;
		qcom,send-defaults;

		BOB: pm6150l_bob: regulator-pm6150l-bob {
			regulator-name = "pm6150l_bob";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3008000>;
			regulator-max-microvolt = <3960000>;
			qcom,init-voltage = <3296000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_PASS>;
		};

		BOB_AO: pm6150l_bob_ao: regulator-pm6150l-bob-ao {
			regulator-name = "pm6150l_bob_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt = <3008000>;
			regulator-max-microvolt = <3960000>;
			qcom,init-voltage = <3296000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_AUTO>;
		};
	};
};
