#define MHZ_TO_KBPS(mhz, w) ((mhz * 1000000 * w) / (1024))
&soc {
	pil_gpu: qcom,kgsl-hyp {
		compatible = "qcom,pil-tz-generic";
		qcom,pas-id = <13>;
		qcom,firmware-name = "a615_zap";
		memory-region = <&pil_gpu_micro_code_mem>;
	};

msm_gpu: qcom,kgsl-3d0@5900000 {
		compatible = "qcom,kgsl-3d0", "qcom,adreno-gpu-a619-holi";
		status = "ok";
		reg = <0x5900000 0x40000>,
		    <0x5961000 0x800>,
		    <0x0596A000 0x30000>,
		    <0x599E000 0x1000>;
		reg-names = "kgsl_3d0_reg_memory", "cx_dbgc", "gmu_wrapper", "cx_misc";
		interrupts = <0 177 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "kgsl_3d0_irq";

		clocks = <&gpucc GPU_CC_GX_GFX3D_CLK>,
			<&gpucc GPU_CC_CXO_CLK>,
			<&gcc GCC_BIMC_GPU_AXI_CLK>,
			<&gpucc GPU_CC_AHB_CLK>,
			<&gcc GCC_GPU_MEMNOC_GFX_CLK>,
			<&gpucc GPU_CC_CX_GMU_CLK>;

		clock-names = "core_clk", "rbbmtimer_clk", "iface_clk",
				"ahb_clk", "mem_clk", "gmu_clk";

		vddcx-supply = <&gpu_cx_gdsc>;
		vdd-supply = <&gpu_gx_gdsc>;
		qcom,chipid = <0x06010900>;

		nvmem-cells = <&gpu_speed_bin>, <&gpu_gaming_bin>;
		nvmem-cell-names = "speed_bin", "gaming_bin";

		qcom,initial-pwrlevel = <4>;
		qcom,gpu-quirk-secvid-set-once;
		qcom,min-access-length = <32>;
		qcom,ubwc-mode = <2>;

		/* Enable context aware freq. scaling */
		qcom,enable-ca-jump;

		/* Context aware jump busy penalty in us */
		qcom,ca-busy-penalty = <12000>;

		interconnects = <&bimc MASTER_GRAPHICS_3D &bimc SLAVE_EBI>;
		interconnect-names = "gpu_icc_path";

		qcom,bus-table-ddr7 =
			<MHZ_TO_KBPS(0, 4)>,    /* index=0  */
			<MHZ_TO_KBPS(451, 4)>,  /* index=1 (LOW SVS) */
			<MHZ_TO_KBPS(547, 4)>,  /* index=2(LOW SVS) */
			<MHZ_TO_KBPS(681, 4)>,  /* index=3 (SVS) */
			<MHZ_TO_KBPS(768, 4)>,  /* index=4 (SVS) */
			<MHZ_TO_KBPS(1017, 4)>, /* index=5 (SVS) */
			<MHZ_TO_KBPS(1353, 4)>, /* index=6 (NOM) */
			<MHZ_TO_KBPS(1555, 4)>, /* index=7 (NOM) */
			<MHZ_TO_KBPS(1804, 4)>, /* index=8 (TURBO) */
			<MHZ_TO_KBPS(2092, 4)>; /* index=9 (TURBO_L1) */

		qcom,gpu-mempools {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "qcom,gpu-mempools";

			/* 4K Page Pool configuration */
			qcom,gpu-mempool@0 {
				reg = <0>;
				qcom,mempool-page-size = <4096>;
				qcom,mempool-allocate;
			};
			/* 8K Page Pool configuration */
			qcom,gpu-mempool@1 {
				reg = <1>;
				qcom,mempool-page-size = <8192>;
				qcom,mempool-allocate;
			};
			/* 64K Page Pool configuration */
			qcom,gpu-mempool@2 {
				reg = <2>;
				qcom,mempool-page-size = <65536>;
				qcom,mempool-reserved = <256>;
			};
			/* 1M Page Pool configuration */
			qcom,gpu-mempool@3 {
				reg = <3>;
				qcom,mempool-page-size = <1048576>;
				qcom,mempool-reserved = <32>;
			};
		};

		/*
		 * Speed-bin zero is default speed bin.
		 * For rest of the speed bins, speed-bin value
		 * is calulated as FMAX/4.8 MHz (round up to zero
		 * decimal places) + 2.
		 */
		qcom,gpu-pwrlevel-bins {
			#address-cells = <1>;
			#size-cells = <0>;

			compatible = "qcom,gpu-pwrlevel-bins";

			qcom,gpu-pwrlevels-0 {
				#address-cells = <1>;
				#size-cells = <0>;
				qcom,speed-bin = <0>;
				qcom,ca-target-pwrlevel = <5>;
				qcom,initial-pwrlevel = <6>;

				/* TURBO_L1 */
				qcom,gpu-pwrlevel@0 {
					reg = <0>;
					qcom,gpu-freq = <875000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_TURBO_L1>;

					qcom,bus-freq-ddr7 = <9>;
					qcom,bus-min-ddr7 = <8>;
					qcom,bus-max-ddr7 = <9>;
				};

				/* TURBO */
				qcom,gpu-pwrlevel@1 {
					reg = <1>;
					qcom,gpu-freq = <800000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_TURBO>;

					qcom,bus-freq-ddr7 = <8>;
					qcom,bus-min-ddr7 = <7>;
					qcom,bus-max-ddr7 = <9>;

				};

				/* NOM_L1 */
				qcom,gpu-pwrlevel@2 {
					reg = <2>;
					qcom,gpu-freq = <650000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM_L1>;

					qcom,bus-freq-ddr7 = <7>;
					qcom,bus-min-ddr7 = <5>;
					qcom,bus-max-ddr7 = <9>;

				};

				/* NOM */
				qcom,gpu-pwrlevel@3 {
					reg = <3>;
					qcom,gpu-freq = <565000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM>;

					qcom,bus-freq-ddr7 = <6>;
					qcom,bus-min-ddr7 = <5>;
					qcom,bus-max-ddr7 = <8>;

				};

				/* SVS_L1 */
				qcom,gpu-pwrlevel@4 {
					reg = <4>;
					qcom,gpu-freq = <430000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L1>;

					qcom,bus-freq-ddr7 = <5>;
					qcom,bus-min-ddr7 = <4>;
					qcom,bus-max-ddr7 = <7>;

				};

				/* SVS */
				qcom,gpu-pwrlevel@5 {
					reg = <5>;
					qcom,gpu-freq = <355000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS>;

					qcom,bus-freq-ddr7 = <4>;
					qcom,bus-min-ddr7 = <2>;
					qcom,bus-max-ddr7= <5>;
				};

				/* LOW SVS */
				qcom,gpu-pwrlevel@6 {
					reg = <6>;
					qcom,gpu-freq = <253000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS>;

					qcom,bus-freq-ddr7 = <2>;
					qcom,bus-min-ddr7 = <1>;
					qcom,bus-max-ddr7 = <4>;
				};

			};

			qcom,gpu-pwrlevels-1 {
				#address-cells = <1>;
				#size-cells = <0>;
				qcom,speed-bin = <138>;
				qcom,ca-target-pwrlevel = <3>;
				qcom,initial-pwrlevel = <4>;

				/* NOM_L1 */
				qcom,gpu-pwrlevel@0 {
					reg = <0>;
					qcom,gpu-freq = <650000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM_L1>;

					qcom,bus-freq-ddr7 = <7>;
					qcom,bus-min-ddr7 = <5>;
					qcom,bus-max-ddr7 = <9>;

				};

				/* NOM */
				qcom,gpu-pwrlevel@1 {
					reg = <1>;
					qcom,gpu-freq = <565000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM>;

					qcom,bus-freq-ddr7 = <6>;
					qcom,bus-min-ddr7 = <5>;
					qcom,bus-max-ddr7 = <8>;

				};

				/* SVS_L1 */
				qcom,gpu-pwrlevel@2 {
					reg = <2>;
					qcom,gpu-freq = <430000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L1>;

					qcom,bus-freq-ddr7 = <5>;
					qcom,bus-min-ddr7 = <4>;
					qcom,bus-max-ddr7 = <7>;

				};

				/* SVS */
				qcom,gpu-pwrlevel@3 {
					reg = <3>;
					qcom,gpu-freq = <355000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS>;

					qcom,bus-freq-ddr7 = <4>;
					qcom,bus-min-ddr7 = <2>;
					qcom,bus-max-ddr7= <5>;
				};

				/* LOW SVS */
				qcom,gpu-pwrlevel@4 {
					reg = <4>;
					qcom,gpu-freq = <253000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS>;

					qcom,bus-freq-ddr7 = <2>;
					qcom,bus-min-ddr7 = <1>;
					qcom,bus-max-ddr7 = <4>;
				};

			};

			qcom,gpu-pwrlevels-2 {
				#address-cells = <1>;
				#size-cells = <0>;
				qcom,speed-bin = <92>;
				qcom,ca-target-pwrlevel = <2>;
				qcom,initial-pwrlevel = <1>;

				/* SVS_L1 */
				qcom,gpu-pwrlevel@0 {
					reg = <0>;
					qcom,gpu-freq = <430000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L1>;

					qcom,bus-freq-ddr7 = <5>;
					qcom,bus-min-ddr7 = <4>;
					qcom,bus-max-ddr7 = <7>;

				};

				/* SVS */
				qcom,gpu-pwrlevel@1 {
					reg = <1>;
					qcom,gpu-freq = <355000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS>;

					qcom,bus-freq-ddr7 = <4>;
					qcom,bus-min-ddr7 = <2>;
					qcom,bus-max-ddr7= <5>;
				};

				/* LOW SVS */
				qcom,gpu-pwrlevel@2 {
					reg = <2>;
					qcom,gpu-freq = <253000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS>;

					qcom,bus-freq-ddr7 = <2>;
					qcom,bus-min-ddr7 = <1>;
					qcom,bus-max-ddr7 = <4>;
				};

			};

		};

	 };

	kgsl_msm_iommu: qcom,kgsl-iommu@5940000 {
		compatible = "qcom,kgsl-smmu-v2";
		reg = <0x5940000 0x10000>;

		vddcx-supply = <&gpu_cx_gdsc>;

		clocks = <&gcc GCC_BIMC_GPU_AXI_CLK>,
			<&gpucc GPU_CC_AHB_CLK>,
			<&gcc GCC_GPU_MEMNOC_GFX_CLK>;

		clock-names = "gcc_bimc_gpu_axi", "gpu_cc_ahb",
			      "gcc_gpu_memnoc_gfx";

		gfx3d_user: gfx3d_user {
			compatible = "qcom,smmu-kgsl-cb";
			iommus = <&kgsl_smmu 0x0>;
			qcom,iommu-dma = "disabled";
		};

		gfx3d_secure: gfx3d_secure {
		      compatible = "qcom,smmu-kgsl-cb";
		      iommus = <&kgsl_smmu 0x2>;
		      qcom,iommu-dma = "disabled";
		};
	};
};
