* Qualcomm Technologies, Inc. MSM MMRM

[Root level node]
MMRM
=====
Required properties:
- compatible : one of:
	- "qcom,msm-mmrm-test"
	- "qcom,waipio-mmrm-test" : Invokes driver specific data for Waipio.
- clock-names: an array of clocks that the driver uses for testing.
	The clocks names here correspond to the clock names used in
	clk_get.
- clocks: Must contain an entry for each clock in clock-names.

Example:

	qcom,mmrm-test {
		compatible = "qcom,msm-mmrm-test";

		clock-names =
			"cam_cc_ife_0_clk_src",
			"cam_cc_ife_1_clk_src",
			"video_cc_mvs1_clk_src",
			"disp_cc_mdss_mdp_clk_src",
			"video_cc_mvs0_clk_src";
		clocks =
			<&clock_camcc CAM_CC_IFE_0_CLK_SRC>,
			<&clock_camcc CAM_CC_IFE_1_CLK_SRC>,
			<&clock_videocc VIDEO_CC_MVS1_CLK_SRC>,
			<&clock_dispcc DISP_CC_MDSS_MDP_CLK_SRC>,
			<&clock_videocc VIDEO_CC_MVS0_CLK_SRC>;
	};
