/dts-v1/;
/plugin/;

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/clock/qcom,gcc-waipio.h>
#include <dt-bindings/interconnect/qcom,waipio.h>
#include <dt-bindings/clock/qcom,videocc-waipio.h>
#include "waipio-vidc.dtsi"

/ {
	model = "Qualcomm Technologies, Inc. waipio/cape/ukee v1 SoC";
	compatible = "qcom,waipio", "qcom,cape", "qcom,ukee";
	qcom,msm-id = <457 0x10000>, <482 0x10000>,
			<457 0x20000>, <482 0x20000>,
			<530 0x10000>, <531 0x10000>,
			<540 0x10000>, <552 0x10000>,
			<591 0x10000>;
	qcom,board-id = <0 0>;
};
