#include <dt-bindings/interconnect/qcom,holi.h>

&soc {
	/* QUPv3 SE Instances
	 * Qup0 0: SE 0: I2C, SPI
	 * Qup0 1: SE 1: HSUART
	 * Qup0 2: SE 2: I2C, SPI
	 * Qup0 3: SE 3: Not bolled out
	 * Qup0 4: SE 4: Not bolled out
	 * Qup0 5: SE 5: Not bolled out
	 * Qup1 0: SE 6: I2C, SPI
	 * Qup1 1: SE 7: I2C
	 * Qup1 2: SE 8: I2C
	 * Qup1 3: SE 9: DEBUG UART
	 * Qup1 4: SE 10: I2C
	 * Qup1 5: SE 11: Not bolled out
	 */

	/* QUPv3_0  wrapper  instance */
	qupv3_0: qcom,qupv3_0_geni_se@4ac0000 {
		compatible = "qcom,qupv3-geni-se";
		reg = <0x4ac0000 0x2000>;
		qcom,msm-bus,num-paths = <2>;
		qcom,msm-bus,vectors-bus-ids =
			<MASTER_QUP_CORE_0 SLAVE_QUP_CORE_0>,
			<MASTER_QUP_0 SLAVE_EBI>;
		qcom,vote-for-bw;
		iommus = <&apps_smmu 0x0003 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0xc0000000>;
		qcom,iommu-dma = "fastmap";
		status = "ok";
	};

	/* GPI Instance */
	gpi_dma0: qcom,gpi-dma@4a00000 {
		compatible = "qcom,gpi-dma";
		#dma-cells = <5>;
		reg = <0x4a00000 0x60000>;
		reg-names = "gpi-top";
		iommus = <&apps_smmu 0x0016 0x0>;
		qcom,max-num-gpii = <10>;
		interrupts = <GIC_SPI 335 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 336 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 337 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 338 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 339 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 340 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 341 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 342 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 343 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 344 IRQ_TYPE_LEVEL_HIGH>;
		qcom,gpii-mask = <0x1f>;
		qcom,ev-factor = <2>;
		qcom,iommu-dma-addr-pool = <0x100000 0x100000>;
		qcom,gpi-ee-offset = <0x10000>;
		status = "ok";
	};

	/* Debug UART Instance */
	qupv3_se9_2uart: qcom,qup_uart@4c8c000 {
		compatible = "qcom,msm-geni-console";
		reg = <0x4c8c000 0x4000>;
		reg-names = "se_phys";
		interrupts = <GIC_SPI 510 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP1_S3_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se9_2uart_active>;
		pinctrl-1 = <&qupv3_se9_2uart_sleep>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se0_i2c: i2c@4a80000 {
		compatible = "qcom,i2c-geni";
		reg = <0x4a80000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		interrupts = <GIC_SPI 327 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP0_S0_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se0_i2c_active>;
		pinctrl-1 = <&qupv3_se0_i2c_sleep>;
		dmas = <&gpi_dma0 0 0 3 64 0>,
			<&gpi_dma0 1 0 3 64 0>;
		dma-names = "tx", "rx";
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se0_spi: spi@4a80000 {
		compatible = "qcom,spi-geni";
		reg = <0x4a80000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		reg-names = "se_phys";
		interrupts = <GIC_SPI 327 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP0_S0_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se0_spi_active>;
		pinctrl-1 = <&qupv3_se0_spi_sleep>;
		dmas = <&gpi_dma0 0 0 1 64 0>,
			<&gpi_dma0 1 0 1 64 0>;
		dma-names = "tx", "rx";
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	/* HS UART Instance */
	qupv3_se1_4uart: qcom,qup_uart@4a84000 {
		compatible = "qcom,msm-geni-serial-hs";
		reg = <0x4a84000 0x4000>;
		reg-names = "se_phys";
		interrupts-extended = <&intc GIC_SPI 328 IRQ_TYPE_LEVEL_HIGH>,
				<&tlmm 64 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP0_S1_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "active", "sleep";
		pinctrl-0 = <&qupv3_se1_default_cts>,
			<&qupv3_se1_default_rtsrx>, <&qupv3_se1_default_tx>;
		pinctrl-1 = <&qupv3_se1_ctsrx>, <&qupv3_se1_rts>,
						<&qupv3_se1_tx>;
		pinctrl-2 = <&qupv3_se1_ctsrx>, <&qupv3_se1_rts>,
						<&qupv3_se1_tx>;
		qcom,wakeup-byte = <0xFD>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se2_i2c: i2c@4a88000 {
		compatible = "qcom,i2c-geni";
		reg = <0x4a88000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		interrupts = <GIC_SPI 329 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP0_S2_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se2_i2c_active>;
		pinctrl-1 = <&qupv3_se2_i2c_sleep>;
		dmas = <&gpi_dma0 0 2 3 64 0>,
			<&gpi_dma0 1 2 3 64 0>;
		dma-names = "tx", "rx";
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	qupv3_se2_spi: spi@4a88000 {
		compatible = "qcom,spi-geni";
		reg = <0x4a88000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		reg-names = "se_phys";
		interrupts = <GIC_SPI 329 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP0_S2_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_0_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se2_spi_active>;
		pinctrl-1 = <&qupv3_se2_spi_sleep>;
		dmas = <&gpi_dma0 0 2 1 64 0>,
			<&gpi_dma0 1 2 1 64 0>;
		dma-names = "tx", "rx";
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_0>;
		status = "disabled";
	};

	/* QUPv3_1  wrapper  instance */
	qupv3_1: qcom,qupv3_1_geni_se@4cc0000 {
		compatible = "qcom,qupv3-geni-se";
		reg = <0x4cc0000 0x2000>;
		qcom,msm-bus,num-paths = <2>;
		qcom,msm-bus,vectors-bus-ids =
			<MASTER_QUP_CORE_1 SLAVE_QUP_CORE_1>,
			<MASTER_QUP_1 SLAVE_EBI>;
		qcom,vote-for-bw;
		iommus = <&apps_smmu 0x00c3 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0xc0000000>;
		qcom,iommu-dma = "fastmap";
		status = "ok";
	};

	/* GPI Instance */
	gpi_dma1: qcom,gpi-dma@4c00000 {
		compatible = "qcom,gpi-dma";
		#dma-cells = <5>;
		reg = <0x4c00000 0x60000>;
		reg-names = "gpi-top";
		iommus = <&apps_smmu 0x00d6 0x0>;
		qcom,max-num-gpii = <10>;
		interrupts = <GIC_SPI 497 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 498 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 499 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 500 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 501 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 502 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 503 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 504 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 505 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 506 IRQ_TYPE_LEVEL_HIGH>;
		qcom,gpii-mask = <0x1f>;
		qcom,ev-factor = <2>;
		qcom,iommu-dma-addr-pool = <0x100000 0x100000>;
		qcom,gpi-ee-offset = <0x10000>;
		status = "ok";
	};

	qupv3_se6_i2c: i2c@4c80000 {
		compatible = "qcom,i2c-geni";
		reg = <0x4c80000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		interrupts = <GIC_SPI 507 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP1_S0_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se6_i2c_active>;
		pinctrl-1 = <&qupv3_se6_i2c_sleep>;
		dmas = <&gpi_dma1 0 0 3 64 0>,
			<&gpi_dma1 1 0 3 64 0>;
		dma-names = "tx", "rx";
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se6_spi: spi@4c80000 {
		compatible = "qcom,spi-geni";
		reg = <0x4c80000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		reg-names = "se_phys";
		interrupts = <GIC_SPI 507 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP1_S0_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se6_spi_active>;
		pinctrl-1 = <&qupv3_se6_spi_sleep>;
		dmas = <&gpi_dma1 0 0 1 64 0>,
			<&gpi_dma1 1 0 1 64 0>;
		dma-names = "tx", "rx";
		spi-max-frequency = <50000000>;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se7_i2c: i2c@4c84000 {
		compatible = "qcom,i2c-geni";
		reg = <0x4c84000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		interrupts = <GIC_SPI 508 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP1_S1_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se7_i2c_active>;
		pinctrl-1 = <&qupv3_se7_i2c_sleep>;
		dmas = <&gpi_dma1 0 1 3 64 0>,
			<&gpi_dma1 1 1 3 64 0>;
		dma-names = "tx", "rx";
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se8_i2c: i2c@4c88000 {
		compatible = "qcom,i2c-geni";
		reg = <0x4c88000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		interrupts = <GIC_SPI 509 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP1_S2_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se8_i2c_active>;
		pinctrl-1 = <&qupv3_se8_i2c_sleep>;
		dmas = <&gpi_dma1 0 2 3 64 0>,
			<&gpi_dma1 1 2 3 64 0>;
		dma-names = "tx", "rx";
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

	qupv3_se10_i2c: i2c@4c90000 {
		compatible = "qcom,i2c-geni";
		reg = <0x4c90000 0x4000>;
		#address-cells = <1>;
		#size-cells = <0>;
		interrupts = <GIC_SPI 511 IRQ_TYPE_LEVEL_HIGH>;
		clock-names = "se-clk", "m-ahb", "s-ahb";
		clocks = <&gcc GCC_QUPV3_WRAP1_S4_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_M_AHB_CLK>,
			<&gcc GCC_QUPV3_WRAP_1_S_AHB_CLK>;
		pinctrl-names = "default", "sleep";
		pinctrl-0 = <&qupv3_se10_i2c_active>;
		pinctrl-1 = <&qupv3_se10_i2c_sleep>;
		dmas = <&gpi_dma1 0 4 3 64 0>,
			<&gpi_dma1 1 4 3 64 0>;
		dma-names = "tx", "rx";
		qcom,shared;
		qcom,wrapper-core = <&qupv3_1>;
		status = "disabled";
	};

};
