/dts-v1/;
/memreserve/ 0x90000000 0x00010000;

#include "parrot.dtsi"
#include "parrot-wcn3990.dtsi"
#include "parrot-rumi.dtsi"

/ {
	model = "Qualcomm Technologies, Inc. Parrot RUMI";
	compatible = "qcom,parrot-rumi", "qcom,parrot", "qcom,rumi";
	qcom,board-id = <0x1000F 0>;
};
