#include <dt-bindings/regulator/qcom,rpmh-regulator-levels.h>

/ {
	VDD_CX_LEVEL:
	S1A_LEVEL:
	pm8150_s1_level: regulator-pm8150-s1-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s1_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_GFX_LEVEL:
	S2A_LEVEL:
	pm8150_s2_level: regulator-pm8150-s2-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s2_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_NSP_LEVEL:
	S3A_LEVEL:
	pm8150_s3_level: regulator-pm8150-s3-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s3_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	S5A:
	pm8150_s5: regulator-pm8150-s5 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s5";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1574000>;
		regulator-max-microvolt = <2040000>;
	};

	VDD_MXA_LEVEL:
	S6A_LEVEL:
	pm8150_s6_level: regulator-pm8150-s6-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s6_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_MM_LEVEL:
	S7A_LEVEL:
	pm8150_s7_level: regulator-pm8150-s7-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s7_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_MXC_LEVEL:
	S8A_LEVEL:
	pm8150_s8_level: regulator-pm8150-s8-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s8_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_MXC_MMCX_VOTER_LEVEL: VDD_MXC_MM_VOTER_LEVEL:
	VDD_MM_MXC_VOTER_LEVEL:
	regulator-pm8150-s8-mmcx-voter-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s8_mmcx_voter_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_MIN_SVS>;
		regulator-max-microvolt =
			<RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_MXC_GFX_VOTER_LEVEL: VDD_GFX_MXC_VOTER_LEVEL:
	regulator-pm8150-s8-gfx-voter-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s8_gfx_voter_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_MIN_SVS>;
		regulator-max-microvolt =
			<RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_EBI_LEVEL:
	S10A_LEVEL:
	pm8150_s10_level: regulator-pm8150-s10-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_s10_level";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	L1A:
	pm8150_l1: regulator-pm8150-l1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l1";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <490000>;
		regulator-max-microvolt = <1304000>;
	};

	L2A:
	pm8150_l2: regulator-pm8150-l2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l2";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <2850000>;
		regulator-max-microvolt = <3544000>;
	};

	L3A:
	pm8150_l3: regulator-pm8150-l3 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l3";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <470000>;
		regulator-max-microvolt = <1050000>;
	};

	L4A:
	pm8150_l4: regulator-pm8150-l4 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l4";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <830000>;
		regulator-max-microvolt = <920000>;
	};

	L5A:
	pm8150_l5: regulator-pm8150-l5 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l5";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <1010000>;
		regulator-max-microvolt = <1170000>;
	};

	L6A:
	pm8150_l6: regulator-pm8150-l6 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l6";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <570000>;
		regulator-max-microvolt = <650000>;
	};

	L7A:
	pm8150_l7: regulator-pm8150-l7 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l7";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1700000>;
		regulator-max-microvolt = <1950000>;
	};

	VDD_LPI_MX_LEVEL:
	L8A_LEVEL:
	pm8150_l8_level: regulator-pm8150-l8-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l8_level";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	VDD_LPI_CX_LEVEL:
	L9A_LEVEL:
	pm8150_l9_level: regulator-pm8150-l9-level {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l9_level";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt =
			<RPMH_REGULATOR_LEVEL_RETENTION>;
		regulator-max-microvolt = <RPMH_REGULATOR_LEVEL_MAX>;
	};

	L10A:
	pm8150_l10: regulator-pm8150-l10 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l10";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <2700000>;
		regulator-max-microvolt = <3544000>;
	};

	L11A:
	pm8150_l11: regulator-pm8150-l11 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l11";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <1250000>;
		regulator-max-microvolt = <1250000>;
	};

	L12A:
	pm8150_l12: regulator-pm8150-l12 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l12";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1504000>;
		regulator-max-microvolt = <2000000>;
	};

	L14A:
	pm8150_l14: regulator-pm8150-l14 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l14";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1700000>;
		regulator-max-microvolt = <1900000>;
	};

	L15A:
	pm8150_l15: regulator-pm8150-l15 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l15";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1620000>;
		regulator-max-microvolt = <2000000>;
	};

	L18A:
	pm8150_l18: regulator-pm8150-l18 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8150_l18";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <720000>;
		regulator-max-microvolt = <950000>;
	};

	S2C:
	pm8009c_s2: regulator-pm8009c-s2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009c_s2";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1140000>;
		regulator-max-microvolt = <1260000>;
	};

	L1C:
	pm8009c_l1: regulator-pm8009c-l1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009c_l1";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
	};

	L2C:
	pm8009c_l2: regulator-pm8009c-l2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009c_l2";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <830000>;
		regulator-max-microvolt = <920000>;
	};

	L3C:
	pm8009c_l3: regulator-pm8009c-l3 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009c_l3";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <750000>;
	};

	L4C:
	pm800c_l4: regulator-pm8009c-l4 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009c_l4";
		qcom,hpm-min-load = <30000>;
		regulator-min-microvolt = <700000>;
		regulator-max-microvolt = <825000>;
	};

	L5C:
	pm8009c_l5: regulator-pm8009c-l5 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009c_l5";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1750000>;
		regulator-max-microvolt = <1850000>;
	};

	L6C:
	pm8009c_l6: regulator-pm8009c-l6 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009c_l6";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1674000>;
		regulator-max-microvolt = <1980000>;
	};

	L7C:
	pm8009c_l7: regulator-pm8009c-l7 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009c_l7";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1700000>;
		regulator-max-microvolt = <2000000>;
	};

	S1E:
	pm8009e_s1: regulator-pm8009e-s1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009e_s1";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <382000>;
		regulator-max-microvolt = <952000>;
	};

	S2E:
	pm8009e_s2: regulator-pm8009e-s2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009e_s2";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <2156000>;
		regulator-max-microvolt = <2400000>;
	};

	L5E:
	pm8009e_l5: regulator-pm8009e-l5 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009e_l5";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1620000>;
		regulator-max-microvolt = <1980000>;
	};

	L6E:
	pm8009e_l6: regulator-pm8009e-l6 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009e_l6";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1504000>;
		regulator-max-microvolt = <3544000>;
	};

	S1G:
	pm8009g_s1: regulator-pm8009g-s1 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009g_s1";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <382000>;
		regulator-max-microvolt = <1336000>;
	};

	S2G:
	pm8009g_s2: regulator-pm8009g-s2 {
		compatible = "qcom,stub-regulator";
		regulator-name = "pm8009g_s2";
		qcom,hpm-min-load = <10000>;
		regulator-min-microvolt = <1574000>;
		regulator-max-microvolt = <1904000>;
	};
};

