#include "neo-pmic-overlay.dtsi"
#include "neo-thermal-overlay.dtsi"

&soc {
};

&sdhc_1 {
	status = "ok";

	vdd-supply = <&L10A>;
	qcom,vdd-voltage-level = <2960000 2960000>;
	qcom,vdd-current-level = <0 570000>;

	vdd-io-supply = <&L7A>;
	qcom,vdd-io-always-on;
	qcom,vdd-io-lpm-sup;
	qcom,vdd-io-voltage-level = <1800000 1800000>;
	qcom,vdd-io-current-level = <0 325000>;

	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&sdc1_on>;
	pinctrl-1 = <&sdc1_off>;
};
