#include <dt-bindings/regulator/qcom,rpmh-regulator-levels.h>

/* RPMh regulators: */
&apps_rsc {
	rpmh-regulator-mxclvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mxc.lvl";
		proxy-supply = <&VDD_MXC_LEVEL>;

		VDD_MXC_LEVEL: S9B_LEVEL:
		pm8350_s9_level: regulator-pm8350-s9-level {
			regulator-name = "pm8350_s9_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MXC_LEVEL_AO: S9B_LEVEL_AO:
		pm8350_s9_level_ao: regulator-pm8350-s9-level-ao {
			regulator-name = "pm8350_s9_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};

		VDD_MXC_MMCX_SUPPLY_LEVEL: regulator-pm8350-s9-mmcx-sup-level {
			regulator-name = "pm8350_s9_mmcx_sup_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			vin-supply = <&VDD_CX_MMCX_SUPPLY_LEVEL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-mxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mx.lvl";
		proxy-supply = <&VDD_MXA_LEVEL>;

		VDD_MXA_LEVEL: S5B_LEVEL:
		pm8350_s5_level: regulator-pm8350-s5-level {
			regulator-name = "pm8350_s5_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			pm8350_s5_level-parent-supply = <&VDD_MXC_LEVEL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,min-dropout-voltage-level = <(-1)>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MXA_LEVEL_AO: S5B_LEVEL_AO:
		pm8350_s5_level_ao: regulator-pm8350-s5-level-ao {
			regulator-name = "pm8350_s5_lvl_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			pm8350_s5_lvl_ao-parent-supply = <&VDD_MXC_LEVEL_AO>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			qcom,min-dropout-voltage-level = <(-1)>;
		};

		VDD_MXA_MMCX_SUPPLY_LEVEL: regulator-pm8350-s5-mmcx-sup-level {
			regulator-name = "pm8350_s5_mmcx_sup_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			vin-supply = <&VDD_MXC_MMCX_SUPPLY_LEVEL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			qcom,min-dropout-voltage-level = <(-1)>;
		};
	};

	rpmh-regulator-gfxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "gfx.lvl";
		VDD_GFX_LEVEL: S6B_LEVEL:
		pm8350_s6_level: regulator-pm8350-s6-level {
			regulator-name = "pm8350_s6_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-smpb10 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb10";
		S10B: pm8350_s10: regulator-pm8350-s10 {
			regulator-name = "pm8350_s10";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
		};
	};

	rpmh-regulator-smpb11 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb11";
		S11B: pm8350_s11: regulator-pm8350-s11 {
			regulator-name = "pm8350_s11";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <752000>;
			regulator-max-microvolt = <1000000>;
			qcom,init-voltage = <952000>;
		};
	};

	rpmh-regulator-smpb12 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpb12";
		qcom,regulator-type = "pmic5-hfsmps";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_RET
			 RPMH_REGULATOR_MODE_AUTO>;
		qcom,mode-threshold-currents = <0 200000>;
		S12B: pm8350_s12: regulator-pm8350-s12 {
			regulator-name = "pm8350_s12";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1224000>;
			regulator-max-microvolt = <1360000>;
			qcom,init-voltage = <1256000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_RET>;
		};
	};

	rpmh-regulator-ldob1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L1B: pm8350_l1: regulator-pm8350-l1 {
			regulator-name = "pm8350_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <912000>;
			regulator-max-microvolt = <920000>;
			qcom,init-voltage = <912000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldob2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		proxy-supply = <&pm8350_l2>;
		L2B: pm8350_l2: regulator-pm8350-l2 {
			regulator-name = "pm8350_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3072000>;
			regulator-max-microvolt = <3072000>;
			qcom,init-voltage = <3072000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-current = <100000>;
		};
	};

	rpmh-regulator-ldob3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L3B: pm8350_l3: regulator-pm8350-l3 {
			regulator-name = "pm8350_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <904000>;
			regulator-max-microvolt = <904000>;
			qcom,init-voltage = <904000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-lmxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "lmx.lvl";
		VDD_LPI_MX_LEVEL: L4B_LEVEL:
		pm8350_l4_level: regulator-pm8350-l4-level {
			regulator-name = "pm8350_l4_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-ldob5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		proxy-supply = <&pm8350_l5>;
		L5B: pm8350_l5: regulator-pm8350-l5 {
			regulator-name = "pm8350_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <888000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-current = <100000>;
		};

		L5B_AO: pm8350_l5_ao: regulator-pm8350-l5-ao {
			regulator-name = "pm8350_l5_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <880000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_LPM>;
		};

		regulator-pm8350-l5-so {
			regulator-name = "pm8350_l5_so";
			qcom,set = <RPMH_REGULATOR_SET_SLEEP>;
			regulator-min-microvolt = <880000>;
			regulator-max-microvolt = <880000>;
			qcom,init-voltage = <880000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_LPM>;
			qcom,init-enable = <0>;
		};
	};

	rpmh-regulator-ldob6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		proxy-supply = <&pm8350_l6>;
		L6B: pm8350_l6: regulator-pm8350-l6 {
			regulator-name = "pm8350_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1208000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-current = <100000>;
		};
	};

	rpmh-regulator-ldob7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L7B: pm8350_l7: regulator-pm8350-l7 {
			regulator-name = "pm8350_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2400000>;
			regulator-max-microvolt = <3008000>;
			qcom,init-voltage = <2504000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-lcxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "lcx.lvl";
		VDD_LPI_CX_LEVEL: L8B_LEVEL:
		pm8350_l8_level: regulator-pm8350-l8-level {
			regulator-name = "pm8350_l8_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-ldob9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldob9";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L9B: pm8350_l9: regulator-pm8350-l9 {
			regulator-name = "pm8350_l9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-smpc1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpc1";
		S1C: pm8350c_s1: regulator-pm8350c-s1 {
			regulator-name = "pm8350c_s1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1952000>;
			qcom,init-voltage = <1880000>;
		};
	};

	rpmh-regulator-ebilvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "ebi.lvl";
		VDD_EBI_LEVEL: S2C_LEVEL:
		pm8350c_s2_level: regulator-pm8350c-s2-level {
			regulator-name = "pm8350c_s2_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-smpc3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpc3";
		S3C: pm8350c_s3: regulator-pm8350c-s3 {
			regulator-name = "pm8350c_s3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <300000>;
			regulator-max-microvolt = <704000>;
			qcom,init-voltage = <496000>;
		};
	};

	rpmh-regulator-msslvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mss.lvl";
		VDD_MODEM_LEVEL: S4C_LEVEL:
		pm8350c_s4_level: regulator-pm8350c-s4-level {
			regulator-name = "pm8350c_s4_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
		};
	};

	rpmh-regulator-cxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "cx.lvl";
		proxy-supply = <&VDD_CX_LEVEL>;

		VDD_CX_LEVEL: S6C_LEVEL:
		pm8350c_s6_level: regulator-pm8350c-s6-level {
			regulator-name = "pm8350c_s6_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			pm8350c_s6_level-parent-supply = <&VDD_MXA_LEVEL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,min-dropout-voltage-level = <(-1)>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_CX_LEVEL_AO: S6C_LEVEL_AO:
		pm8350c_s6_level_ao: regulator-pm8350c-s6-level-ao {
			regulator-name = "pm8350c_s6_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			vin-supply = <&VDD_MXA_LEVEL_AO>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_RETENTION>;
			qcom,min-dropout-voltage-level = <(-1)>;
		};

		VDD_CX_MMCX_SUPPLY_LEVEL: regulator-pm8350c-s6-mmcx-sup-level {
			regulator-name = "pm8350c_s6_mmcx_sup_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_MIN_SVS>;
		};
	};

	rpmh-regulator-mmcxlvl {
		compatible = "qcom,rpmh-arc-regulator";
		qcom,resource-name = "mmcx.lvl";
		proxy-supply = <&VDD_MMCX_LEVEL>;

		VDD_MMCX_LEVEL: S8C_LEVEL: VDD_MM_LEVEL:
		pm8350c_s8_level: regulator-pm8350c-s8-level {
			regulator-name = "pm8350c_s8_level";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			pm8350c_s8_level-parent-supply =
				<&VDD_MXA_MMCX_SUPPLY_LEVEL>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_TURBO>;
			qcom,min-dropout-voltage-level = <(-1)>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-voltage =
				<RPMH_REGULATOR_LEVEL_TURBO
				 RPMH_REGULATOR_LEVEL_MAX>;
		};

		VDD_MMCX_LEVEL_AO: S8C_LEVEL_AO: VDD_MM_LEVEL_AO:
		pm8350c_s8_level_ao: regulator-pm8350c-s8-level-ao {
			regulator-name = "pm8350c_s8_level_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			vin-supply = <&VDD_MXA_LEVEL_AO>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
			qcom,min-dropout-voltage-level = <(-1)>;
		};

		regulator-pm8350c-s8-level-so {
			regulator-name = "pm8350c_s8_level_so";
			qcom,set = <RPMH_REGULATOR_SET_SLEEP>;
			regulator-min-microvolt =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
			regulator-max-microvolt =
				<RPMH_REGULATOR_LEVEL_MAX>;
			qcom,init-voltage-level =
				<RPMH_REGULATOR_LEVEL_LOW_SVS>;
		};
	};

	rpmh-regulator-smpc10 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpc10";
		S10C: pm8350c_s10: regulator-pm8350c-s10 {
			regulator-name = "pm8350c_s10";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1048000>;
			regulator-max-microvolt = <1128000>;
			qcom,init-voltage = <1048000>;
		};
	};

	rpmh-regulator-ldoc1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		proxy-supply = <&pm8350c_l1>;
		L1C: pm8350c_l1: regulator-pm8350c-l1 {
			regulator-name = "pm8350c_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-current = <100000>;
		};

		L1C_AO: pm8350c_l1_ao: regulator-pm8350c-l1-ao {
			regulator-name = "pm8350c_l1_ao";
			qcom,set = <RPMH_REGULATOR_SET_ACTIVE>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_LPM>;
		};

		regulator-pm8350c-l1-so {
			regulator-name = "pm8350c_l1_so";
			qcom,set = <RPMH_REGULATOR_SET_SLEEP>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_LPM>;
			qcom,init-enable = <0>;
		};
	};

	rpmh-regulator-ldoc2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L2C: pm8350c_l2: regulator-pm8350c-l2 {
			regulator-name = "pm8350c_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L3C: pm8350c_l3: regulator-pm8350c-l3 {
			regulator-name = "pm8350c_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3008000>;
			regulator-max-microvolt = <3008000>;
			qcom,init-voltage = <3008000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L4C: pm8350c_l4: regulator-pm8350c-l4 {
			regulator-name = "pm8350c_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1704000>;
			regulator-max-microvolt = <3000000>;
			qcom,init-voltage = <1808000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L5C: pm8350c_l5: regulator-pm8350c-l5 {
			regulator-name = "pm8350c_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1704000>;
			regulator-max-microvolt = <3000000>;
			qcom,init-voltage = <1808000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		proxy-supply = <&pm8350c_l6>;
		L6C: pm8350c_l6: regulator-pm8350c-l6 {
			regulator-name = "pm8350c_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <2960000>;
			qcom,init-voltage = <2960000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-current = <22000>;
		};
	};

	rpmh-regulator-ldoc7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L7C: pm8350c_l7: regulator-pm8350c-l7 {
			regulator-name = "pm8350c_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3008000>;
			regulator-max-microvolt = <3008000>;
			qcom,init-voltage = <3008000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc8 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc8";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L8C: pm8350c_l8: regulator-pm8350c-l8 {
			regulator-name = "pm8350c_l8";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc9 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc9";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		proxy-supply = <&pm8350c_l9>;
		L9C: pm8350c_l9: regulator-pm8350c-l9 {
			regulator-name = "pm8350c_l9";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2960000>;
			regulator-max-microvolt = <3008000>;
			qcom,init-voltage = <2960000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-current = <800000>;
		};
	};

	rpmh-regulator-ldoc10 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc10";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L10C: pm8350c_l10: regulator-pm8350c-l10 {
			regulator-name = "pm8350c_l10";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc11 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc11";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L11C: pm8350c_l11: regulator-pm8350c-l11 {
			regulator-name = "pm8350c_l11";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2400000>;
			regulator-max-microvolt = <3008000>;
			qcom,init-voltage = <2504000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoc12 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc12";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		proxy-supply = <&pm8350c_l12>;
		L12C: pm8350c_l12: regulator-pm8350c-l12 {
			regulator-name = "pm8350c_l12";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <2000000>;
			qcom,init-voltage = <1800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-current = <243000>;
		};
	};

	rpmh-regulator-ldoc13 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoc13";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		proxy-supply = <&pm8350c_l13>;
		L13C: pm8350c_l13: regulator-pm8350c-l13 {
			regulator-name = "pm8350c_l13";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3000000>;
			regulator-max-microvolt = <3000000>;
			qcom,init-voltage = <3000000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
			qcom,proxy-consumer-enable;
			qcom,proxy-consumer-current = <10000>;
		};
	};

	rpmh-regulator-bobc1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "bobc1";
		BOB: pm8350c_bob: regulator-pm8350c-bob {
			regulator-name = "pm8350c_bob";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <3008000>;
			regulator-max-microvolt = <3960000>;
			qcom,init-voltage = <3008000>;
		};
	};

	rpmh-regulator-ldod1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldod1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L1D: pm8350b_l1: regulator-pm8350b-l1 {
			regulator-name = "pm8350b_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-smpe1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe1";
		S1E: pmr735a_s1: regulator-pmr735a-s1 {
			regulator-name = "pmr735a_s1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1280000>;
			qcom,init-voltage = <1256000>;
		};
	};

	rpmh-regulator-smpe2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe2";
		S2E: pmr735a_s2: regulator-pmr735a-s2 {
			regulator-name = "pmr735a_s2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <500000>;
			regulator-max-microvolt = <976000>;
			qcom,init-voltage = <852000>;
		};
	};

	rpmh-regulator-smpe3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "smpe3";
		S3E: pmr735a_s3: regulator-pmr735a-s3 {
			regulator-name = "pmr735a_s3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2200000>;
			regulator-max-microvolt = <2352000>;
			qcom,init-voltage = <2200000>;
		};
	};

	rpmh-regulator-ldoe1 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe1";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L1E: pmr735a_l1: regulator-pmr735a-l1 {
			regulator-name = "pmr735a_l1";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <912000>;
			regulator-max-microvolt = <912000>;
			qcom,init-voltage = <912000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe2 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe2";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L2E: pmr735a_l2: regulator-pmr735a-l2 {
			regulator-name = "pmr735a_l2";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe3 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe3";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L3E: pmr735a_l3: regulator-pmr735a-l3 {
			regulator-name = "pmr735a_l3";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			qcom,init-voltage = <1200000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe4 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe4";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L4E: pmr735a_l4: regulator-pmr735a-l4 {
			regulator-name = "pmr735a_l4";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <1776000>;
			regulator-max-microvolt = <1872000>;
			qcom,init-voltage = <1776000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe5 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe5";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L5E: pmr735a_l5: regulator-pmr735a-l5 {
			regulator-name = "pmr735a_l5";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <800000>;
			regulator-max-microvolt = <800000>;
			qcom,init-voltage = <800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe6 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe6";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 30000>;
		L6E: pmr735a_l6: regulator-pmr735a-l6 {
			regulator-name = "pmr735a_l6";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <480000>;
			regulator-max-microvolt = <904000>;
			qcom,init-voltage = <800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};

	rpmh-regulator-ldoe7 {
		compatible = "qcom,rpmh-vrm-regulator";
		qcom,resource-name = "ldoe7";
		qcom,regulator-type = "pmic5-ldo";
		qcom,supported-modes =
			<RPMH_REGULATOR_MODE_LPM
			 RPMH_REGULATOR_MODE_HPM>;
		qcom,mode-threshold-currents = <0 10000>;
		L7E: pmr735a_l7: regulator-pmr735a-l7 {
			regulator-name = "pmr735a_l7";
			qcom,set = <RPMH_REGULATOR_SET_ALL>;
			regulator-min-microvolt = <2800000>;
			regulator-max-microvolt = <2800000>;
			qcom,init-voltage = <2800000>;
			qcom,init-mode = <RPMH_REGULATOR_MODE_HPM>;
		};
	};
};

&soc {
	refgen: refgen-regulator@88e7000 {
		compatible = "qcom,refgen-kona-regulator";
		reg = <0x88e7000 0x84>;
		regulator-name = "refgen";
		proxy-supply = <&refgen>;
		qcom,proxy-consumer-enable;
		regulator-enable-ramp-delay = <5>;
	};
};
