#include <dt-bindings/msm-camera.h>

&tlmm {
	cci0_active: cci0_active {
		mux {
			/* CLK, DATA */
			pins = "gpio110","gpio111"; // Only 2
			function = "cci_i2c";
		};

		config {
			pins = "gpio110","gpio111";
			bias-pull-up; /* PULL UP*/
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci0_suspend: cci0_suspend {
		mux {
			/* CLK, DATA */
			pins = "gpio110","gpio111";
			function = "cci_i2c";
		};

		config {
			pins = "gpio110","gpio111";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci1_active: cci1_active {
		mux {
			/* CLK, DATA */
			pins = "gpio112","gpio113";
			function = "cci_i2c";
		};

		config {
			pins = "gpio112","gpio113";
			bias-pull-up; /* PULL UP*/
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci1_suspend: cci1_suspend {
		mux {
			/* CLK, DATA */
			pins = "gpio112","gpio113";
			function = "cci_i2c";
		};

		config {
			pins = "gpio112","gpio113";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci2_active: cci2_active {
		mux {
			/* CLK, DATA */
			pins = "gpio114","gpio115";
			function = "cci_i2c";
		};

		config {
			pins = "gpio114","gpio115";
			bias-pull-up; /* PULL UP*/
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci2_suspend: cci2_suspend {
		mux {
			/* CLK, DATA */
			pins = "gpio114","gpio115";
			function = "cci_i2c";
		};

		config {
			pins = "gpio114","gpio115";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cci3_active: cci3_active {
		mux {
			/* CLK, DATA */
			pins = "gpio208","gpio209";
			function = "cci_i2c";
		};

		config {
			pins = "gpio208","gpio209";
			bias-pull-up; /* PULL UP*/
			drive-strength = <2>; /* 2 MA */
			qcom,apps;
		};
	};

	cci3_suspend: cci3_suspend {
		mux {
			/* CLK, DATA */
			pins = "gpio208","gpio209";
			function = "cci_i2c";
		};

		config {
			pins = "gpio208","gpio209";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			qcom,remote;
		};

	};

	cam_sensor_mclk0_active: cam_sensor_mclk0_active {
		/* MCLK0 */
		mux {
			pins = "gpio100";
			function = "cam_mclk";
		};

		config {
			pins = "gpio100";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk0_suspend: cam_sensor_mclk0_suspend {
		/* MCLK0 */
		mux {
			pins = "gpio100";
			function = "cam_mclk";
		};

		config {
			pins = "gpio100";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk1_active: cam_sensor_mclk1_active {
		/* MCLK1 */
		mux {
			pins = "gpio101";
			function = "cam_mclk";
		};

		config {
			pins = "gpio101";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk1_suspend: cam_sensor_mclk1_suspend {
		/* MCLK1 */
		mux {
			pins = "gpio101";
			function = "cam_mclk";
		};

		config {
			pins = "gpio101";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk2_active: cam_sensor_mclk2_active {
		/* MCLK2 */
		mux {
			pins = "gpio102";
			function = "cam_mclk";
		};

		config {
			pins = "gpio102";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk2_suspend: cam_sensor_mclk2_suspend {
		/* MCLK2 */
		mux {
			pins = "gpio102";
			function = "cam_mclk";
		};

		config {
			pins = "gpio102";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk3_active: cam_sensor_mclk3_active {
		/* MCLK3 */
		mux {
			pins = "gpio103";
			function = "cam_mclk";
		};

		config {
			pins = "gpio103";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk3_suspend: cam_sensor_mclk3_suspend {
		/* MCLK3 */
		mux {
			pins = "gpio103";
			function = "cam_mclk";
		};

		config {
			pins = "gpio103";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk4_active: cam_sensor_mclk4_active {
		/* MCLK4 */
		mux {
			pins = "gpio104";
			function = "cam_mclk";
		};

		config {
			pins = "gpio104";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk4_suspend: cam_sensor_mclk4_suspend {
		/* MCLK4 */
		mux {
			pins = "gpio104";
			function = "cam_mclk";
		};

		config {
			pins = "gpio104";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk5_active: cam_sensor_mclk5_active {
		/* MCLK5 */
		mux {
			pins = "gpio105";
			function = "cam_mclk";
		};

		config {
			pins = "gpio105";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk5_suspend: cam_sensor_mclk5_suspend {
		/* MCLK5 */
		mux {
			pins = "gpio105";
			function = "cam_mclk";
		};

		config {
			pins = "gpio105";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk6_active: cam_sensor_mclk6_active {
		/* MCLK6 */
		mux {
			pins = "gpio106";
			function = "cam_mclk";
		};

		config {
			pins = "gpio106";
			bias-disable; /* No PULL */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_mclk6_suspend: cam_sensor_mclk6_suspend {
		/* MCLK6 */
		mux {
			pins = "gpio106";
			function = "cam_mclk";
		};

		config {
			pins = "gpio106";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <6>; /* 6 MA */
		};
	};

	cam_sensor_active_rst1: cam_sensor_active_rst1 {
		/* RESET REARAUX */
		mux {
			pins = "gpio24";
			function = "gpio";
		};

		config {
			pins = "gpio24";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst1: cam_sensor_suspend_rst1 {
		/* RESET REARAUX */
		mux {
			pins = "gpio24";
			function = "gpio";
		};

		config {
			pins = "gpio24";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst2: cam_sensor_active_rst2 {
		/* RESET 2 */
		mux {
			pins = "gpio117";
			function = "gpio";
		};

		config {
			pins = "gpio117";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst2: cam_sensor_suspend_rst2 {
		/* RESET 2 */
		mux {
			pins = "gpio117";
			function = "gpio";
		};

		config {
			pins = "gpio117";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst3: cam_sensor_active_rst3 {
		/* RESET 3 */
		mux {
			pins = "gpio120";
			function = "gpio";
		};

		config {
			pins = "gpio120";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst3: cam_sensor_suspend_rst3 {
		/* RESET 3 */
		mux {
			pins = "gpio120";
			function = "gpio";
		};

		config {
			pins = "gpio120";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst4: cam_sensor_active_rst4 {
		/* RESET 4 */
		mux {
			pins = "gpio119";
			function = "gpio";
		};

		config {
			pins = "gpio119";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst4: cam_sensor_suspend_rst4 {
		/* RESET 4 */
		mux {
			pins = "gpio119";
			function = "gpio";
		};

		config {
			pins = "gpio119";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst5: cam_sensor_active_rst5 {
		/* RESET 5 */
		mux {
			pins = "gpio118";
			function = "gpio";
		};

		config {
			pins = "gpio118";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst5: cam_sensor_suspend_rst5 {
		/* RESET 5 */
		mux {
			pins = "gpio118";
			function = "gpio";
		};

		config {
			pins = "gpio118";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};

	cam_sensor_active_rst6: cam_sensor_active_rst6 {
		/* RESET 6 */
		mux {
			pins = "gpio108";
			function = "gpio";
		};

		config {
			pins = "gpio108";
			bias-disable; /* No PULL */
			drive-strength = <2>; /* 2 MA */
		};
	};

	cam_sensor_suspend_rst6: cam_sensor_suspend_rst6 {
		/* RESET 6 */
		mux {
			pins = "gpio108";
			function = "gpio";
		};

		config {
			pins = "gpio108";
			bias-pull-down; /* PULL DOWN */
			drive-strength = <2>; /* 2 MA */
			output-low;
		};
	};
};

&soc {

	#address-cells = <1>;
	#size-cells = <1>;
	interrupt-parent = <&intc>;

	qcom,cam-req-mgr {
		compatible = "qcom,cam-req-mgr";
		status = "ok";
	};

	qcom,cam-sync {
		compatible = "qcom,cam-sync";
		status = "ok";
	};

	cam_csiphy0: qcom,csiphy0@ace4000 {
		cell-index = <0>;
		compatible = "qcom,csiphy-v2.1.0", "qcom,csiphy";
		reg = < 0x0ace4000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0xe4000>;
		interrupt-names = "CSIPHY0";
		interrupts = <GIC_SPI 477 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L5B>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 59400 147000>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy0_clk",
			"csi0phytimer_clk_src",
			"csi0phytimer_clk";
		clocks = <&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSIPHY0_CLK>,
			<&clock_camcc CAM_CC_CSI0PHYTIMER_CLK_SRC>,
			<&clock_camcc CAM_CC_CSI0PHYTIMER_CLK>;
		src-clock-name = "csi0phytimer_clk_src";
		clock-cntl-level = "lowsvs", "nominal";
		clock-rates =
			<400000000 0 400000000 0>,
			<480000000 0 400000000 0>;
		status = "ok";
	};

	cam_csiphy1: qcom,csiphy1@ace6000 {
		cell-index = <1>;
		compatible = "qcom,csiphy-v2.1.0", "qcom,csiphy";
		reg = <0xace6000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0xe6000>;
		interrupt-names = "CSIPHY1";
		interrupts = <GIC_SPI 478 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L5B>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 59400 147000>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy1_clk",
			"csi1phytimer_clk_src",
			"csi1phytimer_clk";
		clocks = <&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSIPHY1_CLK>,
			<&clock_camcc CAM_CC_CSI1PHYTIMER_CLK_SRC>,
			<&clock_camcc CAM_CC_CSI1PHYTIMER_CLK>;
		src-clock-name = "csi1phytimer_clk_src";
		clock-cntl-level = "lowsvs", "nominal";
		clock-rates =
			<400000000 0 400000000 0>,
			<480000000 0 400000000 0>;

		status = "ok";
	};

	cam_csiphy2: qcom,csiphy2@ace8000 {
		cell-index = <2>;
		compatible = "qcom,csiphy-v2.1.0", "qcom,csiphy";
		reg = <0xace8000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0xe8000>;
		interrupt-names = "CSIPHY2";
		interrupts = <GIC_SPI 479 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L5B>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 59400 147000>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy2_clk",
			"csi2phytimer_clk_src",
			"csi2phytimer_clk";
		clocks = <&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSIPHY2_CLK>,
			<&clock_camcc CAM_CC_CSI2PHYTIMER_CLK_SRC>,
			<&clock_camcc CAM_CC_CSI2PHYTIMER_CLK>;
		src-clock-name = "csi2phytimer_clk_src";
		clock-cntl-level = "lowsvs", "nominal";
		clock-rates =
			<400000000 0 400000000 0>,
			<480000000 0 400000000 0>;
		status = "ok";
	};

	cam_csiphy3: qcom,csiphy3@acea000 {
		cell-index = <3>;
		compatible = "qcom,csiphy-v2.1.0", "qcom,csiphy";
		reg = <0xacea000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0xea000>;
		interrupt-names = "CSIPHY3";
		interrupts = <GIC_SPI 448 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L5B>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 59400 147000>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy3_clk",
			"csi3phytimer_clk_src",
			"csi3phytimer_clk";
		clocks = <&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSIPHY3_CLK>,
			<&clock_camcc CAM_CC_CSI3PHYTIMER_CLK_SRC>,
			<&clock_camcc CAM_CC_CSI3PHYTIMER_CLK>;
		src-clock-name = "csi3phytimer_clk_src";
		clock-cntl-level = "lowsvs", "nominal";
		clock-rates =
			<400000000 0 400000000 0>,
			<480000000 0 400000000 0>;
		status = "ok";
	};

	cam_csiphy4: qcom,csiphy4@acec000 {
		cell-index = <4>;
		compatible = "qcom,csiphy-v2.1.0", "qcom,csiphy";
		reg = <0xacec000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0xec000>;
		interrupt-names = "CSIPHY4";
		interrupts = <GIC_SPI 122 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L5B>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 59400 147000>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy4_clk",
			"csi4phytimer_clk_src",
			"csi4phytimer_clk";
		clocks = <&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSIPHY4_CLK>,
			<&clock_camcc CAM_CC_CSI4PHYTIMER_CLK_SRC>,
			<&clock_camcc CAM_CC_CSI4PHYTIMER_CLK>;
		src-clock-name = "csi4phytimer_clk_src";
		clock-cntl-level = "lowsvs", "nominal";
		clock-rates =
			<400000000 0 400000000 0>,
			<480000000 0 400000000 0>;
		status = "ok";
	};

	cam_csiphy5: qcom,csiphy5@acee000 {
		cell-index = <5>;
		compatible = "qcom,csiphy-v2.1.0", "qcom,csiphy";
		reg = <0xacee000 0x2000>;
		reg-names = "csiphy";
		reg-cam-base = <0xee000>;
		interrupt-names = "CSIPHY5";
		interrupts = <GIC_SPI 89 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr", "csi-vdd-1p2", "csi-vdd-0p9";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		csi-vdd-1p2-supply = <&L6B>;
		csi-vdd-0p9-supply = <&L5B>;
		rgltr-cntrl-support;
		rgltr-enable-sync = <1>;
		rgltr-min-voltage = <0 1200000 880000>;
		rgltr-max-voltage = <0 1248000 912000>;
		rgltr-load-current = <0 59400 147000>;
		shared-clks = <1 0 0 0>;
		clock-names = "cphy_rx_clk_src",
			"csiphy5_clk",
			"csi5phytimer_clk_src",
			"csi5phytimer_clk";
		clocks = <&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSIPHY5_CLK>,
			<&clock_camcc CAM_CC_CSI5PHYTIMER_CLK_SRC>,
			<&clock_camcc CAM_CC_CSI5PHYTIMER_CLK>;
		src-clock-name = "csi5phytimer_clk_src";
		clock-cntl-level = "lowsvs", "nominal";
		clock-rates =
			<400000000 0 400000000 0>,
			<480000000 0 400000000 0>;
		status = "ok";
	};

	cam_cci0: qcom,cci0@ac15000 {
		cell-index = <0>;
		compatible = "qcom,cci", "simple-bus";
		reg = <0xac15000 0x1000>;
		reg-names = "cci";
		reg-cam-base = <0x15000>;
		interrupt-names = "cci0";
		interrupts = <GIC_SPI 460 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cci_0_clk_src",
			"cci_0_clk";
		clocks = <&clock_camcc CAM_CC_CCI_0_CLK_SRC>,
			<&clock_camcc CAM_CC_CCI_0_CLK>;
		clock-rates = <37500000 0>;
		clock-cntl-level = "lowsvs";
		src-clock-name = "cci_0_clk_src";
		pctrl-idx-mapping = <CCI_MASTER_0 CCI_MASTER_1>;
		pctrl-map-names = "m0", "m1";
		pinctrl-names = "m0_active", "m0_suspend",
			"m1_active", "m1_suspend";
		pinctrl-0 = <&cci0_active>;
		pinctrl-1 = <&cci0_suspend>;
		pinctrl-2 = <&cci1_active>;
		pinctrl-3 = <&cci1_suspend>;
		status = "ok";

		i2c_freq_100Khz_cci0: qcom,i2c_standard_mode {
			hw-thigh = <201>;
			hw-tlow = <174>;
			hw-tsu-sto = <204>;
			hw-tsu-sta = <231>;
			hw-thd-dat = <22>;
			hw-thd-sta = <162>;
			hw-tbuf = <227>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <6>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_400Khz_cci0: qcom,i2c_fast_mode {
			hw-thigh = <38>;
			hw-tlow = <56>;
			hw-tsu-sto = <40>;
			hw-tsu-sta = <40>;
			hw-thd-dat = <22>;
			hw-thd-sta = <35>;
			hw-tbuf = <62>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <6>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_custom_cci0: qcom,i2c_custom_mode {
			hw-thigh = <16>;
			hw-tlow = <22>;
			hw-tsu-sto = <17>;
			hw-tsu-sta = <18>;
			hw-thd-dat = <16>;
			hw-thd-sta = <15>;
			hw-tbuf = <24>;
			hw-scl-stretch-en = <1>;
			hw-trdhld = <3>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_1Mhz_cci0: qcom,i2c_fast_plus_mode {
			hw-thigh = <16>;
			hw-tlow = <22>;
			hw-tsu-sto = <17>;
			hw-tsu-sta = <18>;
			hw-thd-dat = <16>;
			hw-thd-sta = <15>;
			hw-tbuf = <24>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <3>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};
	};

	cam_cci1: qcom,cci1@ac16000 {
		cell-index = <1>;
		compatible = "qcom,cci", "simple-bus";
		reg = <0xac16000 0x1000>;
		reg-names = "cci";
		reg-cam-base = <0x16000>;
		interrupt-names = "cci1";
		interrupts = <GIC_SPI 271 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdscr";
		gdscr-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cci_1_clk_src",
			"cci_1_clk";
		clocks = <&clock_camcc CAM_CC_CCI_1_CLK_SRC>,
			<&clock_camcc CAM_CC_CCI_1_CLK>;
		clock-rates = <37500000 0>;
		clock-cntl-level = "lowsvs";
		src-clock-name = "cci_1_clk_src";
		pctrl-idx-mapping = <CCI_MASTER_0 CCI_MASTER_1>;
		pctrl-map-names = "m0", "m1";
		pinctrl-names = "m0_active", "m0_suspend",
			"m1_active", "m1_suspend";
		pinctrl-0 = <&cci2_active>;
		pinctrl-1 = <&cci2_suspend>;
		pinctrl-2 = <&cci3_active>;
		pinctrl-3 = <&cci3_suspend>;
		status = "ok";

		i2c_freq_100Khz_cci1: qcom,i2c_standard_mode {
			hw-thigh = <201>;
			hw-tlow = <174>;
			hw-tsu-sto = <204>;
			hw-tsu-sta = <231>;
			hw-thd-dat = <22>;
			hw-thd-sta = <162>;
			hw-tbuf = <227>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <6>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_400Khz_cci1: qcom,i2c_fast_mode {
			hw-thigh = <38>;
			hw-tlow = <56>;
			hw-tsu-sto = <40>;
			hw-tsu-sta = <40>;
			hw-thd-dat = <22>;
			hw-thd-sta = <35>;
			hw-tbuf = <62>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <6>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_custom_cci1: qcom,i2c_custom_mode {
			hw-thigh = <16>;
			hw-tlow = <22>;
			hw-tsu-sto = <17>;
			hw-tsu-sta = <18>;
			hw-thd-dat = <16>;
			hw-thd-sta = <15>;
			hw-tbuf = <24>;
			hw-scl-stretch-en = <1>;
			hw-trdhld = <3>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};

		i2c_freq_1Mhz_cci1: qcom,i2c_fast_plus_mode {
			hw-thigh = <16>;
			hw-tlow = <22>;
			hw-tsu-sto = <17>;
			hw-tsu-sta = <18>;
			hw-thd-dat = <16>;
			hw-thd-sta = <15>;
			hw-tbuf = <24>;
			hw-scl-stretch-en = <0>;
			hw-trdhld = <3>;
			hw-tsp = <3>;
			cci-clk-src = <37500000>;
			status = "ok";
		};
	};

	qcom,cam_smmu {
		compatible = "qcom,msm-cam-smmu", "simple-bus";
		status = "ok";
		force_cache_allocs;
		need_shared_buffer_padding;

		msm_cam_smmu_ife {
			compatible = "qcom,msm-cam-smmu-cb";
			iommus = <&apps_smmu 0x800 0x460>,
				<&apps_smmu 0x820 0x460>,
				<&apps_smmu 0xC00 0x460>,
				<&apps_smmu 0xC20 0x460>,
				<&apps_smmu 0x840 0x460>,
				<&apps_smmu 0x860 0x460>,
				<&apps_smmu 0xC40 0x460>,
				<&apps_smmu 0xC60 0x460>;
			qcom,iommu-dma-addr-pool = <0x100000 0xffe00000>;
			dma-coherent;
			cam-smmu-label = "ife", "sfe";
			multiple-client-devices;
			ife_iova_mem_map: iova-mem-map {
				/* IO region is approximately 4.0 GB */
				iova-mem-region-io {
					iova-region-name = "io";
					/* 1 MB pad for start */
					iova-region-start = <0x100000>;
					/* 1 MB pad for end */
					iova-region-len = <0xffe00000>;
					iova-region-id = <0x3>;
					status = "ok";
				};
			};
		};

		msm_cam_smmu_jpeg {
			compatible = "qcom,msm-cam-smmu-cb";
			iommus = <&apps_smmu 0x20E0 0x400>,
				<&apps_smmu 0x24E0 0x400>;
			cam-smmu-label = "jpeg";
			qcom,iommu-dma-addr-pool = <0x100000 0xffe00000>;
			dma-coherent;
			jpeg_iova_mem_map: iova-mem-map {
				/* IO region is approximately 4.0 GB */
				iova-mem-region-io {
					iova-region-name = "io";
					/* 1 MB pad for start */
					iova-region-start = <0x100000>;
					/* 1 MB pad for end */
					iova-region-len = <0xffe00000>;
					iova-region-id = <0x3>;
					status = "ok";
				};
			};
		};

		msm_cam_smmu_icp {
			compatible = "qcom,msm-cam-smmu-cb";
			iommus = <&apps_smmu 0x2020 0x420>,
				<&apps_smmu 0x2000 0x420>,
				<&apps_smmu 0x2420 0x420>,
				<&apps_smmu 0x2400 0x420>,
				<&apps_smmu 0x2040 0x420>,
				<&apps_smmu 0x2060 0x420>,
				<&apps_smmu 0x2440 0x420>,
				<&apps_smmu 0x2460 0x420>,
				<&apps_smmu 0x2100 0x420>,
				<&apps_smmu 0x2500 0x420>,
				<&apps_smmu 0x2080 0x400>,
				<&apps_smmu 0x2480 0x400>,
				<&apps_smmu 0x2120 0x420>,
				<&apps_smmu 0x2520 0x420>;
			cam-smmu-label = "icp";
			qcom,iommu-dma-addr-pool = <0x10c00000 0xee300000>;
			iova-region-discard = <0xe0000000 0x800000>;
			dma-coherent;
			icp_iova_mem_map: iova-mem-map {
				iova-mem-region-shared {
					/* Shared region is ~250MB long */
					iova-region-name = "shared";
					iova-region-start = <0x800000>;
					iova-region-len = <0xFC00000>;
					iova-region-id = <0x1>;
					status = "ok";
				};

				iova-mem-region-fwuncached-region {
					/* FW uncached region is 7MB long */
					iova-region-name = "fw_uncached";
					iova-region-start = <0x10400000>;
					iova-region-len = <0x700000>;
					iova-region-id = <0x6>;
					status = "ok";
				};

				iova-mem-region-io {
					/* IO region is approximately 3.8 GB */
					iova-region-name = "io";
					iova-region-start = <0x10c00000>;
					iova-region-len = <0xee300000>;
					iova-region-id = <0x3>;
					iova-region-discard = <0xe0000000 0x800000>;
					status = "ok";
				};

				iova-mem-qdss-region {
					/* QDSS region is appropriate 1MB */
					iova-region-name = "qdss";
					iova-region-start = <0x10b00000>;
					iova-region-len = <0x100000>;
					iova-region-id = <0x5>;
					qdss-phy-addr = <0x16790000>;
					status = "ok";
				};
			};
		};

		msm_cam_smmu_cpas_cdm {
			compatible = "qcom,msm-cam-smmu-cb";
			iommus = <&apps_smmu 0x20C0 0x0400>,
				<&apps_smmu 0x24C0 0x0400>,
				<&apps_smmu 0x20A0 0x0400>,
				<&apps_smmu 0x24A0 0x0400>;
			cam-smmu-label = "cpas-cdm", "rt-cdm";
			qcom,iommu-dma-addr-pool = <0x100000 0xffe00000>;
			dma-coherent;
			multiple-client-devices;
			cpas_cdm_iova_mem_map: iova-mem-map {
				iova-mem-region-io {
					/* IO region is approximately 4.0 GB */
					iova-region-name = "io";
					/* 1 MB pad for start */
					iova-region-start = <0x100000>;
					/* 1 MB pad for end */
					iova-region-len = <0xffe00000>;
					iova-region-id = <0x3>;
					status = "ok";
				};
			};
		};

		msm_cam_smmu_secure {
			compatible = "qcom,msm-cam-smmu-cb";
			cam-smmu-label = "cam-secure";
			qcom,secure-cb;
		};
	};

	qcom,cam-cpas@ac13000 {
		cell-index = <0>;
		compatible = "qcom,cam-cpas";
		label = "cpas";
		arch-compat = "cpas_top";
		reg-names = "cam_cpas_top", "cam_camnoc", "cam_rpmh";
		reg = <0xac13000 0x1000>,
			<0xac19000 0x9000>,
			<0xbbf0000 0x1F00>;
		reg-cam-base = <0x13000 0x19000 0x0bbf0000>;
		interrupt-names = "cpas_camnoc";
		interrupts = <GIC_SPI 459 IRQ_TYPE_EDGE_RISING>;
		camnoc-axi-min-ib-bw = <3000000000>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		clock-names =
			"gcc_ahb_clk",
			"gcc_axi_hf_clk",
			"gcc_axi_sf_clk",
			"cam_cc_slow_ahb_clk_src",
			"cpas_ahb_clk",
			"cpas_core_ahb_clk",
			"cam_cc_fast_ahb_clk_src",
			"cam_cc_cpas_fast_ahb_clk",
			"camnoc_axi_clk_src",
			"camnoc_axi_clk";
		clocks =
			<&clock_gcc GCC_CAMERA_AHB_CLK>,
			<&clock_gcc GCC_CAMERA_HF_AXI_CLK>,
			<&clock_gcc GCC_CAMERA_SF_AXI_CLK>,
			<&clock_camcc CAM_CC_SLOW_AHB_CLK_SRC>,
			<&clock_camcc CAM_CC_CPAS_AHB_CLK>,
			<&clock_camcc CAM_CC_CORE_AHB_CLK>,
			<&clock_camcc CAM_CC_FAST_AHB_CLK_SRC>,
			<&clock_camcc CAM_CC_CPAS_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_CAMNOC_AXI_CLK_SRC>,
			<&clock_camcc CAM_CC_CAMNOC_AXI_CLK>;
		clock-rates =
			<0 0 0 0 0 0 0 0 0 0>,
			<0 0 0 80000000 0 0 100000000 0 300000000 0>,
			<0 0 0 80000000 0 0 200000000 0 400000000 0>,
			<0 0 0 80000000 0 0 300000000 0 400000000 0>,
			<0 0 0 80000000 0 0 400000000 0 400000000 0>,
			<0 0 0 80000000 0 0 400000000 0 400000000 0>,
			<0 0 0 80000000 0 0 400000000 0 400000000 0>;
		clock-cntl-level = "suspend", "lowsvs", "svs", "svs_l1",
			"nominal", "nominal_l1", "turbo";
		src-clock-name = "camnoc_axi_clk_src";
		control-camnoc-axi-clk;
		camnoc-bus-width = <32>;
		camnoc-axi-clk-bw-margin-perc = <20>;
		interconnect-names = "cam_ahb";
		interconnects =<&gem_noc MASTER_APPSS_PROC
			&config_noc SLAVE_CAMERA_CFG>;
		rpmh-bcm-info = <12 0x4 0x800 0 4>;
		cam-ahb-num-cases = <8>;
		cam-ahb-bw-KBps =
			<0 0>, <0 76800>, <0 76800>, <0 150000>, <0 150000>,
			<0 300000>, <0 300000>, <0 300000>;
		vdd-corners = <RPMH_REGULATOR_LEVEL_RETENTION
			RPMH_REGULATOR_LEVEL_MIN_SVS
			RPMH_REGULATOR_LEVEL_LOW_SVS
			RPMH_REGULATOR_LEVEL_SVS
			RPMH_REGULATOR_LEVEL_SVS_L1
			RPMH_REGULATOR_LEVEL_NOM
			RPMH_REGULATOR_LEVEL_NOM_L1
			RPMH_REGULATOR_LEVEL_NOM_L2
			RPMH_REGULATOR_LEVEL_TURBO
			RPMH_REGULATOR_LEVEL_TURBO_L1>;
		vdd-corner-ahb-mapping = "suspend", "lowsvs",
			"lowsvs", "svs", "svs_l1",
			"nominal", "nominal", "nominal",
			"turbo", "turbo";
		client-id-based;
		client-names =
			"csiphy0", "csiphy1", "csiphy2", "csiphy3", "csiphy4", "csiphy5",
			"cci0", "cci1", "csid0", "csid1", "csid2", "csid3", "csid4",
			"csid5", "csid6", "csid7", "ife0", "ife1", "ife2", "ife3", "ife4",
			"ife5", "ife6", "ife7", "sfe0", "sfe1", "custom0", "custom1",
			"ipe0", "cpas-cdm0", "rt-cdm0", "rt-cdm1", "rt-cdm2",
			"cam-cdm-intf0", "bps0", "icp0", "jpeg-dma0", "jpeg-enc0", "tpg13",
			"tpg14", "tpg15";
		sys-cache-names = "small-1", "small-2";
		sys-cache-uids = <34 38>;
		status = "ok";

		camera-bus-nodes {
			level3-nodes {
				level-index = <3>;
				level3_rt0_rd_wr_sum: level3-rt0-rd-wr-sum {
					cell-index = <0>;
					node-name = "level3-rt0-rd-wr-sum";
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
					ib-bw-voting-needed;
					qcom,axi-port-mnoc {
						interconnect-names = "cam_hf_0";
						interconnects =
						<&mmss_noc MASTER_CAMNOC_HF
						&mc_virt SLAVE_EBI1>;
					};
				};

				level3_nrt0_rd_wr_sum: level3-nrt0-rd-wr-sum {
					cell-index = <1>;
					node-name = "level3-nrt0-rd-wr-sum";
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
					qcom,axi-port-mnoc {
						interconnect-names = "cam_sf_0";
						interconnects =
						<&mmss_noc MASTER_CAMNOC_SF
						&mc_virt SLAVE_EBI1>;
					};
				};

				level3_nrt1_rd_wr_sum: level3-nrt1-rd-wr-sum {
					cell-index = <2>;
					node-name = "level3-nrt1-rd-wr-sum";
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
					qcom,axi-port-mnoc {
						interconnect-names =
							"cam_sf_icp";
						interconnects =
						<&mmss_noc MASTER_CAMNOC_ICP
						&mc_virt SLAVE_EBI1>;
					};
				};
			};

			level2-nodes {
				level-index = <2>;
				camnoc-max-needed;
				level2_rt0_wr: level2-rt0-wr {
					cell-index = <3>;
					node-name = "level2-rt0-wr";
					parent-node = <&level3_rt0_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM_INTERLEAVE>;
				};

				level2_rt0_rd: level2-rt0-rd {
					cell-index = <4>;
					node-name = "level2-rt0-rd";
					parent-node = <&level3_rt0_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM_INTERLEAVE>;
				};

				level2_nrt0_wr: level2-nrt0-wr {
					cell-index = <5>;
					node-name = "level2-nrt0-wr";
					parent-node = <&level3_nrt0_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM_INTERLEAVE>;
				};

				level2_nrt0_rd: level2-nrt0-rd {
					cell-index = <6>;
					node-name = "level2-nrt0-rd";
					parent-node = <&level3_nrt0_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM_INTERLEAVE>;
				};

				level2_nrt1_rd: level2-nrt1-rd {
					cell-index = <7>;
					node-name = "level2-nrt1-rd";
					parent-node = <&level3_nrt1_rd_wr_sum>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
					bus-width-factor = <4>;
				};
			};

			level1-nodes {
				level-index = <1>;
				camnoc-max-needed;
				level1_rt0_wr0: level1-rt0-wr0 {
					cell-index = <8>;
					node-name = "level1-ife-ubwc-wr";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_wr1: level1-rt0-wr1 {
					cell-index = <9>;
					node-name = "level1-ife-rdi-wr";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_wr2: level1-rt0-wr2 {
					cell-index = <10>;
					node-name = "level1-ife-pdaf";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_wr3: level1-rt0-wr3 {
					cell-index = <11>;
					node-name = "level1-ife01-linear-stats";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_wr4: level1-rt0-wr4 {
					cell-index = <12>;
					node-name = "level1-ife2-linear-stats";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_wr5: level1-rt0-wr5 {
					cell-index = <13>;
					node-name = "level1-ifelite";
					parent-node = <&level2_rt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_rt0_rd0: level1-rt0-rd0 {
					cell-index = <14>;
					node-name = "level1-sfe-rd";
					parent-node = <&level2_rt0_rd>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_nrt0_wr0: level1-nrt0-wr0 {
					cell-index = <15>;
					node-name = "level1-nrt0-wr0";
					parent-node = <&level2_nrt0_wr>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_nrt0_rd0: level1-nrt0-rd0 {
					cell-index = <16>;
					node-name = "level1-nrt0-rd0";
					parent-node = <&level2_nrt0_rd>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};

				level1_nrt0_rd1: level1-nrt0-rd1 {
					cell-index = <17>;
					node-name = "level1-nrt0-rd1";
					parent-node = <&level2_nrt0_rd>;
					traffic-merge-type =
					<CAM_CPAS_TRAFFIC_MERGE_SUM>;
				};
			};

			level0-nodes {
				level-index = <0>;
				ife0_ubwc_wr: ife0-ubwc-wr {
					cell-index = <18>;
					node-name = "ife0-ubwc-wr";
					client-name = "ife0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_UBWC>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_VID
					CAM_CPAS_PATH_DATA_IFE_DISP>;
					parent-node = <&level1_rt0_wr0>;
				};

				ife1_ubwc_wr: ife1-ubwc-wr {
					cell-index = <19>;
					node-name = "ife1-ubwc-wr";
					client-name = "ife1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_UBWC>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_VID
					CAM_CPAS_PATH_DATA_IFE_DISP>;
					parent-node = <&level1_rt0_wr0>;
				};

				ife2_ubwc_wr: ife2-ubwc-wr {
					cell-index = <20>;
					node-name = "ife2-ubwc-wr";
					client-name = "ife2";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_UBWC>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_VID
					CAM_CPAS_PATH_DATA_IFE_DISP>;
					parent-node = <&level1_rt0_wr0>;
				};

				ife0_rdi_pixel_raw_wr: ife0-rdi-pixel-raw-wr {
					cell-index = <21>;
					node-name = "ife0-rdi-pixel-raw-wr";
					client-name = "ife0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_PIXEL_RAW>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW>;
					parent-node = <&level1_rt0_wr1>;
				};

				ife1_rdi_pixel_raw_wr: ife1-rdi-pixel-raw-wr {
					cell-index = <22>;
					node-name = "ife1-rdi-pixel-raw-wr";
					client-name = "ife1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_PIXEL_RAW>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW>;
					parent-node = <&level1_rt0_wr1>;
				};

				ife2_rdi_pixel_raw_wr: ife2-rdi-pixel-raw-wr {
					cell-index = <23>;
					node-name = "ife2-rdi-pixel-raw-wr";
					client-name = "ife2";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_RDI_PIXEL_RAW>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW>;
					parent-node = <&level1_rt0_wr1>;
				};

				sfe0_rdi_stats_nrdi_wr: sfe0-rdi-stats-nrdi-wr {
					cell-index = <24>;
					node-name = "sfe0-rdi-stats-nrdi-wr";
					client-name = "sfe0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_SFE_NRDI
					CAM_CPAS_PATH_DATA_SFE_STATS
					CAM_CPAS_PATH_DATA_SFE_RDI0
					CAM_CPAS_PATH_DATA_SFE_RDI1
					CAM_CPAS_PATH_DATA_SFE_RDI2
					CAM_CPAS_PATH_DATA_SFE_RDI3
					CAM_CPAS_PATH_DATA_SFE_RDI4>;
					parent-node = <&level1_rt0_wr1>;
				};

				sfe1_rdi_stats_nrdi_wr: sfe1-rdi-stats-nrdi-wr {
					cell-index = <25>;
					node-name = "sfe1-rdi-stats-nrdi-wr";
					client-name = "sfe1";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_SFE_NRDI
					CAM_CPAS_PATH_DATA_SFE_STATS
					CAM_CPAS_PATH_DATA_SFE_RDI0
					CAM_CPAS_PATH_DATA_SFE_RDI1
					CAM_CPAS_PATH_DATA_SFE_RDI2
					CAM_CPAS_PATH_DATA_SFE_RDI3
					CAM_CPAS_PATH_DATA_SFE_RDI4>;
					parent-node = <&level1_rt0_wr1>;
				};

				custom0_wr: custom0-wr {
					cell-index = <26>;
					node-name = "custom0-wr";
					client-name = "custom0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_rt0_wr1>;
				};

				ife0_pdaf_wr: ife0-pdaf-wr {
					cell-index = <27>;
					node-name = "ife0-pdaf-wr";
					client-name = "ife0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_PDAF>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_rt0_wr2>;
				};

				ife1_pdaf_wr: ife1-pdaf-wr {
					cell-index = <28>;
					node-name = "ife1-pdaf-wr";
					client-name = "ife1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_PDAF>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_rt0_wr2>;
				};

				ife2_pdaf_wr: ife2-pdaf-wr {
					cell-index = <29>;
					node-name = "ife2-pdaf-wr";
					client-name = "ife2";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_PDAF>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_rt0_wr2>;
				};

				ife0_linear_stats_wr: ife0-linear-stats-wr {
					cell-index = <30>;
					node-name = "ife0-linear-stats-wr";
					client-name = "ife0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR_STATS>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr3>;
				};

				ife1_linear_stats_wr: ife1-linear-stats-wr {
					cell-index = <31>;
					node-name = "ife1-linear-stats-wr";
					client-name = "ife1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR_STATS>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr3>;
				};

				ife2_linear_stats_wr: ife2-linear-stats-wr {
					cell-index = <32>;
					node-name = "ife2-linear-stats-wr";
					client-name = "ife2";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR_STATS>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_LINEAR
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr4>;
				};

				custom1_wr: custom1-wr {
					cell-index = <33>;
					node-name = "custom1-wr";
					client-name = "custom1";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_rt0_wr5>;
				};

				ife7_rdi_stats_pixel_raw_wr: ife7-rdi-stats-pixel-raw-wr {
					cell-index = <34>;
					node-name = "ife7-rdi-stats-pixel-raw-wr";
					client-name = "ife7";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr5>;
				};

				ife6_rdi_stats_pixel_raw_wr: ife6-rdi-stats-pixel-raw-wr {
					cell-index = <35>;
					node-name = "ife6-rdi-stats-pixel-raw-wr";
					client-name = "ife6";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr5>;
				};

				ife5_rdi_stats_pixel_raw_wr: ife5-rdi-stats-pixel-raw-wr {
					cell-index = <36>;
					node-name = "ife5-rdi-stats-pixel-raw-wr";
					client-name = "ife5";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr5>;
				};

				ife4_rdi_stats_pixel_raw_wr: ife4-rdi-stats-pixel-raw-wr {
					cell-index = <37>;
					node-name = "ife4-rdi-stats-pixel-raw-wr";
					client-name = "ife4";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr5>;
				};

				ife3_rdi_stats_pixel_raw_wr: ife3-rdi-stats-pixel-raw-wr {
					cell-index = <38>;
					node-name = "ife3-rdi-stats-pixel-raw-wr";
					client-name = "ife3";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IFE_RDI0
					CAM_CPAS_PATH_DATA_IFE_RDI1
					CAM_CPAS_PATH_DATA_IFE_RDI2
					CAM_CPAS_PATH_DATA_IFE_RDI3
					CAM_CPAS_PATH_DATA_IFE_PIXEL_RAW
					CAM_CPAS_PATH_DATA_IFE_STATS>;
					parent-node = <&level1_rt0_wr5>;
				};

				sfe0_all_rd: sfe0-all-rd {
					cell-index = <39>;
					node-name = "sfe0-all-rd";
					client-name = "sfe0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_SFE_NRDI
					CAM_CPAS_PATH_DATA_SFE_STATS
					CAM_CPAS_PATH_DATA_SFE_RDI0
					CAM_CPAS_PATH_DATA_SFE_RDI1
					CAM_CPAS_PATH_DATA_SFE_RDI2
					CAM_CPAS_PATH_DATA_SFE_RDI3
					CAM_CPAS_PATH_DATA_SFE_RDI4>;
					parent-node = <&level1_rt0_rd0>;
				};

				sfe1_all_rd: sfe1-all-rd {
					cell-index = <40>;
					node-name = "sfe1-all-rd";
					client-name = "sfe1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_SFE_NRDI
					CAM_CPAS_PATH_DATA_SFE_STATS
					CAM_CPAS_PATH_DATA_SFE_RDI0
					CAM_CPAS_PATH_DATA_SFE_RDI1
					CAM_CPAS_PATH_DATA_SFE_RDI2
					CAM_CPAS_PATH_DATA_SFE_RDI3
					CAM_CPAS_PATH_DATA_SFE_RDI4>;
					parent-node = <&level1_rt0_rd0>;
				};

				custom0_rd: custom0-rd {
					cell-index = <41>;
					node-name = "custom0-rd";
					client-name = "custom0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_rt0_rd0>;
				};

				custom1_rd: custom1-rd {
					cell-index = <42>;
					node-name = "custom1-rd";
					client-name = "custom1";
					traffic-data =
					<CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_rt0_rd0>;
				};

				ipe0_all_wr: ipe0-all-wr {
					cell-index = <43>;
					node-name = "ipe0-all-wr";
					client-name = "ipe0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					constituent-paths =
					<CAM_CPAS_PATH_DATA_IPE_WR_VID
					CAM_CPAS_PATH_DATA_IPE_WR_DISP
					CAM_CPAS_PATH_DATA_IPE_WR_REF>;
					parent-node = <&level2_nrt0_wr>;
				};

				bps0_all_wr: bps0-all-wr {
					cell-index = <44>;
					node-name = "bps0-all-wr";
					client-name = "bps0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level2_nrt0_wr>;
				};

				bps0_all_rd: bps0-all-rd {
					cell-index = <45>;
					node-name = "bps0-all-rd";
					client-name = "bps0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level2_nrt0_rd>;
				};

				jpeg_enc0_all_rd: jpeg-enc0-all-rd {
					cell-index = <46>;
					node-name = "jpeg-enc0-all-rd";
					client-name = "jpeg-enc0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd0>;
				};

				jpeg_dma0_all_rd: jpeg-dma0-all-rd {
					cell-index = <47>;
					node-name = "jpeg-dma0-all-rd";
					client-name = "jpeg-dma0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd0>;
				};

				jpeg_enc0_all_wr: jpeg-enc0-all-wr {
					cell-index = <48>;
					node-name = "jpeg-enc0-all-wr";
					client-name = "jpeg-enc0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_nrt0_wr0>;
				};

				jpeg_dma0_all_wr: jpeg-dma0-all-wr {
					cell-index = <49>;
					node-name = "jpeg-dma0-all-wr";
					client-name = "jpeg-dma0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_WRITE>;
					parent-node = <&level1_nrt0_wr0>;
				};

				ipe0_ref_rd: ipe0-ref-rd {
					cell-index = <50>;
					node-name = "ipe0-ref-rd";
					client-name = "ipe0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IPE_RD_REF>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level2_nrt0_rd>;
				};

				ipe0_in_rd: ipe0-in-rd {
					cell-index = <51>;
					node-name = "ipe0-in-rd";
					client-name = "ipe0";
					traffic-data =
					<CAM_CPAS_PATH_DATA_IPE_RD_IN>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level2_nrt0_rd>;
				};

				rt_cdm0_all_rd: rt-cdm0-all-rd {
					cell-index = <52>;
					node-name = "rt-cdm0-all-rd";
					client-name = "rt-cdm0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd1>;
				};

				rt_cdm1_all_rd: rt-cdm1-all-rd {
					cell-index = <53>;
					node-name = "rt-cdm1-all-rd";
					client-name = "rt-cdm1";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd1>;
				};

				rt_cdm2_all_rd: rt-cdm2-all-rd {
					cell-index = <54>;
					node-name = "rt-cdm2-all-rd";
					client-name = "rt-cdm2";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd1>;
				};

				cpas_cdm0_all_rd: cpas-cdm0-all-rd {
					cell-index = <55>;
					node-name = "cpas-cdm0-all-rd";
					client-name = "cpas-cdm0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level1_nrt0_rd1>;
				};

				icp0_all_rd: icp0-all-rd {
					cell-index = <56>;
					node-name = "icp0-all-rd";
					client-name = "icp0";
					traffic-data = <CAM_CPAS_PATH_DATA_ALL>;
					traffic-transaction-type =
					<CAM_CPAS_TRANSACTION_READ>;
					parent-node = <&level2_nrt1_rd>;
				};
			};
		};
	};

	qcom,cam-cdm-intf {
		compatible = "qcom,cam-cdm-intf";
		cell-index = <0>;
		label = "cam-cdm-intf";
		num-hw-cdm = <1>;
		cdm-client-names = "vfe",
			"jpegdma",
			"jpegenc";
		status = "ok";
	};

	qcom,cpas-cdm0@ac24000 {
		cell-index = <0>;
		compatible = "qcom,cam-cpas-cdm2_1";
		label = "cpas-cdm";
		reg = <0xac24000 0x400>;
		reg-names = "cpas-cdm";
		reg-cam-base = <0x24000>;
		interrupt-names = "cpas-cdm";
		interrupts = <GIC_SPI 461 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cam_cc_cpas_ahb_clk";
		clocks = <&clock_camcc CAM_CC_CPAS_AHB_CLK>;
		clock-rates = <0>;
		clock-cntl-level = "svs";
		nrt-device;
		cdm-client-names = "ife3", "ife4", "ife5", "ife6", "ife7";
		config-fifo;
		fifo-depths = <64 0 0 0>;
		cam_hw_pid = <24>;
		cam-hw-mid = <0>;
		single-context-cdm;
		status = "ok";
	};

	qcom,rt-cdm0@ac25000 {
		cell-index = <0>;
		compatible = "qcom,cam-rt-cdm2_1";
		label = "rt-cdm";
		reg = <0xac25000 0x400>;
		reg-names = "rt-cdm0";
		reg-cam-base = <0x25000>;
		interrupt-names = "rt-cdm0";
		interrupts = <GIC_SPI 456 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cam_cc_cpas_ahb_clk";
		clocks = <&clock_camcc CAM_CC_CPAS_AHB_CLK>;
		clock-rates = <0>;
		clock-cntl-level = "turbo";
		nrt-device;
		cdm-client-names = "ife0", "dualife0";
		config-fifo;
		fifo-depths = <64 0 0 0>;
		cam_hw_pid = <25>;
		cam-hw-mid = <0>;
		single-context-cdm;
		status = "ok";
	};

	qcom,rt-cdm1@ac26000 {
		cell-index = <1>;
		compatible = "qcom,cam-rt-cdm2_1";
		label = "rt-cdm";
		reg = <0xac26000 0x400>;
		reg-names = "rt-cdm1";
		reg-cam-base = <0x26000>;
		interrupt-names = "rt-cdm1";
		interrupts = <GIC_SPI 287 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cam_cc_cpas_ahb_clk";
		clocks = <&clock_camcc CAM_CC_CPAS_AHB_CLK>;
		clock-rates = <0>;
		clock-cntl-level = "turbo";
		nrt-device;
		cdm-client-names = "ife1", "dualife1";
		config-fifo;
		fifo-depths = <64 0 0 0>;
		cam_hw_pid = <26>;
		cam-hw-mid = <0>;
		single-context-cdm;
		status = "ok";
	};

	qcom,rt-cdm2@ac27000 {
		cell-index = <2>;
		compatible = "qcom,cam-rt-cdm2_1";
		label = "rt-cdm";
		reg = <0xac27000 0x400>;
		reg-names = "rt-cdm2";
		reg-cam-base = <0x27000>;
		interrupt-names = "rt-cdm2";
		interrupts = <GIC_SPI 642 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		clock-names = "cam_cc_cpas_ahb_clk";
		clocks = <&clock_camcc CAM_CC_CPAS_AHB_CLK>;
		clock-rates = <0>;
		clock-cntl-level = "turbo";
		nrt-device;
		cdm-client-names = "ife2", "dualife2";
		config-fifo;
		fifo-depths = <64 0 0 0>;
		cam_hw_pid = <27>;
		cam-hw-mid = <0>;
		single-context-cdm;
		status = "ok";
	};

	qcom,cam-isp {
		compatible = "qcom,cam-isp";
		arch-compat = "ife";
		status = "ok";
	};

	cam_sfe0: qcom,sfe0@ac9e000 {
		cell-index = <0>;
		compatible = "qcom,sfe680";
		reg-names = "sfe0";
		reg = <0xac9e000 0x8000>;
		reg-cam-base = <0x9e000>;
		rt-wrapper-base = <0x62000>;
		interrupt-names = "sfe";
		interrupts = <GIC_SPI 462 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc", "sfe0";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		sfe0-supply = <&cam_cc_sfe_0_gdsc>;
		clock-names =
			"sfe_0_fast_ahb",
			"sfe_0_clk_src",
			"sfe_0_clk",
			"cam_cc_cpas_sfe_0_clk";
		clocks =
			<&clock_camcc CAM_CC_SFE_0_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_SFE_0_CLK_SRC>,
			<&clock_camcc CAM_CC_SFE_0_CLK>,
			<&clock_camcc CAM_CC_CPAS_SFE_0_CLK>;
		clock-rates =
			<0 432000000 0 0>,
			<0 594000000 0 0>,
			<0 675000000 0 0>,
			<0 785000000 0 0>,
			<0 785000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "sfe_0_clk_src";
		cam_hw_pid = <11 24>;
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_sfe1: qcom,sfe1@aca6000 {
		cell-index = <1>;
		compatible = "qcom,sfe680";
		reg-names = "sfe1";
		reg = <0xaca6000 0x8000>;
		reg-cam-base = <0xa6000>;
		rt-wrapper-base = <0x62000>;
		interrupt-names = "sfe";
		interrupts = <GIC_SPI 653 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc", "sfe1";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		sfe1-supply = <&cam_cc_sfe_1_gdsc>;
		clock-names =
			"sfe_1_fast_ahb",
			"sfe_1_clk_src",
			"sfe_1_clk",
			"cam_cc_cpas_sfe_1_clk";
		clocks =
			<&clock_camcc CAM_CC_SFE_1_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_SFE_1_CLK_SRC>,
			<&clock_camcc CAM_CC_SFE_1_CLK>,
			<&clock_camcc CAM_CC_CPAS_SFE_1_CLK>;
		clock-rates =
			<0 432000000 0 0>,
			<0 594000000 0 0>,
			<0 675000000 0 0>,
			<0 785000000 0 0>,
			<0 785000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "sfe_1_clk_src";
		cam_hw_pid = <12 25>;
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_csid0: qcom,csid0@acb7000 {
		cell-index = <0>;
		compatible = "qcom,csid680";
		reg-names = "csid", "csid_top";
		reg = <0xacb7000 0xd00>,
			<0xacb6000 0x1000>;
		reg-cam-base = <0xb7000 0xb6000>;
		rt-wrapper-base = <0x62000>;
		interrupt-names = "csid";
		interrupts = <GIC_SPI 464 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <1 0 0>;
		clock-names =
			"csid_clk_src",
			"csid_clk",
			"csiphy_rx_clk";
		clocks =
			<&clock_camcc CAM_CC_CSID_CLK_SRC>,
			<&clock_camcc CAM_CC_CSID_CLK>,
			<&clock_camcc CAM_CC_CSID_CSIPHY_RX_CLK>;
		clock-rates =
			<400000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe0: qcom,ife0@ac62000 {
		cell-index = <0>;
		compatible = "qcom,vfe680";
		reg-names = "ife", "cam_camnoc";
		reg = <0xac62000 0xf000>,
			<0xac19000 0x9000>;
		reg-cam-base = <0x62000 0x19000>;
		rt-wrapper-base = <0x62000>;
		interrupt-names = "ife";
		interrupts = <GIC_SPI 465 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc", "ife0";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		ife0-supply = <&cam_cc_ife_0_gdsc>;
		clock-names =
			"ife_0_fast_ahb",
			"ife_0_clk_src",
			"ife_0_clk",
			"cam_cc_cpas_ife_0_clk";
		clocks =
			<&clock_camcc CAM_CC_IFE_0_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_IFE_0_CLK_SRC>,
			<&clock_camcc CAM_CC_IFE_0_CLK>,
			<&clock_camcc CAM_CC_CPAS_IFE_0_CLK>;
		clock-rates =
			<0 432000000 0 0>,
			<0 594000000 0 0>,
			<0 675000000 0 0>,
			<0 785000000 0 0>,
			<0 785000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "ife_0_clk_src";
		clock-control-debugfs = "true";
		clock-names-option =  "ife_dsp_clk";
		clocks-option = <&clock_camcc CAM_CC_IFE_0_DSP_CLK>;
		clock-rates-option = <594000000>;
		ubwc-static-cfg = <0x1026 0x1036>;
		cam_hw_pid = <16 28 20 8>;
		status = "ok";
	};

	cam_csid1: qcom,csid1@acb9000 {
		cell-index = <1>;
		compatible = "qcom,csid680";
		reg-names = "csid", "csid_top";
		reg = <0xacb9000 0xd00>,
			<0xacb6000 0x1000>;
		reg-cam-base = <0xb9000 0xb6000>;
		rt-wrapper-base = <0x62000>;
		interrupt-names = "csid";
		interrupts = <GIC_SPI 466 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <1 0 0>;
		clock-names =
			"csid_clk_src",
			"csid_clk",
			"csiphy_rx_clk";
		clocks =
			<&clock_camcc CAM_CC_CSID_CLK_SRC>,
			<&clock_camcc CAM_CC_CSID_CLK>,
			<&clock_camcc CAM_CC_CSID_CSIPHY_RX_CLK>;
		clock-rates =
			<400000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe1: qcom,ife1@ac71000 {
		cell-index = <1>;
		compatible = "qcom,vfe680";
		reg-names = "ife", "cam_camnoc";
		reg = <0xac71000 0xf000>,
			<0xac19000 0x9000>;
		reg-cam-base = <0x71000 0x19000>;
		rt-wrapper-base = <0x62000>;
		interrupt-names = "ife";
		interrupts = <GIC_SPI 467 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc", "ife1";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		ife1-supply = <&cam_cc_ife_1_gdsc>;
		clock-names =
			"ife_1_fast_ahb",
			"ife_1_clk_src",
			"ife_1_clk",
			"cam_cc_cpas_ife_1_clk";
		clocks =
			<&clock_camcc CAM_CC_IFE_1_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_IFE_1_CLK_SRC>,
			<&clock_camcc CAM_CC_IFE_1_CLK>,
			<&clock_camcc CAM_CC_CPAS_IFE_1_CLK>;
		clock-rates =
			<0 432000000 0 0>,
			<0 594000000 0 0>,
			<0 675000000 0 0>,
			<0 785000000 0 0>,
			<0 785000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "ife_1_clk_src";
		clock-control-debugfs = "true";
		clock-names-option =  "ife_dsp_clk";
		clocks-option = <&clock_camcc CAM_CC_IFE_1_DSP_CLK>;
		clock-rates-option = <594000000>;
		ubwc-static-cfg = <0x1026 0x1036>;
		cam_hw_pid = <17 29 21 9>;
		status = "ok";
	};

	cam_csid2: qcom,csid2@acbb000 {
		cell-index = <2>;
		compatible = "qcom,csid680";
		reg-names = "csid", "csid_top";
		reg = <0xacbb000 0xd00>,
			<0xacb6000 0x1000>;
		reg-cam-base = <0xbb000 0xb6000>;
		rt-wrapper-base = <0x62000>;
		interrupt-names = "csid";
		interrupts = <GIC_SPI 640 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <1 0 0>;
		clock-names =
			"csid_clk_src",
			"csid_clk",
			"csiphy_rx_clk";
		clocks =
			<&clock_camcc CAM_CC_CSID_CLK_SRC>,
			<&clock_camcc CAM_CC_CSID_CLK>,
			<&clock_camcc CAM_CC_CSID_CSIPHY_RX_CLK>;
		clock-rates =
			<400000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>,
			<480000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe2: qcom,ife2@ac80000 {
		cell-index = <2>;
		compatible = "qcom,vfe680";
		reg-names = "ife", "cam_camnoc";
		reg = <0xac80000 0xf000>,
			<0xac19000 0x9000>;
		reg-cam-base = <0x80000 0x19000>;
		rt-wrapper-base = <0x62000>;
		interrupt-names = "ife";
		interrupts = <GIC_SPI 641 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc", "ife2";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		ife2-supply = <&cam_cc_ife_2_gdsc>;
		clock-names =
			"ife_2_fast_ahb",
			"ife_2_clk_src",
			"ife_2_clk",
			"cam_cc_cpas_ife_2_clk";
		clocks =
			<&clock_camcc CAM_CC_IFE_2_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_IFE_2_CLK_SRC>,
			<&clock_camcc CAM_CC_IFE_2_CLK>,
			<&clock_camcc CAM_CC_CPAS_IFE_2_CLK>;
		clock-rates =
			<0 432000000 0 0>,
			<0 594000000 0 0>,
			<0 675000000 0 0>,
			<0 785000000 0 0>,
			<0 785000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "ife_2_clk_src";
		clock-control-debugfs = "true";
		clock-names-option =  "ife_dsp_clk";
		clocks-option = <&clock_camcc CAM_CC_IFE_2_DSP_CLK>;
		clock-rates-option = <594000000>;
		ubwc-static-cfg = <0x1026 0x1036>;
		cam_hw_pid = <18 30 22 10>;
		status = "ok";
	};

	cam_csid_lite0: qcom,csid-lite0@acc6000 {
		cell-index = <3>;
		compatible = "qcom,csid-lite680";
		reg-names = "csid-lite";
		reg = <0xacc6000 0xa00>;
		reg-cam-base = <0xc6000>;
		interrupt-names = "csid-lite";
		interrupts = <GIC_SPI 468 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <0 1 0 0 0 0>;
		clock-names =
			"ife_lite_ahb",
			"ife_lite_csid_clk_src",
			"ife_lite_csid_clk",
			"ife_lite_cphy_rx_clk",
			"ife_lite_clk",
			"cam_cc_cpas_ife_lite_clk";
		clocks =
			<&clock_camcc CAM_CC_IFE_LITE_AHB_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CSID_CLK_SRC>,
			<&clock_camcc CAM_CC_IFE_LITE_CSID_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CPHY_RX_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CLK>,
			<&clock_camcc CAM_CC_CPAS_IFE_LITE_CLK>;
		clock-rates =
			<0 400000000 0 0 0 0>,
			<0 480000000 0 0 0 0>,
			<0 480000000 0 0 0 0>,
			<0 480000000 0 0 0 0>,
			<0 480000000 0 0 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "ife_lite_csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe_lite0: qcom,ife-lite0@acc6000 {
		cell-index = <3>;
		compatible = "qcom,vfe-lite680";
		reg-names = "ife-lite";
		reg = <0xacc6000 0x2800>;
		reg-cam-base = <0xc6000>;
		interrupt-names = "ife-lite";
		interrupts = <GIC_SPI 469 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <0 0 0 1 0 0>;
		clock-names =
			"ife_lite_ahb",
			"ife_lite_csid_clk",
			"ife_lite_cphy_rx_clk",
			"ife_lite_clk_src",
			"ife_lite_clk",
			"cam_cc_cpas_ife_lite_clk";
		clocks =
			<&clock_camcc CAM_CC_IFE_LITE_AHB_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CSID_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CPHY_RX_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CLK_SRC>,
			<&clock_camcc CAM_CC_IFE_LITE_CLK>,
			<&clock_camcc CAM_CC_CPAS_IFE_LITE_CLK>;
		clock-rates =
			<0 0 0 400000000 0 0>,
			<0 0 0 480000000 0 0>,
			<0 0 0 480000000 0 0>,
			<0 0 0 480000000 0 0>,
			<0 0 0 480000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "ife_lite_clk_src";
		clock-control-debugfs = "true";
		cam_hw_pid = <0>;
		status = "ok";
	};

	cam_csid_lite1: qcom,csid-lite1@acca000 {
		cell-index = <4>;
		compatible = "qcom,csid-lite680";
		reg-names = "csid-lite";
		reg = <0xacca000 0xa00>;
		reg-cam-base = <0xca000>;
		interrupt-names = "csid-lite";
		interrupts = <GIC_SPI 359 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <0 1 0 0 0 0>;
		clock-names =
			"ife_lite_ahb",
			"ife_lite_csid_clk_src",
			"ife_lite_csid_clk",
			"ife_lite_cphy_rx_clk",
			"ife_lite_clk",
			"cam_cc_cpas_ife_lite_clk";
		clocks =
			<&clock_camcc CAM_CC_IFE_LITE_AHB_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CSID_CLK_SRC>,
			<&clock_camcc CAM_CC_IFE_LITE_CSID_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CPHY_RX_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CLK>,
			<&clock_camcc CAM_CC_CPAS_IFE_LITE_CLK>;
		clock-rates =
			<0 400000000 0 0 0 0>,
			<0 480000000 0 0 0 0>,
			<0 480000000 0 0 0 0>,
			<0 480000000 0 0 0 0>,
			<0 480000000 0 0 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "ife_lite_csid_clk_src";
		clock-control-debugfs = "true";
		status = "ok";
	};

	cam_vfe_lite1: qcom,ife-lite1@acca000 {
		cell-index = <4>;
		compatible = "qcom,vfe-lite680";
		reg-names = "ife-lite";
		reg = <0xacca000 0x2800>;
		reg-cam-base = <0xca000>;
		interrupt-names = "ife-lite";
		interrupts = <GIC_SPI 360 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <0 0 0 1 0 0>;
		clock-names =
			"ife_lite_ahb",
			"ife_lite_csid_clk",
			"ife_lite_cphy_rx_clk",
			"ife_lite_clk_src",
			"ife_lite_clk",
			"cam_cc_cpas_ife_lite_clk";
		clocks =
			<&clock_camcc CAM_CC_IFE_LITE_AHB_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CSID_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CPHY_RX_CLK>,
			<&clock_camcc CAM_CC_IFE_LITE_CLK_SRC>,
			<&clock_camcc CAM_CC_IFE_LITE_CLK>,
			<&clock_camcc CAM_CC_CPAS_IFE_LITE_CLK>;
		clock-rates =
			<0 0 0 400000000 0 0>,
			<0 0 0 480000000 0 0>,
			<0 0 0 480000000 0 0>,
			<0 0 0 480000000 0 0>,
			<0 0 0 480000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		src-clock-name = "ife_lite_clk_src";
		clock-control-debugfs = "true";
		cam_hw_pid = <1>;
		status = "ok";
	};

	cam_csiphy_tpg13: qcom,tpg13@acf6000 {
		cell-index = <13>;
		phy-id     = <0>;
		compatible = "qcom,cam-tpg103";
		reg-names = "tpg0", "cam_cpas_top";
		reg = <0xacf6000 0x400>,
			<0xac13000 0x1000>;
		reg-cam-base = <0xf6000 0x13000>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		interrupt-names = "tpg0";
		interrupts = <GIC_SPI 413 IRQ_TYPE_EDGE_RISING>;
		shared-clks = <1 0>;
		clock-names =
			"cphy_rx_clk_src",
			"csid_csiphy_rx_clk";
		clocks =
			<&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSID_CSIPHY_RX_CLK>;
		clock-rates =
			<400000000 0>,
			<480000000 0>;
		clock-cntl-level = "lowsvs", "nominal";
		src-clock-name = "cphy_rx_clk_src";
		status = "ok";
	};

	cam_csiphy_tpg14: qcom,tpg14@acf7000 {
		cell-index = <14>;
		phy-id     = <1>;
		compatible = "qcom,cam-tpg103";
		reg-names = "tpg1", "cam_cpas_top";
		reg = <0xacf7000 0x400>,
			<0xac13000 0x1000>;
		reg-cam-base = <0xf7000 0x13000>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		interrupt-names = "tpg1";
		interrupts = <GIC_SPI 416 IRQ_TYPE_EDGE_RISING>;
		shared-clks = <1 0>;
		clock-names =
			"cphy_rx_clk_src",
			"csid_csiphy_rx_clk";
		clocks =
			<&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSID_CSIPHY_RX_CLK>;
		clock-rates =
			<400000000 0>,
			<480000000 0>;
		clock-cntl-level = "lowsvs", "nominal";
		src-clock-name = "cphy_rx_clk_src";
		status = "ok";
	};

	cam_csiphy_tpg15: qcom,tpg15@acf8000 {
		cell-index = <15>;
		phy-id     = <2>;
		compatible = "qcom,cam-tpg103";
		reg-names = "tpg2", "cam_cpas_top";
		reg = <0xacf8000 0x400>,
			<0xac13000 0x1000>;
		reg-cam-base = <0xf8000 0x13000>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		interrupt-names = "tpg2";
		interrupts = <GIC_SPI 417 IRQ_TYPE_EDGE_RISING>;
		shared-clks = <1 0>;
		clock-names =
			"cphy_rx_clk_src",
			"csid_csiphy_rx_clk";
		clocks =
			<&clock_camcc CAM_CC_CPHY_RX_CLK_SRC>,
			<&clock_camcc CAM_CC_CSID_CSIPHY_RX_CLK>;
		clock-rates =
			<400000000 0>,
			<480000000 0>;
		clock-cntl-level = "lowsvs", "nominal";
		src-clock-name = "cphy_rx_clk_src";
		status = "ok";
	};

	qcom,cam-icp {
		compatible = "qcom,cam-icp";
		compat-hw-name = "qcom,lx7",
			"qcom,ipe0",
			"qcom,bps";
		num-lx7 = <1>;
		num-ipe = <1>;
		num-bps = <1>;
		status = "ok";
		icp_pc_en;
		icp_use_pil;
		ipe_bps_pc_en;
	};

	cam_lx7: qcom,lx7 {
		cell-index = <0>;
		compatible = "qcom,cam-lx7";
		reg = <0xac01000 0x400>,
			<0xac01800 0x400>,
			<0x0ac04000 0x1000>;
		reg-names = "lx7_csr", "lx7_cirq", "lx7_wd0";
		reg-cam-base = <0x1000 0x1800 0x4000>;
		interrupt-names = "lx7";
		interrupts = <GIC_SPI 463 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		memory-region = <&camera_mem>;
		clock-names =
			"icp_ahb_clk",
			"icp_clk_src",
			"icp_clk",
			"camcc_debug_clk";
		clocks =
			<&clock_camcc CAM_CC_ICP_AHB_CLK>,
			<&clock_camcc CAM_CC_ICP_CLK_SRC>,
			<&clock_camcc CAM_CC_ICP_CLK>,
			<&clock_camcc CAM_CC_QDSS_DEBUG_XO_CLK>;
		clock-rates =
			<0 400000000 0 0>,
			<0 480000000 0 0>,
			<0 600000000 0 0>,
			<0 600000000 0 0>,
			<0 600000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		nrt-device;
		src-clock-name = "icp_clk_src";
		clock-control-debugfs = "true";
		fw_name = "CAMERA_ICP";
		ubwc-ipe-fetch-cfg = <0x707b 0x7083>;
		ubwc-ipe-write-cfg = <0x161ef 0x1620f>;
		ubwc-bps-fetch-cfg = <0x707b 0x7083>;
		ubwc-bps-write-cfg = <0x161ef 0x1620f>;
		qos-val = <0x00000A0A>;
		cam_hw_pid = <9>;
		status = "ok";
	};

	cam_ipe0: qcom,ipe0@ac42000 {
		cell-index = <0>;
		compatible = "qcom,cam-ipe680";
		reg = <0xac42000 0x16000>;
		reg-names = "ipe0_top";
		reg-cam-base = <0x42000>;
		regulator-names = "ipe0-vdd";
		ipe0-vdd-supply = <&cam_cc_ipe_0_gdsc>;
		clock-names =
			"ipe_nps_ahb_clk",
			"ipe_nps_fast_ahb_clk",
			"ipe_pps_fast_ahb_clk",
			"ipe_nps_clk_src",
			"ipe_nps_clk",
			"ipe_pps_clk",
			"cam_cc_cpas_ipe_nps_clk";
		clocks =
			<&clock_camcc CAM_CC_IPE_NPS_AHB_CLK>,
			<&clock_camcc CAM_CC_IPE_NPS_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_IPE_PPS_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_IPE_NPS_CLK_SRC>,
			<&clock_camcc CAM_CC_IPE_NPS_CLK>,
			<&clock_camcc CAM_CC_IPE_PPS_CLK>,
			<&clock_camcc CAM_CC_CPAS_IPE_NPS_CLK>;

		clock-rates =
			<0 0 0 364000000 0 0 0>,
			<0 0 0 500000000 0 0 0>,
			<0 0 0 600000000 0 0 0>,
			<0 0 0 700000000 0 0 0>,
			<0 0 0 700000000 0 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		nrt-device;
		src-clock-name = "ipe_nps_clk_src";
		clock-control-debugfs = "true";
		cam_hw_pid = <22 23 30>;
		status = "ok";
	};

	cam_bps: qcom,bps@ac2c000 {
		cell-index = <0>;
		compatible = "qcom,cam-bps680";
		reg = <0xac2c000 0x7800>;
		reg-names = "bps_top";
		reg-cam-base = <0x2c000>;
		regulator-names = "bps-vdd";
		bps-vdd-supply = <&cam_cc_bps_gdsc>;
		clock-names =
			"bps_ahb_clk",
			"bps_fast_ahb_clk",
			"bps_clk_src",
			"bps_clk",
			"cam_cc_cpas_bps_clk";
		clocks =
			<&clock_camcc CAM_CC_BPS_AHB_CLK>,
			<&clock_camcc CAM_CC_BPS_FAST_AHB_CLK>,
			<&clock_camcc CAM_CC_BPS_CLK_SRC>,
			<&clock_camcc CAM_CC_BPS_CLK>,
			<&clock_camcc CAM_CC_CPAS_BPS_CLK>;

		clock-rates =
			<0 0 200000000 0 0>,
			<0 0 400000000 0 0>,
			<0 0 480000000 0 0>,
			<0 0 600000000 0 0>,
			<0 0 600000000 0 0>;
		clock-cntl-level = "lowsvs", "svs", "svs_l1", "nominal",
			"turbo";
		nrt-device;
		src-clock-name = "bps_clk_src";
		clock-control-debugfs = "true";
		cam_hw_pid = <10 16>;
		status = "ok";
	};

	qcom,cam-jpeg {
		compatible = "qcom,cam-jpeg";
		compat-hw-name = "qcom,jpegenc",
			"qcom,jpegdma";
		num-jpeg-enc = <1>;
		num-jpeg-dma = <1>;
		status = "ok";
	};

	cam_jpeg_enc: qcom,jpegenc@ac2a000 {
		cell-index = <0>;
		compatible = "qcom,cam_jpeg_enc_680";
		reg-names = "jpege_hw", "cam_camnoc";
		reg = <0xac2a000 0x1000>,
			<0x0ac19000 0x9000>;
		reg-cam-base = <0x2a000 0x19000>;
		interrupt-names = "jpeg";
		interrupts = <GIC_SPI 474 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <1 0>;
		clock-names =
			"jpegenc_clk_src",
			"jpegenc_clk";
		clocks =
			<&clock_camcc CAM_CC_JPEG_CLK_SRC>,
			<&clock_camcc CAM_CC_JPEG_CLK>;
		clock-rates = <600000000 0>;
		src-clock-name = "jpegenc_clk_src";
		clock-cntl-level = "nominal";
		nrt-device;
		cam_hw_pid = <12 14>;
		cam_hw_rd_mid = <0>;
		cam_hw_wr_mid = <1>;
		status = "ok";
	};

	cam_jpeg_dma: qcom,jpegdma@ac2b000 {
		cell-index = <0>;
		compatible = "qcom,cam_jpeg_dma_680";
		reg-names = "jpegdma_hw", "cam_camnoc";
		reg = <0xac2b000 0x1000>,
			<0x0ac19000 0x9000>;
		reg-cam-base = <0x2b000 0x19000>;
		interrupt-names = "jpegdma";
		interrupts = <GIC_SPI 475 IRQ_TYPE_EDGE_RISING>;
		regulator-names = "gdsc";
		gdsc-supply = <&cam_cc_titan_top_gdsc>;
		shared-clks = <1 0>;
		clock-names =
			"jpegdma_clk_src",
			"jpegdma_clk";
		clocks =
			<&clock_camcc CAM_CC_JPEG_CLK_SRC>,
			<&clock_camcc CAM_CC_JPEG_CLK>;
		clock-rates = <600000000 0>;
		src-clock-name = "jpegdma_clk_src";
		clock-cntl-level = "nominal";
		nrt-device;
		cam_hw_pid = <13 15>;
		cam_hw_rd_mid = <0>;
		cam_hw_wr_mid = <1>;
		status = "ok";
	};
};
