#include "diwali-idp.dtsi"
#include "diwali-idp-pm7250b.dtsi"

&wpss_pas {
	status = "disabled";
};

&icnss2 {
	status = "disabled";
};

&reserved_memory {
	cnss_wlan_mem: cnss_wlan_region {
		compatible = "shared-dma-pool";
		alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
		reusable;
		alignment = <0x0 0x400000>;
		size = <0x0 0x2000000>;
	};
};

&pcie0 {
	status = "ok";
};

&soc {
	bluetooth: bt_wcn6x5x {
		compatible = "qcom,qca6490";
	};

	wlan: qcom,cnss-qca6490@b0000000 {
		compatible = "qcom,cnss-qca6490";
		reg = <0xb0000000 0x10000>;
		reg-names = "smmu_iova_ipa";
		wlan-en-gpio = <&tlmm 49 0>;
		qcom,bt-en-gpio = <&tlmm 114 0>;
		pinctrl-names = "wlan_en_active", "wlan_en_sleep";
		pinctrl-0 = <&cnss_wlan_en_active>;
		pinctrl-1 = <&cnss_wlan_en_sleep>;
		qcom,wlan;
		qcom,wlan-rc-num = <0>;
		qcom,wlan-ramdump-dynamic = <0x420000>;
		qcom,wlan-cbc-enabled;
		use-pm-domain;
		cnss-enable-self-recovery;
		qcom,same-dt-multi-dev;
		mboxes = <&qmp_aop 0>;
		qcom,vreg_ipa="s1c";

		vdd-wlan-aon-supply = <&S7B>;
		qcom,vdd-wlan-aon-config = <950000 952000 0 0 1>;
		vdd-wlan-dig-supply = <&S7B>;
		qcom,vdd-wlan-dig-config = <950000 952000 0 0 1>;
		vdd-wlan-io-supply = <&L18B>;
		qcom,vdd-wlan-io-config = <1800000 1800000 0 0 1>;
		vdd-wlan-rfa1-supply = <&S1B>;
		qcom,vdd-wlan-rfa1-config = <1880000 2040000 0 0 1>;
		vdd-wlan-rfa2-supply = <&S8B>;
		qcom,vdd-wlan-rfa2-config = <1350000 1350000 0 0 1>;

		interconnects =
		<&pcie_noc MASTER_PCIE_0 &pcie_noc SLAVE_ANOC_PCIE_GEM_NOC>,
		<&gem_noc MASTER_ANOC_PCIE_GEM_NOC &mc_virt SLAVE_EBI1>;
		interconnect-names = "pcie_to_memnoc", "memnoc_to_ddr";

		qcom,icc-path-count = <2>;
		qcom,bus-bw-cfg-count = <9>;
		qcom,bus-bw-cfg =
		/** ICC Path 1 **/
		<0 0>, /* no vote */
		/* idle: 0-18 Mbps snoc/anoc: 100 Mhz ddr: 451.2 MHz */
		<2250 700000>,
		/* low: 18-60 Mbps snoc/anoc: 100 Mhz ddr: 451.2 MHz */
		<7500 700000>,
		/* medium: 60-240 Mbps snoc/anoc: 100 Mhz ddr: 451.2 MHz */
		<30000 700000>,
		/* high: 240-1200 Mbps snoc/anoc: 100 Mhz ddr: 451.2 MHz */
		<100000 700000>,
		/* very high: > 1200 Mbps snoc/anoc: 403 Mhz ddr: 1555 MHz */
		<175000 3000000>,
		/* ultra high: DBS mode snoc/anoc: 403 Mhz ddr: 2092 MHz */
		<175000 3000000>,
		/* super high: DBS mode snoc/anoc: 533 Mhz ddr: 3.2GHz */
		<175000 4000000>,
		/* low (latency critical): 18-60 Mbps snoc/anoc: 200 Mhz
		 * ddr: 547.2 MHz
		 */
		<7500 1500000>,

		/** ICC Path 2 **/
		<0 0>,
		/* ddr: 451.2 MHz */
		<2250 2400000>,
		/* ddr: 451.2 MHz */
		<7500 2400000>,
		/* ddr: 451.2 MHz */
		<30000 2400000>,
		/* ddr: 451.2 MHz */
		<100000 2400000>,
		/* ddr: 1555 MHz */
		<175000 8000000>,
		/* ddr: 2092 MHz */
		<175000 9600000>,
		/* ddr: 3.2 GHz */
		<175000 10000000>,
		/* ddr: 547.2 MHz */
		<7500 2400000>;
	};
};

&pcie0_rp {
	#address-cells = <5>;
	#size-cells = <0>;

	cnss_pci: cnss_pci {
		reg = <0 0 0 0 0>;
		qcom,iommu-group = <&cnss_pci_iommu_group>;
		memory-region = <&cnss_wlan_mem>;

		#address-cells = <1>;
		#size-cells = <1>;

		cnss_pci_iommu_group: cnss_pci_iommu_group {
			qcom,iommu-msi-size = <0x1000>;
			qcom,iommu-dma-addr-pool = <0xa0000000 0x10000000>;
			qcom,iommu-dma = "fastmap";
			qcom,iommu-pagetable = "coherent";
			qcom,iommu-faults = "stall-disable", "HUPCF", "no-CFRE",
					    "non-fatal";
		};
	};
};
