* Qualcomm Technologies, Inc. Power State Driver

This binding describes the Qualcomm Technologies, Inc. Power State Driver. Power
State creates power_state device node for user space communication. User space
client can open device node for communication and driver accordingly handles the
request.

Required Properties:

- compatible:
	Usage: required
	Value type: <string>
	Definition: must be "qcom,power-state"
- subsys-name:
	Usage: required
	Value type: <string>
	Description: subsystem names supported
- rproc-handle:
	Usage: required
	Description: phandle to subsys defined in subsys-name.

Example:

	qcom,power-state {
		compatible = "qcom,power-state";
		qcom,subsys-name = "adsp", "modem";
		qcom,rproc-handle = <&adsp_pas>, <&modem_pas>;
	};
