&soc {
  /* smp2p information */
	qcom,smp2p_interrupt_rdbg_2_out {
		compatible = "qcom,smp2p-interrupt-rdbg-2-out";
		qcom,smem-states = <&smp2p_rdbg2_out 0>;
		qcom,smem-state-names = "rdbg-smp2p-out";
	};

	qcom,smp2p_interrupt_rdbg_2_in {
		compatible = "qcom,smp2p-interrupt-rdbg-2-in";
		interrupts-extended = <&smp2p_rdbg2_in 0 0>;
		interrupt-names = "rdbg-smp2p-in";
	};
};
