/*
   this file is for attribution only of unicorn
   And public attribution of xiaomi platforms(like K2 and so and)
*/
#include "unicorn-pinctrl.dtsi"
#include "xiaomi-sm8475-common.dtsi"

&qupv3_se15_i2c {
	status = "ok";
	cs35l41_0: cs35l41@40 {
		status = "ok";
		compatible = "cirrus,cs35l41";
		reset-gpios = <&tlmm 120 0>;
		reg = <0x40>;
		interrupt-parent = <&tlmm>;
		interrupts = <117 0x2008>;
		pinctrl-names = "default";
		pinctrl-0 = <&cirrus_reset_default_0 &cirrus_irq_default_0>;
		cirrus,temp-warn_threshold = <3>;
		cirrus,boost-peak-milliamp = <4000>;
		cirrus,boost-ind-nanohenry = <1000>;
		cirrus,boost-cap-microfarad = <15>;
		cirrus,asp-sdout-hiz = <3>;
		cirrus,right-channel-amp;
		sound-name-prefix = "B";
		cirrus,fast-switch = "B-music.txt", "B-handfree.txt";
		cirrus,gpio-config2 {
			cirrus,gpio-src-select = <0x4>;
			cirrus,gpio-output-enable;
		};
	};
	cs35l41_3: cs35l41@43 {
		status = "ok";
		compatible = "cirrus,cs35l41";
		reset-gpios = <&tlmm 1 0>;
		spk-sw-gpios = <&tlmm 52 0>;
		reg = <0x43>;
		interrupt-parent = <&tlmm>;
		interrupts = <88 0x2008>;
		pinctrl-names = "default";
		pinctrl-0 = <&cirrus_reset_default_3 &cirrus_irq_default_3>;
		cirrus,temp-warn_threshold = <3>;
		cirrus,boost-peak-milliamp = <4000>;
		cirrus,boost-ind-nanohenry = <1000>;
		cirrus,boost-cap-microfarad = <15>;
		cirrus,asp-sdout-hiz = <3>;
		sound-name-prefix = "T";
		cirrus,fast-switch = "T-music.txt", "T-handset.txt", "T-handfree.txt";
		cirrus,gpio-config2 {
			cirrus,gpio-src-select = <0x4>;
			cirrus,gpio-output-enable;
		};
	};
};

&qupv3_se18_i2c {
	#address-cells = <1>;
	#size-cells = <0>;
	clock-frequency = <400000>;
	status = "ok";
	aw8697_haptic@5A {
		compatible = "awinic,aw86297_haptic";
		reg = <0x5a>;
		reset-gpio = <&tlmm 89 0x00>;
		irq-gpio = <&tlmm 90 0x00>;
		pinctrl-names = "awinic_reset_reset","awinic_reset_active","awinic_interrupt_active";
		pinctrl-0 = <&awinic_gpio_reset>;
		pinctrl-1 = <&awinic_gpio_reset_output_high>;
		pinctrl-2 = <&awinic_gpio_int>;
		/*----------------------aw8697----------------------*/
		aw8697_vib_mode = < 0 >; /*mode:   RAM mode->0; CONT mode -> 1*/
		aw8697_vib_f0_pre = < 1300 >;
		aw8697_vib_f0_cali_percen = < 7 >;
		aw8697_vib_cont_drv_lev = < 60 >;
		aw8697_vib_cont_drv_lvl_ov = < 60 >;
		aw8697_vib_cont_td = < 0xef >;
		aw8697_vib_cont_zc_thr = < 0x08f8 >;  /*hq 0x08F8 */
		aw8697_vib_cont_num_brk = < 3 >;
		aw8697_vib_f0_coeff = < 260 >; /*Don't modify it 2.604167*/
		aw8697_vib_f0_trace_parameter = < 9 3 1 31 >;
		aw8697_vib_bemf_config = < 0 0x08 0x03 0xf8 >;
		aw8697_vib_sw_brake = < 0x2c >;
		aw8697_vib_tset = < 0x1a >;
		aw8697_vib_r_spare = < 0x68 >;
		aw8697_vib_bstdbg = < 0x30 0xeb 0xd4 0 0 0 >;
		aw8697_vib_trig_config = < 0 1 0 1 2
					   0 1 0 1 2
					   0 1 0 1 2 >;
		aw8697_vib_bst_vol_default = < 0x0e >;
		aw8697_vib_bst_vol_ram = < 0x0e >;
		aw8697_vib_bst_vol_rtp = < 0x0e >;
		/*----------------------aw8692x----------------------*/
		aw86927_vib_mode = < 0 >; /* mode: RAM mode->0; CONT mode->1 */
		aw86927_vib_f0_pre = < 1300 >;
		aw86927_vib_f0_cali_percen = < 7 >;
		aw86927_vib_cont_drv1_lvl = < 0x7F >;
		aw86927_vib_cont_drv2_lvl = < 0x36 >;
		aw86927_vib_cont_drv1_time = < 0x04 >;
		aw86927_vib_cont_drv2_time = < 0x06 >;
		aw86927_vib_cont_drv_width = < 0x6A >;
		aw86927_vib_cont_wait_num = < 0x06 >;
		aw86927_vib_cont_brk_time = < 0x08 >;
		aw86927_vib_cont_track_margin = < 0x0C >;
		aw86927_vib_brk_bst_md = < 0 >;
		aw86927_vib_cont_tset = < 0x06 >;
		aw86927_vib_cont_bemf_set = < 0x02 >;
		aw86927_vib_cont_bst_brk_gain = < 0x05 >;
		aw86927_vib_cont_brk_gain = < 0x08 >;
		aw86927_vib_d2s_gain = < 0x04 >;
		aw86927_vib_trig_config = < 0 0 0 1 0 2 0 0
					    0 0 0 1 0 2 0 0
					    0 0 0 1 0 2 0 0 >;
		aw86927_vib_bst_vol_default = < 0x47 >;
		aw86927_vib_bst_vol_ram = < 0x47 >;
		aw86927_vib_bst_vol_rtp = < 0x47 >;
		/*--------------------common--------------------*/
		vib_effect_id_boundary = < 10 >;
		vib_effect_max = < 197 >; /*vib_effect_max must bigger than vib_effect_id*/
		vib_rtp_time = < 20 20 20 20 20 20 20 20 20000 15000
				15000 20000 25000 15000 30000 25000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 20000 20000 20000 20000 20000
				20000 20000 20000 20000 20000 >;
		status = "ok";
		wf_0 {
			/*CLICK*/
			qcom,effect-id = <0>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [3e 3e];
			qcom,wf-brake-pattern = [02 01 00 00];
			qcom,wf-play-rate-us = <20000>;
		};
		wf_1 {
			/*DOUBLE CLICK*/
			qcom,effect-id = <1>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [7e 3e];
			qcom,wf-brake-pattern = [03 01 00 00];
			qcom,wf-play-rate-us = <20000>;
		};
		wf_2 {
			/*TICK*/
			qcom,effect-id = <2>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [7e 3e];
			qcom,wf-brake-pattern = [02 01 00 00];
			qcom,wf-play-rate-us = <20000>;
		};
		wf_3 {
			/*THUD*/
			qcom,effect-id = <3>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [3e 3e];
			qcom,wf-brake-pattern = [02 01 00 00];
			qcom,wf-play-rate-us = <20000>;
		};
		wf_4 {
			/*POP*/
			qcom,effect-id = <4>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [3e 3e];
			qcom,wf-brake-pattern = [02 01 00 00];
			qcom,wf-play-rate-us = <28000>;
		};
		wf_5 {
			/*HEAVY CLICK*/
			qcom,effect-id = <5>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [7e 7e 7e];
			qcom,wf-brake-pattern = [03 03 01 00];
			qcom,wf-play-rate-us = <20000>;
		};
		wf_6 {
			/*id 6*/
			qcom,effect-id = <6>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [3e 3e];
			qcom,wf-brake-pattern = [02 01 00 00];
			qcom,wf-play-rate-us = <20000>;
		};
		wf_7 {
			/*id 7*/
			qcom,effect-id = <7>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [3e 3e];
			qcom,wf-brake-pattern = [02 01 00 00];
			qcom,wf-play-rate-us = <20000>;
		};
		wf_8 {
			/*id 8*/
			qcom,effect-id = <8>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [3e 3e];
			qcom,wf-brake-pattern = [02 01 00 00];
			qcom,wf-play-rate-us = <20000>;
		};
		wf_9 {
			/*id 9*/
			qcom,effect-id = <9>;
			qcom,wf-vmax-mv = <3600>;
			qcom,wf-pattern = [3e 3e];
			qcom,wf-brake-pattern = [02 01 00 00];
			qcom,wf-play-rate-us = <20000>;
		};
	};
};

&pm8350b_haptics {
	status = "disabled";
};

&soc {
        fingerprint_goodix {
		compatible = "goodix,fingerprint";
		vdda-supply = <&L11C>;
		goodix,gpio-reset = <&tlmm 41 0x0>;
		goodix,gpio-irq = <&tlmm 40 0x0>;
		status = "ok";
	};
};

&L11C {
	regulator-boot-on;
	regulator-always-on;
	regulator-min-microvolt = <3008000>;
	regulator-max-microvolt = <3008000>;
	qcom,init-voltage = <3008000>;
};


&soc {
	touch_avdd_vreg: touch_avdd_vreg {
		compatible = "regulator-fixed";
		regulator-name = "touch_avdd_vreg";
		enable-active-high;
		gpio = <&tlmm 97 0>;
	};
};

&tlmm {
	mi_ts_active: mi_ts_active {
		mux {
				pins = "gpio21", "gpio20";
				function = "gpio";
		};

		config {
				pins = "gpio21", "gpio20";
				drive-strength = <8>;
				bias-pull-up;
		};
	};
};

&L9C {
		regulator-min-microvolt = <3224000>;
		regulator-max-microvolt = <3224000>;
		qcom,init-voltage = <3224000>;
};

&L2C {
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		qcom,init-voltage = <1800000>;
};

&BOB {
		regulator-min-microvolt = <3296000>;
		regulator-max-microvolt = <3296000>;
		qcom,init-voltage = <3296000>;
};


&qupv3_se4_spi {
	status = "ok";
	qcom,rt;
	fts@0 {
		status = "ok";
		compatible = "st,spi";
		reg = <0x0>;
		interrupt-parent = <&tlmm>;
		interrupts = <21 0x2008>;
		pinctrl-names = "pmx_ts_active", "pmx_ts_suspend";
		pinctrl-0 = <&mi_ts_active>;
		pinctrl-1 = <&ts_int_suspend &ts_reset_suspend>;
		avdd-supply = <&L9C>;
		vdd-supply = <&L2C>;
                fts,pwr-reg-name = "avdd";
		fts,bus-reg-name = "vdd";
		fts,irq-gpio = <&tlmm 21 0x2008>;
		fts,irq-gpio-name = "fts_irq";
		fts,reset-gpio-enable;
		fts,reset-gpio = <&tlmm 20 0x00>;
		fts,reset-gpio-name = "fts_rst";
		fts,irq-flags = <0x2008>;
		fts,x-max = <14400>;
		fts,y-max = <32000>;
		fts,fod-lx = <5860>;
		fts,fod-ly = <23460>;
		fts,fod-x-size = <2680>;
		fts,fod-y-size = <2660>;
		fts,support-fod;
		spi-max-frequency = <12000000>;
		fts,support-super-resolution = <1>;
		fts,default-fw-name = "st_fts_l1.ftb";
		fts,config-array-size = <1>;
		fts,touch-follow-performance-def = <3>;
		fts,touch-tap-sensitivity-def = <4>;
		fts,touch-aim-sensitivity-def = <3>;
		fts,touch-tap-stability-def = <3>;
		fts,cornerfilter-area-step1 = <150>;
		fts,cornerfilter-area-step2 = <280>;
		fts,cornerfilter-area-step3 = <400>;
		fts,touch-deadzone-filter-ver = <2 0 0 0 0 0 0 0
										2 1 0 0 0 0 0 0
										2 2 0 0 0 3199 0 0
										2 3 1439 0 1439 3199 0 0>;
		fts,touch-deadzone-filter-hor = <2 0 0 0 1439 7 0 0
										2 1 0 3192 1439 3199 0 0
										2 2 0 0 0 3199 0 0
										2 3 1439 0 1439 3199 0 0>;
		fts,touch-edgezone-filter-ver = <1 0 0 0 0 0 0 0
										1 1 0 0 0 0 0 0
										1 2 0 0 60 3199 0 0
										1 3 1379 0 1439 3199 0 0>;
		fts,touch-edgezone-filter-hor = <1 0 0 0 1439 70 0 0
										1 1 0 3129 1439 3199 0 0
										1 2 0 0 60 3199 0 0
										1 3 1379 0 1439 3199 0 0>;
		fts,touch-cornerzone-filter-ver = <0 0 0 0 0 0 0 0
										0 1 0 0 0 0 0 0
										0 2 0 2799 250 3199 0 0
										0 3 1189 2799 1439 3199 0 0>;
		fts,touch-cornerzone-filter-hor1 = <0 0 0 0 280 280 0 0
										0 1 0 0 0 0 0 0
										0 2 0 2919 280 3199 0 0
										0 3 0 0 0 0 0 0>;
		fts,touch-cornerzone-filter-hor2 = <0 0 0 0 0 0 0 0
										0 1 1159 0 1439 280 0 0
										0 2 0 0 0 0 0 0
										0 3 1159 2919 1439 3199 0 0>;
		fts,touch-follow-performance = <10 15 1
										8 15 1
										6 15 1
										4 15 1
										2 15 1>;
		fts,touch-tap-sensitivity = <160 150 140 120 100>;
		fts,touch-aim-sensitivity = <10 8 6 4 2>;
		fts,touch-tap-stability = <8 12 15 18 25>;
		fts,touch-expert-array = <6 15 1 120 6 15
								  2 15 1 120 4 15
								  4 15 1 120 2 15>;
		fts,cfg_0 {
			fts,tp-vendor = <0x38>;
			fts,fw-name = "st_fts_l1.ftb";
			fts,limit-name = "stm_fts_production_limits.csv";
		};
	};
};

&pmk8350_vadc {
	pinctrl-names = "default";
	pinctrl-0 = <&pm8350b_rear_tof_therm_default>;

	pm8350_msm_therm {
		reg = <PM8350_ADC7_AMUX_THM1_100K_PU>;
		label = "pm8350_msm_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};

	pm8350_cam_flash_therm {
		reg = <PM8350_ADC7_AMUX_THM2_100K_PU>;
		label = "pm8350_cam_flash_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};

	pm8350_hot_pocket_therm {
		reg = <PM8350_ADC7_AMUX_THM3_100K_PU>;
		label = "pm8350_hot_pocket_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};

	pm8350_wide_rfc_therm {
		reg = <PM8350B_ADC7_GPIO4_100K_PU>;
		label = "pm8350_wide_rfc_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};

	pm8350b_rear_tof_therm {
		reg = <PM8350B_ADC7_GPIO2_100K_PU>;
		label = "pm8350b_rear_tof_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};

	pm8350b_usb_conn_therm {
		reg = <PMR735A_ADC7_GPIO1_100K_PU>;
		label = "pm8350b_usb_conn_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};

	pm8350b_wl_chg_therm {
		reg = <PMR735A_ADC7_GPIO2_100K_PU>;
		label = "pm8350b_wl_chg_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};

	pmk8350_wifi_therm {
		reg = <PMR735A_ADC7_GPIO3_100K_PU>;
		label = "pmk8350_wifi_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};
	pmk8350_xo_therm {
		reg = <PMK8350_ADC7_AMUX_THM1_100K_PU>;
		label = "pmk8350_xo_therm";
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
		qcom,pre-scaling = <1 1>;
	};
};

&pmk8350_adc_tm {
	io-channels = <&pmk8350_vadc PM8350_ADC7_AMUX_THM1_100K_PU>,
			<&pmk8350_vadc PM8350_ADC7_AMUX_THM2_100K_PU>,
			<&pmk8350_vadc PM8350_ADC7_AMUX_THM3_100K_PU>,
			<&pmk8350_vadc PM8350B_ADC7_GPIO4_100K_PU>,
			<&pmk8350_vadc PM8350B_ADC7_GPIO2_100K_PU>,
			<&pmk8350_vadc PMR735A_ADC7_GPIO1_100K_PU>,
			<&pmk8350_vadc PMR735A_ADC7_GPIO2_100K_PU>,
			<&pmk8350_vadc PMR735A_ADC7_GPIO3_100K_PU>;

	pm8350_msm_therm {
		reg = <PM8350_ADC7_AMUX_THM1_100K_PU>;
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
	};

	pm8350_cam_flash_therm {
		reg = <PM8350_ADC7_AMUX_THM2_100K_PU>;
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
	};

	pm8350_hot_pocket_therm {
		reg = <PM8350_ADC7_AMUX_THM3_100K_PU>;
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
	};

	pm8350_wide_rfc_therm {
		reg = <PM8350B_ADC7_GPIO4_100K_PU>;
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
	};

	pm8350b_rear_tof_therm {
		reg = <PM8350B_ADC7_GPIO2_100K_PU>;
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
	};

	pm8350b_usb_conn_therm {
		reg = <PMR735A_ADC7_GPIO1_100K_PU>;
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
	};

	pm8350b_wl_chg_therm {
		reg = <PMR735A_ADC7_GPIO2_100K_PU>;
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
	};

	pmk8350_wifi_therm {
		reg = <PMR735A_ADC7_GPIO3_100K_PU>;
		qcom,ratiometric;
		qcom,hw-settle-time = <200>;
	};
};

&pmk8350 {
	pm8350_adc_tm_iio: adc_tm_e {
		compatible = "qcom,adc-tm7-iio";
		reg = <0x3400>;
		#thermal-sensor-cells = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		io-channels = <&pmk8350_vadc PMK8350_ADC7_AMUX_THM1_100K_PU>;

		pmk8350_xo_therm {
			reg = <PMK8350_ADC7_AMUX_THM1_100K_PU>;
			qcom,ratiometric;
			qcom,hw-settle-time = <200>;
		};
	};
};

&thermal_zones {
	cpu_therm {
		polling-delay-passive = <0>;
		polling-delay = <0>;
		thermal-governor = "user_space";
		thermal-sensors = <&pmk8350_adc_tm PM8350_ADC7_AMUX_THM1_100K_PU>;
		wake-capable-sensor;
		trips {
			active-config0 {
				temperature = <125000>;
				hysteresis = <1000>;
				type = "passive";
			};
		};
	};

	flash_therm {
		polling-delay-passive = <0>;
		polling-delay = <0>;
		thermal-governor = "user_space";
		thermal-sensors = <&pmk8350_adc_tm PM8350_ADC7_AMUX_THM2_100K_PU>;
		wake-capable-sensor;
		trips {
			active-config0 {
				temperature = <125000>;
				hysteresis = <1000>;
				type = "passive";
			};
		};
	};

	quiet_therm {
		polling-delay-passive = <0>;
		polling-delay = <0>;
		thermal-governor = "user_space";
		thermal-sensors = <&pmk8350_adc_tm PM8350_ADC7_AMUX_THM3_100K_PU>;
		wake-capable-sensor;
		trips {
			active-config0 {
				temperature = <125000>;
				hysteresis = <1000>;
				type = "passive";
			};
		};
	};

	charger_therm0 {
		polling-delay-passive = <0>;
		polling-delay = <0>;
		thermal-governor = "user_space";
		thermal-sensors = <&pmk8350_adc_tm PM8350B_ADC7_GPIO4_100K_PU>;
		wake-capable-sensor;
		trips {
			active-config0 {
				temperature = <125000>;
				hysteresis = <1000>;
				type = "passive";
			};
		};
	};

	wireless_therm {
		polling-delay-passive = <0>;
		polling-delay = <0>;
		thermal-governor = "user_space";
		thermal-sensors = <&pmk8350_adc_tm PM8350B_ADC7_GPIO2_100K_PU>;
		wake-capable-sensor;
		trips {
			active-config0 {
				temperature = <125000>;
				hysteresis = <1000>;
				type = "passive";
			};
		};
	};

	pa_therm0 {
		polling-delay-passive = <0>;
		polling-delay = <0>;
		thermal-governor = "user_space";
		thermal-sensors = <&pmk8350_adc_tm PMR735A_ADC7_GPIO1_100K_PU>;
		wake-capable-sensor;
		trips {
			active-config0 {
				temperature = <125000>;
				hysteresis = <1000>;
				type = "passive";
			};
		};
	};

	pa_therm1 {
		polling-delay-passive = <0>;
		polling-delay = <0>;
		thermal-governor = "user_space";
		thermal-sensors = <&pmk8350_adc_tm PMR735A_ADC7_GPIO2_100K_PU>;
		wake-capable-sensor;
		trips {
			active-config0 {
				temperature = <125000>;
				hysteresis = <1000>;
				type = "passive";
			};
		};
	};

	wifi_therm {
		polling-delay-passive = <0>;
		polling-delay = <0>;
		thermal-governor = "user_space";
		thermal-sensors = <&pmk8350_adc_tm PMR735A_ADC7_GPIO3_100K_PU>;
		wake-capable-sensor;
		trips {
			active-config0 {
				temperature = <125000>;
				hysteresis = <1000>;
				type = "passive";
			};
		};
	};
	xo-therm {
                polling-delay-passive = <0>;
                polling-delay = <0>;
                thermal-governor = "user_space";
                thermal-sensors = <&pm8350_adc_tm_iio PMK8350_ADC7_AMUX_THM1_100K_PU>;
                wake-capable-sensor;
                trips {
                        active-config0 {
                                temperature = <125000>;
                                hysteresis = <1000>;
                                type = "passive";
                        };
                };
        };
};

&qseecom_ta_mem {
	size = <0x0 0x2000000>;
};

&qseecom_mem {
	size = <0x0 0x2400000>;
};

&nxp_eusb2_repeater {
	qcom,param-override-seq =
		<0x62 0x08
		0x00 0x07>;
	qcom,param-override-seq-host =
		<0x63 0x08
		0x22 0x07>;
};

&battery_charger {
        qcom,shutdown-voltage = <3350>;
};
