#BCM4375B1 SWB-E43 R03 SEMCO nvram_190405_FW18.38.15.4
# 2G iPA, 5G ePA
NVRAMRev=$Rev: 806135 $
sromrev=11
boardrev=0x1300
boardtype=0x088f
boardflags=0x10401001
boardflags2=0x00800000
boardflags3=0x40000100
#boardnum=57410
macaddr=00:90:4c:30:50:01
jtag_irw=38

#Regulatory specific
ccode=GB
regrev=0

# Board specific
vendid=0x14e4
devid=0x4470
manfid=0x2d0
antswitch=0
pdgain5g=0
pdgain2g=0
aa2g=3
aa5g=3
agbg0=0
agbg1=0
aga0=0
aga1=0
extpagain5g=0
slice/1/extpagain2g=2
slice/1/extpagain5g=0
rxgains2gelnagaina0=1
rxgains2gtrisoa0=6
rxgains2gtrelnabypa0=1
rxgains5gelnagaina0=2
rxgains5gtrisoa0=6
rxgains5gtrelnabypa0=1
rxgains5gmelnagaina0=2
rxgains5gmtrisoa0=6
rxgains5gmtrelnabypa0=1
rxgains5ghelnagaina0=2
rxgains5ghtrisoa0=6
rxgains5ghtrelnabypa0=1
rxgains2gelnagaina1=2
rxgains2gtrisoa1=6
rxgains2gtrelnabypa1=1
rxgains5gelnagaina1=2
rxgains5gtrisoa1=6
rxgains5gtrelnabypa1=1
rxgains5gmelnagaina1=2
rxgains5gmtrisoa1=6
rxgains5gmtrelnabypa1=1
rxgains5ghelnagaina1=2
rxgains5ghtrisoa1=6
rxgains5ghtrelnabypa1=1

rssicorrnorm_c0=0,0
rssicorrnorm_c1=0,0
rssicorrnorm5g_c0=0,0,0,0,0,0,0,0,0,0,0,0
rssicorrnorm5g_c1=0,0,0,0,0,0,0,0,0,0,0,0
rssi_cal_freq_grp_2g= 0x08,0x01,0x91,0x2a,0x23,0xb3,0xc4
rssi_delta_5gl=-7,-6,-7,-6,-11,-6,-11,-6,-10,-6,-10,-6,-3,-3,-3,-3,-8,-3,-8,-3,-6,-3,-6,-3
rssi_delta_5gml=-7,-8,-7,-8,-10,-8,-10,-8,-7,-8,-7,-8,-2,-4,-2,-4,-4,-4,-4,-4,-4,-4,-4,-4
rssi_delta_5gmu=-6,-7,-6,-7,-8,-7,-8,-7,-7,-7,-7,-7,-4,-1,-4,-1,-4,-2,-4,-2,-2,-2,-2,-2
rssi_delta_5gh=-6,-8,-6,-8,-8,-8,-8,-8,-8,-8,-8,-8,-4,-1,-4,-1,-3,-3,-3,-3,-4,-3,-4,-3
rssi_cal_rev=1
rxgaincal_rssical=1
rssi_delta_2gb0=-12,5,-12,5,-12,5,-12,5,-18,-2,-18,-2,-18,-2,-18,-2
rssi_delta_2gb1=-12,5,-12,5,-12,5,-12,5,-18,-2,-18,-2,-18,-2,-18,-2
rssi_delta_2gb2=-12,5,-12,5,-12,5,-12,5,-18,-2,-18,-2,-18,-2,-18,-2
rssi_delta_2gb3=-12,5,-12,5,-12,5,-12,5,-18,-2,-18,-2,-18,-2,-18,-2
rssi_delta_2gb4=-12,5,-12,5,-12,5,-12,5,-18,-2,-18,-2,-18,-2,-18,-2

gain_cal_temp=36
trloss_adj_time_dur=30
trloss_adj_temp_thresh=10
temp_comp_tr_loss=1

slice/1/rxgain_tempcoeff2g_sub=28,31,25,30,25,27,28,24,24,23
rxgain_tempcoeff5gl=32,29
rxgain_tempcoeff5gml=31,46
rxgain_tempcoeff5gmu=26,36
rxgain_tempcoeff5gh=31,36
slice/1/rxgain_tempcoeff2g_sub_elnaoff=28,30,25,25,25,25,22,20,21,23
rxgain_tempcoeff5gl_elnaoff=48,55
rxgain_tempcoeff5gml_elnaoff=50,56
rxgain_tempcoeff5gmu_elnaoff=51,57
rxgain_tempcoeff5gh_elnaoff=49,57

#Two range TSSI
tworangetssi5g=0
slice/1/tworangetssi2g=0
slice/1/lowpowerrange2g=0

nocrc=1
otpimagesize=502

xtalfreq=37400

txchain=3
rxchain=3

## --- 11b ANT selection Diversity ---
cck_onecore_tx=1
#ocl_cm=2
#slice/1/ocl_cm=2

cckdigfilttype=2
slice/1/bphyscale=36
slice/1/cck_txgain_offsetval=54
slice/1/cck_txgain_offsetcal_en=1
cck_txgain_offsetcal_en=1
#bit mask for slice capability bit 0:2G bit 1:5G
bandcap=2
slice/1/bandcap=1

#TXBF Related
rpcal2g=50
rpcal5gb0=5
rpcal5gb1=11
rpcal5gb2=8
rpcal5gb3=10
slice/1/rpcal2g=50
slice/1/rpcal5gb0=5
slice/1/rpcal5gb1=11
slice/1/rpcal5gb2=8
slice/1/rpcal5gb3=10

#FDSS Related
#fdss_level_5g=0,0
#fdss_interp_en=1
#fdss_level_5g_ch36=4,4
#fdss_level_5g_ch64=4,4
#fdss_level_5g_ch100=4,4
#slice/1/fdss_interp_en=1
#slice/1/fdss_bandedge_2g_en=1
#slice/1/fdss_level_2g=0,0
#slice/1/fdss_level_2g_ch1=4,4
#slice/1/fdss_level_2g_ch11=4,4
#slice/1/fdss_level_11ax_2g=0,0
#slice/1/fdss_level_11ax_2g_ch1=1,1
#slice/1/fdss_level_11ax_2g_ch11=1,1

tempthresh=255
tempoffset=-1
rawtempsense=0x1ff
phycal_tempdelta=15
temps_period=15
temps_hysteresis=15

#------------- TSSI Related -------------
tssipos2g=1
tssipos5g=1

AvVmid_c0=2,131,6,43,6,45,6,42,6,42
AvVmid_c1=2,130,6,45,6,51,6,46,6,43

slice/1/AvVmid_c0=3,111,1,159,1,166,1,153,1,153
slice/1/AvVmid_c1=3,111,1,155,1,158,1,147,1,151

# CCK in case of multi mode 5
pa2gccka0=0xff5a,0x1ce0,0xfc93
pa2gccka1=0xff40,0x1b59,0xfcad

# OFDM in case of multi_mode 5
pa2ga0=0xff79,0x1a52,0xfcf9
pa2ga1=0xff8c,0x1c19,0xfce6

slice/1/enable_tssi_war=1

pa5ga0=0xff44,0x17f7,0xfd3e,0xff44,0x17f7,0xfd3e,0xff3a,0x170a,0xfd4e,0xff3a,0x170a,0xfd4e
pa5ga1=0xff42,0x176c,0xfd4d,0xff3f,0x170a,0xfd57,0xff42,0x16f0,0xfd5b,0xff3c,0x16be,0xfd56

# Max power and offsets
maxp2ga0=83
maxp2ga1=83
maxp5ga0=77,76,74,74
maxp5ga1=73,73,72,72
subband5gver=0x4
paparambwver=3
cckpwroffset0=0
cckpwroffset1=0
pdoffset40ma0=0x0000
pdoffset80ma0=0x0000
pdoffset40ma1=0x0000
pdoffset80ma1=0x10F0
slice/1/pdoffset20mRU_c0=1,0,-2,-2,-2,-2,0,2,3,4,0,0,2,1,0,1
slice/1/pdoffset20mRU_c1=2,0,0,0,0,0,0,0,1,0,0,0,0,-2,-3,-3
pdoffset20mRU_c0=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset20mRU_c1=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset40mRU_c0=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset40mRU_c1=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset80mRUset1_c0=-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4
pdoffset80mRUset2_c0=-4,-4,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset80mRUset1_c1=-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-4,-6,-6,-6,-6,-6,-4,-4
pdoffset80mRUset2_c1=-4,-6,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
cckbw202gpo=0
cckbw20ul2gpo=0
mcsbw202gpo=0xDC886666
mcsbw402gpo=0xDA886664
dot11agofdmhrbw202gpo=0x6666
ofdmlrbw202gpo=0x0044
mcsbw205glpo=0x66644440
mcsbw405glpo=0x88866662
mcsbw805glpo=0xAAA88884
mcsbw1605glpo=0
mcsbw205gmpo=0x66644440
mcsbw405gmpo=0x88866662
mcsbw805gmpo=0xAAA88884
mcsbw1605gmpo=0
mcsbw205ghpo=0x66644440
mcsbw405ghpo=0x88866662
mcsbw805ghpo=0xAAA88884

slice/1/powoffs2gtna0=-2,-1,1,2,2,-1,0,-2,-2,1,-3,0,-1,0
slice/1/powoffs2gtna1=-3,0,1,-1,-2,-4,-3,0,1,2,-2,-2,-2,0
#slice/1/pdoffsetcckma0=1
#slice/1/pdoffsetcckma1=1
mcs1024qam2gpo=0xCCBB
mcs1024qam5glpo=0xCCBB66
mcs1024qam5gmpo=0xCCBB66
mcs1024qam5ghpo=0xCCBB66
mcs1024qam5gx1po=0xDDBB66
mcs1024qam5gx2po=0xDDBB66
mcs8poexp=0
mcs9poexp=0
mcs10poexp=0

# 5G power offset per channel for band edge channel
powoffs5g20mtna0=0,0,0,0,0,0,0
powoffs5g20mtna1=0,0,0,0,0,0,0
powoffs5g40mtna0=0,0,0,0,0
powoffs5g40mtna1=0,0,0,0,0
powoffs5g80mtna0=0,0,0,0,0
powoffs5g80mtna1=0,0,0,0,0
mcs11poexp=0

# OLPC Related
disable_olpc=0
olpc_thresh5g=40
olpc_anchor5g=40
slice/1/disable_olpc=0
slice/1/olpc_thresh2g=46
slice/1/olpc_anchor2g=56
slice/1/olpc_thresh2g_hi=0x7f48

hwolpc_offset_c0=-1,-3,-4,-3,-2
hwolpc_offset_c1=-2,-2,-3,-2,-1

#LTE Coex Related
#ltecxmux=0
#ltecxpadnum=0x0504
#ltecxfnsel=0x44
#ltecxgcigpio=0x04
#OOB params
#device_wake_opt=1
host_wake_opt=0

# SWCTRL Related
swctrlmap_5g=0xe0e0c0c0,0xa0a00000,0x80800000,0x000000,0x3FF
swctrlmapext_5g=0x00000000,0x00000000,0x00000000,0x000000,0x000
fem_table_init_val=0x00000000,0x80800000
fem_table_init_val_ext=0x00000000,0x00000000

slice/1/swctrlmap_2g=0x00000000,0x03030000,0x01010000,0x000000,0x3FF
slice/1/swctrlmapext_2g=0x00000000,0x00000000,0x00000000,0x000000,0x003

slice/1/fem_table_init_val=0x01010000,0x00000000
slice/1/fem_table_init_val_ext=0x00000000,0x00000000

#clb2gslice0core0=0x000
clb2gslice1core0=0x003
clb5gslice0core0=0x0E0
#clb5gslice1core0=0x070
#clb2gslice0core1=0x000
clb2gslice1core1=0x003
clb5gslice0core1=0x0E0
#clb5gslice1core1=0x038
btc_prisel_ant_mask=0x2
clb_swctrl_smask_ant0=0x3ff
clb_swctrl_smask_ant1=0x3ff
muxenab=1

#BT Coex 1:TDM
btc_mode=1

# --- PAPD Cal related params ----
txwbpapden=0 # 0:NBPAPD 1:WBPAPD
# NB PAPD Cal params
slice/1/nb_eps_offset=485,487
slice/1/nb_bbmult=35,39
slice/1/nb_papdcalidx=11,11
slice/1/nb_txattn=3,3
slice/1/nb_rxattn=0,0
slice/1/nb_eps_stopidx=63
slice/1/papdgainctrl2g=1
slice/1/pacalshift2g=2,1
slice/1/ampbased_gc=0
slice/1/papd_gainctrl_scaleIdx=52

# energy detect threshold
ed_thresh2g=-60
ed_thresh5g=-63
# energy detect threshold for EU
eu_edthresh2g=-60
eu_edthresh5g=-63

btldopu=1

#Enable LHL PS mode
lhl_ps_mode=3
# to enable he features
he_en=1

# FE Loss comp parameters
slice/1/felossTx2ga0=2,2,2,2,2,1,1,0,1,2,2,2,2,0
slice/1/felossTx2ga1=3,4,4,4,4,3,4,4,4,3,2,4,6,0
slice/1/felossRx2ga0=2,2,2,2,2,1,1,0,1,2,2,2,2,0
slice/1/felossRx2ga1=3,4,4,4,4,3,4,4,4,3,2,4,6,0
felossTx5ga0=3,1,0,0
felossTx5ga1=0,0,0,0
felossRx5ga0=3,1,0,0
felossRx5ga1=0,0,0,0

## ULOFDMA Board limit PPRs for 2G20 ##
ruppr2g20bpska0=0x000318c6
ruppr2g20bpska1=0x00042108
ruppr2g20qpska0=0x000318c6
ruppr2g20qpska1=0x000318c6
ruppr2g20qam16a0=0x00042108
ruppr2g20qam16a1=0x0006318c
ruppr2g20qam64a0=0x0004a529
ruppr2g20qam64a1=0x0006318c
ruppr2g20qam256a0=0x0006b5ad
ruppr2g20qam256a1=0x0007bdef
ruppr2g20qam1024a0=0x0
ruppr2g20qam1024a1=0x0
## ULOFDMA Board limit PPRs for 5G20 ##
ruppr5g20bpska0=0x000e7382
ruppr5g20bpska1=0x0000000b
ruppr5g20qpska0=0x000e7382
ruppr5g20qpska1=0x0000000a
ruppr5g20qam16a0=0x00010843
ruppr5g20qam16a1=0x0002108a
ruppr5g20qam64a0=0x00010842
ruppr5g20qam64a1=0x000318ca
ruppr5g20qam256a0=0x00008422
ruppr5g20qam256a1=0x0005294a
ruppr5g20qam1024a0=0x00060000
ruppr5g20qam1024a1=0x00060000
## ULOFDMA Board limit PPRs for 5G40 ##
ruppr5g40bpska0=0x03ffffe1
ruppr5g40bpska1=0x00210849
ruppr5g40qpska0=0x03ffffe1
ruppr5g40qpska1=0x00210849
ruppr5g40qam16a0=0x00210841
ruppr5g40qam16a1=0x006318c9
ruppr5g40qam64a0=0x005294a3
ruppr5g40qam64a1=0x0084210b
ruppr5g40qam256a0=0x005294a3
ruppr5g40qam256a1=0x0084210b
ruppr5g40qam1024a0=0x00840000
ruppr5g40qam1024a1=0x00a50000
## ULOFDMA Board limit PPRs for 5G80 ##
ruppr5g80bpska0=0x08210843
ruppr5g80bpska1=0x28a5294b
ruppr5g80qpska0=0x08210843
ruppr5g80qpska1=0x1042108a
ruppr5g80qam16a0=0x186318c5
ruppr5g80qam16a1=0x2084210c
ruppr5g80qam64a0=0x20842107
ruppr5g80qam64a1=0x28a5294e
ruppr5g80qam256a0=0x20842107
ruppr5g80qam256a1=0x28a5294e
ruppr5g80qam1024a0=0x30c60000
ruppr5g80qam1024a1=0x30c60000

## powoff 2g temp based comp params
slice/1/powoffcompreftemp=25
slice/1/powoffs2gtempcomploa0=1907
slice/1/powoffs2gtempcomploa1=1754
slice/1/powoffs2gtempcomphia0=0
slice/1/powoffs2gtempcomphia1=0

### SAR HEAD params_MIMO_RSDB
## 2g normal:15dB airplane:15dB
slice/1/dynsar_2g=0xbcbc
slice/1/dynsar_2g_2=0xbcbc
## 5g normal:14dB airplane:14dB
dynsar_5g=0xb8b8
dynsar_5g_2=0xb8b8
## 2g normal:13dB airplane:13dB
slice/1/rsdb_dynsar_2g=0xb4b4
slice/1/rsdb_dynsar_2g_2=0xb4b4
## 5g normal:13dB airplane:13dB
rsdb_dynsar_5g=0xb4b4
rsdb_dynsar_5g_2=0xb4b4

### SAR GRIP params_MIMO_RSDB
## 2g normal:16dB airplane:15dB
slice/1/grip_dynsar_2g=0x0000
slice/1/grip_dynsar_2g_2=0x0000
## 5g normal:14dB airplane:13dB
grip_dynsar_5g=0x0000
grip_dynsar_5g_2=0x0000
## 2g normal:15dB airplane:14dB
slice/1/grip_rsdb_dynsar_2g=0x0000
slice/1/grip_rsdb_dynsar_2g_2=0x0000
## 5g normal:13dB airplane:12dB
grip_rsdb_dynsar_5g=0x0000
grip_rsdb_dynsar_5g_2=0x0000

### Disable Parameters 2G:16dB 5G:13dB
slice/1/rsdb_dynsar_2g_1=0xc0c0
rsdb_dynsar_5g_1=0xb4b4

### RU SAR HEAD params_MIMO_RSDB
## 2g normal:16,16,16dB airplane:16,16,16dB
slice/1/dynsar_2g_ru=0xc0c0,0xc0c0,0xc0c0
slice/1/dynsar_2g_2_ru=0xc0c0,0xc0c0,0xc0c0
## 5g normal:13,13,13dB airplane:13,13,13dB
dynsar_5g_ru=0xb4b4,0xb4b4,0xb4b4
dynsar_5g_2_ru=0xb4b4,0xb4b4,0xb4b4
## 2g normal:13,13,13dB airplane:13,13,13dB
slice/1/rsdb_dynsar_2g_ru=0xb4b4,0xb4b4,0xb4b4
slice/1/rsdb_dynsar_2g_2_ru=0xb4b4,0xb4b4,0xb4b4
## 5g normal:13,13,13dB airplane:13,13,13dB
rsdb_dynsar_5g_ru=0xb4b4,0xb4b4,0xb4b4
rsdb_dynsar_5g_2_ru=0xb4b4,0xb4b4,0xb4b4

### RU SAR GRIP params_MIMO_RSDB
## 2g normal:16,8,1dB airplane:20,12,4dB
slice/1/grip_dynsar_2g_ru=0x0000,0x0000,0x0000
slice/1/grip_dynsar_2g_2_ru=0x0000,0x0000,0x0000
## 5g normal:16,8,1dB airplane:20,12,4dB
grip_dynsar_5g_ru=0x0000,0x0000,0x0000
grip_dynsar_5g_2_ru=0x0000,0x0000,0x0000
## 2g normal:16,8,1dB airplane:20,12,4dB
slice/1/grip_rsdb_dynsar_2g_ru=0x0000,0x0000,0x0000
slice/1/grip_rsdb_dynsar_2g_2_ru=0x0000,0x0000,0x0000
## 5g normal:16,8,1dB airplane:20,12,4dB
grip_rsdb_dynsar_5g_ru=0x0000,0x0000,0x0000
grip_rsdb_dynsar_5g_2_ru=0x0000,0x0000,0x0000

## NR SAR back off - 2G/5G MIMO : 1dB, 2G/5G RSDB : 2dB
slice/1/nr_mw_dynsar_2g=0x0000
slice/1/nr_mw_rsdb_dynsar_2g=0x0000
nr_mw_dynsar_5g=0x0000
nr_mw_rsdb_dynsar_5g=0x0000
## NR SAR only mode - 2G : 14dBm, 5G : 13dBm
slice/1/nr_mw_dynsar_2g_cap=0x0000
nr_mw_dynsar_5g_cap=0x0000

## NR SAR back off - 2G/5G MIMO : 3dB, 2G/5G RSDB : 4dB
slice/1/nr_sub6_dynsar_2g=0x0000
slice/1/nr_sub6_rsdb_dynsar_2g=0x0000
nr_sub6_dynsar_5g=0x0000
nr_sub6_rsdb_dynsar_5g=0x0000
## NR SAR only mode - 2G : 12dBm, 5G : 10dBm
slice/1/nr_sub6_dynsar_2g_cap=0x0000
nr_sub6_dynsar_5g_cap=0x0000

### FCC Mode: 7dB 0.25dB
slice/1/fccpwrch12=28
slice/1/fccpwrch13=1
