#BCM4375B0 SWB-E43 R02 SEMCO nvram_180803_FW18.35.112


# bcm4375 B0, SEMCO E43 R02 nvram
# 2G iPA, 5G ePA
NVRAMRev=$Rev: 506283 $
sromrev=11
boardrev=0x1100
boardtype=0x088e
boardflags=0x10401001
boardflags2=0x00800000
boardflags3=0x40000100
#boardnum=57410
macaddr=00:90:4c:30:40:01
jtag_irw=38

#Regulatory specific
ccode=GB
regrev=0

# Board specific
vendid=0x14e4
devid=0x4470
manfid=0x2d0
antswitch=0
pdgain5g=0
pdgain2g=0
aa2g=3
aa5g=3
agbg0=0
agbg1=0
aga0=0
aga1=0
extpagain5g=0
slice/1/extpagain2g=2
slice/1/extpagain5g=0
rxgains2gelnagaina0=2
rxgains2gtrisoa0=6
rxgains2gtrelnabypa0=1
rxgains5gelnagaina0=2
rxgains5gtrisoa0=6
rxgains5gtrelnabypa0=1
rxgains5gmelnagaina0=2
rxgains5gmtrisoa0=6
rxgains5gmtrelnabypa0=1
rxgains5ghelnagaina0=2
rxgains5ghtrisoa0=6
rxgains5ghtrelnabypa0=1
rxgains2gelnagaina1=2
rxgains2gtrisoa1=6
rxgains2gtrelnabypa1=1
rxgains5gelnagaina1=2
rxgains5gtrisoa1=6
rxgains5gtrelnabypa1=1
rxgains5gmelnagaina1=2
rxgains5gmtrisoa1=6
rxgains5gmtrelnabypa1=1
rxgains5ghelnagaina1=2
rxgains5ghtrisoa1=6
rxgains5ghtrelnabypa1=1

#RSSI related
rssicorrnorm_c0=0,0
rssicorrnorm_c1=0,0
rssicorrnorm5g_c0=0,0,0,0,0,0,0,0,0,0,0,0
rssicorrnorm5g_c1=0,0,0,0,0,0,0,0,0,0,0,0
rssi_cal_freq_grp_2g= 0x08,0x01,0x91,0x2a,0x23,0xb3,0xc4
rssi_delta_5gl=-7 -5 -7 -5 -7 -5 -7 -5 -7 -5 -7 -5 -6 -1 -6 -1 -6 -1 -6 -1 -6 -1 -6 -1
rssi_delta_5gml=-10 -7 -10 -7 -10 -7 -10 -7 -10 -7 -10 -7 -6 -3 -6 -3 -6 -3 -6 -3 -6 -3 -6 -3
rssi_delta_5gmu=-10 -7 -10 -7 -10 -7 -10 -7 -10 -7 -10 -7 -6 -3 -6 -3 -6 -3 -6 -3 -6 -3 -6 -3
rssi_delta_5gh=-10 -5 -10 -5 -10 -5 -10 -5 -10 -5 -10 -5 -6 -1 -6 -1 -6 -1 -6 -1 -6 -1 -6 -1
rssi_cal_rev=1
rxgaincal_rssical=1
rssi_delta_2gb0=-6,8,-6,8,-6,8,-6,8,-22,-10,-22,-10,-22,-10,-22,-10
rssi_delta_2gb1=-6,8,-6,8,-6,8,-6,8,-22,-10,-22,-10,-22,-10,-22,-10
rssi_delta_2gb2=-6,8,-6,8,-6,8,-6,8,-22,-10,-22,-10,-22,-10,-22,-10
rssi_delta_2gb3=-6,8,-6,8,-6,8,-6,8,-22,-10,-22,-10,-22,-10,-22,-10
rssi_delta_2gb4=-6,8,-6,8,-6,8,-6,8,-22,-10,-22,-10,-22,-10,-22,-10
gain_cal_temp=25
trloss_adj_time_dur=30
trloss_adj_temp_thresh=10
temp_comp_tr_loss=1

rxgain_tempcoeff2g_sub=28,31,25,30,25,27,28,24,24,23
rxgain_tempcoeff5gl=32,29
rxgain_tempcoeff5gml=31,46
rxgain_tempcoeff5gmu=26,36
rxgain_tempcoeff5gh=31,36
rxgain_tempcoeff2g_sub_elnaoff=28,30,25,25,25,25,22,20,21,23
rxgain_tempcoeff5gl_elnaoff=48,55
rxgain_tempcoeff5gml_elnaoff=50,56
rxgain_tempcoeff5gmu_elnaoff=51,57
rxgain_tempcoeff5gh_elnaoff=49,57

#Two range TSSI
tworangetssi5g=0
slice/1/tworangetssi2g=0
slice/1/lowpowerrange2g=0

nocrc=1
otpimagesize=502

xtalfreq=37400

txchain=3
rxchain=3

## --- 11b ANT selection Diversity ---
cck_onecore_tx=1
#slice/1/ocl=0
### --- 11b ANT selection Diversity core mask setting ---
#ocl_cm=1
#slice/1/ocl_cm=1

cckdigfilttype=2
slice/1/bphyscale=42
slice/1/cck_txgain_offsetval=36

#bit mask for slice capability bit 0:2G bit 1:5G
bandcap=2
slice/1/bandcap=1

#TXBF Related
rpcal2g=0
rpcal5gb0=0
rpcal5gb1=0
rpcal5gb2=0
rpcal5gb3=0
slice/1/rpcal2g=0
slice/1/rpcal5gb0=0
slice/1/rpcal5gb1=0
slice/1/rpcal5gb2=0
slice/1/rpcal5gb3=0

#FDSS Related
#fdss_level_5g=-1,-1
#fdss_interp_en=0
#slice/1/fdss_level_2g=4,4
#slice/1/fdss_interp_en=1

#PAPRR Related
slice/1/paprdis=1
slice/1/paprrmcsgain2g=128,128,128,128,128,0,0,0,0,0
slice/1/paprrmcsgamma2g=500,500,550,700,700,-1,-1,-1,-1,-1

#Tempsense Related
tempthresh=255
tempoffset=-1
rawtempsense=0x1ff
phycal_tempdelta=15
temps_period=15
temps_hysteresis=15

#------------- TSSI Related -------------
tssipos2g=1
tssipos5g=1

AvVmid_c0=2,131,5,52,6,39,6,39,6,39
AvVmid_c1=2,130,6,39,6,35,6,35,6,37

slice/1/AvVmid_c0=6,70,1,159,1,166,1,153,1,153
slice/1/AvVmid_c1=6,65,1,155,1,158,1,147,1,151
# CCK in case of multi mode 5
pa2gccka0=0xff56,0x1c3c,0xfca5
pa2gccka1=0xff5b,0x1ce9,0xfc97
# OFDM in case of multi_mode 5
pa2ga0=0xffed,0x1ca7,0xfd48
pa2ga1=0xffea,0x1d9b,0xfd23

pa5ga0=0xff44,0x1883,0xfd35,0xff44,0x1877,0xfd32,0xff41,0x1831,0xfd35,0xff35,0x1784,0xfd3a
pa5ga1=0xff42,0x176c,0xfd4d,0xff3f,0x170a,0xfd57,0xff42,0x1730,0xfd55,0xff3c,0x16fe,0xfd50

# Max power and offsets
maxp2ga0=84
maxp2ga1=84
maxp5ga0=74,74,74,74
maxp5ga1=74,74,74,74
subband5gver=0x4
paparambwver=3
cckpwroffset0=0
cckpwroffset1=0
pdoffset40ma0=0x0000
pdoffset80ma0=0x0000
pdoffset40ma1=0x0000
pdoffset80ma1=0x0000
pdoffset20mRU_c0=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset20mRU_c1=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset40mRU_c0=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset40mRU_c1=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset80mRUset1_c0=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset80mRUset2_c0=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset80mRUset1_c1=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
pdoffset80mRUset2_c1=0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
cckbw202gpo=0
cckbw20ul2gpo=0
mcsbw202gpo=0xDA886664
mcsbw402gpo=0xDA886664
dot11agofdmhrbw202gpo=0x6666
ofdmlrbw202gpo=0x0022
mcsbw205glpo=0x66644440
mcsbw405glpo=0x88866662
mcsbw805glpo=0xAAA88884
mcsbw1605glpo=0
mcsbw205gmpo=0x66644440
mcsbw405gmpo=0x88866662
mcsbw805gmpo=0xAAA88884
mcsbw1605gmpo=0
mcsbw205ghpo=0x66644440
mcsbw405ghpo=0x88866662
mcsbw805ghpo=0xAAA88884

slice/1/powoffs2gtna0=0,0,0,0,0,0,0,0,0,0,0,0,0,0
slice/1/powoffs2gtna1=0,0,0,0,0,0,0,0,0,0,0,0,0,0
#slice/1/pdoffsetcckma0=1
#slice/1/pdoffsetcckma1=1
mcs1024qam2gpo=0xCCCC
mcs1024qam5glpo=0xCCAA88
mcs1024qam5gmpo=0xCCAA88
mcs1024qam5ghpo=0xCCAA88
mcs1024qam5gx1po=0xCCAA88
mcs1024qam5gx2po=0xCCAA88
mcs8poexp=0
mcs9poexp=0
mcs10poexp=0

# 5G power offset per channel for band edge channel
powoffs5g20mtna0=0,0,0,0,0,0,0
powoffs5g20mtna1=0,0,0,0,0,0,0
powoffs5g40mtna0=0,0,0,0,0
powoffs5g40mtna1=0,0,0,0,0
powoffs5g80mtna0=0,0,0,0,0
powoffs5g80mtna1=0,0,0,0,0
mcs11poexp=0

# OLPC Related
disable_olpc=0
olpc_thresh5g=44
olpc_anchor5g=48
slice/1/disable_olpc=0
slice/1/olpc_thresh2g=44
slice/1/olpc_anchor2g=48

#LTE Coex Related
#ltecxmux=0
#ltecxpadnum=0x0504
#ltecxfnsel=0x44
#ltecxgcigpio=0x04
#OOB params
#device_wake_opt=1
host_wake_opt=0

# SWCTRL Related
swctrlmap_5g=0xe0e0c0c0,0xa0a00000,0x80800000,0x000000,0x3FF
swctrlmapext_5g=0x00000000,0x00000000,0x00000000,0x000000,0x000
fem_table_init_val=0x00000000,0x80800000
fem_table_init_val_ext=0x00000000,0x00000000

slice/1/swctrlmap_2g=0x00000000,0x03030000,0x01010000,0x000000,0x3FF
slice/1/swctrlmapext_2g=0x00000000,0x00000000,0x00000000,0x000000,0x003

slice/1/fem_table_init_val=0x01010000,0x00000000
slice/1/fem_table_init_val_ext=0x00000000,0x00000000

#clb2gslice0core0=0x000
clb2gslice1core0=0x003
clb5gslice0core0=0x0E0
#clb5gslice1core0=0x070
#clb2gslice0core1=0x000
clb2gslice1core1=0x003
clb5gslice0core1=0x0E0
#clb5gslice1core1=0x038
btc_prisel_ant_mask=0x2
clb_swctrl_smask_ant0=0x3ff
clb_swctrl_smask_ant1=0x3ff
muxenab=1

#BT Coex 1:TDM
btc_mode=1

# --- PAPD Cal related params ----
txwbpapden=0 # 0:NBPAPD 1:WBPAPD
# NB PAPD Cal params
slice/1/nb_eps_offset=485,487
slice/1/nb_bbmult=35,39
slice/1/nb_papdcalidx=11,11
slice/1/nb_txattn=3,3
slice/1/nb_rxattn=0,0
slice/1/nb_eps_stopidx=63
slice/1/papdgainctrl2g=1
slice/1/pacalshift2g=2,1
slice/1/ampbased_gc=0

# energy detect threshold
ed_thresh2g=-63
ed_thresh5g=-63
# energy detect threshold for EU
eu_edthresh2g=-63
eu_edthresh5g=-63

btldopu=1

#Enable LHL PS mode
lhl_ps_mode=3
# to enable he features
he_en=1

# FE Loss comp parameters
slice/1/felossTx2ga0=0,0,0,0,0,0,0,0,0,0,0,0,0,0
slice/1/felossTx2ga1=0,0,0,0,0,0,0,0,0,0,0,0,0,0
slice/1/felossRx2ga0=0,0,0,0,0,0,0,0,0,0,0,0,0,0
slice/1/felossRx2ga1=0,0,0,0,0,0,0,0,0,0,0,0,0,0
felossTx5ga0=0,0,0,0
felossTx5ga1=0,0,0,0
felossRx5ga0=0,0,0,0
felossRx5ga1=0,0,0,0

## ULOFDMA Board limit PPRs for 2G20 ##
ruppr2g20bpska0=0xf62d6
ruppr2g20bpska1=0xf62d6
ruppr2g20qpska0=0xf6b18
ruppr2g20qpska1=0xf6b18
ruppr2g20qam16a0=0xf6b5a
ruppr2g20qam16a1=0xf6b5a
ruppr2g20qam64a0=0x203de
ruppr2g20qam64a1=0x203de
ruppr2g20qam256a0=0x30800
ruppr2g20qam256a1=0x30800
ruppr2g20qam1024a0=0x0
ruppr2g20qam1024a1=0x0
## ULOFDMA Board limit PPRs for 5G20 ##
ruppr5g20bpska0=0xd6316
ruppr5g20bpska1=0xd6316
ruppr5g20qpska0=0xe6316
ruppr5g20qpska1=0xe6316
ruppr5g20qam16a0=0xd6b5a
ruppr5g20qam16a1=0xd6b5a
ruppr5g20qam64a0=0x0
ruppr5g20qam64a1=0x0
ruppr5g20qam256a0=0x10842
ruppr5g20qam256a1=0x10842
ruppr5g20qam1024a0=0x30000
ruppr5g20qam1024a1=0x30000
## ULOFDMA Board limit PPRs for 5G40 ##
ruppr5g40bpska0=0x1cc6316
ruppr5g40bpska1=0x1cc6316
ruppr5g40qpska0=0x1cd6316
ruppr5g40qpska1=0x1cd6316
ruppr5g40qam16a0=0x1cd735a
ruppr5g40qam16a1=0x1cd735a
ruppr5g40qam64a0=0x0
ruppr5g40qam64a1=0x0
ruppr5g40qam256a0=0x210842
ruppr5g40qam256a1=0x210842
ruppr5g40qam1024a0=0x630000
ruppr5g40qam1024a1=0x630000
## ULOFDMA Board limit PPRs for 5G80 ##
ruppr5g80bpska0=0x7bdc
ruppr5g80bpska1=0x7bdc
ruppr5g80qpska0=0x7bdc
ruppr5g80qpska1=0x7bdc
ruppr5g80qam16a0=0x3dc
ruppr5g80qam16a1=0x3dc
ruppr5g80qam64a0=0x0
ruppr5g80qam64a1=0x0
ruppr5g80qam256a0=0x213842
ruppr5g80qam256a1=0x213842
ruppr5g80qam1024a0=0x420000
ruppr5g80qam1024a1=0x420000

### SAR HEAD params
### MIMO Mode Parameters
## 2g normal:16dB airplane:15dB
#slice/1/dynsar_2g=0xc0c0
#slice/1/dynsar_2g_2=0xbcbc
## 5g normal:14dB airplane:13dB
#dynsar_5g=0xb8b8
#dynsar_5g_2=0xb4b4
### RSDB mode Parameters(Both core are active)
## 2g normal:15dB airplane:14dB
#slice/1/rsdb_dynsar_2g=0xbcbc
#slice/1/rsdb_dynsar_2g_2=0xb8b8
## 5g normal:13dB airplane:12dB
#rsdb_dynsar_5g=0xb4b4
#rsdb_dynsar_5g_2=0xb0b0
### Disable Parameters 2G:31.75dB 5G:31.75dB
#slice/1/rsdb_dynsar_2g_1=0xffff
#rsdb_dynsar_5g_1=0xffff
#
### SAR GRIP params
### MIMO Mode Parameters
## 2g normal:16dB airplane:15dB
#slice/1/grip_dynsar_2g=0xc0c0
#slice/1/grip_dynsar_2g_2=0xbcbc
## 5g normal:14dB airplane:13dB
#grip_dynsar_5g=0xb8b8
#grip_dynsar_5g_2=0xb4b4
### RSDB mode Parameters(Both core are active)
## 2g normal:15dB airplane:14dB
#slice/1/grip_rsdb_dynsar_2g=0xbcbc
#slice/1/grip_rsdb_dynsar_2g_2=0xb8b8
## 5g normal:13dB airplane:12dB
#grip_rsdb_dynsar_5g=0xb4b4
#grip_rsdb_dynsar_5g_2=0xb0b0
#
### FCC Mode: 10dB
#slice/1/fccpwrch12=0x28
#slice/1/fccpwrch13=0x28
#
#
### RU SAR HEAD params
### MIMO Mode Parameters
## 2g normal:14,6,0.25dB airplane:18,10,2dB
#slice/1/dynsar_2g_ru=0xb8b8,0x9898,0x8181
#slice/1/dynsar_2g_2_ru=0xc8c8,0xa8a8,0x8888
## 5g normal:14,6,0.25dB airplane:18,10,2dB
#dynsar_5g_ru=0xb8b8,0x9898,0x8181
#dynsar_5g_2_ru=0xc8c8,0xa8a8,0x8888
### RSDB mode Parameters(Both core are active)
## 2g normal:14,6,0.25dB airplane:18,10,2dB
#slice/1/rsdb_dynsar_2g_ru=0xb8b8,0x9898,0x8181
#slice/1/rsdb_dynsar_2g_2_ru=0xc8c8,0xa8a8,0x8888
## 5g normal:14,6,0.25dB airplane:18,10,2dB
#rsdb_dynsar_5g_ru=0xb8b8,0x9898,0x8181
#rsdb_dynsar_5g_2_ru=0xc8c8,0xa8a8,0x8888
#
### RU SAR GRIP params
### MIMO Mode Parameters
## 2g normal:16,8,1dB airplane:20,12,4dB
#slice/1/grip_dynsar_2g_ru=0xc0c0,0xa0a0,0x8484
#slice/1/grip_dynsar_2g_2_ru=0xd0d0,0xb0b0,0x9090
## 5g normal:16,8,1dB airplane:20,12,4dB
#grip_dynsar_5g_ru=0xc0c0,0xa0a0,0x8484
#grip_dynsar_5g_2_ru=0xd0d0,0xb0b0,0x9090
### RSDB mode Parameters(Both core are active)
## 2g normal:16,8,1dB airplane:20,12,4dB
#slice/1/grip_rsdb_dynsar_2g_ru=0xc0c0,0xa0a0,0x8484
#slice/1/grip_rsdb_dynsar_2g_2_ru=0xd0d0,0xb0b0,0x9090
## 5g normal:16,8,1dB airplane:20,12,4dB
#grip_rsdb_dynsar_5g_ru=0xc0c0,0xa0a0,0x8484
#grip_rsdb_dynsar_5g_2_ru=0xd0d0,0xb0b0,0x9090

