/*
 * Copyright 2018 The Android Open Source Project
 *
 * Licensed under the Apache License, Version 2.0 (the "License");
 * you may not use this file except in compliance with the License.
 * You may obtain a copy of the License at
 *
 *      http://www.apache.org/licenses/LICENSE-2.0
 *
 * Unless required by applicable law or agreed to in writing, software
 * distributed under the License is distributed on an "AS IS" BASIS,
 * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
 * See the License for the specific language governing permissions and
 * limitations under the License.
 */

package android.hardware.wifi.supplicant@1.2;

import @1.1::ISupplicantStaIfaceCallback;
import @1.0::Ssid;

/**
 * Callback Interface exposed by the supplicant service
 * for each station mode interface (ISupplicantStaIface).
 *
 * Clients need to host an instance of this HIDL interface object and
 * pass a reference of the object to the supplicant via the
 * corresponding |ISupplicantStaIface.registerCallback_1_2| method.
 */
interface ISupplicantStaIfaceCallback extends @1.1::ISupplicantStaIfaceCallback {
    /**
     * Indicates DPP configuration received success event (Enrolee mode).
     */
    oneway onDppSuccessConfigReceived(Ssid ssid, string password, uint8_t[32] psk,
        DppAkm securityAkm);

    /**
     * Indicates DPP configuration sent success event (Configurator mode).
     */
    oneway onDppSuccessConfigSent();

    /**
     * Indicates a DPP progress event.
     */
    oneway onDppProgress(DppProgressCode code);

    /**
     * Indicates a DPP failure event.
     */
    oneway onDppFailure(DppFailureCode code);
};
