/*
 * Copyright (C) 2020 The Android Open Source Project
 *
 * Licensed under the Apache License, Version 2.0 (the "License");
 * you may not use this file except in compliance with the License.
 * You may obtain a copy of the License at
 *
 *      http://www.apache.org/licenses/LICENSE-2.0
 *
 * Unless required by applicable law or agreed to in writing, software
 * distributed under the License is distributed on an "AS IS" BASIS,
 * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
 * See the License for the specific language governing permissions and
 * limitations under the License.
 */

package android.hardware.gnss;

import android.hardware.gnss.ElapsedRealtime;
import android.hardware.gnss.GnssClock;
import android.hardware.gnss.GnssMeasurement;

/**
 * Represents a reading of GNSS measurements. For devices launched in Android Q or newer, it is
 * mandatory that these be provided, on request, when the GNSS receiver is searching/tracking
 * signals.
 *
 * - Reporting of GNSS constellation measurements is mandatory.
 * - Reporting of all tracked constellations are encouraged.
 */
@VintfStability
parcelable GnssData {
    /** The array of measurements. */
    GnssMeasurement[] measurements;

    /** The GNSS clock time reading. */
    GnssClock clock;

    /**
     * Timing information of the GNSS data synchronized with SystemClock.elapsedRealtimeNanos()
     * clock.
     */
    ElapsedRealtime elapsedRealtime;
}