/*
 * Copyright (C) 2021 The Android Open Source Project
 *
 * Licensed under the Apache License, Version 2.0 (the "License");
 * you may not use this file except in compliance with the License.
 * You may obtain a copy of the License at
 *
 *      http://www.apache.org/licenses/LICENSE-2.0
 *
 * Unless required by applicable law or agreed to in writing, software
 * distributed under the License is distributed on an "AS IS" BASIS,
 * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
 * See the License for the specific language governing permissions and
 * limitations under the License.
 */

package android.hardware.radio.data;

import android.hardware.radio.data.QosBandwidth;

/**
 * LTE/EPS Quality of Service parameters as per 3gpp spec 24.301 sec 9.9.4.3.
 */
@VintfStability
parcelable EpsQos {
    /**
     * Quality of Service Class Identifier (QCI), see 3GPP TS 23.203 and 29.212.
     * The allowed values are standard values(1-9, 65-68, 69-70, 75, 79-80, 82-85)
     * defined in the spec and operator specific values in the range 128-254.
     */
    int qci;
    QosBandwidth downlink;
    QosBandwidth uplink;
}
