/*
 * Copyright (C) 2016 The Android Open Source Project
 *
 * Licensed under the Apache License, Version 2.0 (the "License");
 * you may not use this file except in compliance with the License.
 * You may obtain a copy of the License at
 *
 *      http://www.apache.org/licenses/LICENSE-2.0
 *
 * Unless required by applicable law or agreed to in writing, software
 * distributed under the License is distributed on an "AS IS" BASIS,
 * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
 * See the License for the specific language governing permissions and
 * limitations under the License.
 */

package android.hardware.radio@1.0;

/**
 * Interface declaring response functions to solicited radio requests.
 * Response functions defined in this interface are as per following convention:
 * <xyz>Response is response to IRadio.<xyz>
 */
interface IRadioResponse {
    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param cardStatus ICC card status as defined by CardStatus in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway getIccCardStatusResponse(RadioResponseInfo info, CardStatus cardStatus);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param remainingRetries Number of retries remaining, must be equal to -1 if unknown.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:PASSWORD_INCORRECT
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway supplyIccPinForAppResponse(RadioResponseInfo info, int32_t remainingRetries);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param remainingRetries Number of retries remaining, must be equal to -1 if unknown.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:PASSWORD_INCORRECT (PUK is invalid)
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway supplyIccPukForAppResponse(RadioResponseInfo info, int32_t remainingRetries);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param remainingRetries Number of retries remaining, must be equal to -1 if unknown.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:PASSWORD_INCORRECT
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_PUK2
     */
    oneway supplyIccPin2ForAppResponse(RadioResponseInfo info, int32_t remainingRetries);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param remainingRetries Number of retries remaining, must be equal to -1 if unknown.
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:PASSWORD_INCORRECT (PUK is invalid)
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway supplyIccPuk2ForAppResponse(RadioResponseInfo info, int32_t remainingRetries);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param remainingRetries Number of retries remaining, must be equal to -1 if unknown.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:PASSWORD_INCORRECT
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway changeIccPinForAppResponse(RadioResponseInfo info, int32_t remainingRetries);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param remainingRetries Number of retries remaining, must be equal to -1 if unknown.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:PASSWORD_INCORRECT (old PIN2 is invalid)
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_PUK2
     */
    oneway changeIccPin2ForAppResponse(RadioResponseInfo info, int32_t remainingRetries);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param remainingRetries Number of retries remaining, must be equal to -1 if unknown.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:PASSWORD_INCORRECT (code is invalid)
     *   RadioError:NO_MEMORY
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway supplyNetworkDepersonalizationResponse(RadioResponseInfo info, int32_t remainingRetries);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param calls Current call list
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getCurrentCallsResponse(RadioResponseInfo info, vec<Call> calls);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:DIAL_MODIFIED_TO_USSD
     *   RadioError:DIAL_MODIFIED_TO_SS
     *   RadioError:DIAL_MODIFIED_TO_DIAL
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:INVALID_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:INTERNAL_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:MODEM_ERR
     *   RadioError:NO_SUBSCRIPTION
     *   RadioError:NO_NETWORK_FOUND
     *   RadioError:INVALID_CALL_ID
     *   RadioError:DEVICE_IN_USE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:ABORTED
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:CANCELLED
     */
    oneway dialResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param imsi String containing the IMSI
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:SIM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway getIMSIForAppResponse(RadioResponseInfo info, string imsi);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:INVALID_STATE
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway hangupConnectionResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:NO_RESOURCES
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:CANCELLED
     */
    oneway hangupWaitingOrBackgroundResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:NO_RESOURCES
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway hangupForegroundResumeBackgroundResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_STATE
     *   RadioError:INVALID_CALL_ID
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway switchWaitingOrHoldingAndActiveResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_STATE
     *   RadioError:INVALID_CALL_ID
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway conferenceResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE (radio resetting)
     *   RadioError:INVALID_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway rejectCallResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param failCauseInfo Contains LastCallFailCause and vendor cause code.
     *
     *   The vendor cause code must be used for debugging purpose only.
     *   The implementation must return one of the values of LastCallFailCause
     *   as mentioned below
     *
     *   GSM failure reasons codes for the cause codes defined in TS 24.008 Annex H
     *   where possible.
     *   CDMA failure reasons codes for the possible call failure scenarios
     *   described in the "CDMA IS-2000 Release A (C.S0005-A v6.0)" standard.
     *   Any of the following reason codes if the call is failed or dropped due to reason
     *   mentioned with in the braces.
     *      LastCallFailCause:RADIO_OFF (Radio is OFF)
     *      LastCallFailCause:OUT_OF_SERVICE (No cell coverage)
     *      LastCallFailCause:NO_VALID_SIM (No valid SIM)
     *      LastCallFailCause:RADIO_INTERNAL_ERROR (Modem hit unexpected error scenario)
     *      LastCallFailCause:NETWORK_RESP_TIMEOUT (No response from network)
     *      LastCallFailCause:NETWORK_REJECT (Explicit network reject)
     *      LastCallFailCause:RADIO_ACCESS_FAILURE (RRC connection failure. Eg.RACH)
     *      LastCallFailCause:RADIO_LINK_FAILURE (Radio Link Failure)
     *      LastCallFailCause:RADIO_LINK_LOST (Radio link lost due to poor coverage)
     *      LastCallFailCause:RADIO_UPLINK_FAILURE (Radio uplink failure)
     *      LastCallFailCause:RADIO_SETUP_FAILURE (RRC connection setup failure)
     *      LastCallFailCause:RADIO_RELEASE_NORMAL (RRC connection release, normal)
     *      LastCallFailCause:RADIO_RELEASE_ABNORMAL (RRC connection release, abnormal)
     *      LastCallFailCause:ACCESS_CLASS_BLOCKED (Access class barring)
     *      LastCallFailCause:NETWORK_DETACH (Explicit network detach)
     *   OEM causes (LastCallFailCause:OEM_CAUSE_XX) must be used for debug purpose only
     *
     * If the implementation does not have access to the exact cause codes,
     * then it must return one of the values listed in LastCallFailCause,
     * as the UI layer needs to distinguish these cases for tone generation or
     * error notification.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:NO_MEMORY
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INTERNAL_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getLastCallFailCauseResponse(RadioResponseInfo info,
            LastCallFailCauseInfo failCauseinfo);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param sigStrength Current signal strength
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NOT_PROVISIONED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getSignalStrengthResponse(RadioResponseInfo info, SignalStrength sigStrength);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param voiceRegResponse Current Voice registration response as defined by VoiceRegStateResult
     *        in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway getVoiceRegistrationStateResponse(RadioResponseInfo info,
            VoiceRegStateResult voiceRegResponse);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param dataRegResponse Current Data registration response as defined by DataRegStateResult in
     *        types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NOT_PROVISIONED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getDataRegistrationStateResponse(RadioResponseInfo info,
            DataRegStateResult dataRegResponse);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param longName is long alpha ONS or EONS or empty string if unregistered
     * @param shortName is short alpha ONS or EONS or empty string if unregistered
     * @param numeric is 5 or 6 digit numeric code (MCC + MNC) or empty string if unregistered
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getOperatorResponse(RadioResponseInfo info, string longName, string shortName,
            string numeric);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:DEVICE_IN_USE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setRadioPowerResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_RESOURCES
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway sendDtmfResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param sms Response to sms sent as defined by SendSmsResult in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SMS_SEND_FAIL_RETRY
     *   RadioError:NETWORK_REJECT
     *   RadioError:INVALID_STATE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:INVALID_SMS_FORMAT
     *   RadioError:SYSTEM_ERR
     *   RadioError:ENCODING_ERR
     *   RadioError:INVALID_SMSC_ADDRESS
     *   RadioError:MODEM_ERR
     *   RadioError:NETWORK_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NETWORK_NOT_READY
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway sendSmsResponse(RadioResponseInfo info, SendSmsResult sms);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param sms Response to sms sent as defined by SendSmsResult in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SMS_SEND_FAIL_RETRY
     *   RadioError:NETWORK_REJECT
     *   RadioError:INVALID_STATE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:INVALID_SMS_FORMAT
     *   RadioError:SYSTEM_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:ENCODING_ERR
     *   RadioError:INVALID_SMSC_ADDRESS
     *   RadioError:MODEM_ERR
     *   RadioError:NETWORK_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NETWORK_NOT_READY
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway sendSMSExpectMoreResponse(RadioResponseInfo info, SendSmsResult sms);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param dcResponse SetupDataCallResult defined in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE must be returned on both success and failure of setup with the
     *              DataCallResponse.status containing the actual status
     *              For all other errors the DataCallResponse is ignored.
     *   RadioError:REQUEST_NOT_SUPPORTED may be returned when HAL 1.2 or higher is supported.
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OP_NOT_ALLOWED_BEFORE_REG_TO_NW
     *   RadioError:OP_NOT_ALLOWED_DURING_VOICE_CALL
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway setupDataCallResponse(RadioResponseInfo info, SetupDataCallResult dcResponse);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param iccIo ICC io operation response as defined by IccIoResult in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SIM_PIN2
     *   RadioError:SIM_PUK2
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:SIM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway iccIOForAppResponse(RadioResponseInfo info, IccIoResult iccIo);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:USSD_MODIFIED_TO_DIAL
     *   RadioError:USSD_MODIFIED_TO_SS
     *   RadioError:USSD_MODIFIED_TO_USSD
     *   RadioError:SIM_BUSY
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:ABORTED
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway sendUssdResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SIM_BUSY
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:INVALID_STATE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway cancelPendingUssdResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param n is "n" parameter from TS 27.007 7.7
     * @param m is "m" parameter from TS 27.007 7.7
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getClirResponse(RadioResponseInfo info, int32_t n, int32_t m);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setClirResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param callForwardInfos points to a vector of CallForwardInfo, one for
     *        each distinct registered phone number.
     *
     * For example, if data is forwarded to +18005551212 and voice is forwarded
     * to +18005559999, then two separate CallForwardInfo's must be returned
     *
     * If, however, both data and voice are forwarded to +18005551212, then
     * a single CallForwardInfo must be returned with the service class
     * set to "data + voice = 3")
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SYSTEM_ERR
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getCallForwardStatusResponse(RadioResponseInfo info,
            vec<CallForwardInfo> callForwardInfos);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_STATE
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setCallForwardResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param enable If current call waiting state is disabled, enable = false else true
     * @param serviceClass If enable, then callWaitingResp[1]
     *        must follow, with the TS 27.007 service class bit vector of services
     *        for which call waiting is enabled.
     *        For example, if callWaitingResp[0] is 1 and
     *        callWaitingResp[1] is 3, then call waiting is enabled for data
     *        and voice and disabled for everything else.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getCallWaitingResponse(RadioResponseInfo info, bool enable, int32_t serviceClass);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_STATE
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setCallWaitingResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway acknowledgeLastIncomingGsmSmsResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway acceptCallResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:REQUEST_NOT_SUPPORTED may be returned when HAL 1.2 or higher is supported.
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_CALL_ID
     *   RadioError:INVALID_STATE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway deactivateDataCallResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param response 0 is the TS 27.007 service class bit vector of
     *        services for which the specified barring facility
     *        is active. "0" means "disabled for all"
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getFacilityLockForAppResponse(RadioResponseInfo info, int32_t response);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param retry 0 is the number of retries remaining, or -1 if unknown
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_STATE
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setFacilityLockForAppResponse(RadioResponseInfo info, int32_t retry);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setBarringPasswordResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param selection false for automatic selection, true for manual selection
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getNetworkSelectionModeResponse(RadioResponseInfo info, bool manual);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:ILLEGAL_SIM_OR_ME
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *
     * Returns RadioError:ILLEGAL_SIM_OR_ME when the failure is permanent and
     * no retries needed, such as illegal SIM or ME.
     */
    oneway setNetworkSelectionModeAutomaticResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:ILLEGAL_SIM_OR_ME
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *
     * Returns RadioError:ILLEGAL_SIM_OR_ME when the failure is permanent and
     * no retries needed, such as illegal SIM or ME.
     */
    oneway setNetworkSelectionModeManualResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param networkInfos List of network operator information as OperatorInfos defined in
     *         types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:ABORTED
     *   RadioError:DEVICE_IN_USE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:CANCELLED
     *   RadioError:NO_RESOURCES
     *   RadioError:INTERNAL_ERR
     */
    oneway getAvailableNetworksResponse(RadioResponseInfo info,
            vec<OperatorInfo> networkInfos);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_RESOURCES
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway startDtmfResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_RESOURCES
     *   RadioError:NO_MEMORY
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway stopDtmfResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param version string containing version string for log reporting
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:EMPTY_RECORD
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NOT_PROVISIONED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getBasebandVersionResponse(RadioResponseInfo info, string version);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:NO_MEMORY
     *   RadioError:MODEM_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:CANCELLED
     */
    oneway separateConnectionResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setMuteResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param enable true for "mute enabled" and false for "mute disabled"
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SS_MODIFIED_TO_DIAL
     *   RadioError:SS_MODIFIED_TO_USSD
     *   RadioError:SS_MODIFIED_TO_SS
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getMuteResponse(RadioResponseInfo info, bool enable);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param status indicates CLIP status
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getClipResponse(RadioResponseInfo info, ClipStatus status);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param dcResponse List of DataCallResult as defined in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway getDataCallListResponse(RadioResponseInfo info, vec<SetupDataCallResult> dcResponse);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SIM_BUSY
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway setSuppServiceNotificationsResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param index record index where the message is stored
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SIM_FULL
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SMS_FORMAT
     *   RadioError:INTERNAL_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:ENCODING_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_SMSC_ADDRESS
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:SIM_ABSENT
     */
    oneway writeSmsToSimResponse(RadioResponseInfo info, int32_t index);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SIM_FULL
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NO_SUCH_ENTRY
     *   RadioError:INTERNAL_ERR
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:SIM_ABSENT
     */
    oneway deleteSmsOnSimResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setBandModeResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param bandModes List of RadioBandMode listing supported modes
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getAvailableBandModesResponse(RadioResponseInfo info, vec<RadioBandMode> bandModes);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param commandResponse SAT/USAT response in hexadecimal format
     *        string starting with first byte of response
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SIM_BUSY
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway sendEnvelopeResponse(RadioResponseInfo info, string commandResponse);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway sendTerminalResponseToSimResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway handleStkCallSetupRequestFromSimResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway explicitCallTransferResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:MODE_NOT_SUPPORTED
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setPreferredNetworkTypeResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param nwType RadioPreferredNetworkType defined in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getPreferredNetworkTypeResponse(RadioResponseInfo info,
            PreferredNetworkType nwType);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param cells Vector of neighboring radio cell
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NO_NETWORK_FOUND
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getNeighboringCidsResponse(RadioResponseInfo info, vec<NeighboringCell> cells);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway setLocationUpdatesResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SIM_ABSENT
     *   RadioError:SUBSCRIPTION_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway setCdmaSubscriptionSourceResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway setCdmaRoamingPreferenceResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param type CdmaRoamingType defined in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway getCdmaRoamingPreferenceResponse(RadioResponseInfo info, CdmaRoamingType type);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setTTYModeResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param mode TtyMode
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getTTYModeResponse(RadioResponseInfo info, TtyMode mode);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_CALL_ID
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setPreferredVoicePrivacyResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param enable false for Standard Privacy Mode (Public Long Code Mask)
     *        true for Enhanced Privacy Mode (Private Long Code Mask)
     *
     * Valid errors:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getPreferredVoicePrivacyResponse(RadioResponseInfo info, bool enable);

    /**
     * Response callback for IRadio.sendCDMAFeatureCode()
     *
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:INVALID_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:OPERATION_NOT_ALLOWED
     */
    oneway sendCDMAFeatureCodeResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_CALL_ID
     *   RadioError:INVALID_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:OPERATION_NOT_ALLOWED
     */
    oneway sendBurstDtmfResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param sms Sms result struct as defined by SendSmsResult in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:SMS_SEND_FAIL_RETRY
     *   RadioError:NETWORK_REJECT
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:INVALID_SMS_FORMAT
     *   RadioError:SYSTEM_ERR
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:MODEM_ERR
     *   RadioError:NETWORK_ERR
     *   RadioError:ENCODING_ERR
     *   RadioError:INVALID_SMSC_ADDRESS
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:ENCODING_ERR
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway sendCdmaSmsResponse(RadioResponseInfo info, SendSmsResult sms);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_SMS_TO_ACK
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NETWORK_NOT_READY
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway acknowledgeLastIncomingCdmaSmsResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param configs Vector of GSM/WCDMA Cell broadcast configs
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NO_RESOURCES
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway getGsmBroadcastConfigResponse(RadioResponseInfo info,
            vec<GsmBroadcastSmsConfigInfo> configs);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway setGsmBroadcastConfigResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway setGsmBroadcastActivationResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param configs Vector of CDMA Broadcast SMS configs.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NO_RESOURCES
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway getCdmaBroadcastConfigResponse(RadioResponseInfo info,
            vec<CdmaBroadcastSmsConfigInfo> configs);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway setCdmaBroadcastConfigResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     */
    oneway setCdmaBroadcastActivationResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param mdn MDN if CDMA subscription is available
     * @param hSid is a comma separated list of H_SID (Home SID) if
     *        CDMA subscription is available, in decimal format
     * @param hNid is a comma separated list of H_NID (Home NID) if
     *        CDMA subscription is available, in decimal format
     * @param min MIN (10 digits, MIN2+MIN1) if CDMA subscription is available
     * @param prl PRL version if CDMA subscription is available
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SUBSCRIPTION_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:NOT_PROVISIONED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway getCDMASubscriptionResponse(RadioResponseInfo info, string mdn, string hSid,
            string hNid, string min, string prl);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param index record index where the cmda sms message is stored
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SMS_FORMAT
     *   RadioError:SIM_FULL
     *   RadioError:INTERNAL_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:ENCODING_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:INVALID_SMSC_ADDRESS
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:SIM_ABSENT
     */
    oneway writeSmsToRuimResponse(RadioResponseInfo info, uint32_t index);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NO_SUCH_ENTRY
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:SIM_ABSENT
     */
    oneway deleteSmsOnRuimResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param imei IMEI if GSM subscription is available
     * @param imeisv IMEISV if GSM subscription is available
     * @param esn ESN if CDMA subscription is available
     * @param meid MEID if CDMA subscription is available
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:NOT_PROVISIONED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *
     * If a empty string value is returned for any of the device id, it means that there was error
     * accessing the device.
     *
     */
    oneway getDeviceIdentityResponse(RadioResponseInfo info, string imei, string imeisv,
            string esn, string meid);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OPERATION_NO_ALLOWED
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway exitEmergencyCallbackModeResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param smsc Short Message Service Center address on the device
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NOT_PROVISIONED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway getSmscAddressResponse(RadioResponseInfo info, string smsc);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_SMS_FORMAT
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:MODEM_ERR
     *   RadioError:NO_RESOURCES
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway setSmscAddressResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_MEMORY
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_STATE
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway reportSmsMemoryStatusResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway reportStkServiceIsRunningResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param source CDMA subscription source
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SUBSCRIPTION_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway getCdmaSubscriptionSourceResponse(RadioResponseInfo info, CdmaSubscriptionSource source);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param response response string of the challenge/response algo for ISIM auth in base64 format
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway requestIsimAuthenticationResponse(RadioResponseInfo info, string response);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway acknowledgeIncomingGsmSmsWithPduResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param iccIo IccIoResult as defined in types.hal corresponding to ICC IO response
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SIM_BUSY
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway sendEnvelopeWithStatusResponse(RadioResponseInfo info, IccIoResult iccIo);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param rat Current voice RAT
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway getVoiceRadioTechnologyResponse(RadioResponseInfo info, RadioTechnology rat);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param cellInfo List of current cell information known to radio
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NO_NETWORK_FOUND
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getCellInfoListResponse(RadioResponseInfo info, vec<CellInfo> cellInfo);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway setCellInfoListRateResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SUBSCRIPTION_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:NOT_PROVISIONED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setInitialAttachApnResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param isRegistered false = not registered, true = registered
     * @param ratFamily RadioTechnologyFamily as defined in types.hal. This value is valid only if
     *        isRegistered is true.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway getImsRegistrationStateResponse(RadioResponseInfo info, bool isRegistered,
            RadioTechnologyFamily ratFamily);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param sms Response to sms sent as defined by SendSmsResult in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SMS_SEND_FAIL_RETRY
     *   RadioError:FDN_CHECK_FAILURE
     *   RadioError:NETWORK_REJECT
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INVALID_STATE
     *   RadioError:NO_MEMORY
     *   RadioError:INVALID_SMS_FORMAT
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_RATE_LIMITED
     *   RadioError:MODEM_ERR
     *   RadioError:NETWORK_ERR
     *   RadioError:ENCODING_ERR
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INTERNAL_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NETWORK_NOT_READY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway sendImsSmsResponse(RadioResponseInfo info, SendSmsResult sms);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param result IccIoResult as defined in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway iccTransmitApduBasicChannelResponse(RadioResponseInfo info, IccIoResult result);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param channelId session id of the logical channel.
     * @param selectResponse Contains the select response for the open channel command with one
     *        byte per integer
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:MISSING_RESOURCE
     *   RadioError:NO_SUCH_ELEMENT
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ERR
     *   RadioError:INVALID_SIM_STATE
     *   RadioError:MISSING_RESOURCE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway iccOpenLogicalChannelResponse(RadioResponseInfo info, int32_t channelId,
            vec<int8_t> selectResponse);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway iccCloseLogicalChannelResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param result IccIoResult as defined in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway iccTransmitApduLogicalChannelResponse(RadioResponseInfo info, IccIoResult result);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param result string containing the contents of the NV item
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway nvReadItemResponse(RadioResponseInfo info, string result);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway nvWriteItemResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway nvWriteCdmaPrlResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway nvResetConfigResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SUBSCRIPTION_NOT_SUPPORTED
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setUiccSubscriptionResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:DEVICE_IN_USE
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway setDataAllowedResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param config Array of HardwareConfig of the radio.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway getHardwareConfigResponse(RadioResponseInfo info, vec<HardwareConfig> config);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param result IccIoResult as defined in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:INVALID_MODEM_STATE
     *   RadioError:SIM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway requestIccSimAuthenticationResponse(RadioResponseInfo info, IccIoResult result);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:SUBSCRIPTION_NOT_AVAILABLE
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:SIM_ABSENT
     */
    oneway setDataProfileResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway requestShutdownResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param rc Radio capability as defined by RadioCapability in types.hal
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:INVALID_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway getRadioCapabilityResponse(RadioResponseInfo info, RadioCapability rc);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param rc Radio capability as defined by RadioCapability in types.hal used to
     *        feedback return status
     *
     * Valid errors returned:
     *   RadioError:NONE means a unsol radioCapability() will be sent within 30 seconds.
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:OPERATION_NOT_ALLOWED
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:MODEM_ERR
     *   RadioError:INVALID_STATE
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setRadioCapabilityResponse(RadioResponseInfo info, RadioCapability rc);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param statusInfo LceStatusInfo indicating LCE status
     *
     * Valid errors returned:
     *   RadioError:REQUEST_NOT_SUPPORTED may be returned when HAL 1.2 or higher is supported.
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:LCE_NOT_SUPPORTED
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway startLceServiceResponse(RadioResponseInfo info, LceStatusInfo statusInfo);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param statusInfo LceStatusInfo indicating LCE status
     *
     * Valid errors returned:
     *   RadioError:REQUEST_NOT_SUPPORTED may be returned when HAL 1.2 or higher is supported.
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:LCE_NOT_SUPPORTED
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway stopLceServiceResponse(RadioResponseInfo info, LceStatusInfo statusInfo);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param lceInfo LceDataInfo indicating LCE data as defined in types.hal
     *
     * Valid errors returned:
     *   RadioError:REQUEST_NOT_SUPPORTED may be returned when HAL 1.2 or higher is supported.
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:LCE_NOT_SUPPORTED
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:SIM_ABSENT
     */
    oneway pullLceDataResponse(RadioResponseInfo info, LceDataInfo lceInfo);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param activityInfo modem activity information
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:MODEM_ERR
     *   RadioError:NOT_PROVISIONED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway getModemActivityInfoResponse(RadioResponseInfo info, ActivityStatsInfo activityInfo);

    /**
     * @param info Response info struct containing response type, serial no. and error
     * @param numAllowed number of allowed carriers which have been set correctly.
     *        On success, it must match the length of list Carriers->allowedCarriers.
     *        if Length of allowed carriers list is 0, numAllowed = 0.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway setAllowedCarriersResponse(RadioResponseInfo info, int32_t numAllowed);

    /**
     * Expected modem behavior:
     *  Return list of allowed carriers, and if all carriers are allowed.
     *
     * @param info Response info struct containing response type, serial no. and error
     * @param allAllowed true only when all carriers are allowed. Ignore "carriers" struct.
     *        If false, consider "carriers" struct
     * @param carriers Carrier restriction information.
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:REQUEST_NOT_SUPPORTED
     */
    oneway getAllowedCarriersResponse(RadioResponseInfo info, bool allAllowed,
            CarrierRestrictions carriers);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:REQUEST_NOT_SUPPORTED
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway sendDeviceStateResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:REQUEST_NOT_SUPPORTED may be returned when HAL 1.2 or higher is supported.
     *   RadioError:NONE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:NO_MEMORY
     *   RadioError:INTERNAL_ERR
     *   RadioError:SYSTEM_ERR
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setIndicationFilterResponse(RadioResponseInfo info);

    /**
     * @param info Response info struct containing response type, serial no. and error
     *
     * Valid errors returned:
     *   RadioError:REQUEST_NOT_SUPPORTED may be returned when HAL 1.1 or higher is supported.
     *   RadioError:NONE
     *   RadioError:RADIO_NOT_AVAILABLE
     *   RadioError:INVALID_ARGUMENTS
     *   RadioError:INTERNAL_ERR
     *   RadioError:NO_MEMORY
     *   RadioError:NO_RESOURCES
     *   RadioError:CANCELLED
     */
    oneway setSimCardPowerResponse(RadioResponseInfo info);

    /**
     * Acknowledge the receipt of radio request sent to the vendor. This must be sent only for
     * radio request which take long time to respond.
     * For more details, refer https://source.android.com/devices/tech/connect/ril.html
     *
     * @param serial Serial no. of the request whose acknowledgement is sent.
     */
    oneway acknowledgeRequest(int32_t serial);
};
