
#define MHZ_TO_KBPS(mhz, w) ((mhz * 1000000 * w) / (1024))

&soc {
	msm_gpu: qcom,kgsl-3d0@3d00000 {
		compatible = "qcom,adreno-gpu-gen7-6-0", "qcom,kgsl-3d0";
		status = "ok";
		reg = <0x3d00000 0x40000>, <0x3d61000 0x800>,
			<0x03d50000 0x10000>, <0x03d9e000 0x1000>,
			<0x10900000 0x80000>;
		reg-names = "kgsl_3d0_reg_memory", "cx_dbgc", "rscc",
			"cx_misc", "qdss_gfx";
		interrupts = <0 300 IRQ_TYPE_LEVEL_HIGH>, <0 286 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "kgsl_3d0_irq", "freq_limiter_irq";

		resets = <&gpucc GPUCC_GPU_CC_FREQUENCY_LIMITER_IRQ_CLEAR>;
		reset-names = "freq_limiter_irq_clear";

		/*
		 * HLOS1_VOTE_GPU_SMMU_CLK enables GPU_CC_MEMNOC_GFX_CLK and
		 * GCC_GPU_MEMNOC_GFX_CLK.
		 */
		clocks = <&gpucc GPU_CC_HLOS1_VOTE_GPU_SMMU_CLK>,
			<&gpucc GPU_CC_AHB_CLK>,
			<&gpucc GPU_CC_CX_GMU_CLK>,
			<&gpucc GPU_CC_HUB_CX_INT_CLK>,
			<&gcc GCC_GPU_SNOC_DVM_GFX_CLK>,
			<&aoss_qmp>;
		clock-names = "gpu_cc_hlos1_vote_gpu_smmu",
				"gpu_cc_ahb",
				"gpu_cc_cx_gmu",
				"gpu_cc_hub_cx_int",
				"gcc_gpu_snoc_dvm_gfx",
				"apb_pclk";

		qcom,gpu-model = "Adreno740v3";

		qcom,chipid = <0x43050b00>;

		qcom,no-nap;

		qcom,min-access-length = <32>;

		qcom,ubwc-mode = <4>;

		qcom,gpu-qdss-stm = <0x161c0000 0x40000>; /* base addr, size */

		qcom,tzone-names = "gpuss-0", "gpuss-1", "gpuss-2", "gpuss-3",
				"gpuss-4", "gpuss-5", "gpuss-6", "gpuss-7";

		interconnects = <&gem_noc MASTER_GFX3D &mc_virt SLAVE_EBI1>;
		interconnect-names = "gpu_icc_path";

		qcom,bus-table-cnoc =
			<0>,   /* Off */
			<100>; /* On */

		qcom,bus-table-ddr =
			<MHZ_TO_KBPS(0, 4)>,    /* index=0  */
			<MHZ_TO_KBPS(451, 4)>,  /* index=1  */
			<MHZ_TO_KBPS(547, 4)>,  /* index=2  */
			<MHZ_TO_KBPS(681, 4)>,  /* index=3  */
			<MHZ_TO_KBPS(768, 4)>,  /* index=4  */
			<MHZ_TO_KBPS(1555, 4)>, /* index=5  */
			<MHZ_TO_KBPS(1708, 4)>, /* index=6  */
			<MHZ_TO_KBPS(2092, 4)>, /* index=7  */
			<MHZ_TO_KBPS(2736, 4)>, /* index=8  */
			<MHZ_TO_KBPS(3867, 4)>; /* index=9  */

		nvmem-cells = <&gpu_speed_bin>;
		nvmem-cell-names = "speed_bin";

		zap-shader {
			memory-region = <&gpu_microcode_mem>;
		};

		/* Power levels */
		qcom,gpu-pwrlevel-bins {
			#address-cells = <1>;
			#size-cells = <0>;

			compatible = "qcom,gpu-pwrlevel-bins";

			qcom,gpu-pwrlevels-0 {
				#address-cells = <1>;
				#size-cells = <0>;

				qcom,speed-bin = <0>;
				qcom,initial-pwrlevel = <9>;

				qcom,gpu-pwrlevel@0 {
					reg = <0>;
					qcom,gpu-freq = <690000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <9>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xa82c5ffd>;
				};

				qcom,gpu-pwrlevel@1 {
					reg = <1>;
					qcom,gpu-freq = <640000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L2>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@2 {
					reg = <2>;
					qcom,gpu-freq = <599000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L1>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@3 {
					reg = <3>;
					qcom,gpu-freq = <545000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L0>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@4 {
					reg = <4>;
					qcom,gpu-freq = <492000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@5 {
					reg = <5>;
					qcom,gpu-freq = <456000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_L2>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@6 {
					reg = <6>;
					qcom,gpu-freq = <421000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_L1>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@7 {
					reg = <7>;
					qcom,gpu-freq = <350000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS>;

					qcom,bus-freq = <7>;
					qcom,bus-min = <4>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xc0295ffd>;
				};

				qcom,gpu-pwrlevel@8 {
					reg = <8>;
					qcom,gpu-freq = <317000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_D0>;

					qcom,bus-freq = <5>;
					qcom,bus-min = <2>;
					qcom,bus-max = <5>;

					qcom,acd-level = <0xc0295ffd>;
				};

				qcom,gpu-pwrlevel@9 {
					reg = <9>;
					qcom,gpu-freq = <285000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_D1>;

					qcom,bus-freq = <1>;
					qcom,bus-min = <1>;
					qcom,bus-max = <5>;

					qcom,acd-level = <0xe02a5ffd>;
				};
			};

			qcom,gpu-pwrlevels-1 {
				#address-cells = <1>;
				#size-cells = <0>;

				qcom,speed-bin = <146>;
				qcom,initial-pwrlevel = <9>;

				qcom,gpu-pwrlevel@0 {
					reg = <0>;
					qcom,gpu-freq = <690000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <9>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xa82c5ffd>;
				};

				qcom,gpu-pwrlevel@1 {
					reg = <1>;
					qcom,gpu-freq = <640000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L2>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@2 {
					reg = <2>;
					qcom,gpu-freq = <599000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L1>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@3 {
					reg = <3>;
					qcom,gpu-freq = <545000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L0>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@4 {
					reg = <4>;
					qcom,gpu-freq = <492000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@5 {
					reg = <5>;
					qcom,gpu-freq = <456000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_L2>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@6 {
					reg = <6>;
					qcom,gpu-freq = <421000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_L1>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@7 {
					reg = <7>;
					qcom,gpu-freq = <350000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS>;

					qcom,bus-freq = <7>;
					qcom,bus-min = <4>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xc0295ffd>;
				};

				qcom,gpu-pwrlevel@8 {
					reg = <8>;
					qcom,gpu-freq = <317000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_D0>;

					qcom,bus-freq = <5>;
					qcom,bus-min = <2>;
					qcom,bus-max = <5>;

					qcom,acd-level = <0xc0295ffd>;
				};

				qcom,gpu-pwrlevel@9 {
					reg = <9>;
					qcom,gpu-freq = <285000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_D1>;

					qcom,bus-freq = <1>;
					qcom,bus-min = <1>;
					qcom,bus-max = <5>;

					qcom,acd-level = <0xe02a5ffd>;
				};
			};

			qcom,gpu-pwrlevels-2 {
				#address-cells = <1>;
				#size-cells = <0>;

				qcom,speed-bin = <167>;
				qcom,initial-pwrlevel = <12>;

				qcom,gpu-pwrlevel@0 {
					reg = <0>;
					qcom,gpu-freq = <788000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_TURBO_L1>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <9>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882c5ffd>;
				};

				qcom,gpu-pwrlevel@1 {
					reg = <1>;
					qcom,gpu-freq = <750000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_TURBO>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <9>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xa82c5ffd>;
				};

				qcom,gpu-pwrlevel@2 {
					reg = <2>;
					qcom,gpu-freq = <730000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM_L1>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <8>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xa82c5ffd>;
				};

				qcom,gpu-pwrlevel@3 {
					reg = <3>;
					qcom,gpu-freq = <690000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <7>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xa82c5ffd>;
				};

				qcom,gpu-pwrlevel@4 {
					reg = <4>;
					qcom,gpu-freq = <640000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L2>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@5 {
					reg = <5>;
					qcom,gpu-freq = <599000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L1>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@6 {
					reg = <6>;
					qcom,gpu-freq = <545000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L0>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@7 {
					reg = <7>;
					qcom,gpu-freq = <492000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@8 {
					reg = <8>;
					qcom,gpu-freq = <456000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_L2>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@9 {
					reg = <9>;
					qcom,gpu-freq = <421000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_L1>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@10 {
					reg = <10>;
					qcom,gpu-freq = <350000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS>;

					qcom,bus-freq = <7>;
					qcom,bus-min = <4>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xc0295ffd>;
				};

				qcom,gpu-pwrlevel@11 {
					reg = <11>;
					qcom,gpu-freq = <317000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_D0>;

					qcom,bus-freq = <5>;
					qcom,bus-min = <2>;
					qcom,bus-max = <5>;

					qcom,acd-level = <0xc0295ffd>;
				};

				qcom,gpu-pwrlevel@12 {
					reg = <12>;
					qcom,gpu-freq = <285000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_D1>;

					qcom,bus-freq = <1>;
					qcom,bus-min = <1>;
					qcom,bus-max = <5>;

					qcom,acd-level = <0xe02a5ffd>;
				};
			};

			qcom,gpu-pwrlevels-3 {
				#address-cells = <1>;
				#size-cells = <0>;

				qcom,speed-bin = <168>;
				qcom,initial-pwrlevel = <9>;

				qcom,gpu-pwrlevel@0 {
					reg = <0>;
					qcom,gpu-freq = <690000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_NOM>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <9>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xa82c5ffd>;
				};

				qcom,gpu-pwrlevel@1 {
					reg = <1>;
					qcom,gpu-freq = <640000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L2>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@2 {
					reg = <2>;
					qcom,gpu-freq = <599000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L1>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@3 {
					reg = <3>;
					qcom,gpu-freq = <545000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS_L0>;

					qcom,bus-freq = <9>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@4 {
					reg = <4>;
					qcom,gpu-freq = <492000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_SVS>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@5 {
					reg = <5>;
					qcom,gpu-freq = <456000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_L2>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@6 {
					reg = <6>;
					qcom,gpu-freq = <421000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_L1>;

					qcom,bus-freq = <8>;
					qcom,bus-min = <5>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0x882e5ffd>;
				};

				qcom,gpu-pwrlevel@7 {
					reg = <7>;
					qcom,gpu-freq = <350000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS>;

					qcom,bus-freq = <7>;
					qcom,bus-min = <4>;
					qcom,bus-max = <9>;

					qcom,acd-level = <0xc0295ffd>;
				};

				qcom,gpu-pwrlevel@8 {
					reg = <8>;
					qcom,gpu-freq = <317000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_D0>;

					qcom,bus-freq = <5>;
					qcom,bus-min = <2>;
					qcom,bus-max = <5>;

					qcom,acd-level = <0xc0295ffd>;
				};

				qcom,gpu-pwrlevel@9 {
					reg = <9>;
					qcom,gpu-freq = <285000000>;
					qcom,level = <RPMH_REGULATOR_LEVEL_LOW_SVS_D1>;

					qcom,bus-freq = <1>;
					qcom,bus-min = <1>;
					qcom,bus-max = <5>;

					qcom,acd-level = <0xe02a5ffd>;
				};
			};
		};

		qcom,gpu-mempools {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "qcom,gpu-mempools";

			/* 4K Page Pool configuration */
			qcom,gpu-mempool@0 {
				reg = <0>;
				qcom,mempool-page-size = <4096>;
				qcom,mempool-reserved = <2048>;
			};
			/* 8K Page Pool configuration */
			qcom,gpu-mempool@1 {
				reg = <1>;
				qcom,mempool-page-size = <8192>;
				qcom,mempool-reserved = <1024>;
			};
			/* 64K Page Pool configuration */
			qcom,gpu-mempool@2 {
				reg = <2>;
				qcom,mempool-page-size = <65536>;
				qcom,mempool-reserved = <256>;
			};
			/* 128K Page Pool configuration */
			qcom,gpu-mempool@3 {
				reg = <3>;
				qcom,mempool-page-size = <131072>;
				qcom,mempool-reserved = <128>;
			};
			/* 256K Page Pool configuration */
			qcom,gpu-mempool@4 {
				reg = <4>;
				qcom,mempool-page-size = <262144>;
				qcom,mempool-reserved = <80>;
			};
			/* 1M Page Pool configuration */
			qcom,gpu-mempool@5 {
				reg = <5>;
				qcom,mempool-page-size = <1048576>;
				qcom,mempool-reserved = <32>;
			};
		};
	};

	kgsl_msm_iommu: qcom,kgsl-iommu@3da0000 {
		compatible = "qcom,kgsl-smmu-v2";
		reg = <0x03da0000 0x40000>;

		vddcx-supply = <&gpu_cc_cx_gdsc>;

		gfx3d_user: gfx3d_user {
			compatible = "qcom,smmu-kgsl-cb";
			iommus = <&kgsl_smmu 0x0 0x000>;
			qcom,iommu-dma = "disabled";
		};

		gfx3d_lpac: gfx3d_lpac {
			compatible = "qcom,smmu-kgsl-cb";
			iommus = <&kgsl_smmu 0x1 0x000>;
			qcom,iommu-dma = "disabled";
		};

		gfx3d_secure: gfx3d_secure {
			compatible = "qcom,smmu-kgsl-cb";
			iommus = <&kgsl_smmu 0x2 0x000>;
			qcom,iommu-dma = "disabled";
		};
	};

	gmu: qcom,gmu@3d69000 {
		compatible = "qcom,gen7-gmu";

		reg = <0x3d68000 0x37000>,
		      <0xb290000 0x10000>,
		      <0x03D40000 0x10000>;

		reg-names = "gmu", "gmu_pdc", "gmu_ao_blk_dec0";

		interrupts = <0 304 IRQ_TYPE_LEVEL_HIGH>,
			<0 305 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "hfi", "gmu";

		regulator-names = "vddcx", "vdd";

		vddcx-supply = <&gpu_cc_cx_gdsc>;
		vdd-supply = <&gpu_cc_gx_gdsc>;

		clocks = <&gpucc GPU_CC_CX_GMU_CLK>,
			<&gpucc GPU_CC_CXO_CLK>,
			<&gcc GCC_DDRSS_GPU_AXI_CLK>,
			<&gpucc GPU_CC_HLOS1_VOTE_GPU_SMMU_CLK>,
			<&gpucc GPU_CC_AHB_CLK>,
			<&gpucc GPU_CC_HUB_CX_INT_CLK>,
			<&aoss_qmp>;

		clock-names = "gmu_clk", "cxo_clk", "axi_clk",
			"smmu_vote", "ahb_clk", "hub_clk", "apb_pclk";

		qcom,gmu-freq-table = <220000000 RPMH_REGULATOR_LEVEL_LOW_SVS>,
					<550000000 RPMH_REGULATOR_LEVEL_SVS>;

		iommus = <&kgsl_smmu 0x5 0x000>;
		qcom,iommu-dma = "disabled";

		mboxes = <&qmp_aop 0>;
		mbox-names = "aop";
	};
};
