#include <dt-bindings/clock/qcom,aop-qmp.h>
#include <dt-bindings/clock/qcom,camcc-lahaina.h>
#include <dt-bindings/clock/qcom,dispcc-lahaina.h>
#include <dt-bindings/clock/qcom,gcc-lahaina.h>
#include <dt-bindings/clock/qcom,gpucc-lahaina.h>
#include <dt-bindings/clock/qcom,rpmh.h>
#include <dt-bindings/clock/qcom,videocc-lahaina.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/interconnect/qcom,icc.h>
#include <dt-bindings/interconnect/qcom,epss-l3.h>
#include <dt-bindings/interconnect/qcom,lahaina.h>
#include <dt-bindings/soc/qcom,ipcc.h>
#include <dt-bindings/soc/qcom,dcc_v2.h>
#include <dt-bindings/soc/qcom,rpmh-rsc.h>
#include <dt-bindings/spmi/spmi.h>
#include <dt-bindings/regulator/qcom,rpmh-regulator-levels.h>
#include <dt-bindings/gpio/gpio.h>

#define MHZ_TO_MBPS(mhz, w) ((mhz * 1000000 * w) / (1024 * 1024))
#define BW_OPP_ENTRY(mhz, w) opp-mhz {opp-hz = /bits/ 64 <MHZ_TO_MBPS(mhz, w)>;}
#define BW_OPP_ENTRY_DDR(mhz, w, ddrtype) opp-mhz {\
				opp-hz = /bits/ 64 <MHZ_TO_MBPS(mhz, w)>;\
				opp-supported-hw = <ddrtype>;}
#define DDR_TYPE_LPDDR4X	7
#define DDR_TYPE_LPDDR5		8

/ {
	model = "Qualcomm Technologies, Inc. Lahaina";
	compatible = "qcom,lahaina";
	qcom,msm-id = <415 0x10000>, <456 0x10000>;
	interrupt-parent = <&intc>;

	#address-cells = <2>;
	#size-cells = <2>;
	memory { device_type = "memory"; reg = <0 0 0 0>; };

	mem-offline {
		compatible = "qcom,mem-offline";
		offline-sizes = <0x1 0x40000000 0x0 0x40000000>,
				<0x1 0xc0000000 0x0 0x80000000>,
				<0x2 0xc0000000 0x1 0x40000000>;
		granule = <512>;
		mboxes = <&qmp_aop 0>;
	};

	aliases {
		ufshc1 = &ufshc_mem; /* Embedded UFS Slot */
		sdhc2 = &sdhc_2; /* SDC2 SD card slot */
		serial0 = &qupv3_se3_2uart;
		hsuart0 = &qupv3_se18_4uart;
		pci-domain0 = &pcie0; /* PCIe0 domain */
		pci-domain1 = &pcie1; /* PCIe1 domain */
		usb0 = &usb0;
		usb1 = &usb1;
	};

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		CPU0: cpu@0 {
			device_type = "cpu";
			compatible = "qcom,kryo";
			reg = <0x0 0x0>;
			enable-method = "psci";
			cpu-release-addr = <0x0 0x90000000>;
			cpu-idle-states = <&SILVER_OFF>;
			power-domains = <&CPU_PD0>;
			power-domain-names = "psci";
			qcom,freq-domain = <&cpufreq_hw 0 4>;
			capacity-dmips-mhz = <1024>;
			dynamic-power-coefficient = <100>;
			next-level-cache = <&L2_0>;
			#cooling-cells = <2>;
			L2_0: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;

				L3_0: l3-cache {
				      compatible = "arm,arch-cache";
				      cache-level = <3>;
				};
			};
		};

		CPU1: cpu@100 {
			device_type = "cpu";
			compatible = "qcom,kryo";
			reg = <0x0 0x100>;
			enable-method = "psci";
			cpu-release-addr = <0x0 0x90000000>;
			cpu-idle-states = <&SILVER_OFF>;
			power-domains = <&CPU_PD1>;
			power-domain-names = "psci";
			qcom,freq-domain = <&cpufreq_hw 0 4>;
			capacity-dmips-mhz = <1024>;
			dynamic-power-coefficient = <100>;
			next-level-cache = <&L2_1>;
			#cooling-cells = <2>;
			L2_1: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU2: cpu@200 {
			device_type = "cpu";
			compatible = "qcom,kryo";
			reg = <0x0 0x200>;
			enable-method = "psci";
			cpu-release-addr = <0x0 0x90000000>;
			cpu-idle-states = <&SILVER_OFF>;
			power-domains = <&CPU_PD2>;
			power-domain-names = "psci";
			qcom,freq-domain = <&cpufreq_hw 0 4>;
			capacity-dmips-mhz = <1024>;
			dynamic-power-coefficient = <100>;
			next-level-cache = <&L2_2>;
			#cooling-cells = <2>;
			L2_2: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU3: cpu@300 {
			device_type = "cpu";
			compatible = "qcom,kryo";
			reg = <0x0 0x300>;
			enable-method = "psci";
			cpu-release-addr = <0x0 0x90000000>;
			cpu-idle-states = <&SILVER_OFF>;
			power-domains = <&CPU_PD3>;
			power-domain-names = "psci";
			qcom,freq-domain = <&cpufreq_hw 0 4>;
			capacity-dmips-mhz = <1024>;
			dynamic-power-coefficient = <100>;
			next-level-cache = <&L2_3>;
			#cooling-cells = <2>;
			L2_3: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU4: cpu@400 {
			device_type = "cpu";
			compatible = "qcom,kryo";
			reg = <0x0 0x400>;
			enable-method = "psci";
			cpu-release-addr = <0x0 0x90000000>;
			cpu-idle-states = <&GOLD_OFF>;
			power-domains = <&CPU_PD4>;
			power-domain-names = "psci";
			qcom,freq-domain = <&cpufreq_hw 1 4>;
			capacity-dmips-mhz = <1946>;
			dynamic-power-coefficient = <515>;
			next-level-cache = <&L2_4>;
			#cooling-cells = <2>;
			L2_4: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU5: cpu@500 {
			device_type = "cpu";
			compatible = "qcom,kryo";
			reg = <0x0 0x500>;
			enable-method = "psci";
			cpu-release-addr = <0x0 0x90000000>;
			cpu-idle-states = <&GOLD_OFF>;
			power-domains = <&CPU_PD5>;
			power-domain-names = "psci";
			qcom,freq-domain = <&cpufreq_hw 1 4>;
			capacity-dmips-mhz = <1946>;
			dynamic-power-coefficient = <515>;
			next-level-cache = <&L2_5>;
			#cooling-cells = <2>;
			L2_5: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU6: cpu@600 {
			device_type = "cpu";
			compatible = "qcom,kryo";
			reg = <0x0 0x600>;
			enable-method = "psci";
			cpu-release-addr = <0x0 0x90000000>;
			cpu-idle-states = <&GOLD_OFF>;
			power-domains = <&CPU_PD6>;
			power-domain-names = "psci";
			qcom,freq-domain = <&cpufreq_hw 1 4>;
			capacity-dmips-mhz = <1946>;
			dynamic-power-coefficient = <515>;
			next-level-cache = <&L2_6>;
			#cooling-cells = <2>;
			L2_6: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		CPU7: cpu@700 {
			device_type = "cpu";
			compatible = "qcom,kryo";
			reg = <0x0 0x700>;
			enable-method = "psci";
			cpu-release-addr = <0x0 0x90000000>;
			cpu-idle-states = <&GOLD_OFF>;
			power-domains = <&CPU_PD7>;
			power-domain-names = "psci";
			qcom,freq-domain = <&cpufreq_hw 2 4>;
			capacity-dmips-mhz = <2048>;
			dynamic-power-coefficient = <845>;
			next-level-cache = <&L2_7>;
			#cooling-cells = <2>;
			L2_7: l2-cache {
			      compatible = "arm,arch-cache";
			      cache-level = <2>;
			      next-level-cache = <&L3_0>;
			};
		};

		cpu-map {
			cluster0 {
				core0 {
					cpu = <&CPU0>;
				};

				core1 {
					cpu = <&CPU1>;
				};

				core2 {
					cpu = <&CPU2>;
				};

				core3 {
					cpu = <&CPU3>;
				};
			};

			cluster1 {
				core0 {
					cpu = <&CPU4>;
				};

				core1 {
					cpu = <&CPU5>;
				};

				core2 {
					cpu = <&CPU6>;
				};
			};

			cluster2 {

				core0 {
					cpu = <&CPU7>;
				};
			};
		};
	};

	idle-states {
		SILVER_OFF: silver-c4 {  /* C4 */
			compatible = "arm,idle-state";
			idle-state-name = "rail-pc";
			entry-latency-us = <360>;
			exit-latency-us = <531>;
			min-residency-us = <3934>;
			arm,psci-suspend-param = <0x40000004>;
			local-timer-stop;
		};

		GOLD_OFF: gold-c4 {  /* C4 */
			compatible = "arm,idle-state";
			idle-state-name = "rail-pc";
			entry-latency-us = <702>;
			exit-latency-us = <1061>;
			min-residency-us = <4488>;
			arm,psci-suspend-param = <0x40000004>;
			local-timer-stop;
		};

		CLUSTER_CLK_GATE: cluster-d1 { /* D1 */
			compatible = "domain-idle-state";
			idle-state-name = "l3-wfi";
			entry-latency-us = <48>;
			exit-latency-us = <51>;
			min-residency-us = <99>;
			arm,psci-suspend-param = <0x41000014>;
		};

		CLUSTER_PWR_DN: cluster-d4 { /* D4 */
			compatible = "domain-idle-state";
			idle-state-name = "l3-off";
			entry-latency-us = <1000>;
			exit-latency-us = <1000>;
			min-residency-us = <2000>;
			arm,psci-suspend-param = <0x41000044>;
		};
	};

	soc: soc { };


	firmware: firmware {
		scm {
			compatible = "qcom,scm";
			qcom,dload-mode = <&tcsr 0x13000>;
		};

		android {
			compatible = "android,firmware";
			vbmeta {
				compatible = "android,vbmeta";
				parts = "vbmeta,boot,system,vendor,dtbo";
			};

			fstab {
				compatible = "android,fstab";
				vendor {
					compatible = "android,vendor";
					dev = "/dev/block/platform/soc/1d84000.ufshc/by-name/vendor";
					type = "ext4";
					mnt_flags = "ro,barrier=1,discard";
					fsmgr_flags = "wait,slotselect,avb";
					status = "ok";
				};
			};
		};
	};

	reserved_memory: reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		hyp_mem: hyp_region@80000000 {
			no-map;
			reg = <0x0 0x80000000 0x0 0x600000>;
		};

		xbl_aop_mem: xbl_aop_region@80700000 {
			no-map;
			reg = <0x0 0x80700000 0x0 0x160000>;
		};

		cmd_db: reserved-memory@80860000 {
			compatible = "qcom,cmd-db";
			no-map;
			reg = <0x0 0x80860000 0x0 0x20000>;
		};

		reserved_xbl_uefi_log: res_xbl_uefi_log_region@80880000 {
			no-map;
			reg = <0x0 0x80880000 0x0 0x14000>;
		};

		smem_mem: smem_region@80900000 {
			no-map;
			reg = <0x0 0x80900000 0x0 0x200000>;
		};

		cpucp_fw_mem: cpucp_fw_region@80b00000 {
			no-map;
			reg = <0x0 0x80b00000 0x0 0x100000>;
		};

		cdsp_secure_heap: cdsp_secure_heap@80c00000 {
			no-map;
			reg = <0x0 0x80c00000 0x0 0x4600000>;
		};

		pil_camera_mem: pil_camera_region@85200000 {
			no-map;
			reg = <0x0 0x85200000 0x0 0x500000>;
		};

		pil_video_mem: pil_video_region@85700000 {
			no-map;
			reg = <0x0 0x85700000 0x0 0x500000>;
		};

		pil_cvp_mem: pil_cvp_region@85c00000 {
			no-map;
			reg = <0x0 0x85c00000 0x0 0x500000>;
		};

		pil_adsp_mem: pil_adsp_region@86100000 {
			no-map;
			reg = <0x0 0x86100000 0x0 0x2100000>;
		};

		pil_slpi_mem: pil_slpi_region@88200000 {
			no-map;
			reg = <0x0 0x88200000 0x0 0x1500000>;
		};

		pil_cdsp_mem: pil_cdsp_region@89700000 {
			no-map;
			reg = <0x0 0x89700000 0x0 0x1e00000>;
		};

		pil_ipa_fw_mem: pil_ipa_fw_region@8b500000 {
			no-map;
			reg = <0x0 0x8b500000 0x0 0x10000>;
		};

		pil_ipa_gsi_mem: pil_ipa_gsi_region@8b510000 {
			no-map;
			reg = <0x0 0x8b510000 0x0 0xa000>;
		};

		pil_gpu_mem: pil_gpu_region@8b51a000 {
			no-map;
			reg = <0x0 0x8b51a000 0x0 0x2000>;
		};

		pil_spss_mem: pil_spss_region@8b600000 {
			no-map;
			reg = <0x0 0x8b600000 0x0 0x100000>;
		};

		pil_modem_mem: modem_region@8b800000 {
			no-map;
			reg = <0x0 0x8b800000 0x0 0x10000000>;
		};

		/* First half of the "SPU secure shared memory" region */
		spu_tz_shared_mem: spu_tz_shared_mem@9b800000 {
			no-map;
			reg = <0x0 0x9b800000 0x0 0x10000>;
		};

		/* Second half of the "SPU secure shared memory" region */
		spu_modem_shared_mem: spu_modem_shared_mem@9b810000 {
			no-map;
			reg = <0x0 0x9b810000 0x0 0x10000>;
		};

		hyp_reserved_mem: qheebsp_dbg_vm_hyp_region@d0000000 {
			no-map;
			reg = <0x0 0xd0000000 0x0 0x800000>;
		};

		pil_trustedvm_mem: pil_trustedvm_region@d0800000 {
			no-map;
			reg = <0x0 0xd0800000 0x0 0x76f7000>;
		};

		qrtr_shbuf: qrtr-shmem {
			no-map;
			reg = <0x0 0xd7ef7000 0x0 0x9000>;
		};

		chan0_shbuf: neuron_block@0 {
			no-map;
			reg = <0x0 0xd7f00000 0x0 0x80000>;
		};

		chan1_shbuf: neuron_block@1 {
			no-map;
			reg = <0x0 0xd7f80000 0x0 0x80000>;
		};

		removed_mem: removed_region@d8800000 {
			no-map;
			reg = <0x0 0xd8800000 0x0 0x6800000>;
		};

		adsp_mem: adsp_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0xC00000>;
		};

		sdsp_mem: sdsp_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x800000>;
		};

		cdsp_mem: cdsp_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x400000>;
		};

		user_contig_mem: user_contig_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1000000>;
		};

		qseecom_mem: qseecom_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1400000>;
		};

		qseecom_ta_mem: qseecom_ta_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1000000>;
		};

		secure_display_memory: secure_display_region { /* Secure UI */
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0xA400000>;
		};

		cnss_wlan_mem: cnss_wlan_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1400000>;
		};

		/* global autoconfigured region for contiguous allocations */
		system_cma: linux,cma {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xdfffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x2000000>;
			linux,cma-default;
		};

		dump_mem: mem_dump_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			size = <0 0x3000000>;
		};

		sp_mem: sp_region {  /* SPSS-HLOS ION shared mem */
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1000000>;
		};

		audio_cma_mem: audio_cma_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x1C00000>;
		};

		splash_memory:splash_region {
			reg = <0x0 0xe1000000 0x0 0x02300000>;
			label = "cont_splash_region";
		};

		dfps_data_memory: dfps_data_region {
			reg = <0x0 0xe3300000 0x0 0x0100000>;
			label = "dfps_data_region";
		};

		memshare_mem: memshare_region {
			compatible = "shared-dma-pool";
			no-map;
			/*
			 * Memory shared with modem needs to be outside of
			 * the CLADE address space, which begins at
			 * 0xE0000000 and spans 512 MB.
			 */
			alloc-ranges = <0x0 0x00000000 0x0 0xdfffffff>;
			alignment = <0x0 0x100000>;
			size = <0x0 0x800000>;
		};

		non_secure_display_memory: non_secure_display_region {
			compatible = "shared-dma-pool";
			alloc-ranges = <0x0 0x00000000 0x0 0xffffffff>;
			reusable;
			alignment = <0x0 0x400000>;
			size = <0x0 0x6400000>;
		};
	};

	chosen {
		bootargs = "log_buf_len=256K earlycon=msm_geni_serial,0x98c000 rcupdate.rcu_expedited=1 rcu_nocbs=0-7 cpufreq.default_governor=performance";
	};
};

&soc {
	#address-cells = <1>;
	#size-cells = <1>;
	ranges = <0 0 0 0xffffffff>;
	compatible = "simple-bus";

	psci {
		compatible = "arm,psci-1.0";
		method = "smc";

		CPU_PD0: cpu-pd0 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD1: cpu-pd1 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD2: cpu-pd2 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD3: cpu-pd3 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD4: cpu-pd4 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD5: cpu-pd5 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD6: cpu-pd6 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CPU_PD7: cpu-pd7 {
			#power-domain-cells = <0>;
			power-domains = <&CLUSTER_PD>;
		};

		CLUSTER_PD: cluster-pd {
			#power-domain-cells = <0>;
			domain-idle-states = <&CLUSTER_CLK_GATE &CLUSTER_PWR_DN>;
		};
	};

	slim_aud: slim@3ac0000 {
		cell-index = <1>;
		compatible = "qcom,slim-ngd";
		reg = <0x3ac0000 0x2c000>,
			<0x3a84000 0x22000>;
		reg-names = "slimbus_physical", "slimbus_bam_physical";
		interrupts = <GIC_SPI 163 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 164 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "slimbus_irq", "slimbus_bam_irq";
		qcom,apps-ch-pipes = <0x0>;
		qcom,ea-pc = <0x350>;
		iommus = <&apps_smmu 0x1826 0x0>;
		qcom,iommu-dma-addr-pool = <0x40000000 0xc0000000>;
		qcom,iommu-dma = "fastmap";
		status = "ok";

		/* Slimbus Slave DT for QCA6490 */
		btfmslim_codec: qca6490 {
			compatible = "qcom,btfmslim_slave";
			elemental-addr = [00 01 21 02 17 02];
			qcom,btfm-slim-ifd = "btfmslim_slave_ifd";
			qcom,btfm-slim-ifd-elemental-addr = [00 00 21 02 17 02];
		};
	};

	intc: interrupt-controller@17a00000 {
		compatible = "arm,gic-v3";
		#interrupt-cells = <3>;
		interrupt-controller;
		#redistributor-regions = <1>;
		redistributor-stride = <0x0 0x20000>;
		reg = <0x17a00000 0x10000>,     /* GICD */
		      <0x17a60000 0x100000>;    /* GICR * 8 */
		interrupts = <GIC_PPI 9 IRQ_TYPE_LEVEL_HIGH>;
	};

	arch_timer: timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(8) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(8) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(8) | IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 12 (GIC_CPU_MASK_SIMPLE(8) | IRQ_TYPE_LEVEL_LOW)>;
		clock-frequency = <19200000>;
	};

	memtimer: timer@17c20000 {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "arm,armv7-timer-mem";
		reg = <0x17c20000 0x1000>;
		clock-frequency = <19200000>;

		frame@17c21000 {
			frame-number = <0>;
			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c21000 0x1000>,
			      <0x17c22000 0x1000>;
		};

		frame@17c23000 {
			frame-number = <1>;
			interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c23000 0x1000>;
			status = "disabled";
		};

		frame@17c25000 {
			frame-number = <2>;
			interrupts = <GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c25000 0x1000>;
			status = "disabled";
		};

		frame@17c27000 {
			frame-number = <3>;
			interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c27000 0x1000>;
			status = "disabled";
		};

		frame@17c29000 {
			frame-number = <4>;
			interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c29000 0x1000>;
			status = "disabled";
		};

		frame@17c2b000 {
			frame-number = <5>;
			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c2b000 0x1000>;
			status = "disabled";
		};

		frame@17c2d000 {
			frame-number = <6>;
			interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
			reg = <0x17c2d000 0x1000>;
			status = "disabled";
		};
	};

	dcc: dcc_v2@117f000 {
		compatible = "qcom,dcc-v2";
		reg = <0x117f000 0x1000>,
		      <0x1112000 0x6000>;

		qcom,transaction_timeout = <0>;

		reg-names = "dcc-base", "dcc-ram-base";
		dcc-ram-offset = <0x12000>;

		link_list1 {
			qcom,curr-link-list = <6>;
			qcom,data-sink = "sram";
			qcom,link-list = <DCC_WRITE 0x18080010 0x1 0>,
				<DCC_READ 0x00144018 1 0>,
				<DCC_WRITE 0x00144018 0x1 0>,
				<DCC_READ 0x00144018 1 0>,
				<DCC_READ 0x091a9020 1 0>,
				<DCC_READ_WRITE 0x5 0x1 0>,
				<DCC_READ 0x09102008 1 0>,
				<DCC_READ_WRITE 0x2 0x2 0>,
				<DCC_READ 0x09142008 1 0>,
				<DCC_READ_WRITE 0x2 0x2 0>,
				<DCC_READ 0x09102408 1 0>,
				<DCC_READ_WRITE 0x2 0x2 0>,
				<DCC_READ 0x09142408 1 0>,
				<DCC_READ_WRITE 0x2 0x2 0>,
				<DCC_READ 0x09103808 1 0>,
				<DCC_LOOP 3 0 0>,
				<DCC_READ 0x09103810 1 0>,
				<DCC_READ 0x09103814 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09103888 1 0>,
				<DCC_LOOP 2 0 0>,
				<DCC_READ 0x09103890 1 0>,
				<DCC_READ 0x09103894 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09143808 1 0>,
				<DCC_LOOP 3 0 0>,
				<DCC_READ 0x09143810 1 0>,
				<DCC_READ 0x09143814 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09143888 1 0>,
				<DCC_LOOP 2 0 0>,
				<DCC_READ 0x09143890 1 0>,
				<DCC_READ 0x09143894 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09182808 1 0>,
				<DCC_LOOP 2 0 0>,
				<DCC_READ 0x09182810 1 0>,
				<DCC_READ 0x09182814 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09182888 1 0>,
				<DCC_LOOP 3 0 0>,
				<DCC_READ 0x09182890 1 0>,
				<DCC_READ 0x09182894 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09103008 1 0>,
				<DCC_READ 0x0910300c 1 0>,
				<DCC_WRITE 0x09103028 0x00000001 1>,
				<DCC_LOOP 41 0 0>,
				<DCC_READ 0x09103010 1 0>,
				<DCC_READ 0x09103014 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09103408 1 0>,
				<DCC_READ 0x0910340c 1 0>,
				<DCC_WRITE 0x09103428 0x00000001 1>,
				<DCC_LOOP 41 0 0>,
				<DCC_READ 0x09103410 1 0>,
				<DCC_READ 0x09103414 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09143008 1 0>,
				<DCC_READ 0x0914300c 1 0>,
				<DCC_WRITE 0x09143028 0x00000001 1>,
				<DCC_LOOP 41 0 0>,
				<DCC_READ 0x09143010 1 0>,
				<DCC_READ 0x09143014 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09143408 1 0>,
				<DCC_READ 0x0914340c 1 0>,
				<DCC_WRITE 0x09143428 0x00000001 1>,
				<DCC_LOOP 41 0 0>,
				<DCC_READ 0x09143410 1 0>,
				<DCC_READ 0x09143414 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09182008 1 0>,
				<DCC_READ 0x0918200c 1 0>,
				<DCC_WRITE 0x09182028 0x00000001 1>,
				<DCC_LOOP 11 0 0>,
				<DCC_READ 0x09182010 1 0>,
				<DCC_READ 0x09182014 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x09182408 1 0>,
				<DCC_READ 0x0918240c 1 0>,
				<DCC_WRITE 0x09182428 0x00000001 1>,
				<DCC_LOOP 11 0 0>,
				<DCC_READ 0x09182410 1 0>,
				<DCC_READ 0x09182414 1 0>,
				<DCC_LOOP 1 0 0>,
				<DCC_READ 0x18000024 1 0>,
				<DCC_READ 0x18000040 4 0>,
				<DCC_READ 0x18010024 1 0>,
				<DCC_READ 0x18010040 4 0>,
				<DCC_READ 0x18020024 1 0>,
				<DCC_READ 0x18020040 4 0>,
				<DCC_READ 0x18030024 1 0>,
				<DCC_READ 0x18030040 4 0>,
				<DCC_READ 0x18040024 1 0>,
				<DCC_READ 0x18040040 4 0>,
				<DCC_READ 0x18050024 1 0>,
				<DCC_READ 0x18050040 4 0>,
				<DCC_READ 0x18060024 1 0>,
				<DCC_READ 0x18060040 4 0>,
				<DCC_READ 0x18070024 1 0>,
				<DCC_READ 0x18070040 4 0>,
				<DCC_READ 0x18080024 1 0>,
				<DCC_READ 0x18080040 3 0>,
				<DCC_READ 0x180800f8 1 0>,
				<DCC_READ 0x18080104 1 0>,
				<DCC_READ 0x1808011c 1 0>,
				<DCC_READ 0x18080128 1 0>,
				<DCC_READ 0x18080168 1 0>,
				<DCC_READ 0x18080198 1 0>,
				<DCC_READ 0x9050078 1 0>,
				<DCC_READ 0x9050110 8 0>,
				<DCC_READ 0x9080058 2 0>,
				<DCC_READ 0x90800c8 1 0>,
				<DCC_READ 0x90800d4 1 0>,
				<DCC_READ 0x90800e0 1 0>,
				<DCC_READ 0x90800ec 1 0>,
				<DCC_READ 0x90800f8 1 0>,
				<DCC_READ 0x9084030 1 0>,
				<DCC_READ 0x9084038 2 0>,
				<DCC_READ 0x90840e4 1 0>,
				<DCC_READ 0x90840f4 1 0>,
				<DCC_READ 0x9084104 2 0>,
				<DCC_READ 0x9084194 1 0>,
				<DCC_READ 0x9084804 1 0>,
				<DCC_READ 0x908480c 1 0>,
				<DCC_READ 0x9084844 1 0>,
				<DCC_READ 0x9084850 2 0>,
				<DCC_READ 0x9084860 3 0>,
				<DCC_READ 0x9084888 1 0>,
				<DCC_READ 0x908488c 1 0>,
				<DCC_READ 0x9084900 1 0>,
				<DCC_READ 0x908409c 1 0>,
				<DCC_READ 0x90840a0 1 0>,
				<DCC_READ 0x908426c 1 0>,
				<DCC_READ 0x908439c 1 0>,
				<DCC_READ 0x9085124 1 0>,
				<DCC_READ 0x90ba280 1 0>,
				<DCC_READ 0x90ba288 7 0>,
				<DCC_READ 0x9258610 4 0>,
				<DCC_READ 0x92d8610 4 0>,
				<DCC_READ 0x9358610 4 0>,
				<DCC_READ 0x93d8610 4 0>,
				<DCC_READ 0x9220344 8 0>,
				<DCC_READ 0x9220370 6 0>,
				<DCC_READ 0x9220480 1 0>,
				<DCC_READ 0x9222400 1 0>,
				<DCC_READ 0x922240c 1 0>,
				<DCC_READ 0x9223214 2 0>,
				<DCC_READ 0x9223220 3 0>,
				<DCC_READ 0x9223308 1 0>,
				<DCC_READ 0x9223318 1 0>,
				<DCC_READ 0x9232100 1 0>,
				<DCC_READ 0x9236040 6 0>,
				<DCC_READ 0x92360b0 1 0>,
				<DCC_READ 0x923a004 4 0>,
				<DCC_READ 0x923e030 2 0>,
				<DCC_READ 0x9241000 1 0>,
				<DCC_READ 0x9242028 1 0>,
				<DCC_READ 0x9242044 3 0>,
				<DCC_READ 0x9242070 1 0>,
				<DCC_READ 0x9248030 1 0>,
				<DCC_READ 0x9248048 8 0>,
				<DCC_READ 0x92a0344 8 0>,
				<DCC_READ 0x92a0370 6 0>,
				<DCC_READ 0x92a0480 1 0>,
				<DCC_READ 0x92a2400 1 0>,
				<DCC_READ 0x92a240c 1 0>,
				<DCC_READ 0x92a3214 2 0>,
				<DCC_READ 0x92a3220 3 0>,
				<DCC_READ 0x92a3308 1 0>,
				<DCC_READ 0x92a3318 1 0>,
				<DCC_READ 0x92b2100 1 0>,
				<DCC_READ 0x92b6040 6 0>,
				<DCC_READ 0x92b60b0 1 0>,
				<DCC_READ 0x92ba004 4 0>,
				<DCC_READ 0x92be030 2 0>,
				<DCC_READ 0x92c1000 1 0>,
				<DCC_READ 0x92c2028 1 0>,
				<DCC_READ 0x92c2044 3 0>,
				<DCC_READ 0x92c2070 1 0>,
				<DCC_READ 0x92c8030 1 0>,
				<DCC_READ 0x92c8048 8 0>,
				<DCC_READ 0x9320344 8 0>,
				<DCC_READ 0x9320370 6 0>,
				<DCC_READ 0x9320480 1 0>,
				<DCC_READ 0x9322400 1 0>,
				<DCC_READ 0x932240c 1 0>,
				<DCC_READ 0x9323214 2 0>,
				<DCC_READ 0x9323220 3 0>,
				<DCC_READ 0x9323308 1 0>,
				<DCC_READ 0x9323318 1 0>,
				<DCC_READ 0x9332100 1 0>,
				<DCC_READ 0x9336040 6 0>,
				<DCC_READ 0x93360b0 1 0>,
				<DCC_READ 0x933a004 4 0>,
				<DCC_READ 0x933e030 2 0>,
				<DCC_READ 0x9341000 1 0>,
				<DCC_READ 0x9342028 1 0>,
				<DCC_READ 0x9342044 3 0>,
				<DCC_READ 0x9342070 1 0>,
				<DCC_READ 0x9348030 1 0>,
				<DCC_READ 0x9348048 8 0>,
				<DCC_READ 0x93a0344 8 0>,
				<DCC_READ 0x93a0370 6 0>,
				<DCC_READ 0x93a0480 1 0>,
				<DCC_READ 0x93a2400 1 0>,
				<DCC_READ 0x93a240c 1 0>,
				<DCC_READ 0x93a3214 2 0>,
				<DCC_READ 0x93a3220 3 0>,
				<DCC_READ 0x93a3308 1 0>,
				<DCC_READ 0x93a3318 1 0>,
				<DCC_READ 0x93b2100 1 0>,
				<DCC_READ 0x93b6040 6 0>,
				<DCC_READ 0x93b60b0 1 0>,
				<DCC_READ 0x93ba004 4 0>,
				<DCC_READ 0x93be030 2 0>,
				<DCC_READ 0x93c1000 1 0>,
				<DCC_READ 0x93c2028 1 0>,
				<DCC_READ 0x93c2044 3 0>,
				<DCC_READ 0x93c2070 1 0>,
				<DCC_READ 0x93c8030 1 0>,
				<DCC_READ 0x93c8048 8 0>,
				<DCC_READ 0x9270080 1 0>,
				<DCC_READ 0x9270310 1 0>,
				<DCC_READ 0x9270400 1 0>,
				<DCC_READ 0x9270410 6 0>,
				<DCC_READ 0x9270430 1 0>,
				<DCC_READ 0x9270440 1 0>,
				<DCC_READ 0x9270448 1 0>,
				<DCC_READ 0x92704a0 1 0>,
				<DCC_READ 0x92704b0 1 0>,
				<DCC_READ 0x92704b8 2 0>,
				<DCC_READ 0x92704d0 2 0>,
				<DCC_READ 0x9271400 1 0>,
				<DCC_READ 0x9271408 1 0>,
				<DCC_READ 0x927341c 1 0>,
				<DCC_READ 0x92753b0 1 0>,
				<DCC_READ 0x9275804 1 0>,
				<DCC_READ 0x9275c1c 1 0>,
				<DCC_READ 0x9275c2c 1 0>,
				<DCC_READ 0x9275c38 1 0>,
				<DCC_READ 0x9276418 2 0>,
				<DCC_READ 0x9279100 1 0>,
				<DCC_READ 0x9279110 1 0>,
				<DCC_READ 0x9279120 1 0>,
				<DCC_READ 0x9279180 2 0>,
				<DCC_READ 0x92f0080 1 0>,
				<DCC_READ 0x92f0310 1 0>,
				<DCC_READ 0x92f0400 1 0>,
				<DCC_READ 0x92f0410 6 0>,
				<DCC_READ 0x92f0430 1 0>,
				<DCC_READ 0x92f0440 1 0>,
				<DCC_READ 0x92f0448 1 0>,
				<DCC_READ 0x92f04a0 1 0>,
				<DCC_READ 0x92f04b0 1 0>,
				<DCC_READ 0x92f04b8 2 0>,
				<DCC_READ 0x92f04d0 2 0>,
				<DCC_READ 0x92f1400 1 0>,
				<DCC_READ 0x92f1408 1 0>,
				<DCC_READ 0x92f341c 1 0>,
				<DCC_READ 0x92f53b0 1 0>,
				<DCC_READ 0x92f5804 1 0>,
				<DCC_READ 0x92f5c1c 1 0>,
				<DCC_READ 0x92f5c2c 1 0>,
				<DCC_READ 0x92f5c38 1 0>,
				<DCC_READ 0x92f6418 2 0>,
				<DCC_READ 0x92f9100 1 0>,
				<DCC_READ 0x92f9110 1 0>,
				<DCC_READ 0x92f9120 1 0>,
				<DCC_READ 0x92f9180 2 0>,
				<DCC_READ 0x9370080 1 0>,
				<DCC_READ 0x9370310 1 0>,
				<DCC_READ 0x9370400 1 0>,
				<DCC_READ 0x9370410 6 0>,
				<DCC_READ 0x9370430 1 0>,
				<DCC_READ 0x9370440 1 0>,
				<DCC_READ 0x9370448 1 0>,
				<DCC_READ 0x93704a0 1 0>,
				<DCC_READ 0x93704b0 1 0>,
				<DCC_READ 0x93704b8 2 0>,
				<DCC_READ 0x93704d0 2 0>,
				<DCC_READ 0x9371400 1 0>,
				<DCC_READ 0x9371408 1 0>,
				<DCC_READ 0x937341c 1 0>,
				<DCC_READ 0x93753b0 1 0>,
				<DCC_READ 0x9375804 1 0>,
				<DCC_READ 0x9375c1c 1 0>,
				<DCC_READ 0x9375c2c 1 0>,
				<DCC_READ 0x9375c38 1 0>,
				<DCC_READ 0x9376418 2 0>,
				<DCC_READ 0x9379100 1 0>,
				<DCC_READ 0x9379110 1 0>,
				<DCC_READ 0x9379120 1 0>,
				<DCC_READ 0x9379180 2 0>,
				<DCC_READ 0x93f0080 1 0>,
				<DCC_READ 0x93f0310 1 0>,
				<DCC_READ 0x93f0400 1 0>,
				<DCC_READ 0x93f0410 6 0>,
				<DCC_READ 0x93f0430 1 0>,
				<DCC_READ 0x93f0440 1 0>,
				<DCC_READ 0x93f0448 1 0>,
				<DCC_READ 0x93f04a0 1 0>,
				<DCC_READ 0x93f04b0 1 0>,
				<DCC_READ 0x93f04b8 2 0>,
				<DCC_READ 0x93f04d0 2 0>,
				<DCC_READ 0x93f1400 1 0>,
				<DCC_READ 0x93f1408 1 0>,
				<DCC_READ 0x93f341c 1 0>,
				<DCC_READ 0x93f53b0 1 0>,
				<DCC_READ 0x93f5804 1 0>,
				<DCC_READ 0x93f5c1c 1 0>,
				<DCC_READ 0x93f5c2c 1 0>,
				<DCC_READ 0x93f5c38 1 0>,
				<DCC_READ 0x93f6418 2 0>,
				<DCC_READ 0x93f9100 1 0>,
				<DCC_READ 0x93f9110 1 0>,
				<DCC_READ 0x93f9120 1 0>,
				<DCC_READ 0x93f9180 2 0>,
				<DCC_READ 0x9260080 1 0>,
				<DCC_READ 0x9260400 1 0>,
				<DCC_READ 0x9260410 3 0>,
				<DCC_READ 0x9260420 2 0>,
				<DCC_READ 0x9260430 1 0>,
				<DCC_READ 0x9260440 1 0>,
				<DCC_READ 0x9260448 1 0>,
				<DCC_READ 0x92604a0 1 0>,
				<DCC_READ 0x92604b0 1 0>,
				<DCC_READ 0x92604b8 2 0>,
				<DCC_READ 0x92604d0 2 0>,
				<DCC_READ 0x9261400 1 0>,
				<DCC_READ 0x9263410 1 0>,
				<DCC_READ 0x92653b0 1 0>,
				<DCC_READ 0x9265804 1 0>,
				<DCC_READ 0x9265b1c 1 0>,
				<DCC_READ 0x9265b2c 1 0>,
				<DCC_READ 0x9265b38 1 0>,
				<DCC_READ 0x9269100 1 0>,
				<DCC_READ 0x9269108 1 0>,
				<DCC_READ 0x9269110 1 0>,
				<DCC_READ 0x9269118 1 0>,
				<DCC_READ 0x9269120 1 0>,
				<DCC_READ 0x9269180 2 0>,
				<DCC_READ 0x92e0080 1 0>,
				<DCC_READ 0x92e0400 1 0>,
				<DCC_READ 0x92e0410 3 0>,
				<DCC_READ 0x92e0420 2 0>,
				<DCC_READ 0x92e0430 1 0>,
				<DCC_READ 0x92e0440 1 0>,
				<DCC_READ 0x92e0448 1 0>,
				<DCC_READ 0x92e04a0 1 0>,
				<DCC_READ 0x92e04b0 1 0>,
				<DCC_READ 0x92e04b8 2 0>,
				<DCC_READ 0x92e04d0 2 0>,
				<DCC_READ 0x92e1400 1 0>,
				<DCC_READ 0x92e3410 1 0>,
				<DCC_READ 0x92e53b0 1 0>,
				<DCC_READ 0x92e5804 1 0>,
				<DCC_READ 0x92e5b1c 1 0>,
				<DCC_READ 0x92e5b2c 1 0>,
				<DCC_READ 0x92e5b38 1 0>,
				<DCC_READ 0x92e9100 1 0>,
				<DCC_READ 0x92e9108 1 0>,
				<DCC_READ 0x92e9110 1 0>,
				<DCC_READ 0x92e9118 1 0>,
				<DCC_READ 0x92e9120 1 0>,
				<DCC_READ 0x92e9180 2 0>,
				<DCC_READ 0x9360080 1 0>,
				<DCC_READ 0x9360400 1 0>,
				<DCC_READ 0x9360410 3 0>,
				<DCC_READ 0x9360420 2 0>,
				<DCC_READ 0x9360430 1 0>,
				<DCC_READ 0x9360440 1 0>,
				<DCC_READ 0x9360448 1 0>,
				<DCC_READ 0x93604a0 1 0>,
				<DCC_READ 0x93604b0 1 0>,
				<DCC_READ 0x93604b8 2 0>,
				<DCC_READ 0x93604d0 2 0>,
				<DCC_READ 0x9361400 1 0>,
				<DCC_READ 0x9363410 1 0>,
				<DCC_READ 0x93653b0 1 0>,
				<DCC_READ 0x9365804 1 0>,
				<DCC_READ 0x9365b1c 1 0>,
				<DCC_READ 0x9365b2c 1 0>,
				<DCC_READ 0x9365b38 1 0>,
				<DCC_READ 0x9369100 1 0>,
				<DCC_READ 0x9369108 1 0>,
				<DCC_READ 0x9369110 1 0>,
				<DCC_READ 0x9369118 1 0>,
				<DCC_READ 0x9369120 1 0>,
				<DCC_READ 0x9369180 2 0>,
				<DCC_READ 0x93e0080 1 0>,
				<DCC_READ 0x93e0400 1 0>,
				<DCC_READ 0x93e0410 3 0>,
				<DCC_READ 0x93e0420 2 0>,
				<DCC_READ 0x93e0430 1 0>,
				<DCC_READ 0x93e0440 1 0>,
				<DCC_READ 0x93e0448 1 0>,
				<DCC_READ 0x93e04a0 1 0>,
				<DCC_READ 0x93e04b0 1 0>,
				<DCC_READ 0x93e04b8 2 0>,
				<DCC_READ 0x93e04d0 2 0>,
				<DCC_READ 0x93e1400 1 0>,
				<DCC_READ 0x93e3410 1 0>,
				<DCC_READ 0x93e53b0 1 0>,
				<DCC_READ 0x93e5804 1 0>,
				<DCC_READ 0x93e5b1c 1 0>,
				<DCC_READ 0x93e5b2c 1 0>,
				<DCC_READ 0x93e5b38 1 0>,
				<DCC_READ 0x93e9100 1 0>,
				<DCC_READ 0x93e9108 1 0>,
				<DCC_READ 0x93e9110 1 0>,
				<DCC_READ 0x93e9118 1 0>,
				<DCC_READ 0x93e9120 1 0>,
				<DCC_READ 0x93e9180 2 0>,
				<DCC_READ 0x96b0868 1 0>,
				<DCC_READ 0x96b0870 1 0>,
				<DCC_READ 0x96b1004 1 0>,
				<DCC_READ 0x96b100c 1 0>,
				<DCC_READ 0x96b1014 1 0>,
				<DCC_READ 0x96b1204 1 0>,
				<DCC_READ 0x96b120c 1 0>,
				<DCC_READ 0x96b1214 1 0>,
				<DCC_READ 0x96b1504 1 0>,
				<DCC_READ 0x96b150c 1 0>,
				<DCC_READ 0x96b1514 1 0>,
				<DCC_READ 0x96b1604 1 0>,
				<DCC_READ 0x96b8100 1 0>,
				<DCC_READ 0x96b813c 1 0>,
				<DCC_READ 0x96b8500 1 0>,
				<DCC_READ 0x96b853c 1 0>,
				<DCC_READ 0x96b8a04 1 0>,
				<DCC_READ 0x96b8a18 1 0>,
				<DCC_READ 0x96b8ea8 1 0>,
				<DCC_READ 0x96b9044 1 0>,
				<DCC_READ 0x96b904c 1 0>,
				<DCC_READ 0x96b9054 1 0>,
				<DCC_READ 0x96b905c 1 0>,
				<DCC_READ 0x96b910c 2 0>,
				<DCC_READ 0x96b9204 1 0>,
				<DCC_READ 0x96b920c 1 0>,
				<DCC_READ 0x96b9238 1 0>,
				<DCC_READ 0x96b9240 1 0>,
				<DCC_READ 0x96b926c 1 0>,
				<DCC_READ 0x96b9394 1 0>,
				<DCC_READ 0x96b939c 1 0>,
				<DCC_READ 0x96b9704 1 0>,
				<DCC_READ 0x96b970c 1 0>,
				<DCC_READ 0x96f0868 1 0>,
				<DCC_READ 0x96f0870 1 0>,
				<DCC_READ 0x96f1004 1 0>,
				<DCC_READ 0x96f100c 1 0>,
				<DCC_READ 0x96f1014 1 0>,
				<DCC_READ 0x96f1204 1 0>,
				<DCC_READ 0x96f120c 1 0>,
				<DCC_READ 0x96f1214 1 0>,
				<DCC_READ 0x96f1504 1 0>,
				<DCC_READ 0x96f150c 1 0>,
				<DCC_READ 0x96f1514 1 0>,
				<DCC_READ 0x96f1604 1 0>,
				<DCC_READ 0x96f8100 1 0>,
				<DCC_READ 0x96f813c 1 0>,
				<DCC_READ 0x96f8500 1 0>,
				<DCC_READ 0x96f853c 1 0>,
				<DCC_READ 0x96f8a04 1 0>,
				<DCC_READ 0x96f8a18 1 0>,
				<DCC_READ 0x96f8ea8 1 0>,
				<DCC_READ 0x96f9044 1 0>,
				<DCC_READ 0x96f904c 1 0>,
				<DCC_READ 0x96f9054 1 0>,
				<DCC_READ 0x96f905c 1 0>,
				<DCC_READ 0x96f910c 2 0>,
				<DCC_READ 0x96f9204 1 0>,
				<DCC_READ 0x96f920c 1 0>,
				<DCC_READ 0x96f9238 1 0>,
				<DCC_READ 0x96f9240 1 0>,
				<DCC_READ 0x96f926c 1 0>,
				<DCC_READ 0x96f9394 1 0>,
				<DCC_READ 0x96f939c 1 0>,
				<DCC_READ 0x96f9704 1 0>,
				<DCC_READ 0x96f970c 1 0>,
				<DCC_READ 0x9730868 1 0>,
				<DCC_READ 0x9730870 1 0>,
				<DCC_READ 0x9731004 1 0>,
				<DCC_READ 0x973100c 1 0>,
				<DCC_READ 0x9731014 1 0>,
				<DCC_READ 0x9731204 1 0>,
				<DCC_READ 0x973120c 1 0>,
				<DCC_READ 0x9731214 1 0>,
				<DCC_READ 0x9731504 1 0>,
				<DCC_READ 0x973150c 1 0>,
				<DCC_READ 0x9731514 1 0>,
				<DCC_READ 0x9731604 1 0>,
				<DCC_READ 0x9738100 1 0>,
				<DCC_READ 0x973813c 1 0>,
				<DCC_READ 0x9738500 1 0>,
				<DCC_READ 0x973853c 1 0>,
				<DCC_READ 0x9738a04 1 0>,
				<DCC_READ 0x9738a18 1 0>,
				<DCC_READ 0x9738ea8 1 0>,
				<DCC_READ 0x9739044 1 0>,
				<DCC_READ 0x973904c 1 0>,
				<DCC_READ 0x9739054 1 0>,
				<DCC_READ 0x973905c 1 0>,
				<DCC_READ 0x973910c 2 0>,
				<DCC_READ 0x9739204 1 0>,
				<DCC_READ 0x973920c 1 0>,
				<DCC_READ 0x9739238 1 0>,
				<DCC_READ 0x9739240 1 0>,
				<DCC_READ 0x973926c 1 0>,
				<DCC_READ 0x9739394 1 0>,
				<DCC_READ 0x973939c 1 0>,
				<DCC_READ 0x9739704 1 0>,
				<DCC_READ 0x973970c 1 0>,
				<DCC_READ 0x9770868 1 0>,
				<DCC_READ 0x9770870 1 0>,
				<DCC_READ 0x9771004 1 0>,
				<DCC_READ 0x977100c 1 0>,
				<DCC_READ 0x9771014 1 0>,
				<DCC_READ 0x9771204 1 0>,
				<DCC_READ 0x977120c 1 0>,
				<DCC_READ 0x9771214 1 0>,
				<DCC_READ 0x9771504 1 0>,
				<DCC_READ 0x977150c 1 0>,
				<DCC_READ 0x9771514 1 0>,
				<DCC_READ 0x9771604 1 0>,
				<DCC_READ 0x9778100 1 0>,
				<DCC_READ 0x977813c 1 0>,
				<DCC_READ 0x9778500 1 0>,
				<DCC_READ 0x977853c 1 0>,
				<DCC_READ 0x9778a04 1 0>,
				<DCC_READ 0x9778a18 1 0>,
				<DCC_READ 0x9778ea8 1 0>,
				<DCC_READ 0x9779044 1 0>,
				<DCC_READ 0x977904c 1 0>,
				<DCC_READ 0x9779054 1 0>,
				<DCC_READ 0x977905c 1 0>,
				<DCC_READ 0x977910c 2 0>,
				<DCC_READ 0x9779204 1 0>,
				<DCC_READ 0x977920c 1 0>,
				<DCC_READ 0x9779238 1 0>,
				<DCC_READ 0x9779240 1 0>,
				<DCC_READ 0x977926c 1 0>,
				<DCC_READ 0x9779394 1 0>,
				<DCC_READ 0x977939c 1 0>,
				<DCC_READ 0x9779704 1 0>,
				<DCC_READ 0x977970c 1 0>,
				<DCC_READ 0x910d100 3 0>,
				<DCC_READ 0x914d100 3 0>,
				<DCC_READ 0x918d100 4 0>,
				<DCC_READ 0x91a5100 1 0>,
				<DCC_READ 0x91ad100 1 0>,
				<DCC_READ 0x610110 5 0>,
				<DCC_WRITE 0x06e0a00c 0x00600007 1>,
				<DCC_WRITE 0x06e0a01c 0x00136800 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136810 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136820 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136830 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136840 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136850 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136860 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136870 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003e9a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003c0a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003d1a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003d2a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003d5a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003d6a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003e8a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003eea0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003b1a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003b2a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003b5a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003b6a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003c2a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003c5a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003c6a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a014 0x0002000c 1>,
				<DCC_WRITE 0x06e0a01c 0x000368b0 1>,
				<DCC_WRITE 0x06e0a01c 0x00000ba8 1>,
				<DCC_WRITE 0x06e0a01c 0x0013b6a0 1>,
				<DCC_WRITE 0x06e0a01c 0x00f1e000 1>,
				<DCC_WRITE 0x06e0a008 0x00000007 1>,
				<DCC_READ 0x09067e00 124 0>;
		};

		link_list2 {
			qcom,curr-link-list = <4>;
			qcom,data-sink = "sram";
			qcom,link-list = <DCC_READ 0x9050078 1 0>,
				<DCC_READ 0x9050110 8 0>,
				<DCC_READ 0x9080058 2 0>,
				<DCC_READ 0x90800c8 1 0>,
				<DCC_READ 0x90800d4 1 0>,
				<DCC_READ 0x90800e0 1 0>,
				<DCC_READ 0x90800ec 1 0>,
				<DCC_READ 0x90800f8 1 0>,
				<DCC_READ 0x9084030 1 0>,
				<DCC_READ 0x9084038 2 0>,
				<DCC_READ 0x90840e4 1 0>,
				<DCC_READ 0x90840f4 1 0>,
				<DCC_READ 0x9084104 2 0>,
				<DCC_READ 0x9084194 1 0>,
				<DCC_READ 0x9084804 1 0>,
				<DCC_READ 0x908480c 1 0>,
				<DCC_READ 0x9084844 1 0>,
				<DCC_READ 0x9084850 2 0>,
				<DCC_READ 0x9084860 3 0>,
				<DCC_READ 0x9084888 1 0>,
				<DCC_READ 0x908488c 1 0>,
				<DCC_READ 0x9084900 1 0>,
				<DCC_READ 0x908409c 1 0>,
				<DCC_READ 0x90840a0 1 0>,
				<DCC_READ 0x908426c 1 0>,
				<DCC_READ 0x908439c 1 0>,
				<DCC_READ 0x9085124 1 0>,
				<DCC_READ 0x90ba280 1 0>,
				<DCC_READ 0x90ba288 7 0>,
				<DCC_READ 0x9258610 4 0>,
				<DCC_READ 0x92d8610 4 0>,
				<DCC_READ 0x9358610 4 0>,
				<DCC_READ 0x93d8610 4 0>,
				<DCC_READ 0x9220344 8 0>,
				<DCC_READ 0x9220370 6 0>,
				<DCC_READ 0x9220480 1 0>,
				<DCC_READ 0x9222400 1 0>,
				<DCC_READ 0x922240c 1 0>,
				<DCC_READ 0x9223214 2 0>,
				<DCC_READ 0x9223220 3 0>,
				<DCC_READ 0x9223308 1 0>,
				<DCC_READ 0x9223318 1 0>,
				<DCC_READ 0x9232100 1 0>,
				<DCC_READ 0x9236040 6 0>,
				<DCC_READ 0x92360b0 1 0>,
				<DCC_READ 0x923a004 4 0>,
				<DCC_READ 0x923e030 2 0>,
				<DCC_READ 0x9241000 1 0>,
				<DCC_READ 0x9242028 1 0>,
				<DCC_READ 0x9242044 3 0>,
				<DCC_READ 0x9242070 1 0>,
				<DCC_READ 0x9248030 1 0>,
				<DCC_READ 0x9248048 8 0>,
				<DCC_READ 0x92a0344 8 0>,
				<DCC_READ 0x92a0370 6 0>,
				<DCC_READ 0x92a0480 1 0>,
				<DCC_READ 0x92a2400 1 0>,
				<DCC_READ 0x92a240c 1 0>,
				<DCC_READ 0x92a3214 2 0>,
				<DCC_READ 0x92a3220 3 0>,
				<DCC_READ 0x92a3308 1 0>,
				<DCC_READ 0x92a3318 1 0>,
				<DCC_READ 0x92b2100 1 0>,
				<DCC_READ 0x92b6040 6 0>,
				<DCC_READ 0x92b60b0 1 0>,
				<DCC_READ 0x92ba004 4 0>,
				<DCC_READ 0x92be030 2 0>,
				<DCC_READ 0x92c1000 1 0>,
				<DCC_READ 0x92c2028 1 0>,
				<DCC_READ 0x92c2044 3 0>,
				<DCC_READ 0x92c2070 1 0>,
				<DCC_READ 0x92c8030 1 0>,
				<DCC_READ 0x92c8048 8 0>,
				<DCC_READ 0x9320344 8 0>,
				<DCC_READ 0x9320370 6 0>,
				<DCC_READ 0x9320480 1 0>,
				<DCC_READ 0x9322400 1 0>,
				<DCC_READ 0x932240c 1 0>,
				<DCC_READ 0x9323214 2 0>,
				<DCC_READ 0x9323220 3 0>,
				<DCC_READ 0x9323308 1 0>,
				<DCC_READ 0x9323318 1 0>,
				<DCC_READ 0x9332100 1 0>,
				<DCC_READ 0x9336040 6 0>,
				<DCC_READ 0x93360b0 1 0>,
				<DCC_READ 0x933a004 4 0>,
				<DCC_READ 0x933e030 2 0>,
				<DCC_READ 0x9341000 1 0>,
				<DCC_READ 0x9342028 1 0>,
				<DCC_READ 0x9342044 3 0>,
				<DCC_READ 0x9342070 1 0>,
				<DCC_READ 0x9348030 1 0>,
				<DCC_READ 0x9348048 8 0>,
				<DCC_READ 0x93a0344 8 0>,
				<DCC_READ 0x93a0370 6 0>,
				<DCC_READ 0x93a0480 1 0>,
				<DCC_READ 0x93a2400 1 0>,
				<DCC_READ 0x93a240c 1 0>,
				<DCC_READ 0x93a3214 2 0>,
				<DCC_READ 0x93a3220 3 0>,
				<DCC_READ 0x93a3308 1 0>,
				<DCC_READ 0x93a3318 1 0>,
				<DCC_READ 0x93b2100 1 0>,
				<DCC_READ 0x93b6040 6 0>,
				<DCC_READ 0x93b60b0 1 0>,
				<DCC_READ 0x93ba004 4 0>,
				<DCC_READ 0x93be030 2 0>,
				<DCC_READ 0x93c1000 1 0>,
				<DCC_READ 0x93c2028 1 0>,
				<DCC_READ 0x93c2044 3 0>,
				<DCC_READ 0x93c2070 1 0>,
				<DCC_READ 0x93c8030 1 0>,
				<DCC_READ 0x93c8048 8 0>,
				<DCC_READ 0x9270080 1 0>,
				<DCC_READ 0x9270310 1 0>,
				<DCC_READ 0x9270400 1 0>,
				<DCC_READ 0x9270410 6 0>,
				<DCC_READ 0x9270430 1 0>,
				<DCC_READ 0x9270440 1 0>,
				<DCC_READ 0x9270448 1 0>,
				<DCC_READ 0x92704a0 1 0>,
				<DCC_READ 0x92704b0 1 0>,
				<DCC_READ 0x92704b8 2 0>,
				<DCC_READ 0x92704d0 2 0>,
				<DCC_READ 0x9271400 1 0>,
				<DCC_READ 0x9271408 1 0>,
				<DCC_READ 0x927341c 1 0>,
				<DCC_READ 0x92753b0 1 0>,
				<DCC_READ 0x9275804 1 0>,
				<DCC_READ 0x9275c1c 1 0>,
				<DCC_READ 0x9275c2c 1 0>,
				<DCC_READ 0x9275c38 1 0>,
				<DCC_READ 0x9276418 2 0>,
				<DCC_READ 0x9279100 1 0>,
				<DCC_READ 0x9279110 1 0>,
				<DCC_READ 0x9279120 1 0>,
				<DCC_READ 0x9279180 2 0>,
				<DCC_READ 0x92f0080 1 0>,
				<DCC_READ 0x92f0310 1 0>,
				<DCC_READ 0x92f0400 1 0>,
				<DCC_READ 0x92f0410 6 0>,
				<DCC_READ 0x92f0430 1 0>,
				<DCC_READ 0x92f0440 1 0>,
				<DCC_READ 0x92f0448 1 0>,
				<DCC_READ 0x92f04a0 1 0>,
				<DCC_READ 0x92f04b0 1 0>,
				<DCC_READ 0x92f04b8 2 0>,
				<DCC_READ 0x92f04d0 2 0>,
				<DCC_READ 0x92f1400 1 0>,
				<DCC_READ 0x92f1408 1 0>,
				<DCC_READ 0x92f341c 1 0>,
				<DCC_READ 0x92f53b0 1 0>,
				<DCC_READ 0x92f5804 1 0>,
				<DCC_READ 0x92f5c1c 1 0>,
				<DCC_READ 0x92f5c2c 1 0>,
				<DCC_READ 0x92f5c38 1 0>,
				<DCC_READ 0x92f6418 2 0>,
				<DCC_READ 0x92f9100 1 0>,
				<DCC_READ 0x92f9110 1 0>,
				<DCC_READ 0x92f9120 1 0>,
				<DCC_READ 0x92f9180 2 0>,
				<DCC_READ 0x9370080 1 0>,
				<DCC_READ 0x9370310 1 0>,
				<DCC_READ 0x9370400 1 0>,
				<DCC_READ 0x9370410 6 0>,
				<DCC_READ 0x9370430 1 0>,
				<DCC_READ 0x9370440 1 0>,
				<DCC_READ 0x9370448 1 0>,
				<DCC_READ 0x93704a0 1 0>,
				<DCC_READ 0x93704b0 1 0>,
				<DCC_READ 0x93704b8 2 0>,
				<DCC_READ 0x93704d0 2 0>,
				<DCC_READ 0x9371400 1 0>,
				<DCC_READ 0x9371408 1 0>,
				<DCC_READ 0x937341c 1 0>,
				<DCC_READ 0x93753b0 1 0>,
				<DCC_READ 0x9375804 1 0>,
				<DCC_READ 0x9375c1c 1 0>,
				<DCC_READ 0x9375c2c 1 0>,
				<DCC_READ 0x9375c38 1 0>,
				<DCC_READ 0x9376418 2 0>,
				<DCC_READ 0x9379100 1 0>,
				<DCC_READ 0x9379110 1 0>,
				<DCC_READ 0x9379120 1 0>,
				<DCC_READ 0x9379180 2 0>,
				<DCC_READ 0x93f0080 1 0>,
				<DCC_READ 0x93f0310 1 0>,
				<DCC_READ 0x93f0400 1 0>,
				<DCC_READ 0x93f0410 6 0>,
				<DCC_READ 0x93f0430 1 0>,
				<DCC_READ 0x93f0440 1 0>,
				<DCC_READ 0x93f0448 1 0>,
				<DCC_READ 0x93f04a0 1 0>,
				<DCC_READ 0x93f04b0 1 0>,
				<DCC_READ 0x93f04b8 2 0>,
				<DCC_READ 0x93f04d0 2 0>,
				<DCC_READ 0x93f1400 1 0>,
				<DCC_READ 0x93f1408 1 0>,
				<DCC_READ 0x93f341c 1 0>,
				<DCC_READ 0x93f53b0 1 0>,
				<DCC_READ 0x93f5804 1 0>,
				<DCC_READ 0x93f5c1c 1 0>,
				<DCC_READ 0x93f5c2c 1 0>,
				<DCC_READ 0x93f5c38 1 0>,
				<DCC_READ 0x93f6418 2 0>,
				<DCC_READ 0x93f9100 1 0>,
				<DCC_READ 0x93f9110 1 0>,
				<DCC_READ 0x93f9120 1 0>,
				<DCC_READ 0x93f9180 2 0>,
				<DCC_READ 0x9260080 1 0>,
				<DCC_READ 0x9260400 1 0>,
				<DCC_READ 0x9260410 3 0>,
				<DCC_READ 0x9260420 2 0>,
				<DCC_READ 0x9260430 1 0>,
				<DCC_READ 0x9260440 1 0>,
				<DCC_READ 0x9260448 1 0>,
				<DCC_READ 0x92604a0 1 0>,
				<DCC_READ 0x92604b0 1 0>,
				<DCC_READ 0x92604b8 2 0>,
				<DCC_READ 0x92604d0 2 0>,
				<DCC_READ 0x9261400 1 0>,
				<DCC_READ 0x9263410 1 0>,
				<DCC_READ 0x92653b0 1 0>,
				<DCC_READ 0x9265804 1 0>,
				<DCC_READ 0x9265b1c 1 0>,
				<DCC_READ 0x9265b2c 1 0>,
				<DCC_READ 0x9265b38 1 0>,
				<DCC_READ 0x9269100 1 0>,
				<DCC_READ 0x9269108 1 0>,
				<DCC_READ 0x9269110 1 0>,
				<DCC_READ 0x9269118 1 0>,
				<DCC_READ 0x9269120 1 0>,
				<DCC_READ 0x9269180 2 0>,
				<DCC_READ 0x92e0080 1 0>,
				<DCC_READ 0x92e0400 1 0>,
				<DCC_READ 0x92e0410 3 0>,
				<DCC_READ 0x92e0420 2 0>,
				<DCC_READ 0x92e0430 1 0>,
				<DCC_READ 0x92e0440 1 0>,
				<DCC_READ 0x92e0448 1 0>,
				<DCC_READ 0x92e04a0 1 0>,
				<DCC_READ 0x92e04b0 1 0>,
				<DCC_READ 0x92e04b8 2 0>,
				<DCC_READ 0x92e04d0 2 0>,
				<DCC_READ 0x92e1400 1 0>,
				<DCC_READ 0x92e3410 1 0>,
				<DCC_READ 0x92e53b0 1 0>,
				<DCC_READ 0x92e5804 1 0>,
				<DCC_READ 0x92e5b1c 1 0>,
				<DCC_READ 0x92e5b2c 1 0>,
				<DCC_READ 0x92e5b38 1 0>,
				<DCC_READ 0x92e9100 1 0>,
				<DCC_READ 0x92e9108 1 0>,
				<DCC_READ 0x92e9110 1 0>,
				<DCC_READ 0x92e9118 1 0>,
				<DCC_READ 0x92e9120 1 0>,
				<DCC_READ 0x92e9180 2 0>,
				<DCC_READ 0x9360080 1 0>,
				<DCC_READ 0x9360400 1 0>,
				<DCC_READ 0x9360410 3 0>,
				<DCC_READ 0x9360420 2 0>,
				<DCC_READ 0x9360430 1 0>,
				<DCC_READ 0x9360440 1 0>,
				<DCC_READ 0x9360448 1 0>,
				<DCC_READ 0x93604a0 1 0>,
				<DCC_READ 0x93604b0 1 0>,
				<DCC_READ 0x93604b8 2 0>,
				<DCC_READ 0x93604d0 2 0>,
				<DCC_READ 0x9361400 1 0>,
				<DCC_READ 0x9363410 1 0>,
				<DCC_READ 0x93653b0 1 0>,
				<DCC_READ 0x9365804 1 0>,
				<DCC_READ 0x9365b1c 1 0>,
				<DCC_READ 0x9365b2c 1 0>,
				<DCC_READ 0x9365b38 1 0>,
				<DCC_READ 0x9369100 1 0>,
				<DCC_READ 0x9369108 1 0>,
				<DCC_READ 0x9369110 1 0>,
				<DCC_READ 0x9369118 1 0>,
				<DCC_READ 0x9369120 1 0>,
				<DCC_READ 0x9369180 2 0>,
				<DCC_READ 0x93e0080 1 0>,
				<DCC_READ 0x93e0400 1 0>,
				<DCC_READ 0x93e0410 3 0>,
				<DCC_READ 0x93e0420 2 0>,
				<DCC_READ 0x93e0430 1 0>,
				<DCC_READ 0x93e0440 1 0>,
				<DCC_READ 0x93e0448 1 0>,
				<DCC_READ 0x93e04a0 1 0>,
				<DCC_READ 0x93e04b0 1 0>,
				<DCC_READ 0x93e04b8 2 0>,
				<DCC_READ 0x93e04d0 2 0>,
				<DCC_READ 0x93e1400 1 0>,
				<DCC_READ 0x93e3410 1 0>,
				<DCC_READ 0x93e53b0 1 0>,
				<DCC_READ 0x93e5804 1 0>,
				<DCC_READ 0x93e5b1c 1 0>,
				<DCC_READ 0x93e5b2c 1 0>,
				<DCC_READ 0x93e5b38 1 0>,
				<DCC_READ 0x93e9100 1 0>,
				<DCC_READ 0x93e9108 1 0>,
				<DCC_READ 0x93e9110 1 0>,
				<DCC_READ 0x93e9118 1 0>,
				<DCC_READ 0x93e9120 1 0>,
				<DCC_READ 0x93e9180 2 0>,
				<DCC_READ 0x96b0868 1 0>,
				<DCC_READ 0x96b0870 1 0>,
				<DCC_READ 0x96b1004 1 0>,
				<DCC_READ 0x96b100c 1 0>,
				<DCC_READ 0x96b1014 1 0>,
				<DCC_READ 0x96b1204 1 0>,
				<DCC_READ 0x96b120c 1 0>,
				<DCC_READ 0x96b1214 1 0>,
				<DCC_READ 0x96b1504 1 0>,
				<DCC_READ 0x96b150c 1 0>,
				<DCC_READ 0x96b1514 1 0>,
				<DCC_READ 0x96b1604 1 0>,
				<DCC_READ 0x96b8100 1 0>,
				<DCC_READ 0x96b813c 1 0>,
				<DCC_READ 0x96b8500 1 0>,
				<DCC_READ 0x96b853c 1 0>,
				<DCC_READ 0x96b8a04 1 0>,
				<DCC_READ 0x96b8a18 1 0>,
				<DCC_READ 0x96b8ea8 1 0>,
				<DCC_READ 0x96b9044 1 0>,
				<DCC_READ 0x96b904c 1 0>,
				<DCC_READ 0x96b9054 1 0>,
				<DCC_READ 0x96b905c 1 0>,
				<DCC_READ 0x96b910c 2 0>,
				<DCC_READ 0x96b9204 1 0>,
				<DCC_READ 0x96b920c 1 0>,
				<DCC_READ 0x96b9238 1 0>,
				<DCC_READ 0x96b9240 1 0>,
				<DCC_READ 0x96b926c 1 0>,
				<DCC_READ 0x96b9394 1 0>,
				<DCC_READ 0x96b939c 1 0>,
				<DCC_READ 0x96b9704 1 0>,
				<DCC_READ 0x96b970c 1 0>,
				<DCC_READ 0x96f0868 1 0>,
				<DCC_READ 0x96f0870 1 0>,
				<DCC_READ 0x96f1004 1 0>,
				<DCC_READ 0x96f100c 1 0>,
				<DCC_READ 0x96f1014 1 0>,
				<DCC_READ 0x96f1204 1 0>,
				<DCC_READ 0x96f120c 1 0>,
				<DCC_READ 0x96f1214 1 0>,
				<DCC_READ 0x96f1504 1 0>,
				<DCC_READ 0x96f150c 1 0>,
				<DCC_READ 0x96f1514 1 0>,
				<DCC_READ 0x96f1604 1 0>,
				<DCC_READ 0x96f8100 1 0>,
				<DCC_READ 0x96f813c 1 0>,
				<DCC_READ 0x96f8500 1 0>,
				<DCC_READ 0x96f853c 1 0>,
				<DCC_READ 0x96f8a04 1 0>,
				<DCC_READ 0x96f8a18 1 0>,
				<DCC_READ 0x96f8ea8 1 0>,
				<DCC_READ 0x96f9044 1 0>,
				<DCC_READ 0x96f904c 1 0>,
				<DCC_READ 0x96f9054 1 0>,
				<DCC_READ 0x96f905c 1 0>,
				<DCC_READ 0x96f910c 2 0>,
				<DCC_READ 0x96f9204 1 0>,
				<DCC_READ 0x96f920c 1 0>,
				<DCC_READ 0x96f9238 1 0>,
				<DCC_READ 0x96f9240 1 0>,
				<DCC_READ 0x96f926c 1 0>,
				<DCC_READ 0x96f9394 1 0>,
				<DCC_READ 0x96f939c 1 0>,
				<DCC_READ 0x96f9704 1 0>,
				<DCC_READ 0x96f970c 1 0>,
				<DCC_READ 0x9730868 1 0>,
				<DCC_READ 0x9730870 1 0>,
				<DCC_READ 0x9731004 1 0>,
				<DCC_READ 0x973100c 1 0>,
				<DCC_READ 0x9731014 1 0>,
				<DCC_READ 0x9731204 1 0>,
				<DCC_READ 0x973120c 1 0>,
				<DCC_READ 0x9731214 1 0>,
				<DCC_READ 0x9731504 1 0>,
				<DCC_READ 0x973150c 1 0>,
				<DCC_READ 0x9731514 1 0>,
				<DCC_READ 0x9731604 1 0>,
				<DCC_READ 0x9738100 1 0>,
				<DCC_READ 0x973813c 1 0>,
				<DCC_READ 0x9738500 1 0>,
				<DCC_READ 0x973853c 1 0>,
				<DCC_READ 0x9738a04 1 0>,
				<DCC_READ 0x9738a18 1 0>,
				<DCC_READ 0x9738ea8 1 0>,
				<DCC_READ 0x9739044 1 0>,
				<DCC_READ 0x973904c 1 0>,
				<DCC_READ 0x9739054 1 0>,
				<DCC_READ 0x973905c 1 0>,
				<DCC_READ 0x973910c 2 0>,
				<DCC_READ 0x9739204 1 0>,
				<DCC_READ 0x973920c 1 0>,
				<DCC_READ 0x9739238 1 0>,
				<DCC_READ 0x9739240 1 0>,
				<DCC_READ 0x973926c 1 0>,
				<DCC_READ 0x9739394 1 0>,
				<DCC_READ 0x973939c 1 0>,
				<DCC_READ 0x9739704 1 0>,
				<DCC_READ 0x973970c 1 0>,
				<DCC_READ 0x9770868 1 0>,
				<DCC_READ 0x9770870 1 0>,
				<DCC_READ 0x9771004 1 0>,
				<DCC_READ 0x977100c 1 0>,
				<DCC_READ 0x9771014 1 0>,
				<DCC_READ 0x9771204 1 0>,
				<DCC_READ 0x977120c 1 0>,
				<DCC_READ 0x9771214 1 0>,
				<DCC_READ 0x9771504 1 0>,
				<DCC_READ 0x977150c 1 0>,
				<DCC_READ 0x9771514 1 0>,
				<DCC_READ 0x9771604 1 0>,
				<DCC_READ 0x9778100 1 0>,
				<DCC_READ 0x977813c 1 0>,
				<DCC_READ 0x9778500 1 0>,
				<DCC_READ 0x977853c 1 0>,
				<DCC_READ 0x9778a04 1 0>,
				<DCC_READ 0x9778a18 1 0>,
				<DCC_READ 0x9778ea8 1 0>,
				<DCC_READ 0x9779044 1 0>,
				<DCC_READ 0x977904c 1 0>,
				<DCC_READ 0x9779054 1 0>,
				<DCC_READ 0x977905c 1 0>,
				<DCC_READ 0x977910c 2 0>,
				<DCC_READ 0x9779204 1 0>,
				<DCC_READ 0x977920c 1 0>,
				<DCC_READ 0x9779238 1 0>,
				<DCC_READ 0x9779240 1 0>,
				<DCC_READ 0x977926c 1 0>,
				<DCC_READ 0x9779394 1 0>,
				<DCC_READ 0x977939c 1 0>,
				<DCC_READ 0x9779704 1 0>,
				<DCC_READ 0x977970c 1 0>,
				<DCC_READ 0x910d100 3 0>,
				<DCC_READ 0x914d100 3 0>,
				<DCC_READ 0x918d100 4 0>,
				<DCC_READ 0x91a5100 1 0>,
				<DCC_READ 0x91ad100 1 0>,
				<DCC_READ 0x610110 5 0>,
				<DCC_WRITE 0x06e0a00c 0x00600007 1>,
				<DCC_WRITE 0x06e0a01c 0x00136800 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136810 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136820 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136830 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136840 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136850 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136860 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x00136870 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003e9a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003c0a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003d1a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003d2a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003d5a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003d6a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003e8a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003eea0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003b1a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003b2a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003b5a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003b6a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003c2a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003c5a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a01c 0x0003c6a0 1>,
				<DCC_WRITE 0x06e0a01c 0x001368a0 1>,
				<DCC_READ 0x06e0a014 1 1>,
				<DCC_WRITE 0x06e0a014 0x0002000c 1>,
				<DCC_WRITE 0x06e0a01c 0x000368b0 1>,
				<DCC_WRITE 0x06e0a01c 0x00000ba8 1>,
				<DCC_WRITE 0x06e0a01c 0x0013b6a0 1>,
				<DCC_WRITE 0x06e0a01c 0x00f1e000 1>,
				<DCC_WRITE 0x06e0a008 0x00000007 1>,
				<DCC_READ 0x09067e00 124 0>;
		};

		link_list3 {
			qcom,curr-link-list = <3>;
			qcom,data-sink = "sram";
			qcom,link-list = <DCC_READ 0x18200400 1 0>,
				<DCC_READ 0x18200404 1 0>,
				<DCC_READ 0x18200408 1 0>,
				<DCC_READ 0x18200038 1 0>,
				<DCC_READ 0x18200040 1 0>,
				<DCC_READ 0x18200048 1 0>,
				<DCC_READ 0x18220038 1 0>,
				<DCC_READ 0x18220040 1 0>,
				<DCC_READ 0x182200d0 1 0>,
				<DCC_READ 0x18200030 1 0>,
				<DCC_READ 0x18200010 1 0>,
				<DCC_READ 0x1822000c 1 0>,
				<DCC_READ 0x18220d14 1 0>,
				<DCC_READ 0x18220fb4 1 0>,
				<DCC_READ 0x18221254 1 0>,
				<DCC_READ 0x182214f4 1 0>,
				<DCC_READ 0x18221794 1 0>,
				<DCC_READ 0x18221a34 1 0>,
				<DCC_READ 0x18221cd4 1 0>,
				<DCC_READ 0x18221f74 1 0>,
				<DCC_READ 0x18220d18 1 0>,
				<DCC_READ 0x18220fb8 1 0>,
				<DCC_READ 0x18221258 1 0>,
				<DCC_READ 0x182214f8 1 0>,
				<DCC_READ 0x18221798 1 0>,
				<DCC_READ 0x18221a38 1 0>,
				<DCC_READ 0x18221cd8 1 0>,
				<DCC_READ 0x18221f78 1 0>,
				<DCC_READ 0x18220d00 1 0>,
				<DCC_READ 0x18220d04 1 0>,
				<DCC_READ 0x18220d1c 1 0>,
				<DCC_READ 0x18220fbc 1 0>,
				<DCC_READ 0x1822125c 1 0>,
				<DCC_READ 0x182214fc 1 0>,
				<DCC_READ 0x1822179c 1 0>,
				<DCC_READ 0x18221a3c 1 0>,
				<DCC_READ 0x18221cdc 1 0>,
				<DCC_READ 0x18221f7c 1 0>,
				<DCC_READ 0x18221274 1 0>,
				<DCC_READ 0x18221288 1 0>,
				<DCC_READ 0x1822129c 1 0>,
				<DCC_READ 0x182212b0 1 0>,
				<DCC_READ 0x182212c4 1 0>,
				<DCC_READ 0x182212d8 1 0>,
				<DCC_READ 0x182212ec 1 0>,
				<DCC_READ 0x18221300 1 0>,
				<DCC_READ 0x18221314 1 0>,
				<DCC_READ 0x18221328 1 0>,
				<DCC_READ 0x1822133c 1 0>,
				<DCC_READ 0x18221350 1 0>,
				<DCC_READ 0x18221364 1 0>,
				<DCC_READ 0x18221378 1 0>,
				<DCC_READ 0x1822138c 1 0>,
				<DCC_READ 0x182213a0 1 0>,
				<DCC_READ 0x18221514 1 0>,
				<DCC_READ 0x18221528 1 0>,
				<DCC_READ 0x1822153c 1 0>,
				<DCC_READ 0x18221550 1 0>,
				<DCC_READ 0x18221564 1 0>,
				<DCC_READ 0x18221578 1 0>,
				<DCC_READ 0x1822158c 1 0>,
				<DCC_READ 0x182215a0 1 0>,
				<DCC_READ 0x182215b4 1 0>,
				<DCC_READ 0x182215c8 1 0>,
				<DCC_READ 0x182215dc 1 0>,
				<DCC_READ 0x182215f0 1 0>,
				<DCC_READ 0x18221604 1 0>,
				<DCC_READ 0x18221618 1 0>,
				<DCC_READ 0x1822162c 1 0>,
				<DCC_READ 0x18221640 1 0>,
				<DCC_READ 0x182217b4 1 0>,
				<DCC_READ 0x182217c8 1 0>,
				<DCC_READ 0x182217dc 1 0>,
				<DCC_READ 0x182217f0 1 0>,
				<DCC_READ 0x18221804 1 0>,
				<DCC_READ 0x18221818 1 0>,
				<DCC_READ 0x1822182c 1 0>,
				<DCC_READ 0x18221840 1 0>,
				<DCC_READ 0x18221854 1 0>,
				<DCC_READ 0x18221868 1 0>,
				<DCC_READ 0x1822187c 1 0>,
				<DCC_READ 0x18221890 1 0>,
				<DCC_READ 0x182218a4 1 0>,
				<DCC_READ 0x182218b8 1 0>,
				<DCC_READ 0x182218cc 1 0>,
				<DCC_READ 0x182218e0 1 0>,
				<DCC_READ 0x18221a54 1 0>,
				<DCC_READ 0x18221a68 1 0>,
				<DCC_READ 0x18221a7c 1 0>,
				<DCC_READ 0x18221a90 1 0>,
				<DCC_READ 0x18221aa4 1 0>,
				<DCC_READ 0x18221ab8 1 0>,
				<DCC_READ 0x18221acc 1 0>,
				<DCC_READ 0x18221ae0 1 0>,
				<DCC_READ 0x18221af4 1 0>,
				<DCC_READ 0x18221b08 1 0>,
				<DCC_READ 0x18221b1c 1 0>,
				<DCC_READ 0x18221b30 1 0>,
				<DCC_READ 0x18221b44 1 0>,
				<DCC_READ 0x18221b58 1 0>,
				<DCC_READ 0x18221b6c 1 0>,
				<DCC_READ 0x18221b80 1 0>,
				<DCC_READ 0x18221cf4 1 0>,
				<DCC_READ 0x18221d08 1 0>,
				<DCC_READ 0x18221d1c 1 0>,
				<DCC_READ 0x18221d30 1 0>,
				<DCC_READ 0x18221d44 1 0>,
				<DCC_READ 0x18221d58 1 0>,
				<DCC_READ 0x18221d6c 1 0>,
				<DCC_READ 0x18221d80 1 0>,
				<DCC_READ 0x18221d94 1 0>,
				<DCC_READ 0x18221da8 1 0>,
				<DCC_READ 0x18221dbc 1 0>,
				<DCC_READ 0x18221dd0 1 0>,
				<DCC_READ 0x18221de4 1 0>,
				<DCC_READ 0x18221df8 1 0>,
				<DCC_READ 0x18221e0c 1 0>,
				<DCC_READ 0x18221e20 1 0>,
				<DCC_READ 0x18221f94 1 0>,
				<DCC_READ 0x18221fa8 1 0>,
				<DCC_READ 0x18221fbc 1 0>,
				<DCC_READ 0x18221fd0 1 0>,
				<DCC_READ 0x18221fe4 1 0>,
				<DCC_READ 0x18221ff8 1 0>,
				<DCC_READ 0x1822200c 1 0>,
				<DCC_READ 0x18222020 1 0>,
				<DCC_READ 0x18222034 1 0>,
				<DCC_READ 0x18222048 1 0>,
				<DCC_READ 0x1822205c 1 0>,
				<DCC_READ 0x18222070 1 0>,
				<DCC_READ 0x18222084 1 0>,
				<DCC_READ 0x18222098 1 0>,
				<DCC_READ 0x182220ac 1 0>,
				<DCC_READ 0x182220c0 1 0>,
				<DCC_READ 0x18221278 1 0>,
				<DCC_READ 0x1822128c 1 0>,
				<DCC_READ 0x182212a0 1 0>,
				<DCC_READ 0x182212b4 1 0>,
				<DCC_READ 0x182212c8 1 0>,
				<DCC_READ 0x182212dc 1 0>,
				<DCC_READ 0x182212f0 1 0>,
				<DCC_READ 0x18221304 1 0>,
				<DCC_READ 0x18221318 1 0>,
				<DCC_READ 0x1822132c 1 0>,
				<DCC_READ 0x18221340 1 0>,
				<DCC_READ 0x18221354 1 0>,
				<DCC_READ 0x18221368 1 0>,
				<DCC_READ 0x1822137c 1 0>,
				<DCC_READ 0x18221390 1 0>,
				<DCC_READ 0x182213a4 1 0>,
				<DCC_READ 0x18221518 1 0>,
				<DCC_READ 0x1822152c 1 0>,
				<DCC_READ 0x18221540 1 0>,
				<DCC_READ 0x18221554 1 0>,
				<DCC_READ 0x18221568 1 0>,
				<DCC_READ 0x1822157c 1 0>,
				<DCC_READ 0x18221590 1 0>,
				<DCC_READ 0x182215a4 1 0>,
				<DCC_READ 0x182215b8 1 0>,
				<DCC_READ 0x182215cc 1 0>,
				<DCC_READ 0x182215e0 1 0>,
				<DCC_READ 0x182215f4 1 0>,
				<DCC_READ 0x18221608 1 0>,
				<DCC_READ 0x1822161c 1 0>,
				<DCC_READ 0x18221630 1 0>,
				<DCC_READ 0x18221644 1 0>,
				<DCC_READ 0x182217b8 1 0>,
				<DCC_READ 0x182217cc 1 0>,
				<DCC_READ 0x182217e0 1 0>,
				<DCC_READ 0x182217f4 1 0>,
				<DCC_READ 0x18221808 1 0>,
				<DCC_READ 0x1822181c 1 0>,
				<DCC_READ 0x18221830 1 0>,
				<DCC_READ 0x18221844 1 0>,
				<DCC_READ 0x18221858 1 0>,
				<DCC_READ 0x1822186c 1 0>,
				<DCC_READ 0x18221880 1 0>,
				<DCC_READ 0x18221894 1 0>,
				<DCC_READ 0x182218a8 1 0>,
				<DCC_READ 0x182218bc 1 0>,
				<DCC_READ 0x182218d0 1 0>,
				<DCC_READ 0x182218e4 1 0>,
				<DCC_READ 0x18221a58 1 0>,
				<DCC_READ 0x18221a6c 1 0>,
				<DCC_READ 0x18221a80 1 0>,
				<DCC_READ 0x18221a94 1 0>,
				<DCC_READ 0x18221aa8 1 0>,
				<DCC_READ 0x18221abc 1 0>,
				<DCC_READ 0x18221ad0 1 0>,
				<DCC_READ 0x18221ae4 1 0>,
				<DCC_READ 0x18221af8 1 0>,
				<DCC_READ 0x18221b0c 1 0>,
				<DCC_READ 0x18221b20 1 0>,
				<DCC_READ 0x18221b34 1 0>,
				<DCC_READ 0x18221b48 1 0>,
				<DCC_READ 0x18221b5c 1 0>,
				<DCC_READ 0x18221b70 1 0>,
				<DCC_READ 0x18221b84 1 0>,
				<DCC_READ 0x18221cf8 1 0>,
				<DCC_READ 0x18221d0c 1 0>,
				<DCC_READ 0x18221d20 1 0>,
				<DCC_READ 0x18221d34 1 0>,
				<DCC_READ 0x18221d48 1 0>,
				<DCC_READ 0x18221d5c 1 0>,
				<DCC_READ 0x18221d70 1 0>,
				<DCC_READ 0x18221d84 1 0>,
				<DCC_READ 0x18221d98 1 0>,
				<DCC_READ 0x18221dac 1 0>,
				<DCC_READ 0x18221dc0 1 0>,
				<DCC_READ 0x18221dd4 1 0>,
				<DCC_READ 0x18221de8 1 0>,
				<DCC_READ 0x18221dfc 1 0>,
				<DCC_READ 0x18221e10 1 0>,
				<DCC_READ 0x18221e24 1 0>,
				<DCC_READ 0x18221f98 1 0>,
				<DCC_READ 0x18221fac 1 0>,
				<DCC_READ 0x18221fc0 1 0>,
				<DCC_READ 0x18221fd4 1 0>,
				<DCC_READ 0x18221fe8 1 0>,
				<DCC_READ 0x18221ffc 1 0>,
				<DCC_READ 0x18222010 1 0>,
				<DCC_READ 0x18222024 1 0>,
				<DCC_READ 0x18222038 1 0>,
				<DCC_READ 0x1822204c 1 0>,
				<DCC_READ 0x18222060 1 0>,
				<DCC_READ 0x18222074 1 0>,
				<DCC_READ 0x18222088 1 0>,
				<DCC_READ 0x1822209c 1 0>,
				<DCC_READ 0x182220b0 1 0>,
				<DCC_READ 0x182220c4 1 0>;
		};
	};

	cpu_pmu: cpu-pmu {
		compatible = "arm,armv8-pmuv3";
		qcom,irq-is-percpu;
		interrupts = <GIC_PPI 7 IRQ_TYPE_LEVEL_HIGH>;
	};

	qcom,msm-imem@146bf000 {
		compatible = "qcom,msm-imem";
		reg = <0x146bf000 0x1000>;
		ranges = <0x0 0x146bf000 0x1000>;
		#address-cells = <1>;
		#size-cells = <1>;

		mem_dump_table@10 {
			compatible = "qcom,msm-imem-mem_dump_table";
			reg = <0x10 0x8>;
		};

		restart_reason@65c {
			compatible = "qcom,msm-imem-restart_reason";
			reg = <0x65c 0x4>;
		};

		dload_type@1c {
			compatible = "qcom,msm-imem-dload-type";
			reg = <0x1c 0x4>;
		};

		boot_stats@6b0 {
			compatible = "qcom,msm-imem-boot_stats";
			reg = <0x6b0 0x20>;
		};

		kaslr_offset@6d0 {
			compatible = "qcom,msm-imem-kaslr_offset";
			reg = <0x6d0 0xc>;
		};

		pil@94c {
			compatible = "qcom,msm-imem-pil";
			reg = <0x94c 0xc8>;
		};

		pil@6dc {
			compatible = "qcom,msm-imem-pil-disable-timeout";
			reg = <0x6dc 0x4>;
		};

		diag_dload@c8 {
			compatible = "qcom,msm-imem-diag-dload";
			reg = <0xc8 0xc8>;
		};
	};

	dload_mode {
		compatible = "qcom,dload-mode";
	};

	tlmm: pinctrl@f000000 {
		compatible = "qcom,lahaina-pinctrl";
		reg = <0x0F000000 0x1000000>;
		interrupts = <GIC_SPI 208 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		interrupt-controller;
		#interrupt-cells = <2>;
		wakeup-parent = <&pdc>;
	};

	ipcc_mproc: qcom,ipcc@408000 {
		compatible = "qcom,ipcc";
		reg = <0x408000 0x1000>;
		interrupts = <GIC_SPI 229 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-controller;
		#interrupt-cells = <3>;
		#mbox-cells = <2>;
	};

	qcom,svm_neuron_block {
		compatible = "qcom,neuron-service";
		#address-cells = <1>;
		#size-cells = <0>;
		protocol {
			compatible = "qcom,neuron-protocol-block";
			processes = "server";
		};

		application {
			compatible = "qcom,neuron-block-server";
		};

		channel@0 {
			compatible = "qcom,neuron-channel-haven-shmem";
			reg = <0>;
			class = "message-queue";
			direction = "receive";
			max-size = <0 65536>;
			shared-buffer = <&chan0_shbuf>;
			qcom,primary;
			haven-label = <1>;
			peer-name = <2>;
		};

		channel@1 {
			compatible = "qcom,neuron-channel-haven-shmem";
			reg = <1>;
			class = "message-queue";
			direction = "send";
			max-size = <0 65536>;
			shared-buffer = <&chan1_shbuf>;
			qcom,primary;
			haven-label = <2>;
			peer-name = <2>;
		};
	};

	qcom,qsee_ipc_irq_bridge {
		compatible = "qcom,qsee-ipc-irq-bridge";

		qcom,qsee-ipc-irq-spss {
			qcom,dev-name = "qsee_ipc_irq_spss";
			interrupt-parent = <&ipcc_mproc>;
			interrupts = <IPCC_CLIENT_SPSS
				      IPCC_MPROC_SIGNAL_TZ
				      IRQ_TYPE_EDGE_RISING>;
			label = "spss";
		};
	};

	qrtr-haven {
		compatible = "qcom,qrtr-haven";
		qcom,master;
		haven-label = <3>;
		peer-name = <2>;
		shared-buffer = <&qrtr_shbuf>;
	};

	jtag_mm0: jtagmm@7040000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7040000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU0>;
	};

	jtag_mm1: jtagmm@7140000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7140000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU1>;
	};

	jtag_mm2: jtagmm@7240000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7240000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU2>;
	};

	jtag_mm3: jtagmm@7340000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7340000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU3>;
	};

	jtag_mm4: jtagmm@7440000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7440000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU4>;
	};

	jtag_mm5: jtagmm@7540000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7540000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU5>;
	};

	jtag_mm6: jtagmm@7640000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7640000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU6>;
	};

	jtag_mm7: jtagmm@7740000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7740000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU7>;
	};

	qcom,memshare {
		compatible = "qcom,memshare";

		qcom,client_1 {
			compatible = "qcom,memshare-peripheral";
			qcom,peripheral-size = <0x0>;
			qcom,client-id = <0>;
			qcom,allocate-boot-time;
			label = "modem";
		};

		qcom,client_2 {
			compatible = "qcom,memshare-peripheral";
			qcom,peripheral-size = <0x0>;
			qcom,client-id = <2>;
			label = "modem";
		};

		qcom,client_3 {
			compatible = "qcom,memshare-peripheral";
			qcom,peripheral-size = <0x500000>;
			memory-region = <&memshare_mem>;
			qcom,client-id = <1>;
			qcom,allocate-on-request;
			label = "modem";
		};
	};

	clocks {
		xo_board: xo-board {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <38400000>;
			clock-output-names = "xo_board";
		};

		sleep_clk: sleep-clk {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <32000>;
			clock-output-names = "sleep_clk";
		};
	};

	clock_aop: qcom,aopclk {
		compatible = "qcom,aop-qmp-clk";
		#clock-cells = <1>;
		mboxes = <&qmp_aop 0>;
		mbox-names = "qdss_clk";
	};

	clock_gcc: qcom,gcc@100000 {
		compatible = "qcom,lahaina-gcc", "syscon";
		reg = <0x100000 0x1f0000>;
		reg-names = "cc_base";
		vdd_cx-supply = <&VDD_CX_LEVEL>;
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	clock_videocc: qcom,videocc@abf0000 {
		compatible = "qcom,lahaina-videocc", "syscon";
		reg = <0xabf0000 0x10000>;
		reg-name = "cc_base";
		vdd_mm-supply = <&VDD_MM_LEVEL>;
		vdd_mx-supply = <&VDD_MXA_LEVEL>;
		interconnects = <&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_VENUS_CFG>;
		clocks = <&clock_gcc GCC_VIDEO_AHB_CLK>;
		clock-names = "iface";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	clock_camcc: qcom,camcc@ad00000 {
		compatible = "qcom,lahaina-camcc", "syscon";
		reg = <0xad00000 0x10000>;
		reg-names = "cc_base";
		vdd_mm-supply = <&VDD_MM_LEVEL>;
		vdd_mx-supply = <&VDD_MXA_LEVEL>;
		interconnects = <&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_CAMERA_CFG>;
		clocks = <&clock_gcc GCC_CAMERA_AHB_CLK>;
		clock-names = "iface";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	clock_dispcc: qcom,dispcc@af00000 {
		compatible = "qcom,lahaina-dispcc", "syscon";
		reg = <0xaf00000 0x20000>;
		reg-name = "cc_base";
		vdd_mm-supply = <&VDD_MM_LEVEL>;
		interconnects = <&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_DISPLAY_CFG>;
		clocks = <&clock_gcc GCC_DISP_AHB_CLK>;
		clock-names = "iface";
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	clock_gpucc: qcom,gpucc@3d90000 {
		compatible = "qcom,lahaina-gpucc", "syscon";
		reg = <0x3d90000 0x9000>;
		reg-names = "cc_base";
		vdd_mx-supply = <&VDD_MXA_LEVEL>;
		vdd_cx-supply = <&VDD_CX_LEVEL>;
		#clock-cells = <1>;
		#reset-cells = <1>;
	};

	clock_apsscc: syscon@182a0000 {
		compatible = "syscon";
		reg = <0x182a0000 0x1c>;
	};

	clock_mccc: syscon@90ba000 {
		compatible = "syscon";
		reg = <0x90ba000 0x54>;
	};

	clock_debugcc: qcom,cc-debug {
		compatible = "qcom,lahaina-debugcc";
		qcom,gcc = <&clock_gcc>;
		qcom,videocc = <&clock_videocc>;
		qcom,dispcc = <&clock_dispcc>;
		qcom,camcc = <&clock_camcc>;
		qcom,gpucc = <&clock_gpucc>;
		qcom,apsscc = <&clock_apsscc>;
		qcom,mccc = <&clock_mccc>;
		clock-names = "xo_clk_src";
		clocks = <&clock_rpmh RPMH_CXO_CLK>;
		#clock-cells = <1>;
	};

	cpufreq_hw: qcom,cpufreq-hw {
		compatible = "qcom,cpufreq-hw-epss";
		reg = <0x18591000 0x1000>, <0x18592000 0x1000>,
			<0x18593000 0x1000>;
		reg-names = "freq-domain0", "freq-domain1",
				"freq-domain2";

		clocks = <&clock_rpmh RPMH_CXO_CLK>, <&clock_gcc GCC_GPLL0>;
		clock-names = "xo", "alternate";

		qcom,lut-row-size = <4>;
		qcom,skip-enable-check;

		interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "dcvsh0_int", "dcvsh1_int", "dcvsh2_int";

		#freq-domain-cells = <2>;
	};

	/* CAM_CC GDSCs */
	cam_cc_bps_gdsc: qcom,gdsc@ad07004 {
		compatible = "qcom,gdsc";
		reg = <0xad07004 0x4>;
		regulator-name = "cam_cc_bps_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_CAMERA_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,support-hw-trigger;
		qcom,retain-regs;
	};

	cam_cc_ife_0_gdsc: qcom,gdsc@ad0a004 {
		compatible = "qcom,gdsc";
		reg = <0xad0a004 0x4>;
		regulator-name = "cam_cc_ife_0_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_CAMERA_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,retain-regs;
	};

	cam_cc_ife_1_gdsc: qcom,gdsc@ad0b004 {
		compatible = "qcom,gdsc";
		reg = <0xad0b004 0x4>;
		regulator-name = "cam_cc_ife_1_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_CAMERA_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,retain-regs;
	};

	cam_cc_ife_2_gdsc: qcom,gdsc@ad0b070 {
		compatible = "qcom,gdsc";
		reg = <0xad0b070 0x4>;
		regulator-name = "cam_cc_ife_2_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_CAMERA_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,retain-regs;
	};

	cam_cc_ipe_0_gdsc: qcom,gdsc@ad08004 {
		compatible = "qcom,gdsc";
		reg = <0xad08004 0x4>;
		regulator-name = "cam_cc_ipe_0_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_CAMERA_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,support-hw-trigger;
		qcom,retain-regs;
	};

	cam_cc_sbi_gdsc: qcom,gdsc@ad09004 {
		compatible = "qcom,gdsc";
		reg = <0xad09004 0x4>;
		regulator-name = "cam_cc_sbi_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_CAMERA_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,retain-regs;
	};

	cam_cc_titan_top_gdsc: qcom,gdsc@ad0c120 {
		compatible = "qcom,gdsc";
		reg = <0xad0c120 0x4>;
		regulator-name = "cam_cc_titan_top_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_CAMERA_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,retain-regs;
	};

	/* DISP_CC GDSCs */
	disp_cc_mdss_core_gdsc: qcom,gdsc@af03000 {
		compatible = "qcom,gdsc";
		reg = <0xaf03000 0x4>;
		regulator-name = "disp_cc_mdss_core_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_DISP_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,support-hw-trigger;
		qcom,retain-regs;
		proxy-supply = <&disp_cc_mdss_core_gdsc>;
		qcom,proxy-consumer-enable;
	};

	gcc_apcs_gdsc_vote_ctrl: syscon@152128 {
		compatible = "syscon";
		reg = <0x152128 0x4>;
	};

	/* GCC GDSCs */
	gcc_pcie_0_gdsc: qcom,gdsc@16b004 {
		compatible = "qcom,gdsc";
		reg = <0x16b004 0x4>;
		regulator-name = "gcc_pcie_0_gdsc";
		qcom,gds-timeout = <500>;
		parent-supply = <&VDD_CX_LEVEL>;
		qcom,retain-regs;
		qcom,no-status-check-on-disable;
		qcom,collapse-vote = <&gcc_apcs_gdsc_vote_ctrl 0>;
	};

	gcc_pcie_1_gdsc: qcom,gdsc@18d004 {
		compatible = "qcom,gdsc";
		reg = <0x18d004 0x4>;
		regulator-name = "gcc_pcie_1_gdsc";
		qcom,gds-timeout = <500>;
		parent-supply = <&VDD_CX_LEVEL>;
		qcom,retain-regs;
		qcom,no-status-check-on-disable;
		qcom,collapse-vote = <&gcc_apcs_gdsc_vote_ctrl 1>;
	};

	gcc_ufs_card_gdsc: qcom,gdsc@175004 {
		compatible = "qcom,gdsc";
		reg = <0x175004 0x4>;
		regulator-name = "gcc_ufs_card_gdsc";
		qcom,gds-timeout = <500>;
		parent-supply = <&VDD_CX_LEVEL>;
		qcom,retain-regs;
	};

	gcc_ufs_phy_gdsc: qcom,gdsc@177004 {
		compatible = "qcom,gdsc";
		reg = <0x177004 0x4>;
		regulator-name = "gcc_ufs_phy_gdsc";
		qcom,gds-timeout = <500>;
		parent-supply = <&VDD_CX_LEVEL>;
		qcom,retain-regs;
	};

	gcc_usb30_prim_gdsc: qcom,gdsc@10f004 {
		compatible = "qcom,gdsc";
		reg = <0x10f004 0x4>;
		regulator-name = "gcc_usb30_prim_gdsc";
		qcom,gds-timeout = <500>;
		qcom,retain-regs;
	};

	gcc_usb30_sec_gdsc: qcom,gdsc@110004 {
		compatible = "qcom,gdsc";
		reg = <0x110004 0x4>;
		regulator-name = "gcc_usb30_sec_gdsc";
		qcom,gds-timeout = <500>;
		qcom,retain-regs;
	};

	gcc_hlos1_vote_mmnoc_mmu_tbu_hf0_gdsc: qcom,gdsc@17d050 {
		compatible = "qcom,gdsc";
		reg = <0x17d050 0x4>;
		regulator-name = "gcc_hlos1_vote_mmnoc_mmu_tbu_hf0_gdsc";
		qcom,no-status-check-on-disable;
		qcom,gds-timeout = <500>;
	};

	gcc_hlos1_vote_mmnoc_mmu_tbu_hf1_gdsc: qcom,gdsc@17d058 {
		compatible = "qcom,gdsc";
		reg = <0x17d058 0x4>;
		regulator-name = "gcc_hlos1_vote_mmnoc_mmu_tbu_hf1_gdsc";
		qcom,no-status-check-on-disable;
		qcom,gds-timeout = <500>;
	};

	gcc_hlos1_vote_mmnoc_mmu_tbu_sf0_gdsc: qcom,gdsc@17d054 {
		compatible = "qcom,gdsc";
		reg = <0x17d054 0x4>;
		regulator-name = "gcc_hlos1_vote_mmnoc_mmu_tbu_sf0_gdsc";
		qcom,no-status-check-on-disable;
		qcom,gds-timeout = <500>;
	};

	gcc_hlos1_vote_mmnoc_mmu_tbu_sf1_gdsc: qcom,gdsc@17d06c {
		compatible = "qcom,gdsc";
		reg = <0x17d06c 0x4>;
		regulator-name = "gcc_hlos1_vote_mmnoc_mmu_tbu_sf1_gdsc";
		qcom,no-status-check-on-disable;
		qcom,gds-timeout = <500>;
	};

	/* GPU_CC GDSCs */
	gpu_cc_cx_hw_ctrl: syscon@3d91540 {
		compatible = "syscon";
		reg = <0x3d91540 0x4>;
	};

	gpu_cc_cx_gdsc: qcom,gdsc@3d9106c {
		compatible = "qcom,gdsc";
		reg = <0x3d9106c 0x4>;
		regulator-name = "gpu_cc_cx_gdsc";
		hw-ctrl-addr = <&gpu_cc_cx_hw_ctrl>;
		parent-supply = <&VDD_CX_LEVEL>;
		qcom,no-status-check-on-disable;
		qcom,clk-dis-wait-val = <8>;
		qcom,gds-timeout = <500>;
		qcom,retain-regs;
	};

	gpu_cc_gx_domain_addr: syscon@3d9158c {
		compatible = "syscon";
		reg = <0x3d9158c 0x4>;
	};

	gpu_cc_gx_sw_reset: syscon@3d91008 {
		compatible = "syscon";
		reg = <0x3d91008 0x4>;
	};

	gpu_cc_gx_gdsc: qcom,gdsc@3d9100c {
		compatible = "qcom,gdsc";
		reg = <0x3d9100c 0x4>;
		regulator-name = "gpu_cc_gx_gdsc";
		qcom,gds-timeout = <500>;
		domain-addr = <&gpu_cc_gx_domain_addr>;
		sw-reset = <&gpu_cc_gx_sw_reset>;
		parent-supply = <&VDD_GFX_LEVEL>;
		vdd_parent-supply = <&VDD_GFX_LEVEL>;
		qcom,reset-aon-logic;
		qcom,retain-regs;
	};

	/* VIDEO_CC GDSCs */
	video_cc_mvs0_gdsc: qcom,gdsc@abf0d18 {
		compatible = "qcom,gdsc";
		reg = <0xabf0d18 0x4>;
		regulator-name = "video_cc_mvs0_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_VIDEO_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,support-hw-trigger;
		qcom,retain-regs;
	};

	video_cc_mvs0c_gdsc: qcom,gdsc@abf0bf8 {
		compatible = "qcom,gdsc";
		reg = <0xabf0bf8 0x4>;
		regulator-name = "video_cc_mvs0c_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_VIDEO_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,retain-regs;
	};

	video_cc_mvs1_gdsc: qcom,gdsc@abf0d98 {
		compatible = "qcom,gdsc";
		reg = <0xabf0d98 0x4>;
		regulator-name = "video_cc_mvs1_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_VIDEO_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,support-hw-trigger;
		qcom,retain-regs;
	};

	video_cc_mvs1c_gdsc: qcom,gdsc@abf0c98 {
		compatible = "qcom,gdsc";
		reg = <0xabf0c98 0x4>;
		regulator-name = "video_cc_mvs1c_gdsc";
		qcom,gds-timeout = <500>;
		clock-names = "ahb_clk";
		clocks = <&clock_gcc GCC_VIDEO_AHB_CLK>;
		parent-supply = <&VDD_MM_LEVEL>;
		vdd_parent-supply = <&VDD_MM_LEVEL>;
		qcom,retain-regs;
	};

	thermal_zones: thermal-zones {
	};

	qmi_tmd: qmi-tmd-devices {
		compatible = "qcom,qmi-cooling-devices";
	};

	cache-controller@9200000 {
		compatible = "qcom,lahaina-llcc", "qcom,llcc-v2";
		reg = <0x9200000 0x1d0000> , <0x9600000 0x50000>;
		reg-names = "llcc_base", "llcc_broadcast_base";
		cap-based-alloc-and-pwr-collapse;
		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "qdss_clk";
	};

	qcom_scm {
		compatible = "qcom,secure-chan-manager";
	};

	qtee_shmbridge {
		compatible = "qcom,tee-shared-memory-bridge";
	};

	qcom_smcinvoke {
		compatible = "qcom,smcinvoke";
	};

	qcom-secure-buffer {
		compatible = "qcom,secure-buffer";
		qcom,vmid-cp-camera-preview-ro;
	};

	qcom-mem-buf {
		compatible = "qcom,mem-buf";
		qcom,mem-buf-capabilities = "supplier";
		qcom,vmid = <3>;
	};

	qcom,chd {
		compatible = "qcom,core-hang-detect";
		label = "core";
		qcom,threshold-arr = <0x18000058 0x18010058 0x18020058 0x18030058
			0x18040058 0x18050058 0x18060058 0x18070058>;
		qcom,config-arr = <0x18000060 0x18010060 0x18020060 0x18030060
			0x18040060 0x18050060 0x18060060 0x18070060>;
	};

	apps_rsc: rsc@18200000 {
		label = "apps_rsc";
		compatible = "qcom,rpmh-rsc";
		reg = <0x18200000 0x10000>,
		      <0x18210000 0x10000>,
		      <0x18220000 0x10000>;
		reg-names = "drv-0", "drv-1", "drv-2";
		interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>,
			    <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
		qcom,tcs-offset = <0xd00>;
		qcom,drv-id = <2>;
		qcom,tcs-config = <ACTIVE_TCS    3>,
				  <SLEEP_TCS     2>,
				  <WAKE_TCS      2>,
				  <CONTROL_TCS   0>,
				  <FAST_PATH_TCS 1>;
		power-domains = <&CLUSTER_PD>;

		apps_bcm_voter: bcm_voter {
			compatible = "qcom,bcm-voter";
		};

		clock_rpmh: qcom,rpmhclk {
			compatible = "qcom,lahaina-rpmh-clk";
			#clock-cells = <1>;
		};
	};

	aggre1_noc: interconnect@16e0000 {
		compatible = "qcom,lahaina-aggre1_noc";
		reg = <0x016E0000 0x1f180>;
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
		clocks = <&clock_gcc GCC_AGGRE_UFS_PHY_AXI_CLK>,
			<&clock_gcc GCC_AGGRE_USB3_PRIM_AXI_CLK>,
			<&clock_gcc GCC_AGGRE_USB3_SEC_AXI_CLK>;
	};

	aggre2_noc: interconnect@1700000 {
		reg = <0x1700000 0x3d180>;
		compatible = "qcom,lahaina-aggre2_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
		clocks = <&clock_gcc GCC_AGGRE_NOC_PCIE_0_AXI_CLK>,
			<&clock_gcc GCC_AGGRE_NOC_PCIE_1_AXI_CLK>,
			<&clock_gcc GCC_AGGRE_UFS_CARD_AXI_CLK>,
			<&clock_gcc GCC_AGGRE_UFS_PHY_AXI_CLK>,
			<&clock_rpmh RPMH_IPA_CLK>;
	};

	clk_virt: interconnect {
		compatible = "qcom,lahaina-clk_virt";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	config_noc: interconnect@1500000 {
		reg = <0x1500000 0x28000>;
		compatible = "qcom,lahaina-config_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	dc_noc: interconnect@90e0000 {
		reg = <0x90e0000 0x5080>;
		compatible = "qcom,lahaina-dc_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	gem_noc: interconnect@9100000 {
		reg = <0x9100000 0xb4000>;
		compatible = "qcom,lahaina-gem_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos", "disp";
		qcom,bcm-voters = <&apps_bcm_voter>, <&disp_bcm_voter>;
	};

	lpass_ag_noc: interconnect@3c40000 {
		reg = <0x03c40000 0xf080>;
		compatible = "qcom,lahaina-lpass_ag_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	mc_virt: interconnect@1580000 {
		reg = <0x1580000 0x4>;
		compatible = "qcom,lahaina-mc_virt";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos", "disp";
		qcom,bcm-voters = <&apps_bcm_voter>, <&disp_bcm_voter>;
	};

	mmss_noc: interconnect@1740000 {
		reg = <0x1740000 0x1f080>;
		compatible = "qcom,lahaina-mmss_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos", "disp";
		qcom,bcm-voters = <&apps_bcm_voter>, <&disp_bcm_voter>;
	};

	nsp_noc: interconnect@a0c0000 {
		reg = <0x0a0c0000 0x10000>;
		compatible = "qcom,lahaina-nsp_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	system_noc: interconnect@1680000 {
		reg = <0x1680000 0x1EE00>;
		compatible = "qcom,lahaina-system_noc";
		#interconnect-cells = <1>;
		qcom,bcm-voter-names = "hlos";
		qcom,bcm-voters = <&apps_bcm_voter>;
	};

	epss_l3_cpu: l3_cpu@18590000 {
		reg = <0x18590000 0x4000>;
		compatible = "qcom,lahaina-epss-l3-cpu";
		#interconnect-cells = <1>;
		clock-names = "xo", "alternate";
		clocks = <&clock_rpmh RPMH_CXO_CLK>,
			<&clock_gcc GCC_GPLL0>;
	};

	pil_scm_pas {
		compatible = "qcom,pil-tz-scm-pas";
		interconnects = <&aggre2_noc MASTER_CRYPTO &mc_virt SLAVE_EBI1>;
	};

	qcom,msm-rtb {
		compatible = "qcom,msm-rtb";
		qcom,rtb-size = <0x100000>;
	};

	qcom,mpm2-sleep-counter@c221000 {
		compatible = "qcom,mpm2-sleep-counter";
		reg = <0xc221000 0x1000>;
		clock-frequency = <32768>;
	};

	jtag_mm0: jtagmm@7040000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7040000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU0>;
	};

	jtag_mm1: jtagmm@7140000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7140000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU1>;
	};

	jtag_mm2: jtagmm@7240000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7240000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU2>;
	};

	jtag_mm3: jtagmm@7340000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7340000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU3>;
	};

	jtag_mm4: jtagmm@7440000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7440000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU4>;
	};

	jtag_mm5: jtagmm@7540000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7540000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU5>;
	};

	jtag_mm6: jtagmm@7640000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7640000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU6>;
	};

	jtag_mm7: jtagmm@7740000 {
		compatible = "qcom,jtagv8-mm";
		reg = <0x7740000 0x1000>;
		reg-names = "etm-base";

		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";

		qcom,coresight-jtagmm-cpu = <&CPU7>;
	};

	qcom,rmtfs_sharedmem@0 {
		compatible = "qcom,sharedmem-uio";
		reg = <0x0 0x280000>;
		reg-names = "rmtfs";
		qcom,client-id = <0x00000001>;
	};

	qcom_hwkm: hwkm@10c0000 {
		compatible = "qcom,hwkm";
		reg = <0x10c0000 0x9000>, <0x1d90000 0x9000>;
		reg-names = "km_master", "ice_slave";
		qcom,enable-hwkm-clk;

		clock-names = "km_clk_src";
		clocks = <&clock_rpmh RPMH_HWKM_CLK>;
		qcom,op-freq-hz = <75000000>;
	};

	ufsphy_mem: ufsphy_mem@1d87000 {
		reg = <0x1d87000 0xe10>;
		reg-names = "phy_mem";
		#phy-cells = <0>;

		lanes-per-direction = <2>;
		clock-names = "ref_clk_src",
			"ref_aux_clk";
		clocks = <&clock_rpmh RPMH_CXO_CLK>,
			<&clock_gcc GCC_UFS_PHY_PHY_AUX_CLK>;
		resets = <&ufshc_mem 0>;
		status = "disabled";
	};

	ufshc_mem: ufshc@1d84000 {
		compatible = "qcom,ufshc";
		reg = <0x1d84000 0x3000>,
		      <0x1d88000 0x8000>;
		reg-names = "ufs_mem", "ufs_ice";
		interrupts = <GIC_SPI 265 IRQ_TYPE_LEVEL_HIGH>;
		phys = <&ufsphy_mem>;
		phy-names = "ufsphy";
		#reset-cells = <1>;

		lanes-per-direction = <2>;
		dev-ref-clk-freq = <0>; /* 19.2 MHz */
		clock-names =
			"core_clk",
			"bus_aggr_clk",
			"iface_clk",
			"core_clk_unipro",
			"core_clk_ice",
			"ref_clk",
			"tx_lane0_sync_clk",
			"rx_lane0_sync_clk",
			"rx_lane1_sync_clk";
		clocks =
			<&clock_gcc GCC_UFS_PHY_AXI_CLK>,
			<&clock_gcc GCC_AGGRE_UFS_PHY_AXI_CLK>,
			<&clock_gcc GCC_UFS_PHY_AHB_CLK>,
			<&clock_gcc GCC_UFS_PHY_UNIPRO_CORE_CLK>,
			<&clock_gcc GCC_UFS_PHY_ICE_CORE_CLK>,
			<&clock_rpmh RPMH_CXO_CLK>,
			<&clock_gcc GCC_UFS_PHY_TX_SYMBOL_0_CLK>,
			<&clock_gcc GCC_UFS_PHY_RX_SYMBOL_0_CLK>,
			<&clock_gcc GCC_UFS_PHY_RX_SYMBOL_1_CLK>;
		freq-table-hz =
			<75000000 300000000>,
			<0 0>,
			<0 0>,
			<75000000 300000000>,
			<75000000 300000000>,
			<0 0>,
			<0 0>,
			<0 0>,
			<0 0>;
		interconnects = <&aggre1_noc MASTER_UFS_MEM &mc_virt SLAVE_EBI1>,
		      <&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_UFS_MEM_CFG>;
		interconnect-names = "ufs-ddr", "cpu-ufs";

		qcom,ufs-bus-bw,name = "ufshc_mem";
		qcom,ufs-bus-bw,num-cases = <26>;
		qcom,ufs-bus-bw,num-paths = <2>;
		qcom,ufs-bus-bw,vectors-KBps =
		/*
		 * During HS G3 UFS runs at nominal voltage corner, vote
		 * higher bandwidth to push other buses in the data path
		 * to run at nominal to achieve max throughput.
		 * 4GBps pushes BIMC to run at nominal.
		 * 200MBps pushes CNOC to run at nominal.
		 * Vote for half of this bandwidth for HS G3 1-lane.
		 * For max bandwidth, vote high enough to push the buses
		 * to run in turbo voltage corner.
		 */
		<0 0>, <0 0>,          /* No vote */
		<922 0>, <1000 0>,     /* PWM G1 */
		<1844 0>, <1000 0>,    /* PWM G2 */
		<3688 0>, <1000 0>,    /* PWM G3 */
		<7376 0>, <1000 0>,    /* PWM G4 */
		<1844 0>, <1000 0>,    /* PWM G1 L2 */
		<3688 0>, <1000 0>,    /* PWM G2 L2 */
		<7376 0>, <1000 0>,    /* PWM G3 L2 */
		<14752 0>, <1000 0>,   /* PWM G4 L2 */
		<127796 0>, <1000 0>,  /* HS G1 RA */
		<255591 0>, <1000 0>,  /* HS G2 RA */
		<1492582 0>, <102400 0>,  /* HS G3 RA */
		<2915200 0>, <204800 0>,  /* HS G4 RA */
		<255591 0>, <1000 0>,  /* HS G1 RA L2 */
		<511181 0>, <1000 0>,  /* HS G2 RA L2 */
		<1492582 0>, <204800 0>, /* HS G3 RA L2 */
		<2915200 0>, <409600 0>, /* HS G4 RA L2 */
		<149422 0>, <1000 0>,  /* HS G1 RB */
		<298189 0>, <1000 0>,  /* HS G2 RB */
		<1492582 0>, <102400 0>,  /* HS G3 RB */
		<2915200 0>, <204800 0>,  /* HS G4 RB */
		<298189 0>, <1000 0>,  /* HS G1 RB L2 */
		<596378 0>, <1000 0>,  /* HS G2 RB L2 */
		/* As UFS working in HS G3 RB L2 mode, aggregated
		 * bandwidth (AB) should take care of providing
		 * optimum throughput requested. However, as tested,
		 * in order to scale up CNOC clock, instantaneous
		 * bindwidth (IB) needs to be given a proper value too.
		 */
		<1492582 0>, <204800 409600>, /* HS G3 RB L2 KBPs */
		<2915200 0>, <409600 409600>, /* HS G4 RB L2 */
		<7643136 0>, <307200 0>; /* Max. bandwidth */

		qcom,bus-vector-names = "MIN",
		"PWM_G1_L1", "PWM_G2_L1", "PWM_G3_L1", "PWM_G4_L1",
		"PWM_G1_L2", "PWM_G2_L2", "PWM_G3_L2", "PWM_G4_L2",
		"HS_RA_G1_L1", "HS_RA_G2_L1", "HS_RA_G3_L1", "HS_RA_G4_L1",
		"HS_RA_G1_L2", "HS_RA_G2_L2", "HS_RA_G3_L2", "HS_RA_G4_L2",
		"HS_RB_G1_L1", "HS_RB_G2_L1", "HS_RB_G3_L1", "HS_RB_G4_L1",
		"HS_RB_G1_L2", "HS_RB_G2_L2", "HS_RB_G3_L2", "HS_RB_G4_L2",
		"MAX";

		reset-gpios = <&tlmm 203 GPIO_ACTIVE_LOW>;

		resets = <&clock_gcc GCC_UFS_PHY_BCR>;
		reset-names = "rst";
		iommus = <&apps_smmu 0xE0 0x0>;
		qcom,iommu-dma = "bypass";
		dma-coherent;

		rpm-level = <3>;
		spm-level = <5>;

		status = "disabled";
		qos0 {
			mask = <0xf0>;
			vote = <44>;
		};


		qos1 {
			mask = <0x0f>;
			vote = <44>;
		};
	};

	sdhc_2: sdhci@8804000 {
		compatible = "qcom,sdhci-msm-v5";
		reg = <0x08804000 0x1000>;
		reg-names = "hc_mem";

		interrupts = <GIC_SPI 207 IRQ_TYPE_LEVEL_HIGH>,
				<GIC_SPI 223 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "hc_irq", "pwr_irq";

		qcom,bus-width = <4>;
		qcom,large-address-bus;

		interconnects = <&aggre2_noc MASTER_SDCC_2 &mc_virt SLAVE_EBI1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_SDCC_2>;
		interconnect-names = "sdhc-ddr","cpu-sdhc";
		qcom,msm-bus,name = "sdhc2";
		qcom,msm-bus,num-cases = <8>;
		qcom,msm-bus,num-paths = <2>;
		qcom,msm-bus,vectors-KBps =
			/* No Vote */
			<0 0>, <0 0>,
			/* 400 KB/s*/
			<1046 1600>, <1600 1600>,
			/* 20 MB/s */
			<52286 80000>, <80000 80000>,
			/* 25 MB/s */
			<65360 100000>, <100000 100000>,
			/* 50 MB/s */
			<130718 200000>, <133320 133320>,
			/* 100 MB/s */
			<261438 200000>, <150000 150000>,
			/* 200 MB/s */
			<261438 400000>, <300000 300000>,
			/* Max. bandwidth */
			<1338562 4096000>, <1338562 4096000>;
		qcom,bus-bw-vectors-bps = <0 400000 20000000 25000000 50000000
			100750000 200000000 4294967295>;

		qcom,restore-after-cx-collapse;

		qcom,clk-rates = <400000 20000000 25000000
					50000000 100000000 201500000>;
		qcom,bus-speed-mode = "SDR12", "SDR25", "SDR50", "DDR50",
				      "SDR104";

		qcom,devfreq,freq-table = <50000000 201500000>;
		clocks = <&clock_gcc GCC_SDCC2_AHB_CLK>,
			<&clock_gcc GCC_SDCC2_APPS_CLK>;
		clock-names = "iface", "core";

		/* DLL HSR settings. Refer go/hsr - <Target> DLL settings */
		qcom,dll-hsr-list = <0x0007642C 0xA800 0x10
					0x2C010800 0x80040868>;

		qcom,scaling-lower-bus-speed-mode = "DDR52";

		iommus = <&apps_smmu 0x4a0 0x0>;
		dma-coherent;
		qcom,iommu-dma = "bypass";

		status = "disabled";

		qos0 {
			mask = <0x0f>;
			vote = <44>;
		};

		qos1 {
			mask = <0xf0>;
			vote = <44>;
		};
	};

	kryo-erp {
		compatible = "arm,arm64-kryo-cpu-erp";
		interrupts = <GIC_PPI 0 IRQ_TYPE_LEVEL_HIGH>,
			<GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "l1-l2-faultirq","l3-scu-faultirq";
	};

	tcsr_mutex_block: syscon@1f40000 {
		compatible = "syscon";
		reg = <0x1f40000 0x20000>;
	};

	tcsr_mutex: hwlock {
		compatible = "qcom,tcsr-mutex";
		syscon = <&tcsr_mutex_block 0 0x1000>;
		#hwlock-cells = <1>;
	};

	tcsr: syscon@1fc0000 {
		compatible = "syscon";
		reg = <0x1fc0000 0x30000>;
	};

	smem: qcom,smem {
		compatible = "qcom,smem";
		memory-region = <&smem_mem>;
		hwlocks = <&tcsr_mutex 3>;
	};

	qmp_aop: qcom,qmp-aop@c300000 {
		compatible = "qcom,qmp-mbox";
		mboxes = <&ipcc_mproc IPCC_CLIENT_AOP
			  IPCC_MPROC_SIGNAL_GLINK_QMP>;
		mbox-names = "aop_qmp";
		interrupt-parent = <&ipcc_mproc>;
		interrupts = <IPCC_CLIENT_AOP
			      IPCC_MPROC_SIGNAL_GLINK_QMP
			      IRQ_TYPE_EDGE_RISING>;
		reg = <0xc300000 0x400>;
		reg-names = "msgram";

		label = "aop";
		qcom,early-boot;
		priority = <0>;
		mbox-desc-offset = <0x0>;
		#mbox-cells = <1>;
	};

	aop-msg-client {
		compatible = "qcom,debugfs-qmp-client";
		mboxes = <&qmp_aop 0>;
		mbox-names = "aop";
	};

	qcom,smp2p_sleepstate {
		compatible = "qcom,smp2p-sleepstate";
		qcom,smem-states = <&sleepstate_smp2p_out 0>;
		interrupt-parent = <&sleepstate_smp2p_in>;
		interrupts = <0 0>;
		interrupt-names = "smp2p-sleepstate-in";
	};

	pdc: interrupt-controller@b220000 {
		compatible = "qcom,lahaina-pdc", "qcom,pdc";
		reg = <0xb220000 0x30000>, <0x17c000f0 0x60>;
		qcom,pdc-ranges = <0 480 40>, <40 140 14>, <54 263 1>, <55 306 4>,
				  <59 312 3>, <62 374 2>, <64 434 2>, <66 438 3>,
				  <69 86 1>, <70 520 54>, <124 609 31>, <155 63 1>,
				  <156 716 12>;
		#interrupt-cells = <2>;
		interrupt-parent = <&intc>;
		interrupt-controller;
	};

	disp_rsc: rsc@af20000 {
		label = "disp_rsc";
		compatible = "qcom,rpmh-rsc";
		reg = <0xaf20000 0x10000>;
		reg-names = "drv-0";
		interrupts = <GIC_SPI 129 IRQ_TYPE_LEVEL_HIGH>;
		qcom,tcs-offset = <0x1c00>;
		qcom,drv-id = <0>;
		qcom,tcs-config = <ACTIVE_TCS    0>,
				  <SLEEP_TCS     1>,
				  <WAKE_TCS      1>,
				  <CONTROL_TCS   0>,
				  <FAST_PATH_TCS 0>;

		disp_bcm_voter: bcm_voter {
			compatible = "qcom,bcm-voter";
			qcom,tcs-wait = <QCOM_ICC_TAG_AMC>;
		};

		sde_rsc_rpmh {
			compatible = "qcom,sde-rsc-rpmh";
			cell-index = <0>;
		};
	};

	spmi_bus: qcom,spmi@c440000 {
		compatible = "qcom,spmi-pmic-arb";
		reg = <0xc440000 0x1100>,
		      <0xc600000 0x2000000>,
		      <0xe600000 0x100000>,
		      <0xe700000 0xa0000>,
		      <0xc40a000 0x26000>;
		reg-names = "core", "chnls", "obsrvr", "intr", "cnfg";
		interrupts-extended = <&pdc 1 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "periph_irq";
		interrupt-controller;
		#interrupt-cells = <4>;
		#address-cells = <2>;
		#size-cells = <0>;
		cell-index = <0>;
		qcom,channel = <0>;
		qcom,ee = <0>;
	};

	spmi_debug_bus: qcom,spmi-debug@6b12000 {
		compatible = "qcom,spmi-pmic-arb-debug";
		reg = <0x6b12000 0x60>, <0x7820a8 0x4>;
		reg-names = "core", "fuse";
		clocks = <&clock_aop QDSS_CLK>;
		clock-names = "core_clk";
		qcom,fuse-disable-bit = <24>;
		#address-cells = <2>;
		#size-cells = <0>;
		status = "disabled";

		qcom,pmk8350-debug@0 {
			compatible = "qcom,spmi-pmic";
			reg = <0 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pm8350-debug@1 {
			compatible = "qcom,spmi-pmic";
			reg = <1 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pm8350c-debug@2 {
			compatible = "qcom,spmi-pmic";
			reg = <2 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pm8350b-debug@3 {
			compatible = "qcom,spmi-pmic";
			reg = <3 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pmr735a-debug@4 {
			compatible = "qcom,spmi-pmic";
			reg = <4 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};

		qcom,pmr735b-debug@5 {
			compatible = "qcom,spmi-pmic";
			reg = <5 SPMI_USID>;
			#address-cells = <2>;
			#size-cells = <0>;
			qcom,can-sleep;
		};
	};

	qcom,msm-cdsp-loader {
		compatible = "qcom,cdsp-loader";
		qcom,proc-img-to-load = "cdsp";
	};

	qcom,msm-adsprpc-mem {
		compatible = "qcom,msm-adsprpc-mem-region";
		memory-region = <&adsp_mem>;
		restrict-access;
	};

	msm_fastrpc: qcom,msm_fastrpc {
		compatible = "qcom,msm-fastrpc-compute";
		qcom,adsp-remoteheap-vmid = <22 37>;
		qcom,fastrpc-adsp-audio-pdr;
		qcom,fastrpc-adsp-sensors-pdr;
		qcom,rpc-latency-us = <235>;
		qcom,fastrpc-gids = <2908>;
		qcom,qos-cores = <0 1 2 3>;

		qcom,msm_fastrpc_compute_cb1 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x2161 0x0400>,
					 <&apps_smmu 0x1181 0x0420>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb2 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x2162 0x0400>,
					 <&apps_smmu 0x1182 0x0420>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb3 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x2163 0x0400>,
					 <&apps_smmu 0x1183 0x0420>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb4 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x2164 0x0400>,
					 <&apps_smmu 0x1184 0x0420>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb5 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x2165 0x0400>,
					 <&apps_smmu 0x1185 0x0420>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb6 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x2166 0x0400>,
					 <&apps_smmu 0x1186 0x0420>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb7 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x2167 0x0400>,
					 <&apps_smmu 0x1187 0x0420>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb8 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x2168 0x0400>,
					 <&apps_smmu 0x1188 0x0420>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb9 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			qcom,secure-context-bank;
			iommus = <&apps_smmu 0x2169 0x0400>,
					 <&apps_smmu 0x1189 0x0420>;
			qcom,iommu-dma-addr-pool = <0x60000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			qcom,iommu-vmid = <0xA>;	/* VMID_CP_PIXEL */
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb10 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "adsprpc-smd";
			iommus = <&apps_smmu 0x1803 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb11 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "adsprpc-smd";
			iommus = <&apps_smmu 0x1804 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb12 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "adsprpc-smd";
			iommus = <&apps_smmu 0x1805 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb13 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "sdsprpc-smd";
			iommus = <&apps_smmu 0x0541 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb14 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "sdsprpc-smd";
			iommus = <&apps_smmu 0x0542 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb15 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "sdsprpc-smd";
			iommus = <&apps_smmu 0x0543 0x0>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			shared-cb = <4>;
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb16 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x118B 0x0420>,
					 <&apps_smmu 0x216B 0x0400>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb17 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x118C 0x0420>,
					 <&apps_smmu 0x216C 0x0400>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb18 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x118D 0x0420>,
					 <&apps_smmu 0x216D 0x0400>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};

		qcom,msm_fastrpc_compute_cb19 {
			compatible = "qcom,msm-fastrpc-compute-cb";
			label = "cdsprpc-smd";
			iommus = <&apps_smmu 0x118E 0x0420>,
					 <&apps_smmu 0x216E 0x0400>;
			qcom,iommu-dma-addr-pool = <0x80000000 0x78000000>;
			qcom,iommu-faults = "stall-disable", "HUPCF";
			dma-coherent-hint-cached;
		};
	};

	llcc_pmu: llcc-pmu@9095000 {
		compatible = "qcom,llcc-pmu-ver2";
		reg = <0x09095000 0x300>;
		reg-names = "lagg-base";
	};

	llcc_bw_opp_table: llcc-bw-opp-table {
		compatible = "operating-points-v2";
		BW_OPP_ENTRY(  150, 16); /*  2288 MB/s */
		BW_OPP_ENTRY(  300, 16); /*  4577 MB/s */
		BW_OPP_ENTRY(  466, 16); /*  7110 MB/s */
		BW_OPP_ENTRY(  600, 16); /*  9155 MB/s */
		BW_OPP_ENTRY(  806, 16); /* 12298 MB/s */
		BW_OPP_ENTRY(  933, 16); /* 14236 MB/s */
		BW_OPP_ENTRY( 1000, 16); /* 15258 MB/s */
	};

	ddr_bw_opp_table: ddr-bw-opp-table {
		compatible = "operating-points-v2";
		BW_OPP_ENTRY_DDR(  200, 4, 0x180); /*   762 MB/s */
		BW_OPP_ENTRY_DDR(  451, 4, 0x180); /*  1720 MB/s */
		BW_OPP_ENTRY_DDR(  547, 4, 0x180); /*  2086 MB/s */
		BW_OPP_ENTRY_DDR(  681, 4, 0x180); /*  2597 MB/s */
		BW_OPP_ENTRY_DDR(  768, 4, 0x180); /*  2929 MB/s */
		BW_OPP_ENTRY_DDR( 1017, 4, 0x180); /*  3879 MB/s */
		BW_OPP_ENTRY_DDR( 1353, 4,  0x80); /*  5161 MB/s */
		BW_OPP_ENTRY_DDR( 1555, 4, 0x180); /*  5931 MB/s */
		BW_OPP_ENTRY_DDR( 1708, 4, 0x180); /*  6515 MB/s */
		BW_OPP_ENTRY_DDR( 2092, 4, 0x180); /*  7980 MB/s */
		BW_OPP_ENTRY_DDR( 2133, 4,  0x80); /*  8136 MB/s */
		BW_OPP_ENTRY_DDR( 2736, 4, 0x100); /* 10437 MB/s */
		BW_OPP_ENTRY_DDR( 3196, 4, 0x100); /* 12191 MB/s */
	};

	qoslat_opp_table: qoslat-opp-table {
		compatible = "operating-points-v2";
		opp-1 {
			opp-hz = /bits/ 64 < 1 >;
		};

		opp-2 {
			opp-hz = /bits/ 64 < 2 >;
		};
	};

	cpu_cpu_llcc_bw: qcom,cpu-cpu-llcc-bw {
		compatible = "qcom,devfreq-icc";
		governor = "bw_hwmon";
		interconnects = <&gem_noc MASTER_APPSS_PROC &gem_noc SLAVE_LLCC>;
		qcom,active-only;
		operating-points-v2 = <&llcc_bw_opp_table>;
	};

	cpu_cpu_llcc_bwmon: qcom,cpu-cpu-llcc-bwmon@90b6400 {
		compatible = "qcom,bimc-bwmon4";
		reg = <0x90b6400 0x300>, <0x90b6300 0x200>;
		reg-names = "base", "global_base";
		interrupts = <GIC_SPI 581 IRQ_TYPE_LEVEL_HIGH>;
		qcom,mport = <0>;
		qcom,hw-timer-hz = <19200000>;
		qcom,target-dev = <&cpu_cpu_llcc_bw>;
		qcom,count-unit = <0x10000>;
	};

	cpu_llcc_ddr_bw: qcom,cpu-llcc-ddr-bw {
		compatible = "qcom,devfreq-icc-ddr";
		governor = "bw_hwmon";
		interconnects = <&mc_virt MASTER_LLCC &mc_virt SLAVE_EBI1>;
		qcom,active-only;
		operating-points-v2 = <&ddr_bw_opp_table>;
	};

	cpu_llcc_ddr_bwmon: qcom,cpu-llcc-ddr-bwmon@9091000 {
		compatible = "qcom,bimc-bwmon5";
		reg = <0x9091000 0x1000>;
		reg-names = "base";
		interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
		qcom,hw-timer-hz = <19200000>;
		qcom,target-dev = <&cpu_llcc_ddr_bw>;
		qcom,count-unit = <0x10000>;
	};

	cpu0_cpu_l3_lat: qcom,cpu0-cpu-l3-lat {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "mem_latency";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_CPU0>;
	};

	cpu1_cpu_l3_lat: qcom,cpu1-cpu-l3-lat {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "mem_latency";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_CPU1>;
	};

	cpu2_cpu_l3_lat: qcom,cpu2-cpu-l3-lat {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "mem_latency";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_CPU2>;
	};

	cpu3_cpu_l3_lat: qcom,cpu3-cpu-l3-lat {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "mem_latency";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_CPU3>;
	};

	cpu4_cpu_l3_lat: qcom,cpu4-cpu-l3-lat {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "mem_latency";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_CPU4>;
	};

	cpu5_cpu_l3_lat: qcom,cpu5-cpu-l3-lat {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "mem_latency";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_CPU5>;
	};

	cpu6_cpu_l3_lat: qcom,cpu6-cpu-l3-lat {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "mem_latency";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_CPU6>;
	};

	cpu7_cpu_l3_lat: qcom,cpu7-cpu-l3-lat {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "mem_latency";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_CPU7>;
	};

	cpu7_cpu_l3_latfloor: qcom,cpu7-cpu-l3-latfloor {
		compatible = "qcom,devfreq-icc-l3";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		governor = "compute";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_SHARED>;
	};

	snoop_l3_bw: qcom,snoop-l3-bw {
		compatible = "qcom,devfreq-icc-l3bw";
		reg = <0x18590100 0xa0>;
		reg-names = "ftbl-base";
		qcom,bus-width = <32>;
		governor = "bw_hwmon";
		interconnects =
			<&epss_l3_cpu MASTER_EPSS_L3_APPS
			 &epss_l3_cpu SLAVE_EPSS_L3_SHARED>;
	};

	snoop_l3_bwmon: qcom,snoop-l3-bwmon@9091000 {
		compatible = "qcom,bimc-bwmon4";
		reg = <0x90b9100 0x300>, <0x90b9000 0x200>;
		reg-names = "base", "global_base";
		interrupts = <GIC_SPI 226 IRQ_TYPE_LEVEL_HIGH>;
		qcom,mport = <0>;
		qcom,hw-timer-hz = <19200000>;
		qcom,target-dev = <&snoop_l3_bw>;
		qcom,count-unit = <0x10000>;
	};

	cpu0_cpu_llcc_lat: qcom,cpu0-cpu-llcc-lat {
		compatible = "qcom,devfreq-icc";
		governor = "mem_latency";
		interconnects = <&gem_noc MASTER_APPSS_PROC &gem_noc SLAVE_LLCC>;
		qcom,active-only;
		operating-points-v2 = <&llcc_bw_opp_table>;
	};

	cpu4_cpu_llcc_lat: qcom,cpu4-cpu-llcc-lat {
		compatible = "qcom,devfreq-icc";
		governor = "mem_latency";
		interconnects = <&gem_noc MASTER_APPSS_PROC &gem_noc SLAVE_LLCC>;
		qcom,active-only;
		operating-points-v2 = <&llcc_bw_opp_table>;
	};

	cpu0_llcc_ddr_lat: qcom,cpu0-llcc-ddr-lat {
		compatible = "qcom,devfreq-icc-ddr";
		governor = "mem_latency";
		interconnects = <&mc_virt MASTER_LLCC &mc_virt SLAVE_EBI1>;
		qcom,active-only;
		operating-points-v2 = <&ddr_bw_opp_table>;
	};

	cpu4_llcc_ddr_lat: qcom,cpu4-llcc-ddr-lat {
		compatible = "qcom,devfreq-icc-ddr";
		governor = "mem_latency";
		interconnects = <&mc_virt MASTER_LLCC &mc_virt SLAVE_EBI1>;
		qcom,active-only;
		operating-points-v2 = <&ddr_bw_opp_table>;
	};

	cpu4_cpu_ddr_latfloor: qcom,cpu4-cpu-ddr-latfloor {
		compatible = "qcom,devfreq-icc-ddr";
		governor = "compute";
		interconnects = <&mc_virt MASTER_LLCC &mc_virt SLAVE_EBI1>;
		qcom,active-only;
		operating-points-v2 = <&ddr_bw_opp_table>;
	};

	cpu4_cpu_llcc_latfloor: qcom,cpu4-cpu-llcc-latfloor {
		compatible = "qcom,devfreq-icc";
		governor = "compute";
		interconnects = <&gem_noc MASTER_APPSS_PROC &gem_noc SLAVE_LLCC>;
		qcom,active-only;
		operating-points-v2 = <&llcc_bw_opp_table>;
	};

	cpu7_cpu_ddr_latfloor: qcom,cpu7-cpu-ddr-latfloor {
		compatible = "qcom,devfreq-icc-ddr";
		governor = "mem_latency";
		interconnects = <&mc_virt MASTER_LLCC &mc_virt SLAVE_EBI1>;
		qcom,active-only;
		operating-points-v2 = <&ddr_bw_opp_table>;
	};

	cpu4_cpu_ddr_qoslat: qcom,cpu4-cpu-ddr-qoslat {
		compatible = "qcom,devfreq-qoslat";
		governor = "mem_latency";
		operating-points-v2 = <&qoslat_opp_table>;
		mboxes = <&qmp_aop 0>;
	};

	cpu7_cpu_ddr_qoslatfloor: qcom,cpu7-cpu-ddr-qoslatfloor {
		compatible = "qcom,devfreq-qoslat";
		governor = "mem_latency";
		operating-points-v2 = <&qoslat_opp_table>;
		mboxes = <&qmp_aop 0>;
	};

	cpu0_cpu_l3_tbl: qcom,cpu0-cpu-l3-tbl {
		qcom,core-dev-table =
			<  300000  300000000 >,
			<  403200  403200000 >,
			<  499200  499200000 >,
			<  691200  614400000 >,
			<  806400  710400000 >,
			<  998400  806400000 >,
			< 1190400  998400000 >,
			< 1286400 1094400000 >,
			< 1459200 1248000000 >,
			< 1728000 1344000000 >,
			< 1804800 1440000000 >,
			< 1900800 1516800000 >;
	};

	cpu4_cpu_l3_tbl: qcom,cpu4-cpu-l3-tbl {
		qcom,core-dev-table =
			<  300000  300000000 >,
			<  787200  614400000 >,
			< 1209600  806400000 >,
			< 1497600  998400000 >,
			< 1689600 1248000000 >,
			< 1900800 1344000000 >,
			< 2188800 1440000000 >,
			< 2400000 1516800000 >;
	};

	memlat_cpugrp: qcom,memlat-cpugrp {
		compatible = "qcom,arm-memlat-cpugrp";
		qcom,cpulist = <&CPU0 &CPU1 &CPU2 &CPU3
				&CPU4 &CPU5 &CPU6 &CPU7>;

		cpu0_cpu_l3_latmon: qcom,cpu0-cpu-l3-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU0>;
			qcom,target-dev = <&cpu0_cpu_l3_lat>;
			qcom,cachemiss-ev = <0x17>;
			qcom,core-dev-table = <&cpu0_cpu_l3_tbl>;
		};

		cpu1_cpu_l3_latmon: qcom,cpu1-cpu-l3-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU1>;
			qcom,target-dev = <&cpu1_cpu_l3_lat>;
			qcom,cachemiss-ev = <0x17>;
			qcom,core-dev-table = <&cpu0_cpu_l3_tbl>;
		};

		cpu2_cpu_l3_latmon: qcom,cpu2-cpu-l3-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU2>;
			qcom,target-dev = <&cpu2_cpu_l3_lat>;
			qcom,cachemiss-ev = <0x17>;
			qcom,core-dev-table = <&cpu0_cpu_l3_tbl>;
		};

		cpu3_cpu_l3_latmon: qcom,cpu3-cpu-l3-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU3>;
			qcom,target-dev = <&cpu3_cpu_l3_lat>;
			qcom,cachemiss-ev = <0x17>;
			qcom,core-dev-table = <&cpu0_cpu_l3_tbl>;
		};

		cpu0_cpu_llcc_latmon: qcom,cpu0-cpu-llcc-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU0 &CPU1 &CPU2 &CPU3>;
			qcom,target-dev = <&cpu0_cpu_llcc_lat>;
			qcom,cachemiss-ev = <0x2A>;
			qcom,core-dev-table =
				<  300000 MHZ_TO_MBPS( 150, 16) >,
				<  691200 MHZ_TO_MBPS( 300, 16) >,
				< 1459200 MHZ_TO_MBPS( 466, 16) >,
				< 1900800 MHZ_TO_MBPS( 600, 16) >;
		};

		cpu0_llcc_ddr_latmon: qcom,cpu0-llcc-ddr-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU0 &CPU1 &CPU2 &CPU3>;
			qcom,target-dev = <&cpu0_llcc_ddr_lat>;
			qcom,cachemiss-ev = <0x1000>;
			ddr4-map {
				qcom,ddr-type = <DDR_TYPE_LPDDR4X>;
				qcom,core-dev-table =
					<  300000 MHZ_TO_MBPS(  200, 4) >,
					<  691200 MHZ_TO_MBPS(  451, 4) >,
					< 1190400 MHZ_TO_MBPS(  547, 4) >,
					< 1459200 MHZ_TO_MBPS(  768, 4) >,
					< 1900800 MHZ_TO_MBPS( 1017, 4) >;
			};

			ddr5-map {
				qcom,ddr-type = <DDR_TYPE_LPDDR5>;
				qcom,core-dev-table =
					<  300000 MHZ_TO_MBPS(  200, 4) >,
					<  691200 MHZ_TO_MBPS(  451, 4) >,
					< 1190400 MHZ_TO_MBPS(  547, 4) >,
					< 1459200 MHZ_TO_MBPS(  768, 4) >,
					< 1900800 MHZ_TO_MBPS( 1555, 4) >;
			};
		};

		cpu4_cpu_l3_latmon: qcom,cpu4-cpu-l3-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU4>;
			qcom,target-dev = <&cpu4_cpu_l3_lat>;
			qcom,cachemiss-ev = <0x17>;
			qcom,core-dev-table = <&cpu4_cpu_l3_tbl>;
		};

		cpu5_cpu_l3_latmon: qcom,cpu5-cpu-l3-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU5>;
			qcom,target-dev = <&cpu5_cpu_l3_lat>;
			qcom,cachemiss-ev = <0x17>;
			qcom,core-dev-table = <&cpu4_cpu_l3_tbl>;
		};

		cpu6_cpu_l3_latmon: qcom,cpu6-cpu-l3-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU6>;
			qcom,target-dev = <&cpu6_cpu_l3_lat>;
			qcom,cachemiss-ev = <0x17>;
			qcom,core-dev-table = <&cpu4_cpu_l3_tbl>;
		};

		cpu7_cpu_l3_latmon: qcom,cpu7-cpu-l3-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU7>;
			qcom,target-dev = <&cpu7_cpu_l3_lat>;
			qcom,cachemiss-ev = <0x17>;
			qcom,core-dev-table = <&cpu4_cpu_l3_tbl>;
		};

		cpu7_l3_computemon: qcom,cpu7-l3-computemon {
			compatible = "qcom,arm-compute-mon";
			qcom,cpulist = <&CPU7>;
			qcom,target-dev = <&cpu7_cpu_l3_latfloor>;
			qcom,core-dev-table =
				< 1996800  300000000 >,
				< 2400000 1516800000 >;
		};

		cpu4_cpu_llcc_latmon: qcom,cpu4-cpu-llcc-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU4 &CPU5 &CPU6 &CPU7>;
			qcom,target-dev = <&cpu4_cpu_llcc_lat>;
			qcom,cachemiss-ev = <0x2A>;
			qcom,core-dev-table =
				<  300000 MHZ_TO_MBPS(  150, 16) >,
				<  672000 MHZ_TO_MBPS(  300, 16) >,
				< 1017600 MHZ_TO_MBPS(  466, 16) >,
				< 1305600 MHZ_TO_MBPS(  600, 16) >,
				< 1804800 MHZ_TO_MBPS(  806, 16) >,
				< 2304000 MHZ_TO_MBPS(  933, 16) >,
				< 2400000 MHZ_TO_MBPS( 1000, 16) >;
		};

		cpu4_llcc_ddr_latmon: qcom,cpu4-llcc-ddr-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU4 &CPU5 &CPU6 &CPU7>;
			qcom,target-dev = <&cpu4_llcc_ddr_lat>;
			qcom,cachemiss-ev = <0x1000>;
			ddr4-map {
				qcom,ddr-type = <DDR_TYPE_LPDDR4X>;
				qcom,core-dev-table =
					<  300000 MHZ_TO_MBPS( 200, 4) >,
					<  672000 MHZ_TO_MBPS( 451, 4) >,
					<  902400 MHZ_TO_MBPS( 547, 4) >,
					< 1017600 MHZ_TO_MBPS( 768, 4) >,
					< 1305600 MHZ_TO_MBPS(1017, 4) >,
					< 1593600 MHZ_TO_MBPS(1353, 4) >,
					< 1804800 MHZ_TO_MBPS(1555, 4) >,
					< 2188800 MHZ_TO_MBPS(1708, 4) >,
					< 2400000 MHZ_TO_MBPS(2133, 4) >;
			};

			ddr5-map {
				qcom,ddr-type = <DDR_TYPE_LPDDR5>;
				qcom,core-dev-table =
					<  300000 MHZ_TO_MBPS( 200, 4) >,
					<  672000 MHZ_TO_MBPS( 451, 4) >,
					<  902400 MHZ_TO_MBPS( 547, 4) >,
					< 1017600 MHZ_TO_MBPS( 768, 4) >,
					< 1804800 MHZ_TO_MBPS(1555, 4) >,
					< 2304000 MHZ_TO_MBPS(2092, 4) >,
					< 2400000 MHZ_TO_MBPS(3196, 4) >;
			};
		};

		cpu4_computemon: qcom,cpu4-computemon {
			compatible = "qcom,arm-compute-mon";
			qcom,cpulist = <&CPU4 &CPU5 &CPU6 &CPU7>;
			qcom,target-dev = <&cpu4_cpu_ddr_latfloor>;
			ddr4-map {
				qcom,ddr-type = <DDR_TYPE_LPDDR4X>;
				qcom,core-dev-table =
					< 1804800 MHZ_TO_MBPS( 200, 4) >,
					< 2400000 MHZ_TO_MBPS(1017, 4) >;
			};

			ddr5-map {
				qcom,ddr-type = <DDR_TYPE_LPDDR5>;
				qcom,core-dev-table =
					< 1804800 MHZ_TO_MBPS( 200, 4) >,
					< 2400000 MHZ_TO_MBPS(1555, 4) >;
			};
		};

		cpu4_llcc_computemon: qcom,cpu4-llcc-computemon {
			compatible = "qcom,arm-compute-mon";
			qcom,cpulist = <&CPU4 &CPU5 &CPU6 &CPU7>;
			qcom,target-dev = <&cpu4_cpu_llcc_latfloor>;
			qcom,core-dev-table =
				< 1804800 MHZ_TO_MBPS( 150, 16) >,
				< 2400000 MHZ_TO_MBPS( 600, 16) >;
		};

		cpu7_llcc_ddr_latmon: qcom,cpu7-llcc-ddr-latmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU7>;
			qcom,target-dev = <&cpu7_cpu_ddr_latfloor>;
			qcom,cachemiss-ev = <0x1000>;
			ddr4-map {
				qcom,ddr-type = <DDR_TYPE_LPDDR4X>;
				qcom,core-dev-table =
					< 2304000 MHZ_TO_MBPS( 200, 4) >,
					< 2400000 MHZ_TO_MBPS(2133, 4) >;
			};

			ddr5-map {
				qcom,ddr-type = <DDR_TYPE_LPDDR5>;
				qcom,core-dev-table =
					< 2304000 MHZ_TO_MBPS( 200, 4) >,
					< 2400000 MHZ_TO_MBPS(3196, 4) >;
			};
		};

		cpu4_qoslatmon: qcom,cpu4-qoslatmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU4 &CPU5 &CPU6 &CPU7>;
			qcom,target-dev = <&cpu4_cpu_ddr_qoslat>;
			qcom,cachemiss-ev = <0x1000>;
			qcom,core-dev-table =
				<  300000 1 >,
				< 3000000 2 >;
		};

		cpu7_qoslatmon: qcom,cpu7-qoslatmon {
			compatible = "qcom,arm-memlat-mon";
			qcom,cpulist = <&CPU7>;
			qcom,target-dev = <&cpu7_cpu_ddr_qoslatfloor>;
			qcom,cachemiss-ev = <0x1000>;
			qcom,core-dev-table =
				< 1996800 1 >,
				< 2400000 2 >;
		};
	};

	wdog: qcom,wdt@17c10000{
		compatible = "qcom,msm-watchdog";
		reg = <0x17c10000 0x1000>;
		reg-names = "wdt-base";
		interrupts = <0 0 IRQ_TYPE_LEVEL_HIGH>;
	};

	tsens0:tsens@c222000 {
		compatible = "qcom,tsens24xx";
		reg = <0x0C222000 0x8>,
		      <0x0C263000 0x1ff>;
		reg-names = "tsens_srot_physical",
			"tsens_tm_physical";
		interrupts-extended = <&pdc 26 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 28 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 20 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "tsens-upper-lower", "tsens-critical",
				"tsens-0C";
		#thermal-sensor-cells = <1>;
	};

	tsens1:tsens@c223000 {
		compatible = "qcom,tsens24xx";
		reg = <0x0C223000 0x8>,
			<0x0C265000 0x1ff>;
		reg-names = "tsens_srot_physical",
			"tsens_tm_physical";
		interrupts-extended = <&pdc 27 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 29 IRQ_TYPE_LEVEL_HIGH>,
			<&pdc 21 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "tsens-upper-lower", "tsens-critical",
				"tsens-0C";
		#thermal-sensor-cells = <1>;
	};

	qcom,glink {
		compatible = "qcom,glink";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		glink_modem: modem {
			qcom,remote-pid = <1>;
			transport = "smem";
			mboxes = <&ipcc_mproc IPCC_CLIENT_MPSS
				  IPCC_MPROC_SIGNAL_GLINK_QMP>;
			mbox-names = "mpss_smem";
			interrupt-parent = <&ipcc_mproc>;
			interrupts = <IPCC_CLIENT_MPSS
				      IPCC_MPROC_SIGNAL_GLINK_QMP
				      IRQ_TYPE_EDGE_RISING>;

			label = "modem";
			qcom,glink-label = "mpss";

			qcom,modem_qrtr {
				qcom,glink-channels = "IPCRTR";
				qcom,low-latency;
				qcom,intents = <0x800  5
						0x2000 3
						0x4400 2>;
			};

			qcom,modem_ds {
				qcom,glink-channels = "DS";
				qcom,intents = <0x4000 0x2>;
			};

			qcom,modem_glink_ssr {
				qcom,glink-channels = "glink_ssr";
				qcom,notify-edges = <&glink_adsp>,
						    <&glink_slpi>,
						    <&glink_spss>;
			};
		};

		glink_adsp: adsp {
			qcom,remote-pid = <2>;
			transport = "smem";
			mboxes = <&ipcc_mproc IPCC_CLIENT_LPASS
				  IPCC_MPROC_SIGNAL_GLINK_QMP>;
			mbox-names = "adsp_smem";
			interrupt-parent = <&ipcc_mproc>;
			interrupts = <IPCC_CLIENT_LPASS
				      IPCC_MPROC_SIGNAL_GLINK_QMP
				      IRQ_TYPE_EDGE_RISING>;

			label = "adsp";
			qcom,glink-label = "lpass";

			qcom,adsp_qrtr {
				qcom,glink-channels = "IPCRTR";
				qcom,intents = <0x800  5
						0x2000 3
						0x4400 2>;
			};

			qcom,adsp_glink_ssr {
				qcom,glink-channels = "glink_ssr";
				qcom,notify-edges = <&glink_slpi>,
						    <&glink_modem>;
			};

			qcom,pmic_glink_rpmsg {
				qcom,glink-channels = "PMIC_RTR_ADSP_APPS";
			};

			qcom,pmic_glink_log_rpmsg {
				qcom,glink-channels = "PMIC_LOGS_ADSP_APPS";
				qcom,intents = <0x800 5
						0xc00 3>;
			};
		};

		glink_slpi: dsps {
			qcom,remote-pid = <3>;
			transport = "smem";
			mboxes = <&ipcc_mproc IPCC_CLIENT_SLPI
				  IPCC_MPROC_SIGNAL_GLINK_QMP>;
			mbox-names = "dsps_smem";
			interrupt-parent = <&ipcc_mproc>;
			interrupts = <IPCC_CLIENT_SLPI
				      IPCC_MPROC_SIGNAL_GLINK_QMP
				      IRQ_TYPE_EDGE_RISING>;

			label = "slpi";
			qcom,glink-label = "dsps";

			qcom,slpi_qrtr {
				qcom,glink-channels = "IPCRTR";
				qcom,net-id = <2>;
				qcom,low-latency;
				qcom,intents = <0x800  5
						0x2000 3
						0x4400 2>;
			};

			qcom,slpi_glink_ssr {
				qcom,glink-channels = "glink_ssr";
				qcom,notify-edges = <&glink_adsp>,
						    <&glink_modem>;
			};
		};

		glink_cdsp: cdsp {
			qcom,remote-pid = <5>;
			transport = "smem";
			mboxes = <&ipcc_mproc IPCC_CLIENT_CDSP
				  IPCC_MPROC_SIGNAL_GLINK_QMP>;
			mbox-names = "dsps_smem";
			interrupt-parent = <&ipcc_mproc>;
			interrupts = <IPCC_CLIENT_CDSP
				      IPCC_MPROC_SIGNAL_GLINK_QMP
				      IRQ_TYPE_EDGE_RISING>;

			label = "cdsp";
			qcom,glink-label = "cdsp";

			qcom,cdsp_qrtr {
				qcom,glink-channels = "IPCRTR";
				qcom,intents = <0x800  5
						0x2000 3
						0x4400 2>;
			};

			qcom,msm_cdsprm_rpmsg {
				compatible = "qcom,msm-cdsprm-rpmsg";
				qcom,glink-channels = "cdsprmglink-apps-dsp";
				qcom,intents = <0x20 12>;

				msm_cdsp_rm: qcom,msm_cdsp_rm {
					compatible = "qcom,msm-cdsp-rm";
					qcom,qos-latency-us = <60>;
					qcom,qos-maxhold-ms = <20>;
				};
			};
		};

		glink_spss: spss {
			qcom,remote-pid = <8>;
			transport = "spss";
			mboxes = <&ipcc_mproc IPCC_CLIENT_SPSS
				  IPCC_MPROC_SIGNAL_GLINK_QMP>;
			mbox-names = "spss_spss";
			interrupt-parent = <&ipcc_mproc>;
			interrupts = <IPCC_CLIENT_SPSS
				      IPCC_MPROC_SIGNAL_GLINK_QMP
				      IRQ_TYPE_EDGE_RISING>;

			reg = <0x1885008 0x8>,
			      <0x1885010 0x4>;
			reg-names = "qcom,spss-addr",
				    "qcom,spss-size";

			label = "spss";
			qcom,glink-label = "spss";

			qcom,spss_glink_ssr {
				qcom,glink-channels = "glink_ssr";
				qcom,notify-edges = <&glink_modem>;
			};
		};
	};

	qcom,glinkpkt {
		compatible = "qcom,glinkpkt";

		qcom,glinkpkt-at-mdm0 {
			qcom,glinkpkt-edge = "mpss";
			qcom,glinkpkt-ch-name = "DS";
			qcom,glinkpkt-dev-name = "at_mdm0";
		};

		qcom,glinkpkt-apr-apps2 {
			qcom,glinkpkt-edge = "adsp";
			qcom,glinkpkt-ch-name = "apr_apps2";
			qcom,glinkpkt-dev-name = "apr_apps2";
		};

		qcom,glinkpkt-data40-cntl {
			qcom,glinkpkt-edge = "mpss";
			qcom,glinkpkt-ch-name = "DATA40_CNTL";
			qcom,glinkpkt-dev-name = "smdcntl8";
		};

		qcom,glinkpkt-data1 {
			qcom,glinkpkt-edge = "mpss";
			qcom,glinkpkt-ch-name = "DATA1";
			qcom,glinkpkt-dev-name = "smd7";
		};

		qcom,glinkpkt-data4 {
			qcom,glinkpkt-edge = "mpss";
			qcom,glinkpkt-ch-name = "DATA4";
			qcom,glinkpkt-dev-name = "smd8";
		};

		qcom,glinkpkt-data11 {
			qcom,glinkpkt-edge = "mpss";
			qcom,glinkpkt-ch-name = "DATA11";
			qcom,glinkpkt-dev-name = "smd11";
		};
	};

	pil_modem: qcom,mss@8a800000 {
		compatible = "qcom,pil-tz-generic";
		reg = <0x4080000 0x100>;

		clocks = <&clock_rpmh RPMH_CXO_CLK>;
		clock-names = "xo";
		qcom,proxy-clock-names = "xo";

		vdd_cx-supply = <&VDD_CX_LEVEL>;
		qcom,vdd_cx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 100000>;
		vdd_mss-supply = <&VDD_MODEM_LEVEL>;
		qcom,vdd_mss-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 100000>;
		qcom,proxy-reg-names = "vdd_cx", "vdd_mss";

		qcom,firmware-name = "modem";
		memory-region = <&pil_modem_mem>;
		qcom,proxy-timeout-ms = <10000>;
		qcom,sysmon-id = <0>;
		qcom,minidump-id = <3>;
		qcom,aux-minidump-ids = <4>;
		qcom,ssctl-instance-id = <0x12>;
		qcom,pas-id = <4>;
		qcom,smem-id = <421>;
		qcom,signal-aop;
		qcom,complete-ramdump;

		/* Inputs from mss */
		interrupts-extended = <&intc GIC_SPI 264 IRQ_TYPE_LEVEL_HIGH>,
				<&modem_smp2p_in 0 0>,
				<&modem_smp2p_in 2 0>,
				<&modem_smp2p_in 1 0>,
				<&modem_smp2p_in 3 0>,
				<&modem_smp2p_in 7 0>;

		interrupt-names = "qcom,wdog",
				"qcom,err-fatal",
				"qcom,proxy-unvote",
				"qcom,err-ready",
				"qcom,stop-ack",
				"qcom,shutdown-ack";

		/* Outputs to mss */
		qcom,smem-states = <&modem_smp2p_out 0>;
		qcom,smem-state-names = "qcom,force-stop";

		mboxes = <&qmp_aop 0>;
		mbox-names = "mss-pil";
	};

	qcom,lpass@17300000 {
		compatible = "qcom,pil-tz-generic";
		reg = <0x17300000 0x00100>;

		vdd_cx-supply = <&VDD_LPI_CX_LEVEL>;
		qcom,vdd_cx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 0>;
		vdd_mx-supply = <&VDD_LPI_MX_LEVEL>;
		qcom,vdd_mx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 0>;
		qcom,proxy-reg-names = "vdd_cx","vdd_mx";

		clocks = <&clock_rpmh RPMH_CXO_CLK>;
		clock-names = "xo";
		qcom,proxy-clock-names = "xo";

		qcom,pas-id = <1>;
		qcom,proxy-timeout-ms = <10000>;
		qcom,smem-id = <423>;
		qcom,minidump-id = <5>;
		qcom,sysmon-id = <1>;
		qcom,ssctl-instance-id = <0x14>;
		qcom,firmware-name = "adsp";
		memory-region = <&pil_adsp_mem>;
		qcom,signal-aop;
		qcom,complete-ramdump;
		qcom,minidump-as-elf32;

		/* Inputs from lpass */
		interrupts-extended = <&pdc 6 IRQ_TYPE_LEVEL_HIGH>,
				<&adsp_smp2p_in 0 0>,
				<&adsp_smp2p_in 2 0>,
				<&adsp_smp2p_in 1 0>,
				<&adsp_smp2p_in 3 0>;

		interrupt-names = "qcom,wdog",
				"qcom,err-fatal",
				"qcom,proxy-unvote",
				"qcom,err-ready",
				"qcom,stop-ack";

		/* Outputs to lpass */
		qcom,smem-states = <&adsp_smp2p_out 0>;
		qcom,smem-state-names = "qcom,force-stop";

		mboxes = <&qmp_aop 0>;
		mbox-names = "adsp-pil";
	};

	qcom,turing@0x98900000 {
		compatible = "qcom,pil-tz-generic";
		reg = <0x98900000 0x1400000>;

		vdd_cx-supply = <&VDD_CX_LEVEL>;
		qcom,vdd_cx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 100000>;
		vdd_mx-supply = <&VDD_MXC_LEVEL>;
		qcom,vdd_mx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 100000>;
		qcom,proxy-reg-names = "vdd_cx","vdd_mx";

		clocks = <&clock_rpmh RPMH_CXO_CLK>;
		clock-names = "xo";
		qcom,proxy-clock-names = "xo";

		qcom,pas-id = <18>;
		qcom,proxy-timeout-ms = <10000>;
		qcom,smem-id = <601>;
		qcom,minidump-id = <7>;
		qcom,sysmon-id = <7>;
		qcom,ssctl-instance-id = <0x17>;
		qcom,firmware-name = "cdsp";
		memory-region = <&pil_cdsp_mem>;
		qcom,complete-ramdump;
		qcom,minidump-as-elf32;

		interconnects = <&nsp_noc MASTER_CDSP_PROC &mc_virt SLAVE_EBI1>;

		/* Inputs from turing */
		interrupts-extended = <&intc GIC_SPI 578 IRQ_TYPE_LEVEL_HIGH>,
				<&cdsp_smp2p_in 0 0>,
				<&cdsp_smp2p_in 2 0>,
				<&cdsp_smp2p_in 1 0>,
				<&cdsp_smp2p_in 3 0>;

		interrupt-names = "qcom,wdog",
				"qcom,err-fatal",
				"qcom,proxy-unvote",
				"qcom,err-ready",
				"qcom,stop-ack";

		/* Outputs to turing */
		qcom,smem-states = <&cdsp_smp2p_out 0>;
		qcom,smem-state-names = "qcom,force-stop";

	};


	qcom,venus@aab0000 {
		compatible = "qcom,pil-tz-generic";
		reg = <0xaab0000 0x2000>;

		vdd-supply = <&video_cc_mvs0c_gdsc>;
		qcom,proxy-reg-names = "vdd";
		qcom,complete-ramdump;

		clocks = <&clock_videocc VIDEO_CC_XO_CLK>,
			<&clock_videocc VIDEO_CC_MVS0C_CLK>,
			<&clock_videocc VIDEO_CC_AHB_CLK>;
		clock-names = "xo", "core", "ahb";
		qcom,proxy-clock-names = "xo",  "core", "ahb";

		qcom,core-freq = <200000000>;
		qcom,ahb-freq = <200000000>;

		qcom,pas-id = <9>;
		interconnect-names = "pil-venus";
		interconnects = <&mmss_noc MASTER_VIDEO_P0
				&mc_virt SLAVE_EBI1>;
		qcom,proxy-timeout-ms = <100>;
		qcom,firmware-name = "venus";
		memory-region = <&pil_video_mem>;
	};

	qcom,msm_gsi {
		compatible = "qcom,msm_gsi";
	};

	qcom,sps {
		compatible = "qcom,msm-sps-4k";
		qcom,pipe-attr-ee;
	};

	qcom,rmnet-ipa {
		compatible = "qcom,rmnet-ipa3";
		qcom,rmnet-ipa-ssr;
		qcom,ipa-platform-type-msm;
		qcom,ipa-advertise-sg-support;
		qcom,ipa-napi-enable;
	};

	qcom,ipa_fws {
		compatible = "qcom,pil-tz-generic";
		qcom,pas-id = <0xf>;
		qcom,firmware-name = "ipa_fws";
		qcom,pil-force-shutdown;
		memory-region = <&pil_ipa_gsi_mem>;
	};

	ipa_hw: qcom,ipa@1e00000 {
		compatible = "qcom,ipa";
		mboxes = <&qmp_aop 0>;
		reg =
			<0x1e00000 0x84000>,
			<0x1e04000 0x23000>;
		reg-names = "ipa-base", "gsi-base";
		interrupts =
			<0 654 IRQ_TYPE_LEVEL_HIGH>,
			<0 432 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "ipa-irq", "gsi-irq";
		qcom,ipa-hw-ver = <19>; /* IPA core version = IPAv4.9 */
		qcom,ipa-hw-mode = <0>;
		qcom,platform-type = <1>; /* MSM platform */
		qcom,ee = <0>;
		qcom,use-ipa-tethering-bridge;
		qcom,mhi-event-ring-id-limits = <9 11>; /* start and end */
		qcom,modem-cfg-emb-pipe-flt;
		qcom,ipa-wdi3-over-gsi;
		qcom,arm-smmu;
		qcom,smmu-fast-map;
		qcom,use-64-bit-dma-mask;
		qcom,ipa-endp-delay-wa;
		qcom,lan-rx-napi;
		qcom,tx-napi;
		qcom,wan-use-skb-page;
		qcom,rmnet-ctl-enable;
		qcom,ipa-uc-holb-monitor;
		qcom,ipa-holb-monitor-poll-period = <5>;
		qcom,ipa-holb-monitor-max-cnt-wlan = <10>;
		qcom,ipa-holb-monitor-max-cnt-usb = <10>;
		qcom,ipa-holb-monitor-max-cnt-11ad = <10>;
		qcom,tx-wrapper-cache-max-size = <400>;
		qcom,ipa-gpi-event-rp-ddr;
		clock-names = "core_clk";
		clocks = <&clock_rpmh RPMH_IPA_CLK>;
		qcom,interconnect,num-cases = <5>;
		qcom,interconnect,num-paths = <3>;
		interconnects = <&aggre2_noc MASTER_IPA &gem_noc SLAVE_LLCC>,
			<&mc_virt MASTER_LLCC &mc_virt SLAVE_EBI1>,
			<&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_IPA_CFG>;
		interconnect-names = "ipa_to_llcc", "llcc_to_ebi1", "appss_to_ipa";
		/* No vote */
		qcom,no-vote =
		<0 0 0 0 0 0>;

		/* SVS2 */
		qcom,svs2 =
		<150000 600000 150000 1804000 0 74000>;

		/* SVS */
		qcom,svs =
		<625000 1200000 625000 3072000 0 150000>;

		/* NOMINAL */
		qcom,nominal =
		<1250000 2400000 1250000 6220800 0 400000>;

		/* TURBO */
		qcom,turbo =
		<2000000 3500000 2000000 7219200 0 400000>;

		qcom,bus-vector-names = "MIN", "SVS2", "SVS", "NOMINAL",
			"TURBO";
		qcom,throughput-threshold = <600 2500 5000>;
		qcom,scaling-exceptions = <>;

		/* smp2p information */
		qcom,smp2p_map_ipa_1_out {
			compatible = "qcom,smp2p-map-ipa-1-out";
			qcom,smem-states = <&smp2p_ipa_1_out 0>;
			qcom,smem-state-names = "ipa-smp2p-out";
		};

		qcom,smp2p_map_ipa_1_in {
			compatible = "qcom,smp2p-map-ipa-1-in";
			interrupts-extended = <&smp2p_ipa_1_in 0 0>;
			interrupt-names = "ipa-smp2p-in";
		};

		ipa_smmu_ap: ipa_smmu_ap {
			compatible = "qcom,ipa-smmu-ap-cb";
			iommus = <&apps_smmu 0x5C0 0x0>;
			qcom,iommu-dma-addr-pool = <0x20000000 0x20000000>;
			qcom,additional-mapping =
				/* modem tables in IMEM */
				<0x146BD000 0x146BD000 0x2000>;
			dma-coherent;
			qcom,iommu-dma = "fastmap";
			qcom,ipa-q6-smem-size = <36864>;
		};

		ipa_smmu_wlan: ipa_smmu_wlan {
			compatible = "qcom,ipa-smmu-wlan-cb";
			iommus = <&apps_smmu 0x5C1 0x0>;
			qcom,iommu-dma = "atomic";
			dma-coherent;
		};

		ipa_smmu_uc: ipa_smmu_uc {
			compatible = "qcom,ipa-smmu-uc-cb";
			iommus = <&apps_smmu 0x5C2 0x0>;
			qcom,iommu-dma-addr-pool = <0x20000000 0x20000000>;
			qcom,iommu-dma = "atomic";
		};

		ipa_smmu_11ad: ipa_smmu_11ad {
			compatible = "qcom,ipa-smmu-11ad-cb";
			iommus = <&apps_smmu 0x5C3 0x0>;
			dma-coherent;
			qcom,shared-cb;
			qcom,iommu-group = <>;
		};
	};

	qcom,evass@abb0000 {
		compatible = "qcom,pil-tz-generic";
		reg = <0xabb0000 0x2000>;
		status = "ok";
		qcom,pas-id = <26>;
		qcom,firmware-name = "evass";

		memory-region = <&pil_cvp_mem>;
	};

	mem_dump {
		compatible = "qcom,mem-dump";
		memory-region = <&dump_mem>;

		c0_context {
			qcom,dump-size = <0x800>;
			qcom,dump-id = <0x0>;
		};

		c100_context {
			qcom,dump-size = <0x800>;
			qcom,dump-id = <0x1>;
		};

		c200_context {
			qcom,dump-size = <0x800>;
			qcom,dump-id = <0x2>;
		};

		c300_context {
			qcom,dump-size = <0x800>;
			qcom,dump-id = <0x3>;
		};

		c400_context {
			qcom,dump-size = <0x800>;
			qcom,dump-id = <0x4>;
		};

		c500_context {
			qcom,dump-size = <0x800>;
			qcom,dump-id = <0x5>;
		};

		c600_context {
			qcom,dump-size = <0x800>;
			qcom,dump-id = <0x6>;
		};

		c700_context {
			qcom,dump-size = <0x800>;
			qcom,dump-id = <0x7>;
		};

		c0_scandump {
			qcom,dump-size = <0x10100>;
			qcom,dump-id = <0x130>;
		};

		c100_scandump {
			qcom,dump-size = <0x10100>;
			qcom,dump-id = <0x131>;
		};

		c200_scandump {
			qcom,dump-size = <0x10100>;
			qcom,dump-id = <0x132>;
		};

		c300_scandump {
			qcom,dump-size = <0x10100>;
			qcom,dump-id = <0x133>;
		};

		c400_scandump: c400_scandump {
			qcom,dump-size = <0x1a4c0>;
			qcom,dump-id = <0x134>;
		};

		c500_scandump: c500_scandump {
			qcom,dump-size = <0x1a4c0>;
			qcom,dump-id = <0x135>;
		};

		c600_scandump: c600_scandump {
			qcom,dump-size = <0x1a4c0>;
			qcom,dump-id = <0x136>;
		};

		c700_scandump: c700_scandump {
			qcom,dump-size = <0x1a4c0>;
			qcom,dump-id = <0x137>;
		};

		cpuss_reg {
			qcom,dump-size = <0x30000>;
			qcom,dump-id = <0xef>;
		};

		l1_icache0 {
			qcom,dump-size = <0x10900>;
			qcom,dump-id = <0x60>;
		};

		l1_icache100 {
			qcom,dump-size = <0x10900>;
			qcom,dump-id = <0x61>;
		};

		l1_icache200 {
			qcom,dump-size = <0x10900>;
			qcom,dump-id = <0x62>;
		};

		l1_icache300 {
			qcom,dump-size = <0x10900>;
			qcom,dump-id = <0x63>;
		};

		l1_icache400 {
			qcom,dump-size = <0x15100>;
			qcom,dump-id = <0x64>;
		};

		l1_icache500 {
			qcom,dump-size = <0x15100>;
			qcom,dump-id = <0x65>;
		};

		l1_icache600 {
			qcom,dump-size = <0x15100>;
			qcom,dump-id = <0x66>;
		};

		l1_icache700 {
			qcom,dump-size = <0x32100>;
			qcom,dump-id = <0x67>;
		};

		l1_dcache0 {
			qcom,dump-size = <0x9100>;
			qcom,dump-id = <0x80>;
		};

		l1_dcache100 {
			qcom,dump-size = <0x9100>;
			qcom,dump-id = <0x81>;
		};

		l1_dcache200 {
			qcom,dump-size = <0x9100>;
			qcom,dump-id = <0x82>;
		};

		l1_dcache300 {
			qcom,dump-size = <0x9100>;
			qcom,dump-id = <0x83>;
		};

		l1_dcache400 {
			qcom,dump-size = <0x9100>;
			qcom,dump-id = <0x84>;
		};

		l1_dcache500 {
			qcom,dump-size = <0x9100>;
			qcom,dump-id = <0x85>;
		};

		l1_dcache600 {
			qcom,dump-size = <0x9100>;
			qcom,dump-id = <0x86>;
		};

		l1_dcache700 {
			qcom,dump-size = <0x12100>;
			qcom,dump-id = <0x87>;
		};

		l1_itlb400 {
			qcom,dump-size = <0x300>;
			qcom,dump-id = <0x24>;
		};

		l1_itlb500 {
			qcom,dump-size = <0x300>;
			qcom,dump-id = <0x25>;
		};

		l1_itlb600 {
			qcom,dump-size = <0x300>;
			qcom,dump-id = <0x26>;
		};

		l1_itlb700 {
			qcom,dump-size = <0x400>;
			qcom,dump-id = <0x27>;
		};

		l1_dtlb400 {
			qcom,dump-size = <0x300>;
			qcom,dump-id = <0x44>;
		};

		l1_dtlb500 {
			qcom,dump-size = <0x300>;
			qcom,dump-id = <0x45>;
		};

		l1_dtlb600 {
			qcom,dump-size = <0x300>;
			qcom,dump-id = <0x46>;
		};

		l1_dtlb700 {
			qcom,dump-size = <0x3a0>;
			qcom,dump-id = <0x47>;
		};

		l2_cache400 {
			qcom,dump-size = <0x90100>;
			qcom,dump-id = <0xc4>;
		};

		l2_cache500 {
			qcom,dump-size = <0x90100>;
			qcom,dump-id = <0xc5>;
		};

		l2_cache600 {
			qcom,dump-size = <0x90100>;
			qcom,dump-id = <0xc6>;
		};

		l2_cache700 {
			qcom,dump-size = <0x120100>;
			qcom,dump-id = <0xc7>;
		};

		l2_tlb0 {
			qcom,dump-size = <0x5b00>;
			qcom,dump-id = <0x120>;
		};

		l2_tlb100 {
			qcom,dump-size = <0x5b00>;
			qcom,dump-id = <0x121>;
		};

		l2_tlb200 {
			qcom,dump-size = <0x5b00>;
			qcom,dump-id = <0x122>;
		};

		l2_tlb300 {
			qcom,dump-size = <0x5b00>;
			qcom,dump-id = <0x123>;
		};

		l2_tlb400 {
			qcom,dump-size = <0x6100>;
			qcom,dump-id = <0x124>;
		};

		l2_tlb500 {
			qcom,dump-size = <0x6100>;
			qcom,dump-id = <0x125>;
		};

		l2_tlb600 {
			qcom,dump-size = <0x6100>;
			qcom,dump-id = <0x126>;
		};

		l2_tlb700 {
			qcom,dump-size = <0xc100>;
			qcom,dump-id = <0x127>;
		};

		gemnoc {
			qcom,dump-size = <0x100000>;
			qcom,dump-id = <0x162>;
		};

		mhm_scan {
			qcom,dump-size = <0x20000>;
			qcom,dump-id = <0x161>;
		};

		rpmh {
			qcom,dump-size = <0x2000000>;
			qcom,dump-id = <0xec>;
		};

		rpm_sw {
			qcom,dump-size = <0x28000>;
			qcom,dump-id = <0xea>;
		};

		pmic {
			qcom,dump-size = <0x200000>;
			qcom,dump-id = <0xe4>;
		};

		fcm {
			qcom,dump-size = <0x8400>;
			qcom,dump-id = <0xee>;
		};

		etf_swao {
			qcom,dump-size = <0x10000>;
			qcom,dump-id = <0xf1>;
		};

		etr_reg {
			qcom,dump-size = <0x1000>;
			qcom,dump-id = <0x100>;
		};

		etfswao_reg {
			qcom,dump-size = <0x1000>;
			qcom,dump-id = <0x102>;
		};

		misc_data {
			qcom,dump-size = <0x1000>;
			qcom,dump-id = <0xe8>;
		};

		etf_slpi {
			qcom,dump-size = <0x4000>;
			qcom,dump-id = <0xf3>;
		};

		etfslpi_reg {
			qcom,dump-size = <0x1000>;
			qcom,dump-id = <0x103>;
		};

		etf_lpass {
			qcom,dump-size = <0x4000>;
			qcom,dump-id = <0xf4>;
		};

		etflpass_reg {
			qcom,dump-size = <0x1000>;
			qcom,dump-id = <0x104>;
		};

		LLCC_1: llcc_1_dcache {
			qcom,dump-size = <0x1141c0>;
			qcom,dump-id = <0x140>;
		};

		LLCC_2: llcc_2_dcache {
			qcom,dump-size = <0x1141c0>;
			qcom,dump-id = <0x141>;
		};

		LLCC_3: llcc_3_dcache {
			qcom,dump-size = <0x1141c0>;
			qcom,dump-id = <0x142>;
		};

		LLCC_4: llcc_4_dcache {
			qcom,dump-size = <0x1141c0>;
			qcom,dump-id = <0x143>;
		};
	};

	qcom,ssc@5c00000 {
		compatible = "qcom,pil-tz-generic";
		reg = <0x5c00000 0x4000>;

		vdd_cx-supply = <&VDD_LPI_CX_LEVEL>;
		qcom,vdd_cx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 0>;
		vdd_mx-supply = <&VDD_LPI_MX_LEVEL>;
		qcom,vdd_mx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 0>;
		qcom,proxy-reg-names = "vdd_cx", "vdd_mx";

		clocks = <&clock_rpmh RPMH_CXO_CLK>;
		clock-names = "xo";
		qcom,proxy-clock-names = "xo";

		qcom,pas-id = <12>;
		qcom,proxy-timeout-ms = <10000>;
		qcom,smem-id = <424>;
		qcom,sysmon-id = <3>;
		qcom,ssctl-instance-id = <0x16>;
		qcom,firmware-name = "slpi";
		status = "ok";
		memory-region = <&pil_slpi_mem>;
		qcom,complete-ramdump;
		qcom,signal-aop;

		/* Inputs from ssc */
		interrupts-extended = <&pdc 9 IRQ_TYPE_LEVEL_HIGH>,
				<&dsps_smp2p_in 0 0>,
				<&dsps_smp2p_in 2 0>,
				<&dsps_smp2p_in 1 0>,
				<&dsps_smp2p_in 3 0>;

		interrupt-names = "qcom,wdog",
				"qcom,err-fatal",
				"qcom,proxy-unvote",
				"qcom,err-ready",
				"qcom,stop-ack";

		/* Outputs to ssc */
		qcom,smem-states = <&dsps_smp2p_out 0>;
		qcom,smem-state-names = "qcom,force-stop";

		mboxes = <&qmp_aop 0>;
		mbox-names = "slpi-pil";
	};

	/* PIL spss node - for loading Secure Processor */
	qcom,spss@1880000 {
		compatible = "qcom,pil-tz-generic";
		reg = <0x188101c 0x4>,
		      <0x1881024 0x4>,
		      <0x1881028 0x4>,
		      <0x188103c 0x4>,
		      <0x1881100 0x4>,
		      <0x1882014 0x4>;
		reg-names = "sp2soc_irq_status", "sp2soc_irq_clr",
			    "sp2soc_irq_mask", "rmb_err",
			    "rmb_general_purpose", "rmb_err_spare2";
		interrupts = <0 352 1>;

		vdd_cx-supply = <&VDD_CX_LEVEL>;
		qcom,proxy-reg-names = "vdd_cx";
		qcom,vdd_cx-uV-uA = <RPMH_REGULATOR_LEVEL_TURBO 100000>;
		vdd_mx-supply = <&VDD_MXA_LEVEL>;
		vdd_mx-uV = <RPMH_REGULATOR_LEVEL_TURBO 100000>;

		clocks = <&clock_rpmh RPMH_CXO_CLK>;
		clock-names = "xo";
		qcom,proxy-clock-names = "xo";
		qcom,pil-generic-irq-handler;
		status = "ok";

		qcom,signal-aop;
		qcom,complete-ramdump;

		qcom,boot-enabled;
		qcom,pas-id = <14>;
		qcom,proxy-timeout-ms = <10000>;
		qcom,firmware-name = "spss";
		memory-region = <&pil_spss_mem>;
		qcom,spss-scsr-bits = <24 25>;
		qcom,extra-size = <4096>;

		mboxes = <&qmp_aop 0>;
		mbox-names = "spss-pil";
	};

	qcom,trustedvm@d0800000 {
		compatible = "qcom,pil-tz-generic";
		status = "ok";
		qcom,pas-id = <28>;
		qcom,firmware-name = "trustedvm";
		memory-region = <&pil_trustedvm_mem>;
	};

	qcom,guestvm_loader {
		compatible = "qcom,guestvm-loader";
		image_to_be_loaded = "trustedvm";
	};

	ssc_sensors: qcom,msm-ssc-sensors {
		compatible = "qcom,msm-ssc-sensors";
		status = "ok";
		qcom,firmware-name = "slpi";
	};

	qcom_tzlog: tz-log@146bf720 {
		compatible = "qcom,tz-log";
		reg = <0x146bf720 0x3000>;
		qcom,hyplog-enabled;
		hyplog-address-offset = <0x410>;
		hyplog-size-offset = <0x414>;
	};

	qcom_qseecom: qseecom@c1700000 {
		compatible = "qcom,qseecom";
		memory-region = <&qseecom_mem>;
		qcom,hlos-num-ce-hw-instances = <1>;
		qcom,hlos-ce-hw-instance = <0>;
		qcom,qsee-ce-hw-instance = <0>;
		qcom,disk-encrypt-pipe-pair = <2>;
		qcom,no-clock-support;
		qcom,appsbl-qseecom-support;
		qcom,commonlib64-loaded-by-uefi;
		qcom,qsee-reentrancy-support = <2>;
	};

	qcom,spcom {
		compatible = "qcom,spcom";

		/* predefined channels, remote side is server */
		qcom,spcom-ch-names = "sp_kernel", "sp_ssr";
		/* sp2soc rmb shared register physical address and bmsk */
		qcom,spcom-sp2soc-rmb-reg-addr = <0x01881020>;
		qcom,spcom-sp2soc-rmb-initdone-bit = <24>;
		qcom,spcom-sp2soc-rmb-pbldone-bit = <25>;
		/* soc2sp rmb shared register physical address */
		qcom,spcom-soc2sp-rmb-reg-addr = <0x01881030>;
		qcom,spcom-soc2sp-rmb-sp-ssr-bit = <0>;
		qcom,boot-enabled;
		status = "ok";
	};

	spss_utils: qcom,spss_utils {
		compatible = "qcom,spss-utils";
		/* spss fuses physical address */
		qcom,spss-fuse1-addr = <0x00780204>;
		qcom,spss-fuse1-bit = <9>;
		qcom,spss-fuse2-addr = <0x00780204>;
		qcom,spss-fuse2-bit = <8>;
		qcom,spss-fuse3-addr = <0x007801C0>; // IAR_FEATURE_ENABLED fuse
		qcom,spss-fuse3-bit = <10>;
		qcom,spss-fuse4-addr = <0x00780204>; // IAR_STATE fuse
		qcom,spss-fuse4-bit = <25>; // 0x00780204 bits 25-27
		qcom,spss-dev-firmware-name  = "spss1d";  /* 8 chars max */
		qcom,spss-test-firmware-name = "spss1t";  /* 8 chars max */
		qcom,spss-prod-firmware-name = "spss1p";  /* 8 chars max */
		qcom,spss-debug-reg-addr = <0x01886020>;
		qcom,spss-scsr-regs-addr = <0x01880000>;  /* SPU shared register */
		qcom,spss-emul-type-reg-addr = <0x01fc8004>;
		pil-mem = <&pil_spss_mem>;
		qcom,pil-size = <0x0F0000>; // padding to 960 KB
		status = "ok";
	};

	hyp_core_ctl: qcom,hyp-core-ctl {
		compatible = "qcom,hyp-core-ctl";
		status = "ok";
	};

	eud: qcom,msm-eud@88e0000 {
		compatible = "qcom,msm-eud";
		interrupt-names = "eud_irq";
		interrupt-parent = <&pdc>;
		interrupts = <11 IRQ_TYPE_LEVEL_HIGH>;
		reg = <0x088E0000 0x2000>,
			<0x088E2000 0x1000>;
		reg-names = "eud_base", "eud_mode_mgr2";
		qcom,secure-eud-en;
		status = "ok";
	};

	qcom_rng: qrng@10d3000 {
		compatible = "qcom,msm-rng";
		reg = <0x10d3000 0x1000>;
		qcom,no-qrng-config;
		interconnect-names = "data_path";
		interconnects = <&gem_noc MASTER_APPSS_PROC &config_noc SLAVE_HWKM>;
		clock-names = "km_clk_src";
		clocks = <&clock_rpmh RPMH_HWKM_CLK>;
	};

	qcom_cedev: qcedev@1de0000 {
		compatible = "qcom,qcedev";
		reg = <0x1de0000 0x20000>,
			<0x1dc4000 0x24000>;
		reg-names = "crypto-base","crypto-bam-base";
		interrupts = <GIC_SPI 272 IRQ_TYPE_LEVEL_HIGH>;
		qcom,bam-pipe-pair = <3>;
		qcom,ce-hw-instance = <0>;
		qcom,ce-device = <0>;
		qcom,ce-hw-shared;
		qcom,bam-ee = <0>;
		qcom,smmu-s1-enable;
		qcom,no-clock-support;
		interconnect-names = "data_path";
		interconnects = <&aggre2_noc MASTER_CRYPTO &mc_virt SLAVE_EBI1>;
		iommus = <&apps_smmu 0x0586 0x0011>,
			 <&apps_smmu 0x0596 0x0011>;
		qcom,iommu-dma = "atomic";

		qcom_cedev_ns_cb {
			compatible = "qcom,qcedev,context-bank";
			label = "ns_context";
			iommus = <&apps_smmu 0x592 0>,
				 <&apps_smmu 0x598 0>,
				 <&apps_smmu 0x599 0>,
				 <&apps_smmu 0x59F 0>;
		};

		qcom_cedev_s_cb {
			compatible = "qcom,qcedev,context-bank";
			label = "secure_context";
			iommus = <&apps_smmu 0x593 0>,
				 <&apps_smmu 0x59C 0>,
				 <&apps_smmu 0x59D 0>,
				 <&apps_smmu 0x59E 0>;
			qcom,iommu-vmid = <0x9>; /* VMID_CP_BITSTREAM */
			qcom,secure-context-bank;
		};
	};

	qcom_crypto: qcrypto@1de0000 {
		compatible = "qcom,qcrypto";
		reg = <0x1de0000 0x20000>,
			 <0x1dc4000 0x24000>;
		reg-names = "crypto-base","crypto-bam-base";
		interrupts = <GIC_SPI 272 IRQ_TYPE_LEVEL_HIGH>;
		qcom,bam-pipe-pair = <2>;
		qcom,ce-hw-instance = <0>;
		qcom,ce-device = <0>;
		qcom,bam-ee = <0>;
		qcom,ce-hw-shared;
		qcom,clk-mgmt-sus-res;
		qcom,use-sw-aes-cbc-ecb-ctr-algo;
		qcom,use-sw-aes-xts-algo;
		qcom,use-sw-aes-ccm-algo;
		qcom,use-sw-ahash-algo;
		qcom,use-sw-aead-algo;
		qcom,use-sw-hmac-algo;
		qcom,smmu-s1-enable;
		qcom,no-clock-support;
		interconnect-names = "data_path";
		interconnects = <&aggre2_noc MASTER_CRYPTO &mc_virt SLAVE_EBI1>;
		iommus = <&apps_smmu 0x0584 0x0011>,
			 <&apps_smmu 0x0594 0x0011>;
		qcom,iommu-dma = "atomic";
	};

	wlan: qcom,cnss-qca6490@b0000000 {
		compatible = "qcom,cnss-qca6490";
		reg = <0xb0000000 0x10000>,
		      <0xb2e5510 0x690>;
		reg-names = "smmu_iova_ipa", "tcs_cmd";
		wlan-en-gpio = <&tlmm 64 0>;
		qcom,bt-en-gpio = <&tlmm 65 0>;
		pinctrl-names = "wlan_en_active", "wlan_en_sleep";
		pinctrl-0 = <&cnss_wlan_en_active>;
		pinctrl-1 = <&cnss_wlan_en_sleep>;
		qcom,wlan-rc-num = <0>;
		qcom,wlan-ramdump-dynamic = <0x420000>;
		qcom,wlan-cbc-enabled;
		/* RPMH_PDC_WLAN_RF_TCS<6>_CMD<2> offset */
		qcom,tcs_offset_int_pow_amp_vreg = <0x4D0>;
		use-pm-domain;
		cnss-enable-self-recovery;

		vdd-wlan-aon-supply = <&S2E>;
		qcom,vdd-wlan-aon-config = <950000 952000 0 0 1>;
		vdd-wlan-dig-supply = <&S11B>;
		qcom,vdd-wlan-dig-config = <950000 952000 0 0 1>;
		vdd-wlan-io-supply = <&S10B>;
		qcom,vdd-wlan-io-config = <1800000 1800000 0 0 1>;
		vdd-wlan-rfa1-supply = <&S1C>;
		qcom,vdd-wlan-rfa1-config = <1880000 1880000 0 0 1>;
		vdd-wlan-rfa2-supply = <&S12B>;
		qcom,vdd-wlan-rfa2-config = <1350000 1350000 0 0 1>;
		wlan-ant-switch-supply = <&L7E>;
		qcom,wlan-ant-switch-config = <2800000 2800000 0 0 0>;

		interconnects =
		<&aggre2_noc MASTER_PCIE_0 &aggre2_noc SLAVE_ANOC_PCIE_GEM_NOC>,
		<&gem_noc MASTER_ANOC_PCIE_GEM_NOC &mc_virt SLAVE_EBI1>;
		interconnect-names = "pcie_to_memnoc", "memnoc_to_ddr";

		qcom,icc-path-count = <2>;
		qcom,bus-bw-cfg-count = <7>;
		qcom,bus-bw-cfg =
		/** ICC Path 1 **/
		<0 0>, /* no vote */
		/* idle: 0-18 Mbps snoc/anoc: 100 Mhz ddr: 451.2 MHz */
		<2250 390000>,
		/* low: 18-60 Mbps snoc/anoc: 100 Mhz ddr: 451.2 MHz */
		<7500 390000>,
		/* medium: 60-240 Mbps snoc/anoc: 200 Mhz ddr: 451.2 MHz */
		<30000 790000>,
		/* high: 240-1080 Mbps snoc/anoc: 200 Mhz ddr: 451.2 MHz */
		<100000 790000>,
		/* very high: > 1080 Mbps snoc/anoc: 403 Mhz ddr: 451.2 MHz */
		<175000 1600000>,
		/* low (latency critical): 18-60 Mbps snoc/anoc: 200 Mhz
		 * ddr: 547.2 MHz
		 */
		<7500 390000>,

		/** ICC Path 2 **/
		<0 0>,
		<2250 1804800>,
		<7500 1804800>,
		<30000 1804800>,
		<100000 1804800>,
		<175000 6220800>,
		<7500 2188800>;

		mhi,max-channels = <30>;
		mhi,timeout = <10000>;
		mhi,buffer-len = <0x8000>;
		mhi,m2-no-db-access;

		mhi_channels {
			#address-cells = <1>;
			#size-cells = <0>;

			mhi_chan@0 {
				reg = <0>;
				label = "LOOPBACK";
				mhi,num-elements = <32>;
				mhi,event-ring = <1>;
				mhi,chan-dir = <1>;
				mhi,data-type = <0>;
				mhi,doorbell-mode = <2>;
				mhi,ee = <0x14>;
			};

			mhi_chan@1 {
				reg = <1>;
				label = "LOOPBACK";
				mhi,num-elements = <32>;
				mhi,event-ring = <1>;
				mhi,chan-dir = <2>;
				mhi,data-type = <0>;
				mhi,doorbell-mode = <2>;
				mhi,ee = <0x14>;
			};

			mhi_chan@4 {
				reg = <4>;
				label = "DIAG";
				mhi,num-elements = <32>;
				mhi,event-ring = <1>;
				mhi,chan-dir = <1>;
				mhi,data-type = <0>;
				mhi,doorbell-mode = <2>;
				mhi,ee = <0x14>;
			};

			mhi_chan@5 {
				reg = <5>;
				label = "DIAG";
				mhi,num-elements = <32>;
				mhi,event-ring = <1>;
				mhi,chan-dir = <2>;
				mhi,data-type = <0>;
				mhi,doorbell-mode = <2>;
				mhi,ee = <0x14>;
			};

			mhi_chan@20 {
				reg = <20>;
				label = "IPCR";
				mhi,num-elements = <32>;
				mhi,event-ring = <1>;
				mhi,chan-dir = <1>;
				mhi,data-type = <1>;
				mhi,doorbell-mode = <2>;
				mhi,ee = <0x14>;
				mhi,auto-start;
			};

			mhi_chan@21 {
				reg = <21>;
				label = "IPCR";
				mhi,num-elements = <32>;
				mhi,event-ring = <1>;
				mhi,chan-dir = <2>;
				mhi,data-type = <0>;
				mhi,doorbell-mode = <2>;
				mhi,ee = <0x14>;
				mhi,auto-queue;
				mhi,auto-start;
			};
		};

		mhi_events {
			mhi_event@0 {
				mhi,num-elements = <32>;
				mhi,intmod = <0>;
				mhi,msi = <1>;
				mhi,priority = <0>;
				mhi,brstmode = <2>;
				mhi,data-type = <1>;
			};

			mhi_event@1 {
				mhi,num-elements = <256>;
				mhi,intmod = <0>;
				mhi,msi = <2>;
				mhi,priority = <1>;
				mhi,brstmode = <2>;
			};

			mhi_event@2 {
				mhi,num-elements = <32>;
				mhi,intmod = <0>;
				mhi,msi = <0>;
				mhi,priority = <2>;
				mhi,brstmode = <2>;
				mhi,data-type = <3>;
			};
		};

		mhi_devices {
			mhi_qrtr {
				mhi,chan = "IPCR";
				qcom,net-id = <0>;
				qcom,low-latency;
			};
		};
	};

	qcom,pmic_glink {
		compatible = "qcom,pmic-glink";
		qcom,pmic-glink-channel = "PMIC_RTR_ADSP_APPS";
		qcom,subsys-name = "adsp";
		qcom,protection-domain = "tms/servreg", "msm/adsp/charger_pd";

		battery_charger: qcom,battery_charger {
			compatible = "qcom,battery-charger";
		};

		qcom,ucsi {
			compatible = "qcom,ucsi-glink";
			port {
				usb_port0_connector: endpoint {
					remote-endpoint = <&usb_port0>;
				};
			};
		};

		altmode: qcom,altmode {
			compatible = "qcom,altmode-glink";
			#altmode-cells = <1>;
		};
	};

	qcom,pmic_glink_log {
		compatible = "qcom,pmic-glink";
		qcom,pmic-glink-channel = "PMIC_LOGS_ADSP_APPS";

		qcom,battery_debug {
			compatible = "qcom,battery-debug";
		};

		spmi_glink_debug: qcom,spmi_glink_debug {
			compatible = "qcom,spmi-glink-debug";
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";

			/* Primary SPMI bus */
			spmi@0 {
				reg = <0>;
				#address-cells = <2>;
				#size-cells = <0>;

				qcom,pm8350b-debug@3 {
					compatible = "qcom,spmi-pmic";
					reg = <0x3 SPMI_USID>;
					qcom,can-sleep;
				};
			};

			/* Secondary (QUP) SPMI bus */
			spmi@1 {
				reg = <1>;
				#address-cells = <2>;
				#size-cells = <0>;

				qcom,smb1396-debug@b {
					compatible = "qcom,spmi-pmic";
					reg = <0xb SPMI_USID>;
					qcom,can-sleep;
				};

				qcom,smb1396-debug@c {
					compatible = "qcom,spmi-pmic";
					reg = <0xc SPMI_USID>;
					qcom,can-sleep;
				};

				smb1398_debug: qcom,smb1398-debug@d {
					compatible = "qcom,spmi-pmic";
					reg = <0xd SPMI_USID>;
					qcom,can-sleep;
					status = "disabled";
				};
			};
		};
	};

	bluetooth: bt_qca6490 {
		compatible = "qcom,qca6490";
		reg = <0xb2e5510 0x690>;
		reg-names = "tcs_cmd";
		pinctrl-names = "default";
		pinctrl-0 = <&bt_en_sleep>;
		/* offset=(0xC8*6) + (0x10*2) */
		qcom,tcs_offset_ipa = <0x4D0>;
		qcom,bt-reset-gpio = <&tlmm 65 0>; /* BT_EN */
		qcom,bt-sw-ctrl-gpio = <&tlmm 153 0>; /* SW_CTRL */
		qcom,bt-vdd-aon-supply = <&S11B>;
		qcom,bt-vdd-dig-supply = <&S11B>;
		qcom,bt-vdd-rfa1-supply = <&S1C>;
		qcom,bt-vdd-rfa2-supply = <&S12B>;
		qcom,bt-vdd-asd-supply = <&L7E>;

		qcom,bt-vdd-aon-config = <950000 950000 0 1>;
		qcom,bt-vdd-dig-config = <950000 950000 0 1>;
		qcom,bt-vdd-rfa1-config = <1880000 1880000 0 1>;
		qcom,bt-vdd-rfa2-config = <1350000 1350000 0 1>;
		qcom,bt-vdd-asd-config = <2800000 2800000 0 1>;
	};

	wil6210: qcom,wil6210 {
		compatible = "qcom,wil6210";
		qcom,pcie-parent = <&pcie1>;
		qcom,wigig-en = <&tlmm 47 0>;
		pinctrl-names = "default";
		pinctrl-0 = <&wil6210_refclk_en_pin>;
		qcom,11ad-bus-bw,name = "wil6210";
		qcom,11ad-bus-bw,num-cases = <3>;
		qcom,11ad-bus-bw,num-paths = <1>;
		qcom,11ad-bus-bw,vectors-KBps =
			<100 512 0 0>,
			<100 512 600000 800000>,  /* ~4.6Gbps (MCS12) */
			<100 512 1300000 1300000>; /* ~10.1Gbps */
		qcom,use-ext-supply;
		vdd-s1c-supply = <&S1C>;
		qcom,use-ext-clocks;
		clocks = <&clock_rpmh RPMH_RF_CLK5>;
		clock-names = "rf_clk";
		qcom,keep-radio-on-during-sleep;
		qcom,use-ap-power-save;
		status = "disabled";
	};

	cpuss-sleep-stats@18000054 {
	      compatible = "qcom,cpuss-sleep-stats";
	      reg = <0x18000054 0x4>, <0x18010054 0x4>, <0x18020054 0x4>,
		    <0x18030054 0x4>, <0x18040054 0x4>, <0x18050054 0x4>,
		    <0x18060054 0x4>, <0x18070054 0x4>, <0x18080098 0x4>,
		    <0x180C0000 0x10000>;
	      reg-names = "seq_lpm_cntr_cfg_cpu0", "seq_lpm_cntr_cfg_cpu1",
			  "seq_lpm_cntr_cfg_cpu2", "seq_lpm_cntr_cfg_cpu3",
			  "seq_lpm_cntr_cfg_cpu4", "seq_lpm_cntr_cfg_cpu5",
			  "seq_lpm_cntr_cfg_cpu6", "seq_lpm_cntr_cfg_cpu7",
			  "l3_seq_lpm_cntr_cfg", "apss_seq_mem_base";
	      num-cpus = <8>;
	};

	soc-sleep-stats@c3f0000 {
		compatible = "qcom,rpmh-sleep-stats";
		reg = <0xc3f0000 0x400>;
	};

	sys-pm-vx@c320000 {
		compatible = "qcom,sys-pm-violators", "qcom,sys-pm-lahaina";
		reg = <0xc320000 0x0400>;
		mboxes = <&qmp_aop 0>;
		mbox-names = "aop";
	};

};

#include "ipcc-test.dtsi"
#include "lahaina-regulators.dtsi"
#include "lahaina-pinctrl.dtsi"
#include "lahaina-smp2p.dtsi"
#include "lahaina-ion.dtsi"
#include "waipio-dma-heaps.dtsi"
#include "msm-arm-smmu-lahaina.dtsi"
#include "lahaina-usb.dtsi"
#include "lahaina-coresight.dtsi"
#include "lahaina-qupv3.dtsi"
#include "lahaina-vidc.dtsi"
#include "lahaina-cvp.dtsi"
#include "lahaina-pcie.dtsi"
#include "msm-qvr-external.dtsi"

&pcie0_rp {
	#address-cells = <5>;
	#size-cells = <0>;

	cnss_pci: cnss_pci {
		reg = <0 0 0 0 0>;
		qcom,iommu-group = <&cnss_pci_iommu_group>;
		memory-region = <&cnss_wlan_mem>;

		#address-cells = <1>;
		#size-cells = <1>;

		cnss_pci_iommu_group: cnss_pci_iommu_group {
			qcom,iommu-dma-addr-pool = <0xa0000000 0x10000000>;
			qcom,iommu-dma = "fastmap";
			qcom,iommu-pagetable = "coherent";
			qcom,iommu-faults = "stall-disable", "HUPCF", "no-CFRE",
					    "non-fatal";
		};
	};
};

&pcie1_rp {
	#address-cells = <5>;
	#size-cells = <0>;

	wil6210_pci: wil6210_pci {
		reg = <0 0 0 0 0>;
		qcom,iommu-group = <&wil6210_pci_iommu_group>;

		#address-cells = <1>;
		#size-cells = <1>;

		wil6210_pci_iommu_group: wil6210_pci_iommu_group {
			reg = <0 0>;
			qcom,iommu-dma-addr-pool = <0x60000000 0xa0000000>;
			qcom,iommu-dma = "fastmap";
			qcom,iommu-pagetable = "coherent";
		};
	};
};

#include "lahaina-gpu.dtsi"
#include "lahaina-thermal.dtsi"

&qupv3_se18_4uart {
	status = "ok";
};

&qupv3_se13_i2c {
	status = "ok";
	nq@64 {
		compatible = "rtc6226";
		reg = <0x64>;
		fmint-gpio = <&tlmm 50 0>;
		vdd-supply = <&L7E>;
		rtc6226,vdd-supply-voltage = <2800000 2800000>;
		vio-supply = <&S10B>;
		rtc6226,vio-supply-voltage = <1800000 1800000 >;
	};
};

#include "msm-rdbg.dtsi"
