#include "holi-sde-display.dtsi"

&dsi_rm69299_visionox_amoled_video {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_dcs";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <255>;
	qcom,platform-te-gpio = <&tlmm 23 0>;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&dsi_rm69299_visionox_amoled_cmd {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_dcs";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <255>;
	qcom,platform-te-gpio = <&tlmm 23 0>;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};


&dsi_sim_vid {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_dcs";
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&dsi_sharp_qsync_fhd_video {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply_labibb>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_wled";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <4095>;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&dsi_sharp_qsync_fhd_cmd {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply_labibb>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_wled";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <4095>;
	qcom,platform-te-gpio = <&tlmm 23 0>;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&dsi_sharp_qsync_fhd_60hz_cmd {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply_labibb>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_wled";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <4095>;
	qcom,platform-te-gpio = <&tlmm 23 0>;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&dsi_r66451_amoled_cmd {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply_vddio_182>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_dcs";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <4095>;
	qcom,mdss-brightness-max-level = <255>;
	qcom,mdss-dsi-bl-inverted-dbv;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&dsi_r66451_amoled_video {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply_vddio_182>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_dcs";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <4095>;
	qcom,mdss-brightness-max-level = <255>;
	qcom,mdss-dsi-bl-inverted-dbv;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&dsi_r66451_amoled_60hz_video {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_dcs";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <4095>;
	qcom,mdss-brightness-max-level = <255>;
	qcom,mdss-dsi-bl-inverted-dbv;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&dsi_r66451_amoled_60hz_cmd {
	qcom,panel-supply-entries = <&dsi_panel_pwr_supply>;
	qcom,mdss-dsi-bl-pmic-control-type = "bl_ctrl_dcs";
	qcom,mdss-dsi-bl-min-level = <1>;
	qcom,mdss-dsi-bl-max-level = <4095>;
	qcom,mdss-brightness-max-level = <255>;
	qcom,mdss-dsi-bl-inverted-dbv;
	qcom,platform-reset-gpio = <&pm6150l_gpios 9 0>;
};

&sde_dsi {
	qcom,dsi-default-panel = <&dsi_rm69299_visionox_amoled_video>;
};
