&soc {
	audio_etm0 {
		compatible = "qcom,coresight-remote-etm";

		coresight-name = "coresight-audio-etm0";
		qcom,inst-id = <5>;
		atid = <40>;

		out-ports {
			port {
				audio_etm0_out_funnel_lpass_lpi: endpoint {
					remote-endpoint =
					<&funnel_lpass_lpi_in_audio_etm0>;
				};
			};
		};
	};

	tpdm_lpass_lpi: tpdm_lpass_lpi {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-tpdm-lpass-lpi";
		qcom,dummy-source;

		atid = <26>;

		out-ports {
			port {
				tpdm_lpass_lpi_out_funnel_lpass_lpi: endpoint {
					remote-endpoint =
					<&funnel_lpass_lpi_in_tpdm_lpass_lpi>;
				};
			};
		};
	};

	tpdm_lpass: tpdm@10844000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10844000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-lpass";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		atid = <74>;
		out-ports {
			port {
				tpdm_lpass_out_funnel_lpass: endpoint {
					remote-endpoint =
					<&funnel_lpass_in_tpdm_lpass>;
				};
			};
		};
	};

	tpdm_dl_lpass: tpdm@10c38000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c38000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-dl-lpass";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		atid = <74>;
		out-ports {
			port {
				tpdm_dl_lpass_out_tpda_dl_lpass_10: endpoint {
					remote-endpoint =
					<&tpda_dl_lpass_10_in_tpdm_dl_lpass>;
				};
			};
		};
	};

	lpass_stm: lpass_stm {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-lpass-stm";
		qcom,dummy-source;

		atid = <25>;

		out-ports {
			port {
				lpass_stm_out_funnel_lpass_lpi: endpoint {
					remote-endpoint =
					<&funnel_lpass_lpi_in_lpass_stm>;
				};
			};
		};
	};

	tpdm_swao_prio_0: tpdm@10b09000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b09000 0x1000>;
		reg-names = "tpdm-base";

		atid = <71>;
		coresight-name = "coresight-tpdm-swao-prio-0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_prio_0_out_tpda_aoss_0: endpoint {
					remote-endpoint =
					<&tpda_aoss_0_in_tpdm_swao_prio_0>;
				};
			};
		};
	};

	tpdm_swao_prio_1: tpdm@10b0a000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b0a000 0x1000>;
		reg-names = "tpdm-base";

		atid = <71>;
		coresight-name = "coresight-tpdm-swao-prio-1";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_prio_1_out_tpda_aoss_1: endpoint {
					remote-endpoint =
					<&tpda_aoss_1_in_tpdm_swao_prio_1>;
				};
			};
		};
	};

	tpdm_swao_prio_2: tpdm@10b0b000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b0b000 0x1000>;
		reg-names = "tpdm-base";

		atid = <71>;
		coresight-name = "coresight-tpdm-swao-prio-2";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_prio_2_out_tpda_aoss_2: endpoint {
					remote-endpoint =
					<&tpda_aoss_2_in_tpdm_swao_prio_2>;
				};
			};
		};
	};

	tpdm_swao_prio_3: tpdm@10b0c000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b0c000 0x1000>;
		reg-names = "tpdm-base";

		atid = <71>;
		coresight-name = "coresight-tpdm-swao-prio-3";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_prio_3_out_tpda_aoss_3: endpoint {
					remote-endpoint =
					<&tpda_aoss_3_in_tpdm_swao_prio_3>;
				};
			};
		};
	};

	tpdm_swao_1: tpdm@10b0d000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b0d000 0x1000>;
		reg-names = "tpdm-base";

		atid = <71>;
		coresight-name = "coresight-tpdm-swao";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_out_tpda_aoss_4: endpoint {
					remote-endpoint =
					<&tpda_aoss_4_in_tpdm_swao>;
				};
			};
		};
	};

	tpdm_ddr_ch01: tpdm@10d20000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10d20000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-ddr-ch01";

		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_ddr_ch01_out_funnel_ddr_ch01: endpoint {
					remote-endpoint =
					<&funnel_ddr_ch01_in_tpdm_ddr_ch01>;
				};
			};
		};
	};

	tpdm_ddr: tpdm@10d00000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10d00000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-ddr";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_ddr_dl0_out_funnel_ddr_dl0: endpoint {
					remote-endpoint =
					<&funnel_ddr_dl0_in_tpdm_ddr_dl0>;
				};
			};
		};
	};

	tpdm_shrm: tpdm@10d01000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10d01000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-shrm";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;
		out-ports {
			port {
				tpdm_shrm_out_funnel_ddr_dl0: endpoint {
					remote-endpoint =
					<&funnel_ddr_dl0_in_tpdm_shrm>;
				};
			};
		};
	};

	tpdm_turing: tpdm@10980000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10980000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-turing";

		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_turing_out_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_in_tpdm_turing>;
				};
			};
		};
	};

	tpdm_turing_llm: tpdm_turing_llm {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-tpdm-turing-llm";
		qcom,dummy-source;

		atid = <78>;

		out-ports {
			port {
				tpdm_turing_llm_out_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_in_tpdm_turing_llm>;
				};
			};
		};
	};

	tpdm_gpu: tpdm@10900000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10900000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-gpu";

		atid = <79>;
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_gpu_out_funnel_gfx_dl: endpoint {
					remote-endpoint =
					<&funnel_gfx_dl_in_tpdm_gpu>;
				};
			};
		};
	};

	tpdm_prng: tpdm@10841000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10841000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-prng";

		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_prng_out_tpda_dl_center_19: endpoint {
					remote-endpoint =
					<&tpda_dl_center_19_in_tpdm_prng>;
				};
			};
		};
	};

	tpdm_qm: tpdm@109d0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x109d0000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-qm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_qm_out_tpda_dl_center_20: endpoint {
					remote-endpoint =
					<&tpda_dl_center_20_in_tpdm_qm>;
				};
			};
		};
	};

	tpdm_gcc: tpdm@1082c000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x1082c000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-gcc";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_gcc_out_tpda_dl_center_21: endpoint {
					remote-endpoint =
					<&tpda_dl_center_21_in_tpdm_gcc>;
				};
			};
		};
	};

	tpdm_vsense: tpdm@10840000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10840000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-vsense";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_vsense_out_tpda_dl_center_22: endpoint {
					remote-endpoint =
					<&tpda_dl_center_22_in_tpdm_vsense>;
				};
			};
		};
	};

	tpdm_emmc: tpdm@10c23000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c23000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-emmc";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_sdcc_out_tpda_dl_center_23: endpoint {
					remote-endpoint =
					<&tpda_dl_center_23_in_tpdm_sdcc>;
				};
			};
		};
	};

	tpdm_sdcc: tpdm@10c20000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c20000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-sdcc";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;

		out-ports {
			port {
				tpdm_sdcc2_out_tpda_dl_lpass_0: endpoint {
					remote-endpoint =
					<&tpda_dl_lpass_0_in_tpdm_sdcc2>;
				};
			};
		};
	};

	tpdm_ipa: tpdm@10c22000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c22000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-ipa";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;

		out-ports {
			port {
				tpdm_ipa_out_tpda_dl_center_24: endpoint {
					remote-endpoint =
					<&tpda_dl_center_24_in_tpdm_ipa>;
				};
			};
		};
	};

	tpdm_pimem: tpdm@10850000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10850000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-pimem";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_pimem_out_tpda_dl_center_25: endpoint {
					remote-endpoint =
					<&tpda_dl_center_25_in_tpdm_pimem>;
				};
			};
		};
	};

	tpdm_dlct: tpdm@10c28000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c28000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-dlct";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_dlct_out_tpda_dl_center_26: endpoint {
					remote-endpoint =
					<&tpda_dl_center_26_in_tpdm_dlct>;
				};
			};
		};
	};

	tpdm_ipcc: tpdm@10c29000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c29000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-ipcc";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_ipcc_out_tpda_dl_center_27: endpoint {
					remote-endpoint =
					<&tpda_dl_center_27_in_tpdm_ipcc>;
				};
			};
		};
	};

	snoc: snoc {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-snoc";
		qcom,dummy-source;

		atid = <125>;
		out-ports {
			port {
				snoc_out_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_in_snoc>;
				};
			};
		};
	};

	tpdm_spdm: tpdm@1000f000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x1000f000 0x1000>;
		reg-names = "tpdm-base";

		atid = <65>;
		coresight-name = "coresight-tpdm-spdm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_spdm_out_tpda_qdss_1: endpoint {
					remote-endpoint =
					<&tpda_qdss_1_in_tpdm_spdm>;
				};
			};
		};
	};

	stm: stm@10002000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb962>;
		reg = <0x10002000 0x1000>,
			<0x16280000 0x180000>;
		reg-names = "stm-base", "stm-stimulus-base";

		atid = <16>;
		coresight-name = "coresight-stm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				stm_out_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_in_stm>;
				};
			};
		};
	};

	tpdm_dcc: tpdm@10003000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10003000 0x1000>;
		reg-names = "tpdm-base";

		atid = <65>;
		coresight-name = "coresight-tpdm-dcc";

		qcom,hw-enable-check;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_dcc_out_tpda_qdss_0: endpoint {
					remote-endpoint =
					<&tpda_qdss_0_in_tpdm_dcc>;
				};
			};
		};
	};

	turing_etm0: turing_etm0 {
		compatible = "qcom,coresight-remote-etm";

		coresight-name = "coresight-turing-etm0";
		qcom,inst-id = <13>;

		atid = <38 39>;

		out-ports {
			port {
				turing_etm0_out_funnel_turing_dup: endpoint {
					remote-endpoint =
						<&funnel_turing_dup_in_turing_etm0>;
				};
			};
		};
	};

	tpdm_east: tpdm@10c24000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c24000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-east";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_east_out_tpda_dl_center_19: endpoint {
					remote-endpoint =
					<&tpda_dl_center_19_in_tpdm_east>;
				};
			};
		};
	};

	tpdm_dl_center2_dsb: tpdm@10ac0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10ac0000 0x1000>;
		reg-names = "tpdm-base";

		atid = <79>;
		coresight-name = "coresight-tpdm-dlct2-dsb";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_dlct0_out_tpda_dl_center2_26: endpoint {
					remote-endpoint =
					<&tpda_dl_center2_26_in_tpdm_dlct0>;
				};
			};
		};
	};

	tpdm_dl_center2_cmb: tpdm@10ac1000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10ac1000 0x1000>;
		reg-names = "tpdm-base";

		atid = <79>;
		coresight-name = "coresight-tpdm-dlct2-cmb";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;
		status = "disabled";
		out-ports {
			port {
				tpdm_dlct1_out_tpda_dl_center2_27: endpoint {
					remote-endpoint =
					<&tpda_dl_center2_27_in_tpdm_dlct1>;
				};
			};
		};
	};

	tpdm_dl_south0: tpdm@109c0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x109c0000 0x1000>;
		reg-names = "tpdm-base";

		atid = <79>;
		coresight-name = "coresight-tpdm-dl-south-dsb";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;

		out-ports {
			port {
				tpdm_dl_south0_out_funnel_dl_south: endpoint {
					remote-endpoint =
					<&funnel_dl_south_in_tpdm_dl_south0>;
				};
			};
		};
	};

	tpdm_dl_south1: tpdm@109c1000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x109c1000 0x1000>;
		reg-names = "tpdm-base";

		atid = <79>;
		coresight-name = "coresight-tpdm-dl-south-cmb";

		clocks = <&aoss_qmp>;
		status = "disabled";
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;

		out-ports {
			port {
				tpdm_dl_south1_out_funnel_dl_south: endpoint {
					remote-endpoint =
					<&funnel_dl_south_in_tpdm_dl_south1>;
				};
			};
		};
	};

	tpdm_rdpm: tpdm@10c00000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c00000 0x1000>;
		reg-names = "tpdm-base";

		atid = <79>;
		coresight-name = "coresight-tpdm-rdpm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;
		status = "disabled";
		out-ports {
			port {
				tpdm_rdpm_out_funnel_dl_center_1: endpoint {
					remote-endpoint =
					<&funnel_dl_center_1_in_tpdm_rdpm>;
				};
			};
		};
	};

	tpdm_rdpm_mx: tpdm@10c01000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c01000 0x1000>;
		reg-names = "tpdm-base";

		atid = <79>;
		coresight-name = "coresight-tpdm-rdpm-mx";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;
		status = "disabled";
		out-ports {
			port {
				tpdm_rdpm_mx_out_funnel_dl_center_1: endpoint {
					remote-endpoint =
					<&funnel_dl_center_1_in_tpdm_rdpm_mx>;
				};
			};
		};
	};

	tpdm_llm_silver: tpdm@128a0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x128a0000 0x1000>;
		reg-names = "tpdm-base";

		atid = <66>;
		coresight-name = "coresight-tpdm-llm-silver";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_llm_silver_out_tpda_apss_0: endpoint {
					remote-endpoint =
					<&tpda_apss_0_in_tpdm_llm_silver>;
				};
			};
		};
	};

	tpdm_llm_gold: tpdm@138b0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x128b0000 0x1000>;
		reg-names = "tpdm-base";

		atid = <66>;
		coresight-name = "coresight-tpdm-llm-gold";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_llm_gold_out_tpda_apss_1: endpoint {
					remote-endpoint =
					<&tpda_apss_1_in_tpdm_llm_gold>;
				};
			};
		};
	};


	tpdm_actpm: tpdm@12860000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x12860000 0x1000>;
		reg-names = "tpdm-base";

		atid = <66>;
		coresight-name = "coresight-tpdm-actpm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_apss0_out_tpda_apss_3: endpoint {
					remote-endpoint =
					<&tpda_apss_3_in_tpdm_apss0>;
				};
			};
		};
	};

	tpdm_apss: tpdm@12861000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x12861000 0x1000>;
		reg-names = "tpdm-base";

		atid = <66>;
		coresight-name = "coresight-tpdm-apss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_apps1_out_tpda_apss_4: endpoint {
					remote-endpoint =
					<&tpda_apss_4_in_tpdm_apps1>;
				};
			};
		};
	};

	tpdm_modem_0: tpdm@10800000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10800000 0x1000>;
		reg-names = "tpdm-base";

		atid = <67>;
		coresight-name = "coresight-tpdm-modem-0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_modem_0_out_tpda_modem_0: endpoint {
					remote-endpoint =
					<&tpda_modem_0_in_tpdm_modem_0>;
				};
			};
		};
	};

	tpdm_modem_1: tpdm@10801000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10801000 0x1000>;
		reg-names = "tpdm-base";

		atid = <67>;
		coresight-name = "coresight-tpdm-modem-1";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-msr-skip;

		out-ports {
			port {
				tpdm_modem_1_out_tpda_modem_1: endpoint {
					remote-endpoint =
					<&tpda_modem_1_in_tpdm_modem_1>;
				};
			};
		};
	};

	modem_etm0 {
		compatible = "qcom,coresight-remote-etm";

		coresight-name = "coresight-modem-etm0";
		qcom,inst-id = <2>;

		atid = <36 37>;
		out-ports {
			port {
				modem_etm0_out_funnel_modem_q6_dup: endpoint {
					remote-endpoint =
						<&funnel_modem_q6_dup_in_modem_etm0>;
				};
			};
		};
	};

	modem2_etm0 {
		compatible = "qcom,coresight-remote-etm";

		coresight-name = "coresight-modem2-etm0";
		qcom,inst-id = <11>;

		atid = <39>;
		out-ports {
			port {
				modem2_etm0_out_funnel_modem: endpoint {
					remote-endpoint =
						<&funnel_modem_in_modem2_etm0>;
				};
			};
		};
	};

	modem_diag: modem_diag {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-modem-diag";
		qcom,dummy-source;

		atid = <50>;
		out-ports {
			port {
				modem_diag_out_funnel_modem_q6: endpoint {
					remote-endpoint =
					<&funnel_modem_q6_in_modem_diag>;
				};
			};
		};
	};

	tpdm_wcss: tpdm@109A4000 {
		compatible = "qcom,coresight-dummy";
		qcom,dummy-source;

		atid = <67>;
		coresight-name = "coresight-tpdm-wcss";

		out-ports {
			port {
				tpdm_wcss_out_funnel_dl_south: endpoint {
					remote-endpoint =
					<&funnel_dl_south_in_tpdm_wcss>;
				};
			};
		};
	};

	tpdm_tmess_prng: tpdm@10cc9000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10cc9000 0x1000>;
		reg-names = "tpdm-base";

		atid = <85>;
		coresight-name = "coresight-tpdm-tmess-prng";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		status = "disabled";

		out-ports {
			port {
				tpdm_tmess_prng_out_tpda_tmess_0: endpoint {
					remote-endpoint =
					<&tpda_tmess_0_in_tpdm_tmess_prng>;
				};
			};
		};
	};

	tpdm_tmess_0: tpdm@10cc0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10cc0000 0x1000>;
		reg-names = "tpdm-base";

		atid = <85>;
		coresight-name = "coresight-tpdm-tmess-irq";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		status = "disabled";

		out-ports {
			port {
				tpdm_tmess_0_out_tpda_tmess_1: endpoint {
					remote-endpoint =
					<&tpda_tmess_1_in_tpdm_tmess_0>;
				};
			};
		};
	};

	tpdm_tmess_1: tpdm@10cc1000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10cc1000 0x1000>;
		reg-names = "tpdm-base";

		atid = <85>;
		coresight-name = "coresight-tpdm-tmess-dsb";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		status = "disabled";

		out-ports {
			port {
				tpdm_tmess_1_out_tpda_tmess_2: endpoint {
					remote-endpoint =
					<&tpda_tmess_2_in_tpdm_tmess_1>;
				};
			};
		};
	};

	tpdm_wpss: tpdm@10c70000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c70000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-wpss-dsb";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_wpss_out_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_in_tpdm_wpss>;
				};
			};
		};
	};

	tpdm_wpss1: tpdm@10c71000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c71000 0x1000>;
		reg-names = "tpdm-base";

		atid = <78>;
		coresight-name = "coresight-tpdm-wpss-cmb";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_wpss_1_out_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_in_tpdm_wpss_1>;
				};
			};
		};
	};

	wpss_etm: wpss_etm0 {
		compatible = "qcom,coresight-remote-etm";

		coresight-name = "coresight-wpss-etm0";
		qcom,inst-id = <3>;
		atid = <44>;

		out-ports {
			port {
				wpss_etm0_out_funnel_wpss: endpoint {
					remote-endpoint =
						<&funnel_wpss_in_wpss_etm0>;
				};
			};
		};
	};

	funnel_wpss: funnel@10c73000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c73000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-wpss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_wpss_in_tpdm_wpss: endpoint {
					remote-endpoint =
					<&tpdm_wpss_out_funnel_wpss>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_wpss_in_tpdm_wpss_1: endpoint {
					remote-endpoint =
					<&tpdm_wpss_1_out_funnel_wpss>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_wpss_in_wpss_etm0: endpoint {
					remote-endpoint =
					<&wpss_etm0_out_funnel_wpss>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_wpss_out_tpda_dl_center_5: endpoint {
					remote-endpoint =
					<&tpda_dl_center_5_in_funnel_wpss>;
					source = <&tpdm_wpss>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_wpss_out_tpda_dl_center_6: endpoint {
					remote-endpoint =
					<&tpda_dl_center_6_in_funnel_wpss>;
					source = <&tpdm_wpss1>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_wpss_out_funnel_dl_center: endpoint {
					remote-endpoint =
					<&funnel_dl_center_in_funnel_wpss>;
					source = <&wpss_etm>;
				};
			};

		};
	};

	funnel_lpass_lpi: funnel@10b44000 {
		compatible = "arm,coresight-static-funnel";
		coresight-name = "coresight-funnel-lpass_lpi";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_lpass_lpi_in_audio_etm0: endpoint {
					remote-endpoint =
					<&audio_etm0_out_funnel_lpass_lpi>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_lpass_lpi_in_lpass_stm: endpoint {
					remote-endpoint =
					<&lpass_stm_out_funnel_lpass_lpi>;
				};
			};

			port@5 {
				reg = <5>;
				funnel_lpass_lpi_in_tpdm_lpass_lpi: endpoint {
					remote-endpoint =
					<&tpdm_lpass_lpi_out_funnel_lpass_lpi>;
				};
			};

		};

		out-ports {
			port {
				funnel_lpass_lpi_out_funnel_aoss: endpoint {
					remote-endpoint =
					<&funnel_aoss_in_funnel_lpass_lpi>;
				};
			};

		};
	};

	funnel_gfx_dl: funnel@10902000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10902000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-gfx_dl";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				funnel_gfx_dl_in_tpdm_gpu: endpoint {
					remote-endpoint =
					<&tpdm_gpu_out_funnel_gfx_dl>;
				};
			};

		};

		out-ports {
			port {
				funnel_gfx_out_tpda_dl_center2_17: endpoint {
					remote-endpoint =
					<&tpda_dl_center2_17_in_funnel_gfx>;
				};
			};

		};
	};


	funnel_lpass: funnel@10846000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10846000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-lpass";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				funnel_lpass_in_tpdm_lpass: endpoint {
					remote-endpoint =
					<&tpdm_lpass_out_funnel_lpass>;
				};
			};

		};

		out-ports {
			port {
				funnel_lpass_out_tpda_dl_lpass_2: endpoint {
					remote-endpoint =
					<&tpda_dl_lpass_2_in_funnel_lpass>;
				};
			};

		};
	};

	funnel_ddr_ch01: funnel@10d22000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10d22000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-ddr_ch01";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				funnel_ddr_ch01_in_tpdm_ddr_ch01: endpoint {
					remote-endpoint =
					<&tpdm_ddr_ch01_out_funnel_ddr_ch01>;
				};
			};

		};

		out-ports {
			port {
				funnel_ddr_ch01_out_funnel_ddr_dl0: endpoint {
					remote-endpoint =
					<&funnel_ddr_dl0_in_funnel_ddr_ch01>;
				};
			};

		};
	};

	funnel_ddr_dl0: funnel@10d03000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10d03000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-ddr_dl0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_ddr_dl0_in_funnel_ddr_ch01: endpoint {
					remote-endpoint =
					<&funnel_ddr_ch01_out_funnel_ddr_dl0>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_ddr_dl0_in_tpdm_ddr_dl0: endpoint {
					remote-endpoint =
					<&tpdm_ddr_dl0_out_funnel_ddr_dl0>;
				};
			};

			port@3 {
				reg = <3>;
				funnel_ddr_dl0_in_tpdm_shrm: endpoint {
					remote-endpoint =
					<&tpdm_shrm_out_funnel_ddr_dl0>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_ddr_out_tpda_dl_center_9: endpoint {
					remote-endpoint =
					<&tpda_dl_center_9_in_funnel_ddr>;
					source = <&tpdm_ddr_ch01>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_ddr_out_tpda_dl_center_11: endpoint {
					remote-endpoint =
					<&tpda_dl_center_11_in_funnel_ddr>;
					source = <&tpdm_ddr>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_ddr_out_tpda_dl_center_12: endpoint {
					remote-endpoint =
					<&tpda_dl_center_12_in_funnel_ddr>;
					source = <&tpdm_shrm>;
				};
			};

		};
	};

	funnel_turing_dup: funnel@10984000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10984000 0x1000>,
			<0x10983000 0x1000>;
		reg-names = "funnel-base-dummy", "funnel-base-real";

		coresight-name = "coresight-funnel-turing_dup";

		qcom,duplicate-funnel;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;
			port@3 {
				reg = <3>;
				funnel_turing_dup_in_turing_etm0: endpoint {
					remote-endpoint =
					<&turing_etm0_out_funnel_turing_dup>;
				};
			};

		};

		out-ports {
			port {
				funnel_turing_dup_out_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_in_funnel_turing_dup>;
				};
			};

		};
	};

	funnel_turing: funnel@10983000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10983000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-turing";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_turing_in_tpdm_turing: endpoint {
					remote-endpoint =
					<&tpdm_turing_out_funnel_turing>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_turing_in_tpdm_turing_llm: endpoint {
					remote-endpoint =
					<&tpdm_turing_llm_out_funnel_turing>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_turing_in_funnel_turing_dup: endpoint {
					remote-endpoint =
					<&funnel_turing_dup_out_funnel_turing>;
				};
			};

		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_turing_out_tpda_dl_center_15: endpoint {
					remote-endpoint =
					<&tpda_dl_center_15_in_funnel_turing>;
					source = <&tpdm_turing>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_turing_out_tpda_dl_center_16: endpoint {
					remote-endpoint =
					<&tpda_dl_center_16_in_funnel_turing>;
					source = <&tpdm_turing_llm>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_turing_out_funnel_dl_center: endpoint {
					remote-endpoint =
					<&funnel_dl_center_in_funnel_turing>;
				};
			};

		};
	};

	funnel_dlct_1: funnel@10c02000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c02000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dlct1";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				funnel_dl_center_1_in_tpdm_rdpm: endpoint {
					remote-endpoint =
					<&tpdm_rdpm_out_funnel_dl_center_1>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_dl_center_1_in_tpdm_rdpm_mx: endpoint {
					remote-endpoint =
					<&tpdm_rdpm_mx_out_funnel_dl_center_1>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;
			port@0 {
				reg = <0>;
				funnel_dl_center_1_out_tpda_dl_center_10: endpoint {
					remote-endpoint =
					<&tpda_dl_center_10_in_funnel_dl_center_1>;
					source = <&tpdm_rdpm>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_dl_center_1_out_tpda_dl_center_11: endpoint {
					remote-endpoint =
					<&tpda_dl_center_11_in_funnel_dl_center_1>;
					source = <&tpdm_rdpm_mx>;
				};
			};
		};
	};

	tpda_tmess: tpda@10cc4000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10cc4000 0x1000>;
		reg-names = "tpda-base";

		qcom,cmb-elem-size = <0 64>,
				     <1 64>,
				     <2 32>;
		qcom,dsb-elem-size = <1 32>;

		qcom,tpda-atid = <85>;
		coresight-name = "coresight-tpda-tmess";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				tpda_tmess_0_in_tpdm_tmess_prng: endpoint {
					remote-endpoint =
					<&tpdm_tmess_prng_out_tpda_tmess_0>;
				};
			};

			port@1 {
				reg = <1>;
				tpda_tmess_1_in_tpdm_tmess_0: endpoint {
					remote-endpoint =
					<&tpdm_tmess_0_out_tpda_tmess_1>;
				};
			};

			port@2 {
				reg = <2>;
				tpda_tmess_2_in_tpdm_tmess_1: endpoint {
					remote-endpoint =
					<&tpdm_tmess_1_out_tpda_tmess_2>;
				};
			};

		};

		out-ports {

			port {
				tpda_tmess_out_funnel_tmess: endpoint {
					remote-endpoint =
					<&funnel_tmess_in_tpda_tmess>;
				};
			};

		};
	};

	funnel_tmess: funnel@10cc5000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10cc5000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-tmess";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				funnel_tmess_in_tpda_tmess: endpoint {
					remote-endpoint =
					<&tpda_tmess_out_funnel_tmess>;
				};
			};

		};

		out-ports {
			port {
				funnel_tmess_out_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_in_funnel_tmess>;
				};
			};

		};
	};

	tpda_modem: tpda@10803000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10803000 0x1000>;
		reg-names = "tpda-base";

		qcom,tpda-atid = <67>;
		qcom,dsb-elem-size = <0 32>;
		qcom,cmb-elem-size = <0 64>;

		coresight-name = "coresight-tpda-modem";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				tpda_modem_0_in_tpdm_modem_0: endpoint {
					remote-endpoint =
					<&tpdm_modem_0_out_tpda_modem_0>;
				};
			};

			port@1 {
				reg = <1>;
				tpda_modem_1_in_tpdm_modem_1: endpoint {
					remote-endpoint =
					<&tpdm_modem_1_out_tpda_modem_1>;
				};
			};

		};

		out-ports {

			port {
				tpda_modem_out_funnel_modem: endpoint {
					remote-endpoint =
					<&funnel_modem_in_tpda_modem>;
				};
			};

		};
	};

	funnel_modem_q6_dup: funnel@1080d000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x1080d000 0x1000>,
			<0x1080c000 0x1000>;
		reg-names = "funnel-base-dummy", "funnel-base-real";

		coresight-name = "coresight-funnel-modem_q6_dup";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,duplicate-funnel;

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_modem_q6_dup_in_modem_etm0: endpoint {
					remote-endpoint =
					<&modem_etm0_out_funnel_modem_q6_dup>;
				};
			};

		};

		out-ports {
			port {
				funnel_modem_q6_dup_out_funnel_modem_q6: endpoint {
					remote-endpoint =
					<&funnel_modem_q6_in_funnel_modem_q6_dup>;
				};
			};

		};
	};

	funnel_modem_q6: funnel@1080c000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x1080c000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-modem_q6";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				funnel_modem_q6_in_funnel_modem_q6_dup: endpoint {
					remote-endpoint =
					<&funnel_modem_q6_dup_out_funnel_modem_q6>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_modem_q6_in_modem_diag: endpoint {
					remote-endpoint =
					<&modem_diag_out_funnel_modem_q6>;
				};
			};

		};

		out-ports {
			port {
				funnel_modem_q6_out_funnel_modem: endpoint {
					remote-endpoint =
					<&funnel_modem_in_funnel_modem_q6>;
				};
			};

		};
	};

	funnel_modem: funnel@10804000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10804000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-modem";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				funnel_modem_in_modem2_etm0: endpoint {
					remote-endpoint =
					<&modem2_etm0_out_funnel_modem>;
				};
			};

			port@0 {
				reg = <0>;
				funnel_modem_in_tpda_modem: endpoint {
					remote-endpoint =
					<&tpda_modem_out_funnel_modem>;
				};
			};

			port@3 {
				reg = <3>;
				funnel_modem_in_funnel_modem_q6: endpoint {
					remote-endpoint =
					<&funnel_modem_q6_out_funnel_modem>;
				};
			};

		};

		out-ports {
			port {
				funnel_modem_out_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_in_funnel_modem>;
				};
			};

		};
	};

	tpda_apss: tpda@12863000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x12863000 0x1000>;
		reg-names = "tpda-base";

		qcom,tpda-atid = <66>;
		qcom,dsb-elem-size = <4 32>;
		qcom,cmb-elem-size = <0 32>,
				     <1 32>,
				     <3 64>;

		coresight-name = "coresight-tpda-apss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				tpda_apss_0_in_tpdm_llm_silver: endpoint {
					remote-endpoint =
					<&tpdm_llm_silver_out_tpda_apss_0>;
				};
			};

			port@1 {
				reg = <1>;
				tpda_apss_1_in_tpdm_llm_gold: endpoint {
					remote-endpoint =
					<&tpdm_llm_gold_out_tpda_apss_1>;
				};
			};

			port@3 {
				reg = <3>;
				tpda_apss_3_in_tpdm_apss0: endpoint {
					remote-endpoint =
					<&tpdm_apss0_out_tpda_apss_3>;
				};
			};

			port@4 {
				reg = <4>;
				tpda_apss_4_in_tpdm_apps1: endpoint {
					remote-endpoint =
					<&tpdm_apps1_out_tpda_apss_4>;
				};
			};

		};

		out-ports {
			port {
				tpda_apss_out_funnel_apss: endpoint {
					remote-endpoint =
					<&funnel_apss_in_tpda_apss>;
				};
			};

		};
	};

	funnel_apss: funnel@12810000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x12810000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-apss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_apss_in_funnel_ete: endpoint {
					remote-endpoint =
					<&funnel_ete_out_funnel_apss>;
				};
			};

			port@3 {
				reg = <3>;
				funnel_apss_in_tpda_apss: endpoint {
					remote-endpoint =
					<&tpda_apss_out_funnel_apss>;
				};
			};

		};

		out-ports {
			port {
				funnel_apss_out_funnel_dl_center: endpoint {
					remote-endpoint =
					<&funnel_dl_center_in_funnel_apss>;
				};
			};

		};
	};

	tpda_dl_center: tpda@10c2b000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10c2b000 0x1000>;
		reg-names = "tpda-base";

		qcom,tpda-atid = <78>;

		qcom,dsb-elem-size = <5 32>,
							 <9 32>,
							 <11 32>,
							 <15 32>,
							 <20 32>,
							 <21 32>,
							 <25 32>,
							 <26 32>;

		qcom,cmb-elem-size = <6 32>,
							 <11 32>,
							 <12 64>,
							 <16 32>,
							 <19 64>,
							 <22 32>,
							 <23 32>,
							 <24 64>,
							 <25 64>,
							 <27 64>;

		coresight-name = "coresight-tpda-dlct0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@5 {
				reg = <5>;
				tpda_dl_center_5_in_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_out_tpda_dl_center_5>;
				};
			};

			port@6 {
				reg = <6>;
				tpda_dl_center_6_in_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_out_tpda_dl_center_6>;
				};
			};

			port@9 {
				reg = <9>;
				tpda_dl_center_9_in_funnel_ddr: endpoint {
					remote-endpoint =
					<&funnel_ddr_out_tpda_dl_center_9>;
				};
			};

			port@c {
				reg = <11>;
				tpda_dl_center_11_in_funnel_ddr: endpoint {
					remote-endpoint =
					<&funnel_ddr_out_tpda_dl_center_11>;
				};
			};

			port@d {
				reg = <12>;
				tpda_dl_center_12_in_funnel_ddr: endpoint {
					remote-endpoint =
					<&funnel_ddr_out_tpda_dl_center_12>;
				};
			};

			port@f {
				reg = <15>;
				tpda_dl_center_15_in_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_out_tpda_dl_center_15>;
				};
			};

			port@10 {
				reg = <16>;
				tpda_dl_center_16_in_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_out_tpda_dl_center_16>;
				};
			};

			port@13 {
				reg = <19>;
				tpda_dl_center_19_in_tpdm_prng: endpoint {
					remote-endpoint =
					<&tpdm_prng_out_tpda_dl_center_19>;
				};
			};

			port@14 {
				reg = <20>;
				tpda_dl_center_20_in_tpdm_qm: endpoint {
					remote-endpoint =
					<&tpdm_qm_out_tpda_dl_center_20>;
				};
			};

			port@15 {
				reg = <21>;
				tpda_dl_center_21_in_tpdm_gcc: endpoint {
					remote-endpoint =
					<&tpdm_gcc_out_tpda_dl_center_21>;
				};
			};

			port@16 {
				reg = <22>;
				tpda_dl_center_22_in_tpdm_vsense: endpoint {
					remote-endpoint =
					<&tpdm_vsense_out_tpda_dl_center_22>;
				};
			};

			port@17 {
				reg = <23>;
				tpda_dl_center_23_in_tpdm_sdcc: endpoint {
					remote-endpoint =
					<&tpdm_sdcc_out_tpda_dl_center_23>;
				};
			};

			port@18 {
				reg = <24>;
				tpda_dl_center_24_in_tpdm_ipa: endpoint {
					remote-endpoint =
					<&tpdm_ipa_out_tpda_dl_center_24>;
				};
			};

			port@19 {
				reg = <25>;
				tpda_dl_center_25_in_tpdm_pimem: endpoint {
					remote-endpoint =
					<&tpdm_pimem_out_tpda_dl_center_25>;
				};
			};

			port@1a {
				reg = <26>;
				tpda_dl_center_26_in_tpdm_dlct: endpoint {
					remote-endpoint =
					<&tpdm_dlct_out_tpda_dl_center_26>;
				};
			};

			port@1b {
				reg = <27>;
				tpda_dl_center_27_in_tpdm_ipcc: endpoint {
					remote-endpoint =
					<&tpdm_ipcc_out_tpda_dl_center_27>;
				};
			};

		};

		out-ports {

			port {
				tpda_dl_center_out_funnel_dl_center: endpoint {
					remote-endpoint =
					<&funnel_dl_center_in_tpda_dl_center>;
				};
			};

		};
	};

	funnel_dlct0: funnel@10c2c000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c2c000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dlct0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_dl_center_in_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_out_funnel_dl_center>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_dl_center_in_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_out_funnel_dl_center>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_dl_center_in_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_out_funnel_dl_center>;
				};
			};

			port@7 {
				reg = <7>;
				funnel_dl_center_in_funnel_apss: endpoint {
					remote-endpoint =
					<&funnel_apss_out_funnel_dl_center>;
				};
			};
		};

		out-ports {
			port {
				funnel_dl_center_out_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_in_funnel_dl_center>;
				};
			};

		};
	};

	funnel_dl_south: funnel@109c3000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x109c3000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dl_south";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@2 {
				reg = <2>;
				funnel_dl_south_in_tpdm_dl_south0: endpoint {
					remote-endpoint =
					<&tpdm_dl_south0_out_funnel_dl_south>;
				};
			};

			port@3 {
				reg = <3>;
				funnel_dl_south_in_tpdm_dl_south1: endpoint {
					remote-endpoint =
					<&tpdm_dl_south1_out_funnel_dl_south>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_dl_south_in_tpdm_wcss: endpoint {
					remote-endpoint =
					<&tpdm_wcss_out_funnel_dl_south>;
				};
			};

		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_dl_south_out_tpda_dl_center2_7: endpoint {
					remote-endpoint =
					<&tpda_dl_center2_7_in_funnel_dl_south>;
					source = <&tpdm_dl_south0>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_dl_south_out_tpda_dl_center2_8: endpoint {
					remote-endpoint =
					<&tpda_dl_center2_8_in_funnel_dl_south>;
					source = <&tpdm_dl_south1>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_dl_south_out_funnel_dl_center2: endpoint {
					remote-endpoint =
					<&funnel_dl_center2_in_funnel_dl_south>;
				};
			};
		};
	};

	tpda_dl_center2: tpda@10ac3000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10ac3000 0x1000>;
		reg-names = "tpda-base";

		qcom,tpda-atid = <79>;

		qcom,dsb-elem-size = <7 32>,
							 <9 32>,
							 <17 32>,
							 <19 32>,
							 <26 32>;

		qcom,cmb-elem-size = <8 64>,
							 <13 64>,
							 <14 64>,
							 <27 64>;

		coresight-name = "coresight-tpda-dlct2";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@7 {
				reg = <7>;
				tpda_dl_center2_7_in_funnel_dl_south: endpoint {
					remote-endpoint =
					<&funnel_dl_south_out_tpda_dl_center2_7>;
				};
			};

			port@8 {
				reg = <8>;
				tpda_dl_center2_8_in_funnel_dl_south: endpoint {
					remote-endpoint =
					<&funnel_dl_south_out_tpda_dl_center2_8>;
				};
			};


			port@d {
				reg = <13>;
				tpda_dl_center_10_in_funnel_dl_center_1: endpoint {
					remote-endpoint =
					<&funnel_dl_center_1_out_tpda_dl_center_10>;
				};
			};

			port@e {
				reg = <14>;
				tpda_dl_center_11_in_funnel_dl_center_1: endpoint {
					remote-endpoint =
					<&funnel_dl_center_1_out_tpda_dl_center_11>;
				};
			};

			port@11 {
				reg = <17>;
				tpda_dl_center2_17_in_funnel_gfx: endpoint {
					remote-endpoint =
					<&funnel_gfx_out_tpda_dl_center2_17>;
				};
			};

			port@13 {
				reg = <19>;
				tpda_dl_center_19_in_tpdm_east: endpoint {
					remote-endpoint =
					<&tpdm_east_out_tpda_dl_center_19>;
				};
			};

			port@1a {
				reg = <26>;
				tpda_dl_center2_26_in_tpdm_dlct0: endpoint {
					remote-endpoint =
					<&tpdm_dlct0_out_tpda_dl_center2_26>;
				};
			};

			port@1b {
				reg = <27>;
				tpda_dl_center2_27_in_tpdm_dlct1: endpoint {
					remote-endpoint =
					<&tpdm_dlct1_out_tpda_dl_center2_27>;
				};
			};

		};

		out-ports {

			port {
				tpda_dl_center2_out_funnel_dl_center2: endpoint {
					remote-endpoint =
					<&funnel_dl_center2_in_tpda_dl_center2>;
				};
			};

		};
	};


funnel_dl_center2: funnel@10ac4000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10ac4000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dlct2";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_dl_center2_in_tpda_dl_center2: endpoint {
					remote-endpoint =
					<&tpda_dl_center2_out_funnel_dl_center2>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_dl_center2_in_funnel_dl_south: endpoint {
					remote-endpoint =
					<&funnel_dl_south_out_funnel_dl_center2>;
				};
			};

		};

		out-ports {
			port {
				funnel_dl_center2_out_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_in_funnel_dl_center2>;
				};
			};

		};
	};

	tpda_dl_lpass: tpda@10c3a000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10c3a000 0x1000>;
		reg-names = "tpda-base";

		qcom,tpda-atid = <74>;
		coresight-name = "coresight-tpda-dl-lpass";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,cmb-elem-size = <0 32>;
		qcom,dsb-elem-size = <2 32>,
							<10 32>;

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				tpda_dl_lpass_0_in_tpdm_sdcc2: endpoint {
					remote-endpoint =
					<&tpdm_sdcc2_out_tpda_dl_lpass_0>;
				};
			};

			port@2 {
				reg = <2>;
				tpda_dl_lpass_2_in_funnel_lpass: endpoint {
					remote-endpoint =
					<&funnel_lpass_out_tpda_dl_lpass_2>;
				};
			};

			port@10 {
				reg = <10>;
				tpda_dl_lpass_10_in_tpdm_dl_lpass: endpoint {
					remote-endpoint =
					<&tpdm_dl_lpass_out_tpda_dl_lpass_10>;
				};
			};

		};

		out-ports {

			port {
				tpda_dl_lpass_out_funnel_dl_lpass: endpoint {
					remote-endpoint =
					<&funnel_dl_lpass_in_tpda_dl_lpass>;
				};
			};

		};
	};

	funnel_dl_lpass: funnel@10c3b000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c3b000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dl-lpass";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			port {
				funnel_dl_lpass_in_tpda_dl_lpass: endpoint {
					remote-endpoint =
					<&tpda_dl_lpass_out_funnel_dl_lpass>;
				};
			};

		};

		out-ports {
			port {
				funnel_dl_lpass_out_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_in_funnel_dl_lpass>;
				};
			};

		};
	};

	tpda_qdss: tpda@10004000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10004000 0x1000>;
		reg-names = "tpda-base";

		qcom,tpda-atid = <65>;
		coresight-name = "coresight-tpda-qdss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,cmb-elem-size = <0 32>,
							<1 32>;

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				tpda_qdss_0_in_tpdm_dcc: endpoint {
					remote-endpoint =
					<&tpdm_dcc_out_tpda_qdss_0>;
				};
			};

			port@1 {
				reg = <1>;
				tpda_qdss_1_in_tpdm_spdm: endpoint {
					remote-endpoint =
					<&tpdm_spdm_out_tpda_qdss_1>;
				};
			};


		};

		out-ports {

			port {
				tpda_qdss_out_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_in_tpda_qdss>;
				};
			};

		};
	};

	funnel_in0: funnel@10041000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10041000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-in0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_in0_in_snoc: endpoint {
					remote-endpoint =
					<&snoc_out_funnel_in0>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_in0_in_funnel_tmess: endpoint {
					remote-endpoint =
					<&funnel_tmess_out_funnel_in0>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_in0_in_tpda_qdss: endpoint {
					remote-endpoint =
					<&tpda_qdss_out_funnel_in0>;
				};
			};

			port@7 {
				reg = <7>;
				funnel_in0_in_stm: endpoint {
					remote-endpoint =
					<&stm_out_funnel_in0>;
				};
			};
		};

		out-ports {
			port {
				funnel_in0_out_funnel_qdss: endpoint {
					remote-endpoint =
					<&funnel_qdss_in_funnel_in0>;
				};
			};

		};
	};

	funnel_in1: funnel@10042000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10042000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-in1";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@4 {
				reg = <4>;
				funnel_in1_in_funnel_modem: endpoint {
					remote-endpoint =
					<&funnel_modem_out_funnel_in1>;
				};
			};

			port@5 {
				reg = <5>;
				funnel_in1_in_funnel_dl_lpass: endpoint {
					remote-endpoint =
					<&funnel_dl_lpass_out_funnel_in1>;
				};
			};


			port@6 {
				reg = <6>;
				funnel_in1_in_funnel_dl_center: endpoint {
					remote-endpoint =
					<&funnel_dl_center_out_funnel_in1>;
				};
			};

			port@7 {
				reg = <7>;
				funnel_in1_in_funnel_dl_center2: endpoint {
					remote-endpoint =
					<&funnel_dl_center2_out_funnel_in1>;
				};
			};

		};

		out-ports {
			port {
				funnel_in1_out_funnel_qdss: endpoint {
					remote-endpoint =
					<&funnel_qdss_in_funnel_in1>;
				};
			};

		};
	};

	funnel_merg: funnel@10045000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10045000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-merg";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				funnel_qdss_in_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_out_funnel_qdss>;
				};
			};

			port@0 {
				reg = <0>;
				funnel_qdss_in_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_out_funnel_qdss>;
				};
			};

		};

		out-ports {
			port {
				funnel_qdss_out_funnel_aoss: endpoint {
					remote-endpoint =
					<&funnel_aoss_in_funnel_qdss>;
				};
			};

		};
	};

	tpda_aoss: tpda@10b08000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10b08000 0x1000>;
		reg-names = "tpda-base";

		coresight-name = "coresight-tpda-aoss";

		qcom,tpda-atid = <71>;
		qcom,cmb-elem-size = <0 64>,
				     <1 64>,
				     <2 64>,
				     <3 64>;

		qcom,dsb-elem-size = <4 32>;

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				tpda_aoss_0_in_tpdm_swao_prio_0: endpoint {
					remote-endpoint =
					<&tpdm_swao_prio_0_out_tpda_aoss_0>;
				};
			};

			port@1 {
				reg = <1>;
				tpda_aoss_1_in_tpdm_swao_prio_1: endpoint {
					remote-endpoint =
					<&tpdm_swao_prio_1_out_tpda_aoss_1>;
				};
			};

			port@2 {
				reg = <2>;
				tpda_aoss_2_in_tpdm_swao_prio_2: endpoint {
					remote-endpoint =
					<&tpdm_swao_prio_2_out_tpda_aoss_2>;
				};
			};

			port@3 {
				reg = <3>;
				tpda_aoss_3_in_tpdm_swao_prio_3: endpoint {
					remote-endpoint =
					<&tpdm_swao_prio_3_out_tpda_aoss_3>;
				};
			};

			port@4 {
				reg = <4>;
				tpda_aoss_4_in_tpdm_swao: endpoint {
					remote-endpoint =
					<&tpdm_swao_out_tpda_aoss_4>;
				};
			};

		};

		out-ports {

			port {
				tpda_aoss_out_funnel_aoss: endpoint {
					remote-endpoint =
					<&funnel_aoss_in_tpda_aoss>;
				};
			};

		};
	};

	funnel_aoss: funnel@10b04000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10b04000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-aoss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@5 {
				reg = <5>;
				funnel_aoss_in_funnel_lpass_lpi: endpoint {
					remote-endpoint =
					<&funnel_lpass_lpi_out_funnel_aoss>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_aoss_in_tpda_aoss: endpoint {
					remote-endpoint =
					<&tpda_aoss_out_funnel_aoss>;
				};
			};

			port@7 {
				reg = <7>;
				funnel_aoss_in_funnel_qdss: endpoint {
					remote-endpoint =
					<&funnel_qdss_out_funnel_aoss>;
				};
			};
		};

		out-ports {
			port {
				funnel_aoss_out_tmc_etf: endpoint {
					remote-endpoint =
					<&tmc_etf_in_funnel_aoss>;
				};
			};

		};
	};

	dummy_eud: dummy_sink {
		compatible = "qcom,coresight-dummy";

		coresight-name = "coresight-eud";

		qcom,dummy-sink;
		in-ports {
			port {
				eud_in_replicator_swao: endpoint {
					remote-endpoint =
						<&replicator_swao_out_eud>;
				};
			};
		};
	};

	tmc_etf: tmc@10b05000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb961>;
		reg = <0x10b05000 0x1000>;
		reg-names = "tmc-base";

		coresight-name = "coresight-tmc-etf";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				tmc_etf_in_funnel_aoss: endpoint {
					remote-endpoint =
					<&funnel_aoss_out_tmc_etf>;
				};
			};
		};

		out-ports {
			port {
				tmc_etf_out_replicator_swao: endpoint {
					remote-endpoint =
					<&replicator_swao_in_tmc_etf>;
				};
			};
		};
	};

	replicator_swao: replicator@10b06000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb909>;

		reg = <0x10b06000 0x1000>;
		reg-names = "replicator-base";

		coresight-name = "coresight-replicator_swao";

		qcom,replicator-loses-context;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		in-ports {
			port {
				replicator_swao_in_tmc_etf: endpoint {
					remote-endpoint =
					<&tmc_etf_out_replicator_swao>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				replicator_swao_out_replicator_qdss: endpoint {
					remote-endpoint =
					<&replicator_qdss_in_replicator_swao>;
				};
			};

			port@1 {
				reg = <1>;
				replicator_swao_out_eud: endpoint {
					remote-endpoint =
					  <&eud_in_replicator_swao>;
				};
			};
		};
	};

	replicator_qdss: replicator@10046000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb909>;

		reg = <0x10046000 0x1000>;
		reg-names = "replicator-base";

		coresight-name = "coresight-replicator_qdss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		in-ports {
			port {
				replicator_qdss_in_replicator_swao: endpoint {
					remote-endpoint =
					<&replicator_swao_out_replicator_qdss>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				replicator_qdss_out_replicator_etr: endpoint {
					remote-endpoint =
					<&replicator_etr_in_replicator_qdss>;
				};
			};
		};
	};

	replicator_etr: replicator@1004e000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb909>;

		reg = <0x1004e000 0x1000>;
		reg-names = "replicator-base";

		coresight-name = "coresight-replicator_etr";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				replicator_etr_in_replicator_qdss: endpoint {
					remote-endpoint =
					<&replicator_qdss_out_replicator_etr>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				replicator_etr_out_tmc_etr: endpoint {
					remote-endpoint =
					<&tmc_etr_in_replicator_etr>;
				};
			};

			port@1 {
				reg = <1>;
				replicator_etr_out_tmc_etr1: endpoint {
					remote-endpoint =
					<&tmc_etr1_in_replicator_etr>;
				};
			};
		};
	};

	tmc_etr: tmc@10048000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb961>;

		reg = <0x10048000 0x1000>,
			<0x10064000 0x16000>;
		reg-names = "tmc-base", "bam-base";

		qcom,iommu-dma = "bypass";
		iommus = <&apps_smmu 0x04e0 0>,
			<&apps_smmu 0x0520 0>;

		qcom,iommu-dma-addr-pool = <0x0 0xffc00000>;

		qcom,sw-usb;
		dma-coherent;
		coresight-name = "coresight-tmc-etr";

		coresight-csr = <&csr>;
		csr-atid-offset = <0xf8>;
		csr-irqctrl-offset = <0x6c>;
		byte-cntr-name = "byte-cntr";
		byte-cntr-class-name = "coresight-tmc-etr-stream";

		interrupts = <GIC_SPI 270 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "byte-cntr-irq";

		arm,scatter-gather;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				tmc_etr_in_replicator_etr: endpoint {
					remote-endpoint =
					<&replicator_etr_out_tmc_etr>;
				};
			};
		};
	};

	tmc_etr1: tmc@1004f000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb961>;

		reg = <0x1004f000 0x1000>;
		reg-names = "tmc-base";

		coresight-name = "coresight-tmc-etr1";

		iommus = <&apps_smmu 0x0500 0>;
		qcom,iommu-dma-addr-pool = <0x0 0xffc00000>;
		dma-coherent;

		coresight-csr = <&csr>;
		csr-atid-offset = <0x108>;
		csr-irqctrl-offset = <0x70>;
		byte-cntr-name = "byte-cntr1";
		byte-cntr-class-name = "coresight-tmc-etr1-stream";

		interrupts = <GIC_SPI 269 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "byte-cntr-irq";

		arm,scatter-gather;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				tmc_etr1_in_replicator_etr: endpoint {
					remote-endpoint =
					<&replicator_etr_out_tmc_etr1>;
				};
			};
		};
	};

	csr: csr@10001000 {
		compatible = "qcom,coresight-csr";

		reg = <0x10001000 0x1000>;
		reg-names = "csr-base";

		coresight-name = "coresight-csr";
		qcom,usb-bam-support;
		qcom,perflsheot-set-support;
		qcom,hwctrl-set-support;
		qcom,set-byte-cntr-support;
		qcom,blk-size = <1>;
	};

	swao_csr: csr@10b11000 {
		compatible = "qcom,coresight-csr";

		reg = <0x10b11000 0x1000>,
		      <0x10b110f8 0x50>;
		reg-names = "csr-base", "msr-base";

		coresight-name = "coresight-swao-csr";
		qcom,timestamp-support;
		qcom,msr-support;
		qcom,blk-size = <1>;

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	qc_cti: cti@10010000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10010000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-qc_cti";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,cti-gpio-trigout = <16>;
		pinctrl-names = "cti-trigout-pctrl";
		pinctrl-0 = <&trigout_a>;
	};

	cti0: cti@10c2a000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10c2a000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-cti0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	south_cti: cti@109C2000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x109C2000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-dl_south_cti0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	ddr_dl_0_cti_0: cti@10d02000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10d02000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-ddr_dl_0_cti_0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	ddr_dl_1_cti_0: cti@10d0c000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10d0c000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-ddr_dl_1_cti_0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	ddr_ch01_dl_cti_0: cti@10d21000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10d21000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-ddr_ch01_dl_cti_0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	lpass_dl_cti: cti@10845000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10845000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-lpass_dl_cti";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	gpu_isdb_cti: cti@10961000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10961000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-gpu_isdb_cti";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	gpu_cortex_m3: cti@10962000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10962000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-gpu_cortex_m3";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	turing_dl_cti_0: cti@10982000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10982000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-turing_dl_cti_0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	turing_q6_cti: cti@1098b000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x1098b000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-turing_q6_cti";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	wlan_q6_cti: cti@10C7B000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10C7B000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-wlan_q6_cti";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	swao_cti: cti@10b00000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10b00000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-swao_cti";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,extended_cti;
	};

	cortex_m3: cti@10b13000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10b13000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-cortex_m3";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	lpass_lpi_cti: cti@10b41000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10b41000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-lpass_lpi_cti";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	lpass_q6_cti: cti@10b4b000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10b4b000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-lpass_q6_cti";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	apss_cti0: cti@128e0000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x128e0000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-apss_cti0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	apss_cti1: cti@128f0000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x128f0000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-apss_cti1";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	apss_cti2: cti@12900000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x12900000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-apss_cti2";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	riscv_cti: cti@1282b000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x1282b000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-riscv_cti";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	mss_q6_cti: cti@1080b000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x1080b000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-mss_q6_cti";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	mss_vq6_cti: cti@10813000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10813000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-mss_vq6_cti";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	tmess_cti_0: cti@10cc2000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10cc2000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-tmess_cti_0";

		qcom,extended_cti;
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	tmess_cti_1: cti@10cc3000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10cc3000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-tmess_cti_1";

		qcom,extended_cti;
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	tmess_cpu: cti@10cd1000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10cd1000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-tmess_cpu";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	apss_atb_cti: cti@12862000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x12862000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-apss_atb_cti";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	ddrss_shrm2: cti@10d11000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10d11000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-ddrss_shrm2";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	Sierra_A6: cti@10C13000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10C13000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-sierra_a6";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	wcss0: cti@109AC000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x109AC000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-sierra_a6";
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	wcss1: cti@109ad000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x109ad000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-wcss1";
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	wcss2: cti@109Ae000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x109Ae000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-wcss2";
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	ipcb_tgu: tgu@10b0e000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb999>;

		reg = <0x10b0e000 0x1000>;
		reg-names = "tgu-base";

		tgu-steps = <3>;
		tgu-conditions = <4>;
		tgu-regs = <4>;
		tgu-timer-counters = <8>;

		coresight-name = "coresight-tgu-ipcb";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	spmi_tgu0: tgu@10b0f000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb999>;

		reg = <0x10b0f000 0x1000>;
		reg-names = "tgu-base";

		tgu-steps = <3>;
		tgu-conditions = <4>;
		tgu-regs = <9>;
		tgu-timer-counters = <8>;

		coresight-name = "coresight-tgu-spmi0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	spmi_tgu1: tgu@10b10000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb999>;

		reg = <0x10b10000 0x1000>;
		reg-names = "tgu-base";

		tgu-steps = <3>;
		tgu-conditions = <4>;
		tgu-regs = <9>;
		tgu-timer-counters = <8>;

		coresight-name = "coresight-tgu-spmi1";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	etm0 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12040000 0x1000>;
		cpu = <&CPU0>;

		coresight-name = "coresight-etm0";
		qcom,skip-power-up;

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <1>;
		out-ports {
			port {
				ete0_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete0>;
				};
			};
		};
	};

	etm1 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12140000 0x1000>;
		cpu = <&CPU1>;

		coresight-name = "coresight-etm1";
		qcom,skip-power-up;

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <2>;
		out-ports {
			port {
				ete1_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete1>;
				};
			};
		};
	};

	etm2 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12240000 0x1000>;
		cpu = <&CPU2>;

		coresight-name = "coresight-etm2";
		qcom,skip-power-up;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <3>;
		out-ports {
			port {
				ete2_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete2>;
				};
			};
		};
	};

	etm3 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12340000 0x1000>;
		cpu = <&CPU3>;

		coresight-name = "coresight-etm3";
		qcom,skip-power-up;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <4>;
		out-ports {
			port {
				ete3_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete3>;
				};
			};
		};
	};

	etm4 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12440000 0x1000>;
		cpu = <&CPU4>;

		coresight-name = "coresight-etm4";
		qcom,skip-power-up;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <5>;
		out-ports {
			port {
				ete4_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete4>;
				};
			};
		};
	};

	etm5 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12540000 0x1000>;
		cpu = <&CPU5>;

		coresight-name = "coresight-etm5";
		qcom,skip-power-up;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <6>;
		out-ports {
			port {
				ete5_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete5>;
				};
			};
		};
	};

	etm6 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12640000 0x1000>;
		cpu = <&CPU6>;

		coresight-name = "coresight-etm6";
		qcom,skip-power-up;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <7>;
		out-ports {
			port {
				ete6_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete6>;
				};
			};
		};
	};

	etm7 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12740000 0x1000>;
		cpu = <&CPU7>;

		coresight-name = "coresight-etm7";
		qcom,skip-power-up;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <8>;
		out-ports {
			port {
				ete7_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete7>;
				};
			};
		};
	};

	funnel_etm: funnel@12800000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x12800000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-etm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				funnel_ete_out_funnel_apss: endpoint {
					remote-endpoint =
					<&funnel_apss_in_funnel_ete>;
				};
			};
		};

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_ete_in_ete0: endpoint {
					remote-endpoint =
					<&ete0_out_funnel_ete>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_ete_in_ete1: endpoint {
				remote-endpoint =
					<&ete1_out_funnel_ete>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_ete_in_ete2: endpoint {
				remote-endpoint =
					<&ete2_out_funnel_ete>;
				};
			};

			port@3 {
				reg = <3>;
				funnel_ete_in_ete3: endpoint {
				remote-endpoint =
					<&ete3_out_funnel_ete>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_ete_in_ete4: endpoint {
				remote-endpoint =
					<&ete4_out_funnel_ete>;
				};
			};

			port@5 {
				reg = <5>;
				funnel_ete_in_ete5: endpoint {
					remote-endpoint =
					<&ete5_out_funnel_ete>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_ete_in_ete6: endpoint {
					remote-endpoint =
					<&ete6_out_funnel_ete>;
				};
			};

			port@7 {
				reg = <7>;
				funnel_ete_in_ete7: endpoint {
					remote-endpoint =
					<&ete7_out_funnel_ete>;
				};
			};
		};
	};
};
