&soc {

	stm: stm@10002000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb962>;
		reg = <0x10002000 0x1000>,
			<0x16280000 0x180000>;
		reg-names = "stm-base", "stm-stimulus-base";

		atid = <16>;
		coresight-name = "coresight-stm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				stm_out_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_in_stm>;
				};
			};
		};
	};

	snoc: snoc {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-snoc";
		qcom,dummy-source;

		atid = <125>;
		out-ports {
			port {
				snoc_out_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_in_snoc>;
				};
			};
		};
	};

	csr: csr@10001000 {
		compatible = "qcom,coresight-csr";
		reg = <0x10001000 0x1000>;
		reg-names = "csr-base";

		coresight-name = "coresight-csr";
		qcom,usb-bam-support;
		qcom,hwctrl-set-support;
		qcom,set-byte-cntr-support;

		qcom,blk-size = <1>;
	};

	swao_csr: csr@10b11000 {
		compatible = "qcom,coresight-csr";

		reg = <0x10b11000 0x1000>,
		      <0x10b110f8 0x50>;
		reg-names = "csr-base", "msr-base";

		coresight-name = "coresight-swao-csr";
		qcom,timestamp-support;
		qcom,msr-support;
		qcom,blk-size = <1>;

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	audio_etm0 {
		compatible = "qcom,coresight-remote-etm";

		coresight-name = "coresight-audio-etm0";
		qcom,inst-id = <5>;

		atid = <40 41>;

		out-ports {
			port {
				audio_etm0_out_funnel_lpass_lpi: endpoint {
					remote-endpoint =
						<&funnel_lpass_lpi_in_audio_etm0>;
				};
			};
		};
	};

	lpass_stm: lpass_stm {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-lpass-stm";
		qcom,dummy-source;

		atid = <25>;

		out-ports {
			port {
				lpass_stm_out_funnel_lpass_lpi: endpoint {
					remote-endpoint =
					<&funnel_lpass_lpi_in_lpass_stm>;
				};
			};
		};
	};

	tpdm_lpass_lpi: tpdm@10b46000 {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-tpdm-lpass-lpi";
		qcom,dummy-source;

		atid = <26>;

		out-ports {
			port {
				tpdm_lpass_lpi_out_funnel_lpass_lpi: endpoint {
					remote-endpoint =
					<&funnel_lpass_lpi_in_tpdm_lpass_lpi>;
				};
			};
		};
	};

	turing_etm0: turing_etm0 {
		compatible = "qcom,coresight-remote-etm";

		coresight-name = "coresight-turing-etm0";
		qcom,inst-id = <13>;

		atid = <38 39>;

		out-ports {
			port {
				turing_etm0_out_funnel_turing_dup: endpoint {
					remote-endpoint =
						<&funnel_turing_dup_in_turing_etm0>;
				};
			};
		};
	};

	tpdm_swao_prio0: tpdm@10b09000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b09000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-swao-prio-0";
		atid = <71>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_prio0_out_tpda_aoss: endpoint {
					remote-endpoint =
					<&tpda_aoss_in_tpdm_swao_prio0>;
				};
			};
		};
	};

	tpdm_swao_prio1: tpdm@10b0a000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b0a000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-swao-prio-1";
		atid = <71>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_prio1_out_tpda_aoss: endpoint {
					remote-endpoint =
					<&tpda_aoss_in_tpdm_swao_prio1>;
				};
			};
		};
	};

	tpdm_swao_prio2: tpdm@10b0b000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b0b000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-swao-prio-2";
		atid = <71>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_prio2_out_tpda_aoss: endpoint {
					remote-endpoint =
					<&tpda_aoss_in_tpdm_swao_prio2>;
				};
			};
		};
	};

	tpdm_swao_prio3: tpdm@10b0c000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b0c000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-swao-prio-3";
		atid = <71>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_prio3_out_tpda_aoss: endpoint {
					remote-endpoint =
					<&tpda_aoss_in_tpdm_swao_prio3>;
				};
			};
		};
	};

	tpdm_lpass: tpdm@10844000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10844000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-lpass";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_lpass_out_funnel_lpass_dl: endpoint {
					remote-endpoint =
					<&funnel_lpass_dl_in_tpdm_lpass>;
				};
			};
		};
	};

	tpdm_ddr_ch0: tpdm@10d20000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10d20000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-ddr-ch0";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_ddr_ch0_out_funnel_ddr_ch0: endpoint {
					remote-endpoint =
					<&funnel_ddr_ch0_in_tpdm_ddr_ch0>;
				};
			};
		};
	};

	tpdm_ddr: tpdm@10d00000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10d00000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-ddr";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		status = "disabled";

		out-ports {
			port {
				tpdm_ddr_out_funnel_ddr0: endpoint {
					remote-endpoint =
					<&funnel_ddr0_in_tpdm_ddr>;
				};
			};
		};
	};

	tpdm_shrm: tpdm@10d01000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10d01000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-shrm";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		status = "disabled";

		out-ports {
			port {
				tpdm_shrm_out_funnel_ddr0: endpoint {
					remote-endpoint =
					<&funnel_ddr0_in_tpdm_shrm>;
				};
			};
		};
	};

	tpdm_video: tpdm@10830000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10830000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-video";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_video_out_funnel_video: endpoint {
					remote-endpoint =
					<&funnel_video_in_tpdm_video>;
				};
			};
		};
	};

	tpdm_mdss: tpdm@10c60000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c60000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-mdss";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		status = "disabled";

		out-ports {
			port {
				tpdm_mdss_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_tpdm_mdss>;
				};
			};
		};
	};

	tpdm_dlmm: tpdm@10c08000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c08000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-mm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <79>;

		out-ports {
			port {
				tpdm_dlmm_out_funnel_dlmm: endpoint {
					remote-endpoint =
					<&funnel_dlmm_in_tpdm_dlmm>;
				};
			};
		};
	};

	tpdm_rdpm: tpdm@10c38000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c38000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-rdpm";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		status = "disabled";

		out-ports {
			port {
				tpdm_dl_west0_out_funnel_dl_west: endpoint {
					remote-endpoint =
					<&funnel_dl_west_in_tpdm_dl_west0>;
				};
			};
		};
	};

	tpdm_rdpm_mx: tpdm@10c39000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c39000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-rdpm-mx";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		status = "disabled";

		out-ports {
			port {
				tpdm_dl_west1_out_funnel_dl_west: endpoint {
					remote-endpoint =
					<&funnel_dl_west_in_tpdm_dl_west1>;
				};
			};
		};
	};

	tpdm_turing: tpdm@10980000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10980000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-turing";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_turing_out_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_in_tpdm_turing>;
				};
			};
		};
	};

	tpdm_turing_llm: tpdm@10981000 {
		compatible = "qcom,coresight-dummy";
		coresight-name = "coresight-tpdm-turing-llm";
		qcom,dummy-source;

		atid = <78>;

		out-ports {
			port {
				tpdm_turing_llm_out_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_in_tpdm_turing_llm>;
				};
			};
		};
	};

	tpdm_gpu: tpdm@10900000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10900000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-gpu";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_gpu_out_funnel_gpu_dl: endpoint {
					remote-endpoint =
					<&funnel_gpu_dl_in_tpdm_gpu>;
				};
			};
		};
	};

	tpdm_prng: tpdm@10841000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10841000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-prng";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_prng_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_tpdm_prng>;
				};
			};
		};
	};

	tpdm_qm: tpdm@109d0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x109d0000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-qm";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_qm_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_tpdm_qm>;
				};
			};
		};
	};

	tpdm_gcc: tpdm@1082c000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x1082c000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-gcc";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_gcc_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_tpdm_gcc>;
				};
			};
		};
	};

	tpdm_vsense: tpdm@10840000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10840000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-vsense";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_vsense_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_tpdm_vsense>;
				};
			};
		};
	};

	tpdm_pimem: tpdm@10850000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10850000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-pimem";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_pime_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_tpdm_pime>;
				};
			};
		};
	};

	tpdm_dlct0: tpdm@10c28000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c28000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-dlct";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <78>;

		out-ports {
			port {
				tpdm_dl_ct0_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_tpdm_dl_ct0>;
				};
			};
		};
	};

	tpdm_dlct1: tpdm@10c29000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c29000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-ipcc";
		atid = <78>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_dl_ct1_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_tpdm_dl_ct1>;
				};
			};
		};
	};

	tpdm_swao: tpdm@10b0d000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10b0d000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-swao-1";
		atid = <71>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_swao_out_tpda_aoss: endpoint {
					remote-endpoint =
					<&tpda_aoss_in_tpdm_swao>;
				};
			};
		};
	};

	tpdm_dlct3: tpdm@10c30000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c30000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-dlct3";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <79>;

		out-ports {
			port {
				tpdm_dlct3_out_tpda_dlct3: endpoint {
					remote-endpoint =
					<&tpda_dlct3_in_tpdm_dlct3>;
				};
			};
		};
	};

	tpdm_spdm: tpdm@1000f000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x1000f000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-spdm";
		atid = <65>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_spdm_out_tpda_qdss: endpoint {
					remote-endpoint =
					<&tpda_qdss_in_tpdm_spdm>;
				};
			};
		};
	};

	tpdm_wpss: tpdm@10c70000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c70000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-wpss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <79>;

		out-ports {
			port {
				tpdm_wpss_out_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_in_tpdm_wpss>;
				};
			};
		};
	};

	tpdm_wpss1: tpdm@10c71000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c71000 0x1000>;
		reg-names = "tpdm-base";

		atid = <97>;
		coresight-name = "coresight-tpdm-wpss-1";
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_wpss1_out_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_in_tpdm_wpss1>;
				};
			};
		};
	};

	wpss_etm: wpss_etm {
		compatible = "qcom,coresight-remote-etm";

		coresight-name = "coresight-wpss-etm0";
		qcom,inst-id = <3>;
		atid = <44>;

		out-ports {
			port {
				wpss_etm_out_funnel_wpss: endpoint {
					remote-endpoint =
						<&funnel_wpss_in_wpss_etm>;
				};
			};
		};
	};

	tpdm_dcc: tpdm@10003000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10003000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-dcc";
		atid = <65>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,hw-enable-check;
		out-ports {
			port {
				tpdm_dcc_out_tpda_qdss: endpoint {
					remote-endpoint =
					<&tpda_qdss_in_tpdm_dcc>;
				};
			};
		};
	};

	tpdm_dl_north: tpdm@10ac0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10ac0000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-dl-north";
		atid = <97>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_dl_north_out_tpda_dl_north: endpoint {
					remote-endpoint =
					<&tpda_dl_north_in_tpdm_dl_north>;
				};
			};
		};
	};

	tpdm_llm_silver: tpdm@128a0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x128a0000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-llm-silver";
		atid = <66>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_llm_silver_out_tpda_apss: endpoint {
					remote-endpoint =
					<&tpda_apss_in_tpdm_llm_silver>;
				};
			};
		};
	};

	tpdm_apss0: tpdm@12860000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x12860000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-actpm";
		atid = <66>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_apss0_out_tpda_apss: endpoint {
					remote-endpoint =
					<&tpda_apss_in_tpdm_apss0>;
				};
			};
		};
	};

	tpdm_apss1: tpdm@12861000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x12861000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-apss";
		atid = <66>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_apss1_out_tpda_apss: endpoint {
					remote-endpoint =
					<&tpda_apss_in_tpdm_apss1>;
				};
			};
		};
	};

	tpdm_sdcc5: tpdm@10c20000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10c20000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-sdcc5";
		atid = <97>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		status = "disabled";

		out-ports {
			port {
				tpdm_sdcc5_out_tpda_dl_north: endpoint {
					remote-endpoint =
					<&tpda_dl_north_in_tpdm_sdcc5>;
				};
			};
		};
	};

	tpdm_tmess_prng: tpdm@10cc9000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10cc9000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-tmess-prng";
		atid = <85>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		status = "disabled";

		out-ports {
			port {
				tpdm_tmess_prng_out_tpda_tmess: endpoint {
					remote-endpoint =
					<&tpda_tmess_in_tpdm_tmess_prng>;
				};
			};
		};
	};

	tpdm_tmess1: tpdm@10cc1000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10cc1000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-tmess-1";
		atid = <85>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_tmess0_out_tpda_tmess: endpoint {
					remote-endpoint =
					<&tpda_tmess_in_tpdm_tmess0>;
				};
			};
		};
	};

	tpdm_tmess0: tpdm@10cc0000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb968>;
		reg = <0x10cc0000 0x1000>;
		reg-names = "tpdm-base";

		coresight-name = "coresight-tpdm-tmess-0";
		atid = <85>;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		out-ports {
			port {
				tpdm_tmess1_out_tpda_tmess: endpoint {
					remote-endpoint =
					<&tpda_tmess_in_tpdm_tmess1>;
				};
			};
		};
	};


	funnel_lpass_lpi: funnel@10b44000 {
		compatible = "arm,coresight-static-funnel";
		coresight-name = "coresight-funnel-lpass_lpi";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_lpass_lpi_in_audio_etm0: endpoint {
					remote-endpoint =
					<&audio_etm0_out_funnel_lpass_lpi>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_lpass_lpi_in_lpass_stm: endpoint {
					remote-endpoint =
					<&lpass_stm_out_funnel_lpass_lpi>;
				};
			};

			port@5 {
				reg = <5>;
				funnel_lpass_lpi_in_tpdm_lpass_lpi: endpoint {
					remote-endpoint =
					<&tpdm_lpass_lpi_out_funnel_lpass_lpi>;
				};
			};

		};

		out-ports {

			port {
				funnel_lpass_lpi_out_funnel_aoss: endpoint {
					remote-endpoint =
					<&funnel_aoss_in_funnel_lpass_lpi>;
				};
			};

		};
	};

	funnel_gpu_dl: funnel@10902000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10902000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-gpu_dl";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;


			port@0 {
				reg = <0>;
				funnel_gpu_dl_in_tpdm_gpu: endpoint {
					remote-endpoint =
					<&tpdm_gpu_out_funnel_gpu_dl>;
				};
			};

		};

		out-ports {

			port {
				funnel_gpu_dl_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_funnel_gpu_dl>;
				};
			};

		};
	};

	funnel_video: funnel@10832000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10832000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-video";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_video_in_tpdm_video: endpoint {
					remote-endpoint =
					<&tpdm_video_out_funnel_video>;
				};
			};

		};

		out-ports {

			port {
				funnel_video_out_funnel_dlmm: endpoint {
					remote-endpoint =
					<&funnel_dlmm_in_funnel_video>;
				};
			};

		};
	};


	funnel_dlmm: funnel@10c0a000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c0a000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dlmm";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_dlmm_in_funnel_video: endpoint {
					remote-endpoint =
					<&funnel_video_out_funnel_dlmm>;
				};
			};

			port@3 {
				reg = <3>;
				funnel_dlmm_in_tpdm_dlmm: endpoint {
					remote-endpoint =
					<&tpdm_dlmm_out_funnel_dlmm>;
				};
			};


		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_dlmm_out_tpda_dlct3_2: endpoint {
					remote-endpoint =
					<&tpda_dlct3_2_in_funnel_dlmm>;
					source = <&tpdm_video>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_dlmm_out_tpda_dlct3_5: endpoint {
					remote-endpoint =
					<&tpda_dlct3_5_in_funnel_dlmm>;
					source = <&tpdm_dlmm>;
				};
			};

		};
	};

	funnel_lpass_dl: funnel@10846000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10846000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-lpass_dl";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_lpass_dl_in_tpdm_lpass: endpoint {
					remote-endpoint =
					<&tpdm_lpass_out_funnel_lpass_dl>;
				};
			};

		};

		out-ports {

			port {
				funnel_lpass_dl_out_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_in_funnel_lpass_dl>;
				};
			};

		};
	};

	funnel_ddr_ch0: funnel@10d22000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10d22000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-ddr_ch0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_ddr_ch0_in_tpdm_ddr_ch0: endpoint {
					remote-endpoint =
					<&tpdm_ddr_ch0_out_funnel_ddr_ch0>;
				};
			};

		};

		out-ports {

			port {
				funnel_ddr_ch0_out_funnel_ddr0: endpoint {
					remote-endpoint =
					<&funnel_ddr0_in_funnel_ddr_ch0>;
				};
			};

		};
	};


	funnel_ddr0: funnel@10d03000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10d03000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-ddr0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_ddr0_in_funnel_ddr_ch0: endpoint {
					remote-endpoint =
					<&funnel_ddr_ch0_out_funnel_ddr0>;
				};
			};

			port@3 {
				reg = <3>;
				funnel_ddr0_in_tpdm_shrm: endpoint {
					remote-endpoint =
					<&tpdm_shrm_out_funnel_ddr0>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_ddr0_in_tpdm_ddr: endpoint {
					remote-endpoint =
					<&tpdm_ddr_out_funnel_ddr0>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_ddr0_out_tpda_dl_center_5: endpoint {
					remote-endpoint =
					<&tpda_dl_center_5_in_funnel_ddr0>;
					source = <&tpdm_ddr_ch0>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_ddr0_out_tpda_dl_center_7: endpoint {
					remote-endpoint =
					<&tpda_dl_center_7_in_funnel_ddr0>;
					source = <&tpdm_ddr>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_ddr0_out_tpda_dl_center_8: endpoint {
					remote-endpoint =
					<&tpda_dl_center_8_in_funnel_ddr0>;
					source = <&tpdm_shrm>;
				};
			};
		};
	};

	funnel_wpss: funnel@10c73000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c73000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-wpss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_wpss_in_tpdm_wpss: endpoint {
					remote-endpoint =
					<&tpdm_wpss_out_funnel_wpss>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_wpss_in_tpdm_wpss1: endpoint {
					remote-endpoint =
					<&tpdm_wpss1_out_funnel_wpss>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_wpss_in_wpss_etm: endpoint {
					remote-endpoint =
					<&wpss_etm_out_funnel_wpss>;
				};
			};

		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_wpss_out_tpda_dlct3: endpoint {
					remote-endpoint =
					<&tpda_dlct3_in_funnel_wpss>;
					source = <&tpdm_wpss>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_wpss_out_funnel_dlct3: endpoint {
					remote-endpoint =
					<&funnel_dlct3_in_funnel_wpss>;
				};
			};

		};
	};

	funnel_dl_west: funnel@10c3a000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c3a000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dl_west";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@5 {
				reg = <5>;
				funnel_dl_west_in_tpdm_dl_west1: endpoint {
					remote-endpoint =
					<&tpdm_dl_west1_out_funnel_dl_west>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_dl_west_in_tpdm_dl_west0: endpoint {
					remote-endpoint =
					<&tpdm_dl_west0_out_funnel_dl_west>;
				};
			};

		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_dl_west_out_tpda_dl_center_13: endpoint {
					remote-endpoint =
					<&tpda_dl_center_13_in_funnel_dl_west>;
					source = <&tpdm_rdpm>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_dl_west_out_tpda_dl_center_14: endpoint {
					remote-endpoint =
					<&tpda_dl_center_14_in_funnel_dl_west>;
					source = <&tpdm_rdpm_mx>;
				};
			};
		};
	};

	funnel_turing_dup: funnel@10984000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10984000 0x1000>,
			<0x10983000 0x1000>;
		reg-names = "funnel-base-dummy", "funnel-base-real";

		coresight-name = "coresight-funnel-turing_dup";

		qcom,duplicate-funnel;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			#address-cells = <1>;
			#size-cells = <0>;
			port@3 {
				reg = <3>;
				funnel_turing_dup_in_turing_etm0: endpoint {
					remote-endpoint =
					<&turing_etm0_out_funnel_turing_dup>;
				};
			};

		};

		out-ports {
			port {
				funnel_turing_dup_out_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_in_funnel_turing_dup>;
				};
			};

		};
	};

	funnel_turing: funnel@10983000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10983000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-turing";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				funnel_turing_in_tpdm_turing_llm: endpoint {
					remote-endpoint =
					<&tpdm_turing_llm_out_funnel_turing>;
				};
			};

			port@0 {
				reg = <0>;
				funnel_turing_in_tpdm_turing: endpoint {
					remote-endpoint =
					<&tpdm_turing_out_funnel_turing>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_turing_in_funnel_turing_dup: endpoint {
					remote-endpoint =
					<&funnel_turing_dup_out_funnel_turing>;
				};
			};


		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_turing_out_tpda_dl_center_15: endpoint {
					remote-endpoint =
					<&tpda_dl_center_15_in_funnel_turing>;
					source = <&tpdm_turing>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_turing_out_tpda_dl_center_16: endpoint {
					remote-endpoint =
					<&tpda_dl_center_16_in_funnel_turing>;
					source = <&tpdm_turing_llm>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_turing_out_funnel_dl_center: endpoint {
					remote-endpoint =
					<&funnel_dl_center_in_funnel_turing>;
				};
			};
		};
	};

	tpda_dlct3: tpda@10c32000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10c32000 0x1000>;
		reg-names = "tpda-base";

		coresight-name = "coresight-tpda-dlct3";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,tpda-atid = <79>;
		qcom,dsb-elem-size = <0 32>,
							<2 32>,
							<5 32>,
							<10 32>;

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@a {
				reg = <10>;
				tpda_dlct3_in_tpdm_dlct3: endpoint {
					remote-endpoint =
					<&tpdm_dlct3_out_tpda_dlct3>;
				};
			};

			port@2 {
				reg = <2>;
				tpda_dlct3_2_in_funnel_dlmm: endpoint {
					remote-endpoint =
					<&funnel_dlmm_out_tpda_dlct3_2>;
				};
			};

			port@5 {
				reg = <5>;
				tpda_dlct3_5_in_funnel_dlmm: endpoint {
					remote-endpoint =
					<&funnel_dlmm_out_tpda_dlct3_5>;
				};
			};

			port@0 {
				reg = <0>;
				tpda_dlct3_in_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_out_tpda_dlct3>;
				};
			};

		};

		out-ports {

			port {
				tpda_dlct3_out_funnel_dlct3: endpoint {
					remote-endpoint =
					<&funnel_dlct3_in_tpda_dlct3>;
				};
			};

		};
	};

	funnel_dlct3: funnel@10c33000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c33000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dlct3";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				funnel_dlct3_in_funnel_wpss: endpoint {
					remote-endpoint =
					<&funnel_wpss_out_funnel_dlct3>;
				};
			};

			port@0 {
				reg = <0>;
				funnel_dlct3_in_tpda_dlct3: endpoint {
					remote-endpoint =
					<&tpda_dlct3_out_funnel_dlct3>;
				};
			};

		};

		out-ports {

			port {
				funnel_dlct3_out_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_in_funnel_dlct3>;
				};
			};

		};
	};

	tpda_tmess: tpda@10cc4000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10cc4000 0x1000>;
		reg-names = "tpda-base";

		coresight-name = "coresight-tpda-tmess";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,tpda-atid = <85>;

		qcom,dsb-elem-size = <2 64>;
		qcom,cmb-elem-size = <0 32>,
							<1 32>;

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				tpda_tmess_in_tpdm_tmess_prng: endpoint {
					remote-endpoint =
					<&tpdm_tmess_prng_out_tpda_tmess>;
				};
			};

			port@1 {
				reg = <1>;
				tpda_tmess_in_tpdm_tmess1: endpoint {
					remote-endpoint =
					<&tpdm_tmess1_out_tpda_tmess>;
				};
			};

			port@2 {
				reg = <2>;
				tpda_tmess_in_tpdm_tmess0: endpoint {
					remote-endpoint =
					<&tpdm_tmess0_out_tpda_tmess>;
				};
			};
		};

		out-ports {

			port {
				tpda_tmess_out_funnel_tmess: endpoint {
					remote-endpoint =
					<&funnel_tmess_in_tpda_tmess>;
				};
			};

		};
	};

	funnel_tmess: funnel@10cc5000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10cc5000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-tmess";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_tmess_in_tpda_tmess: endpoint {
					remote-endpoint =
					<&tpda_tmess_out_funnel_tmess>;
				};
			};

		};

		out-ports {

			port {
				funnel_tmess_out_funnel_dl_north: endpoint {
					remote-endpoint =
					<&funnel_dl_north_in_funnel_tmess>;
				};
			};

		};
	};

	tpda_dl_north: tpda@10ac1000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10ac1000 0x1000>;
		reg-names = "tpda-base";

		coresight-name = "coresight-tpda-dl_north";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,tpda-atid = <97>;

		qcom,dsb-elem-size = <2 32>;
		qcom,cmb-elem-size = <1 32>;

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				tpda_dl_north_in_tpdm_sdcc5: endpoint {
					remote-endpoint =
					<&tpdm_sdcc5_out_tpda_dl_north>;
				};
			};

			port@2 {
				reg = <2>;
				tpda_dl_north_in_tpdm_dl_north: endpoint {
					remote-endpoint =
					<&tpdm_dl_north_out_tpda_dl_north>;
				};
			};

		};

		out-ports {

			port {
				tpda_dl_north_out_funnel_dl_north: endpoint {
					remote-endpoint =
					<&funnel_dl_north_in_tpda_dl_north>;
				};
			};

		};
	};

	funnel_dl_north: funnel@10ac2000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10ac2000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dl_north";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_dl_north_in_tpda_dl_north: endpoint {
					remote-endpoint =
					<&tpda_dl_north_out_funnel_dl_north>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_dl_north_in_funnel_tmess: endpoint {
					remote-endpoint =
					<&funnel_tmess_out_funnel_dl_north>;
				};
			};

		};

		out-ports {

			port {
				funnel_dl_north_out_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_in_funnel_dl_north>;
				};
			};

		};
	};

	tpda_apss: tpda@12863000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x12863000 0x1000>;
		reg-names = "tpda-base";

		coresight-name = "coresight-tpda-apss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,tpda-atid = <66>;

		qcom,dsb-elem-size = <4 32>;
		qcom,cmb-elem-size = <0 32>,
							<3 64>;

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				tpda_apss_in_tpdm_llm_silver: endpoint {
					remote-endpoint =
					<&tpdm_llm_silver_out_tpda_apss>;
				};
			};

			port@3 {
				reg = <3>;
				tpda_apss_in_tpdm_apss0: endpoint {
					remote-endpoint =
					<&tpdm_apss0_out_tpda_apss>;
				};
			};

			port@4 {
				reg = <4>;
				tpda_apss_in_tpdm_apss1: endpoint {
					remote-endpoint =
					<&tpdm_apss1_out_tpda_apss>;
				};
			};

		};

		out-ports {

			port {
				tpda_apss_out_funnel_apss: endpoint {
					remote-endpoint =
					<&funnel_apss_in_tpda_apss>;
				};
			};

		};
	};

	ipcb_tgu: tgu@10b0e000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb999>;

		reg = <0x10b0e000 0x1000>;
		reg-names = "tgu-base";

		tgu-steps = <3>;
		tgu-conditions = <4>;
		tgu-regs = <4>;
		tgu-timer-counters = <8>;

		coresight-name = "coresight-tgu-ipcb";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	spmi_tgu0: tgu@10b0f000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb999>;

		reg = <0x10b0f000 0x1000>;
		reg-names = "tgu-base";

		tgu-steps = <3>;
		tgu-conditions = <4>;
		tgu-regs = <9>;
		tgu-timer-counters = <8>;

		coresight-name = "coresight-tgu-spmi0";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	spmi_tgu1: tgu@10b10000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb999>;

		reg = <0x10b10000 0x1000>;
		reg-names = "tgu-base";

		tgu-steps = <3>;
		tgu-conditions = <4>;
		tgu-regs = <9>;
		tgu-timer-counters = <8>;

		coresight-name = "coresight-tgu-spmi1";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	etm0 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12040000 0x1000>;
		cpu = <&CPU0>;

		coresight-name = "coresight-etm0";
		qcom,skip-power-up;

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <1>;
		out-ports {
			port {
				ete0_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete0>;
				};
			};
		};
	};

	etm1 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12140000 0x1000>;
		cpu = <&CPU1>;

		coresight-name = "coresight-etm1";
		qcom,skip-power-up;

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <2>;
		out-ports {
			port {
				ete1_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete1>;
				};
			};
		};
	};

	etm2 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12240000 0x1000>;
		cpu = <&CPU2>;

		coresight-name = "coresight-etm2";
		qcom,skip-power-up;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <3>;
		out-ports {
			port {
				ete2_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete2>;
				};
			};
		};
	};

	etm3 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb95d>;
		reg = <0x12340000 0x1000>;
		cpu = <&CPU3>;

		coresight-name = "coresight-etm3";
		qcom,skip-power-up;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		atid = <4>;
		out-ports {
			port {
				ete3_out_funnel_ete: endpoint {
				remote-endpoint = <&funnel_ete_in_ete3>;
				};
			};
		};
	};

	funnel_apss: funnel@12810000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x12810000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-apss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_ete_in_ete0: endpoint {
					remote-endpoint =
					<&ete0_out_funnel_ete>;
				};
			};

			port@1 {
				reg = <1>;
				funnel_ete_in_ete1: endpoint {
				remote-endpoint =
					<&ete1_out_funnel_ete>;
				};
			};

			port@2 {
				reg = <2>;
				funnel_ete_in_ete2: endpoint {
				remote-endpoint =
					<&ete2_out_funnel_ete>;
				};
			};

			port@3 {
				reg = <3>;
				funnel_ete_in_ete3: endpoint {
				remote-endpoint =
					<&ete3_out_funnel_ete>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_apss_in_tpda_apss: endpoint {
					remote-endpoint =
					<&tpda_apss_out_funnel_apss>;
				};
			};

		};

		out-ports {

			port {
				funnel_apss_out_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_in_funnel_apss>;
				};
			};

		};
	};

	tpda_dl_center: tpda@10c2b000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10c2b000 0x1000>;
		reg-names = "tpda-base";

		coresight-name = "coresight-tpda-dl_center";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,tpda-atid = <78>;

		qcom,dsb-elem-size = <0 32>,
							<4 32>,
							<5 32>,
							<7 32>,
							<15 32>,
							<17 32>,
							<20 32>,
							<21 32>,
							<25 32>,
							<26 32>;
		qcom,cmb-elem-size = <0 32>,
							<7 32>,
							<8 64>,
							<13 64>,
							<14 64>,
							<16 32>,
							<19 32>,
							<22 32>,
							<25 64>,
							<27 64>;

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@19 {
				reg = <25>;
				tpda_dl_center_in_tpdm_pime: endpoint {
					remote-endpoint =
					<&tpdm_pime_out_tpda_dl_center>;
				};
			};

			port@d {
				reg = <13>;
				tpda_dl_center_13_in_funnel_dl_west: endpoint {
					remote-endpoint =
					<&funnel_dl_west_out_tpda_dl_center_13>;
				};
			};

			port@1b {
				reg = <27>;
				tpda_dl_center_in_tpdm_dl_ct1: endpoint {
					remote-endpoint =
					<&tpdm_dl_ct1_out_tpda_dl_center>;
				};
			};

			port@f {
				reg = <15>;
				tpda_dl_center_15_in_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_out_tpda_dl_center_15>;
				};
			};

			port@e {
				reg = <14>;
				tpda_dl_center_14_in_funnel_dl_west: endpoint {
					remote-endpoint =
					<&funnel_dl_west_out_tpda_dl_center_14>;
				};
			};

			port@11 {
				reg = <17>;
				tpda_dl_center_in_funnel_gpu_dl: endpoint {
					remote-endpoint =
					<&funnel_gpu_dl_out_tpda_dl_center>;
				};
			};

			port@10 {
				reg = <16>;
				tpda_dl_center_16_in_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_out_tpda_dl_center_16>;
				};
			};

			port@13 {
				reg = <19>;
				tpda_dl_center_in_tpdm_prng: endpoint {
					remote-endpoint =
					<&tpdm_prng_out_tpda_dl_center>;
				};
			};

			port@16 {
				reg = <22>;
				tpda_dl_center_in_tpdm_vsense: endpoint {
					remote-endpoint =
					<&tpdm_vsense_out_tpda_dl_center>;
				};
			};

			port@1a {
				reg = <26>;
				tpda_dl_center_in_tpdm_dl_ct0: endpoint {
					remote-endpoint =
					<&tpdm_dl_ct0_out_tpda_dl_center>;
				};
			};

			port@14 {
				reg = <20>;
				tpda_dl_center_in_tpdm_qm: endpoint {
					remote-endpoint =
					<&tpdm_qm_out_tpda_dl_center>;
				};
			};

			port@0 {
				reg = <0>;
				tpda_dl_center_in_tpdm_mdss: endpoint {
					remote-endpoint =
					<&tpdm_mdss_out_tpda_dl_center>;
				};
			};

			port@5 {
				reg = <5>;
				tpda_dl_center_5_in_funnel_ddr0: endpoint {
					remote-endpoint =
					<&funnel_ddr0_out_tpda_dl_center_5>;
				};
			};

			port@4 {
				reg = <4>;
				tpda_dl_center_in_funnel_lpass_dl: endpoint {
					remote-endpoint =
					<&funnel_lpass_dl_out_tpda_dl_center>;
				};
			};

			port@7 {
				reg = <7>;
				tpda_dl_center_7_in_funnel_ddr0: endpoint {
					remote-endpoint =
					<&funnel_ddr0_out_tpda_dl_center_7>;
				};
			};

			port@8 {
				reg = <8>;
				tpda_dl_center_8_in_funnel_ddr0: endpoint {
					remote-endpoint =
					<&funnel_ddr0_out_tpda_dl_center_8>;
				};
			};

			port@15 {
				reg = <21>;
				tpda_dl_center_in_tpdm_gcc: endpoint {
					remote-endpoint =
					<&tpdm_gcc_out_tpda_dl_center>;
				};
			};

		};

		out-ports {

			port {
				tpda_dl_center_out_funnel_dl_center: endpoint {
					remote-endpoint =
					<&funnel_dl_center_in_tpda_dl_center>;
				};
			};

		};
	};

	funnel_dl_center: funnel@10c2c000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10c2c000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-dl_center";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_dl_center_in_tpda_dl_center: endpoint {
					remote-endpoint =
					<&tpda_dl_center_out_funnel_dl_center>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_dl_center_in_funnel_turing: endpoint {
					remote-endpoint =
					<&funnel_turing_out_funnel_dl_center>;
				};
			};

		};

		out-ports {

			port {
				funnel_dl_center_out_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_in_funnel_dl_center>;
				};
			};

		};
	};

	tpda_qdss: tpda@10004000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10004000 0x1000>;
		reg-names = "tpda-base";

		coresight-name = "coresight-tpda-qdss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,tpda-atid = <65>;

		qcom,cmb-elem-size = <0 32>,
							<1 32>;

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				tpda_qdss_in_tpdm_spdm: endpoint {
					remote-endpoint =
					<&tpdm_spdm_out_tpda_qdss>;
				};
			};

			port@0 {
				reg = <0>;
				tpda_qdss_in_tpdm_dcc: endpoint {
					remote-endpoint =
					<&tpdm_dcc_out_tpda_qdss>;
				};
			};

		};

		out-ports {

			port {
				tpda_qdss_out_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_in_tpda_qdss>;
				};
			};

		};
	};

	funnel_in0: funnel@10041000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10041000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-in0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				funnel_in0_in_snoc: endpoint {
					remote-endpoint =
					<&snoc_out_funnel_in0>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_in0_in_tpda_qdss: endpoint {
					remote-endpoint =
					<&tpda_qdss_out_funnel_in0>;
				};
			};

			port@7 {
				reg = <7>;
				funnel_in0_in_stm: endpoint {
					remote-endpoint =
					<&stm_out_funnel_in0>;
				};
			};

		};

		out-ports {

			port {
				funnel_in0_out_funnel_merge: endpoint {
					remote-endpoint =
					<&funnel_merge_in_funnel_in0>;
				};
			};

		};
	};

	funnel_in1: funnel@10042000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10042000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-in1";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				funnel_in1_in_funnel_dl_north: endpoint {
					remote-endpoint =
					<&funnel_dl_north_out_funnel_in1>;
				};
			};

			port@5 {
				reg = <5>;
				funnel_in1_in_funnel_dlct3: endpoint {
					remote-endpoint =
					<&funnel_dlct3_out_funnel_in1>;
				};
			};

			port@4 {
				reg = <4>;
				funnel_in1_in_funnel_apss: endpoint {
					remote-endpoint =
					<&funnel_apss_out_funnel_in1>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_in1_in_funnel_dl_center: endpoint {
					remote-endpoint =
					<&funnel_dl_center_out_funnel_in1>;
				};
			};

		};

		out-ports {

			port {
				funnel_in1_out_funnel_merge: endpoint {
					remote-endpoint =
					<&funnel_merge_in_funnel_in1>;
				};
			};

		};
	};

	funnel_merge: funnel@10045000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10045000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-merge";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				funnel_merge_in_funnel_in1: endpoint {
					remote-endpoint =
					<&funnel_in1_out_funnel_merge>;
				};
			};

			port@0 {
				reg = <0>;
				funnel_merge_in_funnel_in0: endpoint {
					remote-endpoint =
					<&funnel_in0_out_funnel_merge>;
				};
			};

		};

		out-ports {

			port {
				funnel_merge_out_funnel_aoss: endpoint {
					remote-endpoint =
					<&funnel_aoss_in_funnel_merge>;
				};
			};

		};
	};

	tpda_aoss: tpda@10b08000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb969>;

		reg = <0x10b08000 0x1000>;
		reg-names = "tpda-base";

		coresight-name = "coresight-tpda-aoss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		qcom,tpda-atid = <71>;

		qcom,dsb-elem-size = <4 32>;
		qcom,cmb-elem-size = <0 64>,
							<1 64>,
							<2 64>,
							<3 64>;


		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@1 {
				reg = <1>;
				tpda_aoss_in_tpdm_swao_prio1: endpoint {
					remote-endpoint =
					<&tpdm_swao_prio1_out_tpda_aoss>;
				};
			};

			port@0 {
				reg = <0>;
				tpda_aoss_in_tpdm_swao_prio0: endpoint {
					remote-endpoint =
					<&tpdm_swao_prio0_out_tpda_aoss>;
				};
			};

			port@3 {
				reg = <3>;
				tpda_aoss_in_tpdm_swao_prio3: endpoint {
					remote-endpoint =
					<&tpdm_swao_prio3_out_tpda_aoss>;
				};
			};

			port@2 {
				reg = <2>;
				tpda_aoss_in_tpdm_swao_prio2: endpoint {
					remote-endpoint =
					<&tpdm_swao_prio2_out_tpda_aoss>;
				};
			};

			port@4 {
				reg = <4>;
				tpda_aoss_in_tpdm_swao: endpoint {
					remote-endpoint =
					<&tpdm_swao_out_tpda_aoss>;
				};
			};

		};

		out-ports {

			port {
				tpda_aoss_out_funnel_aoss: endpoint {
					remote-endpoint =
					<&funnel_aoss_in_tpda_aoss>;
				};
			};

		};
	};

	funnel_aoss: funnel@10b04000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb908>;

		reg = <0x10b04000 0x1000>;
		reg-names = "funnel-base";

		coresight-name = "coresight-funnel-aoss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {

			#address-cells = <1>;
			#size-cells = <0>;

			port@5 {
				reg = <5>;
				funnel_aoss_in_funnel_lpass_lpi: endpoint {
					remote-endpoint =
					<&funnel_lpass_lpi_out_funnel_aoss>;
				};
			};

			port@7 {
				reg = <7>;
				funnel_aoss_in_funnel_merge: endpoint {
					remote-endpoint =
					<&funnel_merge_out_funnel_aoss>;
				};
			};

			port@6 {
				reg = <6>;
				funnel_aoss_in_tpda_aoss: endpoint {
					remote-endpoint =
					<&tpda_aoss_out_funnel_aoss>;
				};
			};

		};

		out-ports {

			port {
				funnel_aoss_out_tmc_etf: endpoint {
					remote-endpoint =
					<&tmc_etf_in_funnel_aoss>;
				};
			};

		};
	};

	dummy_eud: dummy_sink {
		compatible = "qcom,coresight-dummy";

		coresight-name = "coresight-eud";

		qcom,dummy-sink;
		in-ports {
			port {
				eud_in_replicator_swao: endpoint {
					remote-endpoint =
						<&replicator_swao_out_eud>;
				};
			};
		};
	};

	tmc_etf: tmc@10b05000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb961>;
		reg = <0x10b05000 0x1000>;
		reg-names = "tmc-base";

		coresight-name = "coresight-tmc-etf";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				tmc_etf_in_funnel_aoss: endpoint {
					remote-endpoint =
					<&funnel_aoss_out_tmc_etf>;
				};
			};
		};

		out-ports {
			port {
				tmc_etf_out_replicator_swao: endpoint {
					remote-endpoint =
					<&replicator_swao_in_tmc_etf>;
				};
			};
		};
	};

	replicator_swao: replicator@10b06000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb909>;
		reg = <0x10b06000 0x1000>;
		reg-names = "replicator-base";

		coresight-name = "coresight-replicator-swao";

		//qcom,replicator-loses-context;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				replicator_swao_in_tmc_etf: endpoint {
					remote-endpoint =
					<&tmc_etf_out_replicator_swao>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				replicator_swao_out_replicator_qdss: endpoint {
					remote-endpoint =
					<&replicator_qdss_in_replicator_swao>;
				};
			};

			port@1 {
				reg = <1>;
				replicator_swao_out_eud: endpoint {
					remote-endpoint =
					  <&eud_in_replicator_swao>;
				};
			};
		};
	};

	replicator_qdss: replicator@10046000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb909>;
		reg = <0x10046000 0x1000>;
		reg-names = "replicator-base";

		coresight-name = "coresight-replicator-qdss";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				replicator_qdss_in_replicator_swao: endpoint {
					remote-endpoint =
					<&replicator_swao_out_replicator_qdss>;
				};
			};
		};

		out-ports {

			port@0 {
				replicator_qdss_out_replicator_etr: endpoint {
					remote-endpoint =
					<&replicator_etr_in_replicator_qdss>;
				};
			};
		};
	};

	replicator_etr: replicator@1004e000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb909>;
		reg = <0x1004e000 0x1000>;
		reg-names = "replicator-base";

		coresight-name = "coresight-replicator-etr";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				replicator_etr_in_replicator_qdss: endpoint {
					remote-endpoint =
					<&replicator_qdss_out_replicator_etr>;
				};
			};
		};

		out-ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				replicator_etr_out_tmc_etr: endpoint {
					remote-endpoint =
					<&tmc_etr_in_replicator_etr>;
				};
			};

			port@1 {
				reg = <1>;
				replicator_etr_out_tmc_etr1: endpoint {
					remote-endpoint =
					<&tmc_etr1_in_replicator_etr>;
				};
			};
		};
	};

	tmc_etr: tmc@10048000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb961>;
		reg = <0x10048000 0x1000>,
			<0x10064000 0x16000>;
		reg-names = "tmc-base", "bam-base";

		qcom,iommu-dma = "bypass";
		iommus = <&apps_smmu 0x00c0 0>,
			<&apps_smmu 0x00a0 0>;

		qcom,iommu-dma-addr-pool = <0x0 0xffc00000>;

		qcom,sw-usb;
		dma-coherent;
		coresight-name = "coresight-tmc-etr";

		coresight-csr = <&csr>;
		csr-atid-offset = <0xf8>;
		csr-irqctrl-offset = <0x6c>;
		byte-cntr-name = "byte-cntr";
		byte-cntr-class-name = "coresight-tmc-etr-stream";

		interrupts = <GIC_SPI 270 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "byte-cntr-irq";

		arm,scatter-gather;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				tmc_etr_in_replicator_etr: endpoint {
					remote-endpoint =
					<&replicator_etr_out_tmc_etr>;
				};
			};
		};
	};

	tmc_etr1: tmc@1004f000 {
		compatible = "arm,primecell";
		arm,primecell-periphid = <0x000bb961>;
		reg = <0x1004f000 0x1000>;
		reg-names = "tmc-base";

		coresight-name = "coresight-tmc-etr1";

		iommus = <&apps_smmu 0x00e0 0>;
		qcom,iommu-dma-addr-pool = <0x0 0xffc00000>;
		dma-coherent;

		coresight-csr = <&csr>;
		csr-atid-offset = <0x108>;
		csr-irqctrl-offset = <0x70>;
		byte-cntr-name = "byte-cntr1";
		byte-cntr-class-name = "coresight-tmc-etr1-stream";

		interrupts = <GIC_SPI 269 IRQ_TYPE_EDGE_RISING>;
		interrupt-names = "byte-cntr-irq";

		arm,scatter-gather;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";

		in-ports {
			port {
				tmc_etr1_in_replicator_etr: endpoint {
					remote-endpoint =
					<&replicator_etr_out_tmc_etr1>;
				};
			};
		};
	};

	qc_cti: cti@10010000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10010000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-qc_cti";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	iris_dl_cti: cti@10831000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10831000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-iris_dl_cti";
		status = "disabled";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	lpass_cti: cti@10845000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10845000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-lpass_cti";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	gpu_cti: cti@10901000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10901000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-gpu";
		status = "disabled";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	apss_cti: cti@12862000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x12862000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-apss_dl_cti";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	apss_cti0: cti@128e0000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x128e0000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-apss_cti0";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	apss_cti1: cti@128f0000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x128f0000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-apss_cti1";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	apss_cti2: cti@12900000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x12900000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-apss_cti2";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	cortex_m3: cti@10b13000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10b13000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-cortex_m3";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	cti0: cti@10c2a000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10c2a000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-cti0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	ddr_ch01_dl_cti_0: cti@10d21000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10d21000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-ddr_ch01_dl_cti_0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	ddr_dl_0_cti_0: cti@10d02000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10d02000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-ddr_dl_0_cti_0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	ddr_dl_1_cti_0: cti@10d0c000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10d0c000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-ddr_dl_1_cti_0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	gpu_cortex_m3: cti@10962000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10962000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-gpu_cortex_m3";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	lpass_dl_cti: cti@10845000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10845000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-lpass_dl_cti";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	lpass_lpi_cti: cti@10b41000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10b41000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-lpass_lpi_cti";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	lpass_q6_cti: cti@10b4b000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10b4b000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-lpass_q6_cti";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	mdss_dl_cti: cti@10c61000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10c61000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-mdss_dl_cti";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		status= "disabled";
	};

	riscv_cti: cti@1282b000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x1282b000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-riscv_cti";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	swao_cti: cti@10b00000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10b00000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-swao_cti";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
		qcom,extended_cti;
	};

	tmess_cpu: cti@10cd1000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10cd1000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-tmess_cpu";

		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	tmess_cti_0: cti@10cc2000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10cc2000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-tmess_cti_0";

		qcom,extended_cti;
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	tmess_cti_1: cti@10cc3000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10cc3000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-tmess_cti_1";

		qcom,extended_cti;
		status = "disabled";
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	turing_dl_cti_0: cti@10982000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10982000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-turing_dl_cti_0";

		qcom,extended_cti;
		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	turing_q6_cti: cti@1098b000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x1098b000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-turing_q6_cti";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};

	wlan_q6_cti: cti@10C7B000 {
		compatible = "arm,coresight-cti", "arm,primecell";
		reg = <0x10C7B000 0x1000>;

		arm,primecell-periphid = <0x000bb922>;
		coresight-name = "coresight-cti-wlan_q6_cti";

		clocks = <&aoss_qmp>;
		clock-names = "apb_pclk";
	};
};
